The Device Kit: Master Index

Table of Contents

# The Device Kit: Master Index

C

ClearInput() | BSerialPort
ClearOutput() | BSerialPort
Close() | BJoystick
Close() | BSerialPort
Constructor and Destructor | BJoystick
Constructor and Destructor | BSerialPort
CountAxes() | BJoystick
CountButtons() | BJoystick
CountDevices() | BJoystick
CountHats() | BJoystick
CountSticks() | BJoystick

D

DataBits() | BSerialPort
Data Members | BJoystick
DataRate() | BSerialPort
data_bits | BSerialPort
data_rate | BSerialPort
The Device Kit | The Device Kit
The Device Kit | The Device Kit

E

EnableCalibration() | BJoystick
EnterEnhancedMode() | BJoystick

F

FlowControl() | BSerialPort

G

GetAxisNameAt() | BJoystick
GetAxisValues() | BJoystick
GetButtonNameAt() | BJoystick
GetButtonValues() | BJoystick
GetControllerModule() | BJoystick
GetControllerName() | BJoystick
GetDeviceName() | BJoystick
GetHatNameAt() | BJoystick
GetHatValues() | BJoystick

H

B_HARDWARE_CONT | BSerialPort

I

IsCTS() | BSerialPort
IsCalibrationEnabled() | BJoystick
IsDCD() | BSerialPort
IsDSR() | BSerialPort
IsRI() | BSerialPort

J

BJoystick | BJoystick
BJoystick() | BJoystick
~BJoystick() | BJoystick

M

Member Functions | BJoystick
Member Functions | BSerialPort

O

Open() | BJoystick
Open() | BSerialPort

P

ParityMode() | BSerialPort
parity_mode | BSerialPort

R

Read() | BSerialPort

S

BSerialPort | BSerialPort
BSerialPort() | BSerialPort
~BSerialPort() | BSerialPort
SetBlocking() | BSerialPort
SetDTR() | BSerialPort
SetDataBits() | BSerialPort
SetDataRate() | BSerialPort
SetFlowControl() | BSerialPort
SetMaxLatency() | BJoystick
SetParityMode() | BSerialPort
SetRTS() | BSerialPort
SetStopBits() | BSerialPort
SetTimeout() | BSerialPort
B_SOFTWARE_CONT | BSerialPort
StopBits() | BSerialPort
stop_bits | BSerialPort

U

Update() | BJoystick

W

WaitForInput() | BSerialPort
Write() | BSerialPort

The Be Book,
...in lovely HTML...
for BeOS Release 5.

Copyright © 2000 Be, Inc. All rights reserved..