
# bebox -- an ansi style termcap entry without all the tc= fields which
# gnu termcap doesn't grok properly (we put this at the top of the file
# so the termcap library finds this faster).
ansi|beterm|ANSI BeOS Terminal:\
	:am:eo:mi:ms:xn:xo:\
	:Co#8:co#80:it#8:li#25:pa#64:\
	:&7=^Z:@7=\E[4~:AB=\E[4%p1%dm:AF=\E[3%p1%dm:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:F1=\E[21~:F2=\E[22~:\
	:IC=\E[%d@:\
	:K2=\E[G:Sb=\E[%+(m:Sf=\E[%+^^m:\
	:al=\E[L::bl=^G:cd=\E[J:ce=\E[K:\
	:ch=\E[%i%dG:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:\
	:cs=\E[%i%d;%dr:ct=\E[3g:cv=\E[%i%dd:dc=\E[P:dl=\E[M:\
	:do=^J:ei=\E[4l:ho=\E[H:ic=\E[@:im=\E[4h:k1=\E[11~:\
	:k2=\E[12~:k3=\E[13~:k4=\E[14~:k5=\E[15~:k6=\E[16~:\
	:k7=\E[17~:k8=\E[18~:k9=\E[19~:k;=\E[20~:\
	:kI=\E[2~:kN=\E[6~:kP=\E[5~:kb=^h:kd=\E[B:\
	:kh=\E[1~:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[0;10m:mh=\E[2m:mk=\E[8m:mr=\E[7m:\
	:nd=\E[C:nw=^M^J:op=\E[m:r1=\Ec:rc=\E8:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:u6=\E[%i%d;%dR:u7=\E[6n:u8=\E[?6c:u9=\E[c:ue=\E[24m:\
	:up=\E[A:us=\E[4m:vb=200\E[?5h\E[?5l:ve=\E[?25h:\
	:vi=\E[?25l:

####### TERMINAL TYPE DESCRIPTIONS SOURCE FILE
#
#	Version 9.8.1
#	termcap syntax
#
#	Eric S. Raymond		(current maintainer)
#	John Kunze, Berkeley
#	Craig Leres, Berkeley
#
# Please e-mail changes to terminfo@ccil.org.  The old termcap@berkeley.edu
# address is no longer valid.
#
# PURPOSE OF THIS FILE:
#
# This file describes the capabilities of various character-cell terminals,
# as needed by software such as screen-oriented editors.
#
# Pointers to related resources (including the ncurses distribution) may
# be found at <http://www.ccil.org/~esr/ncurses.html>.
#
# FILE FORMAT:
#
# The version you are looking at may be in any of three formats: master
# (terminfo with OT capabilities), stock terminfo, or termcap.  You can tell
# which by the format given in the header above.
#
# The master format is accepted and generated by the terminfo tools in the
# ncurses suite; it differs from stock (System V-compatible) terminfo only
# in that it admits a group of capabilities (prefixed `OT') equivalent to
# various obsolete termcap capabilities.  You can, thus, convert from master
# to stock terminfo simply by filtering with `sed "/OT[^,]*,/s///"'; but if
# you have ncurses `tic -I' is nicer.
#
# The termcap version is generated automatically from the master version
# using tic -C.  This filtering leaves in the OT capabilities under their
# original termcap names.  All translated entries fit within the
# 1023-byte string-table limit of archaic termcap libraries except where
# explicitly noted below.
#
# For details on these formats, see terminfo(5) in the ncurses distribution,
# and termcap(5) in the 4.4BSD Unix Programmer's Manual.  Be aware that 4.4BSD
# curses has been declared obsolete by the caretakers of the 4.4BSD sources
# as of June 1995; they are encouraging everyone to migrate to ncurses.
#
# Note: unlike some other distributed terminfo files (Novell Unix & SCO's),
# no entry in this file has embedded comments.  This is so source translation
# to termcap only has to carry over leading comments.  Also, no name field
# contains embedded whitespace (such whitespace confuses rdist).
#
# Further note: older versions of this file were often installed with an editor
# script (reorder) that moved the most common terminal types to the front of
# the file.  This should no longer be necessary, as the file is now ordered
# roughly by type frequency with ANSI/VT100 and other common types up front.
#
# CONTINUITY WITH HISTORICAL VERSIONS:
#
# The last /etc/termcap version maintained by John Kunze was 8.3, dated 8/5/94.
# Releases 9 and up are maintained by Eric Raymond as part of the ncurses
# project.
#
# This file contains all the capability information present in John Kunze's
# last version of the termcap master file, except as noted in the change 
# comments at end of file.  Some information about very ancient obsolete
# capabilities has been moved to comments.  Some all-numeric names of older
# terminals have been retired.
#
# The 9.1.0 version of this file was translated from a syntax-corrected copy of
# 8.3, then mechanically checked against 8.3 using Emacs Lisp code written for
# the purpose.  Unless the ncurses tic implementation and the Lisp code were
# making perfectly synchronized mistakes which I then failed to catch by
# eyeball, the translation was correct and perfectly information-preserving.
#
# Some information has been merged in from terminfo files distributed by
# USL and SCO (see COPYRIGHTS AND OTHER DELUSIONS below).  Much information
# comes from vendors who maintain official terminfos for their hardware
# (notably DEC and Wyse).
#
# A detailed change history is included at the end of this file.
#
# FILE ORGANIZATION:
#
# Comments in this file begin with # - they cannot appear in the middle
# of a terminfo/termcap entry.  Individual capabilities are commented out by
# placing a period between the colon and the capability name.
#
# Starting with version 9.0.0, the file is divided up into major sections
# (headed by lines beginning with "########") and minor sections (beginning
# with "####"); do
#
#	grep "^####" <file> | more
#
# to see a listing of section headings.  The intent of the divisions is
# (a) to make it easier to find things, and (b) to order the database so
# that important and frequently-encountered terminal types are near the
# front (so that you'll get reasonable search efficiency even if you don't
# use reorder).  Minor sections usually correspond to manufacturers or
# standard terminal classes.  Parenthesized words following manufacturer
# names are type prefixes or product line names used by that manufacturers.
#
# Finally, because this file is released in both terminfo and termcap formats,
# most references to termcap names in comments are bracketed with colons (the
# termcap separator) so they can be distinguished from terminfo capability
# names.
#
# HOW TO READ THE ENTRIES:
#
# The first name in an entry is the canonical name for the model or
# type, last entry is a verbose description.  Others are mnemonic synonyms for
# the terminal.
#
# Terminal names look like <manufacturer> <model> - <modes/options>
# The part to the left of the dash, if a dash is present, describes the
# particular hardware of the terminal.  The part to the right may be used
# for flags indicating special ROMs, extra memory, particular terminal modes,
# or user preferences.
#
# All names should be in lower case, for consistency in typing.
#
# The following are conventionally used suffixes:
#	mono	suppress color support
#	rv	Terminal in reverse video mode (black on white)
#	2p	Has two pages of memory.  Likewise 4p, 8p, etc.
#	w	Wide - in 132 column mode.
#	pp	Has a printer port which is used.
#	na	No arrow keys - termcap ignores arrow keys which are
#		actually there on the terminal, so the user can use
#		the arrow keys locally.
#	nam	No auto-margin - suppress am capability
#	mc	Magic-cookie.  Some terminals (notably older Wyses) can
#		only support one attribute without magic-cookie lossage.
#		Their base entry is usually paired with another that
#		uses magic cookies to support multiple attributes.
#	vb	Use visible bell (flash) rather than beep.
#
# To easily test a new terminal description, put it in $HOME/.termcap
# and programs will look there before looking in /etc/termcap.
# You can also setenv TERMPATH to a list of full pathnames (separated
# by spaces or colons) to be searched by tgetent() in the order listed.
# The TERMCAP environment variable is usually set to the termcap
# entry itself to avoid reading files when starting up a program.
#
# RELEASE 9 COMMENTS:
#
# To avoid search clashes, some older all-numeric names for terminals have
# been removed (i.e., "33" for the Model 33 Teletype, "2621" for the HP2621).
# All primary names of terminals now have alphanumeric prefixes.
#
# Comments marked "esr" are mostly results of applying the termcap-compiler
# code packaged with ncurses and contemplating the resulting error messages. 
# In many cases, these indicated obvious fixes to syntax garbled by the
# composers.  In a few cases, I was able to deduce corrected forms for garbled
# capabilities by looking at context.  All the information in the original
# entries is preserved in the comments.
#
# I changed :MT: to :km: (the 4.4BSD name) everywhere.  I commented out some
# capabilities (EP, dF, dT, dV, kn, ko, ma, ml, mu, xr, xx) that are no longer
# used by BSD curses.
#
# Entries derived from XENIX use a termcap-extension set that showed up in
# several entries, notably those for scoansi, ibmpcx, lisa, trs16, fos, and
# the altos terminals.  Its signature is the use of GS/GE as an as/ae pair.
# This set of extensions and their translations are described in the extended
# comment at the end of this file.
#
# There is a second, smaller set of extensions used by AT&T terminals and
# also described in the trailing comment.
#
# Besides these and the terminals mentioned above, only the psterm variants,
# zen50, wsiris and minitel had unknown capabilities that weren't obviously
# garbled.
#
# INTERPRETATION OF USER CAPABILITIES
#
# The System V Release 4 and XPG4 terminfo format defines ten string
# capabilities for use by applications, u0...u9.   In this file, we use
# certain of these capabilities to describe functions which are not covered
# by terminfo.  The mapping is as follows:
#
#	u9	terminal enquire string (equivalent to ANSI DA)
#	u8	terminal answerback description
#	u7	cursor position request (equivalent to VT100 DSR 6)
#	u6	cursor position report (equivalent to ANSI CPR)
#
# The terminal enquire string u9 should elicit an answerback response
# from the terminal.  Common values for u9 will be ^E (on older ASCII
# terminals) or \E[c (on newer VT100/ANSI-compatible terminals).
#
# The cursor position request (u7) string should elicit a cursor position
# report.  A typical value (for ANSI/VT100 terminals) is \E[6n.
#
# The terminal answerback description (u8) must consist of an expected
# answerback string.  The string may contain the following scanf(3)-like
# escapes:
#
#	%c	Accept any character
#	%[...]	Accept any number of characters in the given set
#
# The cursor position report (u6) string must contain two scanf(3)-style 
# %d format elements.  The first of these must correspond to the Y coordinate
# and the second to the %d.  The typical CPR value is \E[%d;%dR (on VT100/
# ANSI-compatible terminals).
#
# These capabilities are used by tac(1m), the terminfo action checker soon
# to be distributed with ncurses.
# 
# REQUEST FOR CONTACT INFORMATION AND HISTORICAL MATERIAL:
#
# As the ANSI standard and variants take firmer hold, and as character-cell
# terminals are increasingly replaced by X displays, much of this file
# is becoming a historical document (this is part of the reason for the
# new organization, which puts ANSI types, xterm, and vt100 up front in
# confidence that this will catch 95% of new hardware).
#
# For the terminal types still alive, I'd like to have manufacturer's
# contact data (Internet address and/or snail-mail + phone).
#
# I'm also interested in enriching the comments so that the latter portions of
# the file do in fact become a potted history of VDT technology as seen by
# UNIX hackers.  Ideally, I'd like the headers for each manufacturer to
# include its live/dead/out-of-the-business status, and for as many
# terminal types as possible to be tagged with information like years
# of heaviest use, popularity, and interesting features.
#
# I'm especially interested in identifying the obscure entries listed under
# `Manufacturer unknown' and `Utter unknowns', before the tribal wisdom 
# about them gets lost.
#
# If you have been around long enough to contribute, please read the file
# with this in mind and send me your annotations.
#
# COPYRIGHTS AND OTHER DELUSIONS
#
# The BSD ancestor of this file had a standard Regents of the University of
# California copyright with dates from 1980 to 1993.
#
# Some information has been merged in from a terminfo file SCO distributes.
# It has an obnoxious boilerplate copyright which I'm ignoring because they 
# took so much of the content from the ancestral BSD versions of this file
# and didn't attribute it, thereby violating the BSD Regents' copyright.
#
# Not that anyone should care.  However many valid functions copyrights may
# serve, putting one on a termcap/terminfo file with hundreds of anonymous
# contributors makes about as much sense as copyrighting a wall-full of
# graffiti -- it's legally dubious, ethically bogus, and patently ridiculous.
#
# This file deliberately has no copyright.  It belongs to no one and everyone.
# If you claim you own it, you will merely succeed in looking like a fool. 
# Use it as you like.  Use it at your own risk.  Copy and redistribute freely.
# There are no guarantees anywhere.  Svaha!

######## STANDARD AND SPECIAL TYPES
#
# This section describes terminal classes and maker brands that are still
# quite common.
#

#### Specials
#
# Special "terminals".  These are used to label tty lines when you don't
# know what kind of terminal is on it.  The characteristics of an unknown
# terminal are the lowest common denominator - they look about like a ti 700.
# The last one, "other", is like unknown but it allows an escape from software
# that insists that a "real" unknown terminal is merely so far unspecified.
#

dumb:\
	:am:\
	:co#80:\
	:bl=^G:cr=^M:do=^J:sf=^J:
unknown:\
	:gn:\
	:tc=dumb:
other|none of the above, but not exactly unknown:\
	:am:gn:\
	:co#80:\
	:cl=^M^J:do=^J:ho=^M:

arpanet|bussiplexer|dialup|ethernet|network|net|patch|plugboard|switch|network switch or dialup:\
	:tc=unknown:
lpr|printer|print|printing|line printer:\
	:hc:os:\
	:co#132:li#66:\
	:bl=^G:cr=^M:do=^J:ff=^L:le=^H:sf=^J:

#### ANSI terminals and terminal emulators
#
# See near the end of this file for details on ANSI conformance.
# Don't mess with these entries!  Lots of other entries depend on them!
#
# This section lists entries in a least-capable to most-capable order.
# if you're in doubt about what `ANSI' matches yours, try them in that
# order and back off from the first that breaks.

# (ansi: changed ":pt:" to ":it#8:" -- esr)
ansi-mini|any ansi terminal with pessimistic assumptions:\
	:am:bs:\
	:co#80:it#8:li#24:\
	:ce=\E[K:cl=\E[;H\E[2J:cm=\E[%i%d;%dH:do=\E[B:\
	:ho=\E[H:le=\E[D:nd=\E[C:up=\E[A:

# Color controls corresponding to the ANSI.SYS de-facto standard
# (This is not a standalone entry)
ansi-pc-color:\
	:Co#8:NC#3:pa#64:\
	:AB=\E[4%p1%dm:AF=\E[3%p1%dm:\
	:..Sb=\E[4%?%p1%{1}%=%t4%e%p1%{3}%=%t6%e%p1%{4}%=%t1%e%p1%{6}%=%t3%e%p1%d%;m:\
	:..Sf=\E[3%?%p1%{1}%=%t4%e%p1%{3}%=%t6%e%p1%{4}%=%t1%e%p1%{6}%=%t3%e%p1%d%;m:\
	:op=\E[37;40m:

# Procomm and some other ANSI emulations don't recognize all of the ANSI-
# standard capabilities.  This entry deletes cuu, cuf, cud, cub, and vpa/hpa
# capabilities, forcing curses to use repetitions of cuu1, cuf1, cud1 and cub1.
# Also deleted ich and ich1, as QModem up to 5.03 doesn't recognize these.
# Finally, we delete rep and ri, which seem to confuse many emulators.
# On the other hand, we can count on these programs doing rmacs/smacs/sgr.
# From: Eric S. Raymond <esr@snark.thyrsus.com> July 25 1995
pcansi-mono|ibm-pc terminal programs claiming to be ansi (mono mode):\
	:am:bs:mi:ms:pt:\
	:co#80:it#8:li#24:\
	:ae=\E[10m:al=\E[L:as=\E[12m:bl=^G:bt=\E[Z:cd=\E[J:\
	:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:ct=\E[2g:\
	:dc=\E[P:dl=\E[M:do=\E[B:ho=\E[H:kb=^H:kd=\E[B:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:le=\E[D:mb=\E[5m:\
	:md=\E[1m:me=\E[0m:mk=\E[9m:mr=\E[7m:nd=\E[C:\
	:..sa=\E[0;10%?%p1%t;7%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p6%t;1%;%?%p7%t;8%;%?%p8%t;11%;%?%p9%t;12%;m:\
	:se=\E[m:sf=^J:so=\E[7m:st=\EH:ta=^I:ue=\E[m:up=\E[A:\
	:us=\E[4m:
pcansi-mono25|ansi25|ibm-pc terminal programs with 25 lines (mono mode):\
	:li#25:\
	:tc=pcansi-mono:
pcansi-mono33|ansi33|ibm-pc terminal programs with 33 lines (mono mode):\
	:li#33:\
	:tc=pcansi-mono:
pcansi-mono43|ansi43|ibm-pc terminal programs with 43 lines (mono mode):\
	:li#43:\
	:tc=pcansi-mono:
# The color versions.  All PC emulators do color...
pcansi|ibm-pc terminal programs claiming to be ansi:\
	:tc=ansi-pc-color:tc=pcansi-mono:
pcansi-25|ansi25|ibm-pc terminal programs with 25 lines:\
	:li#25:\
	:tc=pcansi:
pcansi-33|ansi33|ibm-pc terminal programs with 33 lines:\
	:li#33:\
	:tc=pcansi:
pcansi-43|ansi43|ibm-pc terminal programs with 43 lines:\
	:li#43:\
	:tc=pcansi:

# From: Eric S. Raymond <esr@snark.thyrsus.com> Feb 3 1995
# ansi-mono -- full X.364 with ANSI.SYS-compatible attributes, no color.
# Function-key mappings aren't in X3.64 but these are pretty standard.
# If you want pound signs rather than dollars, replace `B' with `A'
# in the s?ds capabilities.
ansi-mono|ANSI X3.64-1979 terminal with ANSI.SYS compatible attributes:\
	:5i:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[W:\
	:F2=\E[X:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:SF=\E[%dS:\
	:SR=\E[%dT:UP=\E[%dA:cb=\E[1K:ch=\E[%dG:ct=\E[2g:\
	:cv=\E[%dd:ec=\E[%dX:ei=:im=:k1=\E[M:k2=\E[N:k3=\E[O:\
	:k4=\E[P:k5=\E[Q:k6=\E[R:k7=\E[S:k8=\E[T:k9=\E[U:\
	:k;=\E[V:kB=\E[Z:kI=\E[L:kb=^H:kd=\E[B:kl=\E[D:\
	:kr=\E[C:ku=\E[A:me=\E[0;10m:nw=\r\E[S:pf=\E[4i:\
	:po=\E[5i:..rp=%p1%c\E[%p2%{1}%-%db:s0=\E(B:s1=\E)B:\
	:s2=\E*B:s3=\E+B:\
	:..sa=\E[0;10%?%p1%t;7%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p6%t;1%;%?%p7%t;8%;%?%p8%t;11%;%?%p9%t;12%;m:\
	:ta=\E[I:tc=pcansi:

# ansi -- this terminfo expresses the largest subset of X3.64 that will fit in
# standard terminfo.  Assumes ANSI.SYS-compatible attributes and color
# From: Eric S. Raymond <esr@snark.thyrsus.com> Feb 12 1995
#ansi|ansi/pc-term compatible with color:\
#	:u6=\E[%d;%dR:u7=\E[6n:..u8=\E[?%[;0123456789]c:\
#	:u9=\E[c:tc=ansi-pc-color:tc=ansi-mono:

#
# ANSI.SYS entries
#
# Cannot use :pt:, it does not work (why?).  :ho: seems required (why?). [gts]
# Caution: 4.3 BSD tset does not pass li#25 to stty rows except during login?
# :cl: clears attributes and sets wrap at margin before clearing the screen.
# (ansi.sys: removed obsolete ":ma=^Hh^Jj^Kk^Ll^^H:" -- esr)
# From: greg small <gts@populi.berkeley.edu>
ansi.sys|ansisys|PC-DOS 3.1 ANSI.SYS:\
	:am:bs:ms:\
	:co#80:li#25:\
	:ae=\E[10:as=\E[12:ce=\E[K:cl=\E[m\E[7h\E[2J:\
	:cm=\E[%i%d;%dH:ho=\E[H:\
	:is=U1 PC-DOS 3.1 ANSI.SYS 9-23-86\n\E[m\E[7h:kd=^J:\
	:kh=^^:kl=^H:kr=^L:ku=^K:md=\E[1m:me=\E[0;10m:\
	:mr=\E[7m:nd=\E[C:se=\E[m:so=\E[1m:ue=\E[m:up=\E[A:\
	:us=\E[4m:
#
# Define IBM PC keypad keys for vi as per MS-Kermit while using ANSI.SYS.
# This should only be used when the terminal emulator cannot redefine the keys.
# Since redefining keys with ansi.sys also affects PC-DOS programs, the key
# definitions must be restored.  If the terminal emulator is quit while in vi
# or others using :ks:ke:, the keypad keys will not be defined as per PC-DOS.
# The PgUp and PgDn are prefixed with ESC so that tn3270 can be used on Unix
# (^U and ^D are already defined for tn3270).  The ESC is safe for vi but it
# does "beep".  ESC ESC i is used for Ins to avoid tn3270 ESC i for coltab.
# Left arrow is always BS, because PC-dos can tolerate this change.
# Caution: vi is limited to 256 string bytes, longer crashes or weirds out vi.
# Consequently the End keypad key could not be set (it is relatively safe and
# actually useful because it sends ^@ O, which beeps and opens a line above).
ansi.sysk|ansisysk|PC-DOS 3.1 ANSI.SYS with keypad redefined for vi:\
	:is=U2 PC-DOS 3.1 ANSI.SYS with keypad redefined for vi 9-29-86\n\E[;75;8p:\
	:ke=\E[;71;0;71p\E[;72;0;72p\E[;73;0;73p\E[;77;0;77p\E[;80;0;80p\E[;81;0;81p\E[;82;0;82p\E[;83;0;83p:\
	:ks=\E[;71;30p\E[;72;11p\E[;73;27;21p\E[;77;12p\E[;80;10p\E[;81;27;4p\E[;82;27;27;105p\E[;83;127p:tc=ansi.sys:
#
# Adds ins/del line/character, hence vi reverse scrolls/inserts/deletes nicer.
nansi.sys|nansisys|PC-DOS Public Domain NANSI.SYS:\
	:al=\E[1L:dc=\E[1P:dl=\E[1M:ei=:ic=\E[1@:im=:\
	:is=U3 PC-DOS Public Domain NANSI.SYS 9-23-86\n:tc=ansi.sys:
#
# See ansi.sysk and nansi.sys above.
nansi.sysk|nansisysk|PC-DOS Public Domain NANSI.SYS with keypad redefined for vi:\
	:al=\E[1L:dc=\E[1P:dl=\E[1M:ei=:ic=\E[1@:im=:\
	:is=U4 PC-DOS Public Domain NANSI.SYS with keypad redefined for vi 9-29-86\n\E[;75;8p:tc=ansi.sysk:

#### ANSI console types
#

# This entry is good for the 1.1.47 version of the Linux console driver.
#
# It assumes that you want A_PROTECT mapped to the alternate character set
# mode that permits IBM ROM characters to be displayed (this is the assumption
# used by ncurses version 1.9 and after, in order not to collide with the
# internationalization attribute values specified in the XSI Curses standard).
#
# We use \E11m for rmacs rather than \E12m so the acsc string can use the ROM
# graphics for control characters such as the diamond, up arrow and down-arrow.
# This trick could work with other Intel consoles like the att6386 and pc3.
#
# Note: there are numerous broken linux entries out there, which didn't screw
# up BSD termcap but hose ncurses's smarter cursor-movement optimization.
# One common pathology is an incorrect tab length of 4.  Also note that the 
# hpa=\E[%dG/vpa=\E[%dd capabilities seem not to be reliable.  To reproduce
# the bug, re-introduce them and run worm -T 200 212 from the ncurses
# test suite, save the trace, then worm -N -T 200 212.  Observe that the first
# run fails to properly delete some worm segments, then diff the trace files.
#
# From: Eric S. Raymond <esr@snark.thyrsus.com> 23 July 1995
linux|linux console:\
	:am:bs:eo:mi:ms:ut:xn:xo:\
	:Co#8:co#80:it#8:li#25:pa#64:\
	:&7=^Z:@7=\E[4~:AB=\E[4%p1%dm:AF=\E[3%p1%dm:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:F1=\E[23~:F2=\E[24~:\
	:F3=\E[25~:F4=\E[26~:F5=\E[28~:F6=\E[29~:F7=\E[31~:\
	:F8=\E[32~:F9=\E[33~:FA=\E[34~:IC=\E[%d@:K2=\E[G:\
	:S2=\E[11m:S3=\E[10m:Sb=\E[%+(m:Sf=\E[%+^^m:\
	:ac=`\004a\261f\370g\361h\260j\331k\277l\332m\300n\305o~q\304r\362s_t\303u\264v\301w\302x\263y\371z\372{\373|\374}\375~\376.\031-\030\054\021+^P0\333:\
	:ae=\E[10m:al=\E[L:as=\E[11m:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:ho=\E[H:\
	:ic=\E[@:im=\E[4h:k1=\E[[A:k2=\E[[B:k3=\E[[C:\
	:k4=\E[[D:k5=\E[[E:k6=\E[17~:k7=\E[18~:k8=\E[19~:\
	:k9=\E[20~:k;=\E[21~:kD=\E[3~:kI=\E[2~:kN=\E[6~:\
	:kP=\E[5~:kb=^H:kd=\E[B:kh=\E[1~:kl=\E[D:kr=\E[C:\
	:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[0;10m:\
	:mr=\E[7m:nd=\E[C:nw=^M^J:op=\E[37;40m:r1=\Ec:rc=\E8:\
	:..sa=\E[0;10%?%p1%t;7%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p6%t;1%;%?%p7%t;8%;%?%p8%t;11%;%?%p9%t;11%;m:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:u6=\E[%d;%dR:u7=\E[6n:u8=\E[?6c:u9=\E[c:ue=\E[24m:\
	:up=\E[A:us=\E[4m:vb=\E[?5h\E[?5l:ve=\E[?25h:\
	:vi=\E[?25l:
linux-mono|Linux console, no color:\
	:Co@:pa@:\
	:AB@:Sb@:Sf@:tc=linux:

# See the note on ICH/ICH1 VERSUS RMIR/SMIR near the end of file
linux-nic|linux with ich/ich1 suppressed for non-curses programs:\
	:IC@:ei=:ic@:im=:tc=linux:

# SCO console and SOS-Syscons console for 386bsd
# (scoansi: had unknown capabilities
#	:Gc=N:Gd=K:Gh=M:Gl=L:Gu=J:Gv=\072:\
#	:GC=E:GD=B:GH=D:GL=\64:GU=A:GV=\63:GR=C:RT=^J:
#	:G1=?:G2=Z:G3=@:G4=Y:G5=;:G6=I:G7=H:G8=<:\
#	:CW=\E[M:NU=\E[N:RF=\E[O:RC=\E[P:\
#	:WL=\E[S:WR=\E[T:CL=\E[U:CR=\E[V:\
# I renamed GS/GE/HM/EN/PU/PD and mapped ":pt:" to ":it#8:" -- esr)
scoansi|SCO Extended ANSI standard crt:\
	:am:bs:eo:pt:\
	:co#80:it#8:li#25:\
	:@7=\E[F:ae=\E[10m:al=\E[L:as=\E[12m:bt=\E[Z:cd=\E[J:\
	:ce=\E[K:cl=\E[2J\E[H:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:\
	:do=\E[B:ei=:ho=\E[H:ic=\E[@:im=:k1=\E[M:k2=\E[N:\
	:k3=\E[O:k4=\E[P:k5=\E[Q:k6=\E[R:k7=\E[S:k8=\E[T:\
	:k9=\E[U:k;=\E[V:kN=\E[G:kP=\E[I:kb=^H:kd=\E[B:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:mb=\E[5m:md=\E[1m:\
	:me=\E[m:nd=\E[C:se=\E[m:sf=\E[S:so=\E[7m:sr=\E[T:\
	:ue=\E[m:up=\E[A:us=\E[4m:


#
# FreeBSD console types
#
# for syscons
# common entry without semigraphics
cons25w|ansiw|ansi80x25-raw:\
	:al=\E[L:am:bs:NP:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:co#80:\
	:dc=\E[P:dl=\E[M:do=\E[B:bt=\E[Z:ho=\E[H:ic=\E[@:li#25:cb=\E[1K:\
	:ms:nd=\E[C:pt:rs=\E[x\E[m\Ec:so=\E[7m:se=\E[m:up=\E[A:\
	:pa#64:Co#8:Sf=\E[3%dm:Sb=\E[4%dm:op=\E[x:\
	:k1=\E[M:k2=\E[N:k3=\E[O:k4=\E[P:k5=\E[Q:k6=\E[R:k7=\E[S:k8=\E[T:\
	:k9=\E[U:k;=\E[V:F1=\E[W:F2=\E[X:K2=\E[E:nw=\E[E:ec=\E[%dX:\
	:kb=^H:kh=\E[H:ku=\E[A:kd=\E[B:kl=\E[D:kr=\E[C:le=^H:eo:sf=\E[S:sr=\E[T:\
	:kN=\E[G:kP=\E[I:@7=\E[F:kI=\E[L:kD=\177:kB=\E[Z:\
	:IC=\E[%d@:DC=\E[%dP:SF=\E[%dS:SR=\E[%dT:AL=\E[%dL:DL=\E[%dM:\
	:DO=\E[%dB:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:cv=\E[%i%dd:ch=\E[%i%d`:bw:\
	:mb=\E[5m:md=\E[1m:mh=\E[30;1m:mr=\E[7m:me=\E[m:bl=^G:ut:it#8:km:
cons25|ansis|ansi80x25:\
	:ac=l\332m\300k\277j\331u\264t\303v\301w\302q\304x\263n\305`^Da\260f\370g\361~\371.^Y-^Xh\261I^U0\333y\363z\362:\
	:tc=cons25w:
cons25-m|ansis-mono|ansi80x25-mono:\
	:pa@:Co@:Sf@:Sb@:op@:us=\E[4m:ue=\E[m:md@:mh@:tc=cons25:
cons30|ansi80x30:\
	:li#30:tc=cons25:
cons30-m|ansi80x30-mono:\
	:li#30:tc=cons25-m:
cons43|ansi80x43:\
	:li#43:tc=cons25:
cons43-m|ansi80x43-mono:\
	:li#43:tc=cons25-m:
cons50|ansil|ansi80x50:\
	:li#50:tc=cons25:
cons50-m|ansil-mono|ansi80x50-mono:\
	:li#50:tc=cons25-m:
cons60|ansi80x60:\
	:li#60:tc=cons25:
cons60-m|ansi80x60-mono:\
	:li#60:tc=cons25-m:
# Syscons console with koi8-r russian code table.
cons25r|pc3r|ibmpc3r|cons25-koi8-r:\
	:ac=q\200x\201m\204v\211j\205t\206n\212u\207l\202w\210k\203y\230z\231f\234~\225a\220h\221`^D.^Y-^XI^U0\215:\
	:kD=\E[K:tc=cons25w:
cons25r-m|pc3r-m|ibmpc3r-mono|cons25-koi8-r-mono:\
	:pa@:Co@:Sf@:Sb@:op@:us=\E[4m:ue=\E[m:md@:mh@:tc=cons25r:
cons30r|cons30-koi8-r:\
	:li#30:tc=cons25r:
cons30r-m|cons30-koi8-r-mono:\
	:li#30:tc=cons25r-m:
cons43r|cons43-koi8-r:\
	:li#43:tc=cons25r:
cons43r-m|cons43-koi8-r-mono:\
	:li#43:tc=cons25r-m:
cons50r|cons50-koi8-r:\
	:li#50:tc=cons25r:
cons50r-m|cons50-koi8-r-mono:\
	:li#50:tc=cons25r-m:
cons60r|cons60-koi8-r:\
	:li#60:tc=cons25r:
cons60r-m|cons60-koi8-r-mono:\
	:li#60:tc=cons25r-m:
# 80x25 ISO 8859-1 FreeBSD console
cons25l1|cons25-iso8859-1:\
	:ac=l\215m\216k\214j\213u\226t\225v\227w\230q\222x\231n\217o\220s\224p\221r\223`\201a\202f\207g\210~\237.^Y-^X+\253,\273I\247y\232z\233:\
	:tc=cons25w:
cons25l1-m|cons25-iso8859-1-mono:\
	:pa@:Co@:Sf@:Sb@:op@:us=\E[4m:ue=\E[m:md@:mh@:tc=cons25l1:
cons30l1|cons30-iso8859-1:\
	:li#30:tc=cons25l1:
cons30l1-m|cons30-iso8859-1-mono:\
	:li#30:tc=cons25l1-m:
cons43l1|cons43-iso8859-1:\
	:li#43:tc=cons25l1:
cons43l1-m|cons43-iso8859-1-mono:\
	:li#43:tc=cons25l1-m:
cons50l1|cons50-iso8859-1:\
	:li#50:tc=cons25l1:
cons50l1-m|cons50-iso8859-1-mono:\
	:li#50:tc=cons25l1-m:
cons60l1|cons60-iso8859-1:\
	:li#60:tc=cons25l1:
cons60l1-m|cons60-iso8859-1-mono:\
	:li#60:tc=cons25l1-m:

# From: Eric Raymond <esr@snark.thyrsus.com> Wed Jan 18 17:14:34 EST 1995
att6386|AT386|at386|386AT|386at|AT&T WGS 6386 console:\
	:am:bw:eo:xo:\
	:co#80:it#8:li#25:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\EOZ:\
	:F2=\EOA:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:SF=\E[%dS:\
	:SR=\E[%dT:UP=\E[%dA:\
	:ac=``a1fxgqh0jYk?lZm@nEooppqDrrsstCu4vAwBx3yyzz{{||}}~~:\
	:ae=\E[10m:al=\E[1L:as=\E[12m:bl=^G:bt=\E[Z:cd=\E[J:\
	:ce=\E[K:ch=\E[%i%dG:cl=\E[2J\E[H:cm=\E[%i%d;%dH:\
	:cr=^M:ct=\E[2g:cv=\E[%dd:dc=\E[P:dl=\E[1M:do=\E[B:\
	:ec=\E[%dX:ei=:ho=\E[H:ic=\E[1@:im=:is=\E[0;10;39m:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\EOT:k6=\EOU:\
	:k7=\EOV:k8=\EOW:k9=\EOX:k;=\EOY:kD=\E[P:kI=\E[@:\
	:kM=\E0:kN=\E[U:kP=\E[V:kb=^H:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=\E[D:mb=\E[5m:md=\E[1m:\
	:me=\E[0;10m:mk=\E[9m:mr=\E[7m:nd=\E[C:nw=\r\E[S:\
	:..sa=\E[10m\E[0%?%p1%p3%|%t;7%;%?%p2%t;4%;%?%p4%t;5%;%?%p6%t;1%;%?%p9%t;12%e;10%;%?%p7%t;9%;m:\
	:se=\E[m:sf=\E[S:so=\E[7m:sr=\E[T:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:vb=^G:tc=ansi-pc-color:
# (pc6300plus: ":KM=/usr/lib/ua/kmap.s5:"; renamed BO/EE/CI/CV -- esr)
pc6300plus|6300plus:\
	:am:bs:\
	:co#80:li#24:\
	:al=\E[1L:bl=^G:cd=\E[0J:ce=\E[0K:cl=\E[2J\E[H:\
	:cm=\E[%i%2;%2H:cr=^M:ct=\E[3g:dc=\E[1P:dl=\E[1M:\
	:do=\E[B:ei=:ho=\E[H:ic=\E[1@:im=:k1=\EOc:k2=\EOd:\
	:k3=\EOe:k4=\EOf:k5=\EOg:k6=\EOh:k7=\EOi:k8=\EOj:\
	:k9=\EOk:k;=\EOu:kb=^H:kd=\E[B:kl=\E[D:kr=\E[C:\
	:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[m:mh=\E[2m:\
	:mk=\E[9m:mr=\E[7m:nd=\E[C:nw=^M^J:se=\E[m:sf=^J:\
	:so=\E[7m:st=\EH:ue=\E[m:up=\E[A:us=\E[4m:ve=\E[=1C:\
	:vi=\E[=C:

#
#	Terminfo entry for the AT&T Unix PC 7300
#	from escape(7) in Unix PC 7300 Manual.
#	Somewhat similar to a vt100-am (but different enough
#	to redo this from scratch.)
#
#	/***************************************************************
#	*
#	*           FONT LOADING PROGRAM FOR THE UNIX PC
#	*
#	*     This routine loads a font defined in the file ALTFONT
#	*     into font memory slot #1.  Once the font has been loaded,
#	*     it can be used as an alternative character set.
#	*
#	*     The call to ioctl with the argument WIOCLFONT is the key 
#	*     to this routine.  For more information, see window(7) in 
#	*     the PC 7300 documentation.
#	***************************************************************/
#	#include <string.h>		/* needed for strcpy call */
#	#include <sys/window.h>         /* needed for ioctl call */
#	#define FNSIZE	60		/* font name size */
#	#define ALTFONT  "/usr/lib/wfont/special.8.ft"  /* font file */
#	/*
#	*     The file /usr/lib/wfont/special.8.ft comes with the
#	*     standard PC software.  It defines a graphics character set
#	*     similar to that of the Teletype 5425 terminal.  To view
#	*     this or other fonts in /usr/lib/wfont, use the command
#	*     cfont <filename>.  For further information on fonts see
#	*     cfont(1) in the PC 7300 documentation.
#	*/
#	
#	struct altfdata 	/* structure for alt font data */
#	{
#	short	altf_slot;		/* memory slot number */
#	char	altf_name[FNSIZE];	/* font name (file name) */
#	};
#	ldfont()
#	{
#		int wd;		/* window in which altfont will be */
#		struct altfdata altf;
#		altf.altf_slot=1;
#		strcpy(altf.altf_name,ALTFONT);
#		for (wd =1; wd < 12; wd++) {
#		     ioctl(wd, WIOCLFONT,&altf);
#	        }
#	}
#
att7300|unixpc|pc7300|3b1|s4|AT&T UNIX PC Model 7300:\
	:am:xn:xo:\
	:co#80:it#8:li#24:\
	:!1=\ESV:!3=\EUD:#1=\EHL:#2=\EHM:#3=\ENJ:#4=\EBW:\
	:%0=\Ero:%1=\Ehl:%2=\Emk:%4=\Emv:%5=\Enx:%6=\Eop:\
	:%7=\Eot:%8=\Epv:%9=\Epr:%b=\EMV:%c=\ENX:%d=\EOT:\
	:%e=\EPV:%g=\ERO:%h=\ERP:%i=\EFW:&0=\ECN:&1=\Ere:\
	:&2=\Erf:&3=\Erp:&4=\Ers:&6=\Esv:&8=\Eud:&9=\EBG:\
	:*0=\EFI:*2=\ECP:*3=\ECR:*4=\EDC:*5=\EDL:*6=\Esl:\
	:*7=\EEN:*8=\ECI:@0=\Efi:@1=\Ebg:@2=\Ecn:@3=\Ecl:\
	:@4=\Ecm:@5=\Ecp:@6=\Ecr:@7=\Een:@9=\Eex:AL=\E[%dL:\
	:DL=\E[%dM:DO=\E[%dB:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ae=\E[10m:al=\E[L:as=\E[11m:bl=^G:bt=\E^I:cd=\E[0J:\
	:ce=\E[0K:cl=\E[2J\E[H:cm=\E[%i%d;%dH:cr=^M:dl=\E[M:\
	:do=\E[B:ho=\E[H:i1=^O:k1=\EOP:k2=\EOQ:k3=\EOR:\
	:k4=\EOS:k5=\E5:k6=\E6:k7=\E7:k8=\E8:kB=\E^I:kC=\Ece:\
	:kD=\Edc:kE=\Eci:kF=\Erd:kI=\Eim:kN=\Epg:kP=\EPG:\
	:kR=\Eru:kS=\Ece:kb=^H:kd=\E[B:kh=\Ehm:kl=\E[D:\
	:kr=\E[C:ku=\E[A:md=\E[7m:me=\E[0;10m:mh=\E[2m:\
	:mr=\E[7m:nd=\E[C:nw=\EE:se=\E[0m:sf=^J:so=\E[7m:\
	:sr=\EM:ue=\E[0m:up=\E[A:us=\E[4m:

# From: <davis@unidata.ucar.edu>
iris-ansi|iris-ansi-net|IRIS emulating ANSI terminal:\
	:am:\
	:co#80:it#8:li#40:\
	:!2=\E[218q:#2=\E[143q:#4=\E[158q:%9=\E[209q:\
	:%f=\E[210q:%i=\E[167q:&7=\E[217q:*4=\E[P:*7=\E[147q:\
	:@7=\E[146q:@8=^M:AL=\E[%dL:DL=\E[%dM:DO=\E[%dB:\
	:F1=\EOR:F2=\EOS:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:al=\E[L:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:ct=\E[3g:dl=\E[M:do=^J:ho=\E[H:\
	:is=\E[?1l\E>\E[?7h\E[100g\E[0m\E7\E[r\E8:k1=\E[001q:\
	:k2=\E[002q:k3=\E[003q:k4=\E[004q:k5=\E[005q:\
	:k6=\E[006q:k7=\E[007q:k8=\E[008q:k9=\EOP:k;=\EOQ:\
	:kB=\E[Z:kD=\177:kI=\E[139q:kM=\E[146q:kN=\E[154q:\
	:kP=\E[150q:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:\
	:ku=\E[A:le=\E[D:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:\
	:nw=\EE:pk=\EP101;%d.y%s\E\\:rc=\E8:sc=\E7:se=\E[m:\
	:sf=\ED:so=\E[1;7m:sr=\EM:st=\EH:ta=^I:ue=\E[m:\
	:up=\E[A:us=\E[4m:ve=\E[9/y\E[12/y\E[=6l:\
	:vs=\E[10/y\E[=1h\E[=2l\E[=6h:

# From: Alex R.N. Wetmore <aw2t@andrew.cmu.edu>
oldpc3|oibmpc3|IBM PC 386BSD Console:\
	:am:bs:bw:eo:\
	:co#80:li#25:\
	:ac=l\332q\304k\277x\263j\331m\300w\302u\264v\301t\303n\305:\
	:cd=\E[J:ce=\E[K:cl=\Ec:cm=\E[%i%2;%2H:do=\E[B:\
	:ho=\E[;H:kd=\E[B:kh=\E[Y:kl=\E[D:kr=\E[C:ku=\E[A:\
	:md=\E[7m:me=\E[0m\E[1;0x\E[2;7x:nd=\E[C:\
	:se=\E[1;0x\E[2;7x:sf=\E[S:so=\E[1;7x\E[2;0x:sr=\E[T:\
	:ue=\E[1;0x\E[2;7x:up=\E[A:us=\E[1;7x\E[2;0x:

# BSD/OS console emulator
# The emulator supports many of the additional console features
# listed in the iBSC2 (e.g. color and character-set selection).
# The console will also work with fewer lines after doing
# "stty rows NN", e.g. to use 24 lines.
# (This is the entry BSDI ships)
pc3|ibmpc3|IBM PC BSD/OS Console:\
	:am:bw:eo:km:\
	:co#80:it#8:li#25:\
	:AL=\E[%dL:DL=\E[%dM:DO=\E[%dB:LE=\E[%dD:RI=\E[%dC:\
	:UP=\E[%dA:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\Ec:\
	:cm=\E[%i%d;%dH:cr=^M:dl=\E[M:do=^J:ho=\E[H:kH=\E[F:\
	:kI=\E[L:kN=\E[G:kP=\E[I:kb=^H:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[0m:mh=\E[=8F:mr=\E[7m:nd=\E[C:nw=^M^J:\
	:rc=\E[=u:sc=\E[=s:se=\E[0m:sf=^J:so=\E[7m:ta=^I:\
	:up=\E[A:
pc3-bold|ibmpc3|IBM PC BSD/OS Console with bold instead of underline:\
	:ue=\E[0m:us=\E[1m:tc=pc3:

# The following is a version of the ibm-pc entry distributed with PC/IX,
# (Interactive Systems' System 3 for the Big Blue), modified by Richard
# McIntosh at UCB/CSM.  The :pt: and :uc: have been removed from the original,
# (the former is untrue, and the latter failed under UCB/man); standout and
# underline modes have been added.  Note: this entry describes the "native"
# capabilities of the PC monochrome display, without ANY emulation; most
# communications packages (but NOT PC/IX connect) do some kind of emulation.
pcix|PC/IX console:\
	:am:bs:bw:eo:\
	:co#80:li#24:\
	:cd=\E[J:ce=\E[K:cl=\Ec:cm=\E[%i%2;%2H:do=\E[B:\
	:ho=\E[;H:nd=\E[C:se=\E[0m:so=\E[7m:ue=\E[0m:up=\E[A:\
	:us=\E[4m:

# (ibmx: this entry formerly included the following unknown capabilities:
#	:GC=b:GL=v:GR=t:RT=^J:\
#	:GH=\E[196g:GV=\E[179g:\
#	:GU=\E[193g:GD=\E[194g:\
#	:G1=\E[191g:G2=\E[218g:G3=\E[192g:G4=\E[217g:\
#	:CW=\E[E:NU=\E[F:RF=\E[G:RC=\E[H:\
#	:WL=\E[K:WR=\E[L:CL=\E[M:CR=\E[N:\
# I renamed GS/GE/WL/WR/CL/CR/PU/PD/HM/EN; also, removed a duplicate
# ":kh=\E[Y:" -- esr)
ibmpcx|xenix|ibmx|IBM PC xenix console display:\
	:am:bs:ms:\
	:co#80:li#25:\
	:@7=\E[d:MR=\E[0m:ae=\E[10m:al=\E[L:as=\E[11m:\
	:cd=\E[J:ce=\E[K:cl=^L:cm=\E[%d;%dH:dc=\E[P:dl=\E[M:\
	:do=\E[B:ei=:ho=\E[H:ic=\E[@:im=:k1=\E[K:k2=\E[L:\
	:k3=\E[M:k4=\E[N:kN=\E[e:kP=\E[Z:kb=^H:kd=\E[B:\
	:kh=\E[Y:kl=\E[D:kr=\E[C:ku=\E[A:nd=\E[C:se=\E[0m:\
	:so=\E[7m:ue=\E[m:up=\E[A:us=\E[4m:
ibmc|ibmcpc|IBM PC xenix color console display:\
	:tc=ibmpcx:
ibmcx|ibmcpcx:\
	:tc=ibmpcx:

pcvt25h|386BSD pcvt rel 2.10 vt220 emulator video driver:\
	:am:km:mi:ms:xn:\
	:it#8:pb#9216:vt#3:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:\
	:LE=\E[%dD:RI=\E[%dC:SF=\E%dD:SR=\E%dM:UP=\E[%dA:\
	:ae=^O:al=\E[L:as=^N:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:ho=\E[H:\
	:i1=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h\E[1;25r\E[25;1H:\
	:ic=\E[@:im=\E[4h:k1=\E[17~:k2=\E[18~:k3=\E[19~:\
	:k4=\E[20~:k5=\E[21~:k6=\E[23~:k7=\E[24~:k8=\E[25~:\
	:kD=\E[3~:kH=\E[4~:kI=\E[2~:kN=\E[6~:kP=\E[5~:kb=^_:\
	:kd=\EOB:ke=\E[?1l\E>:kh=\E[1~:kl=\EOD:kr=\EOC:\
	:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[m:mr=\E[7m:nd=\E[C:nw=^M^J:\
	:r1=\Ec\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:rf=/usr/share/tabset/vt100:sc=\E7:se=\E[27m:sf=\ED:\
	:so=\E[7m:sr=\EM:st=\EH:ta=^I:ue=\E[24m:up=\E[A:\
	:us=\E[4m:

#### DEC VT100 and compatibles
#
# DEC terminals from the vt100 forward are collected here.  Older DEC terminals
# and micro consoles can be found in the `obsolete' section.  More details
# on the relationship between the VT100 and ANSI X3.64 may be found near the
# end of this file.
#
# Except where noted, these entries are DEC's official terminfos.
# Contact Bill Hedberg <hedberg@hannah.enet.dec.com> of Terminal Support
# Engineering for more information.  Updated terminfos and termcaps 
# are kept available at ftp://gatekeeper.dec.com/pub/DEC/termcaps.
#

# Note that the xenl glitch in vt100 is not quite the same as on the Concept,
# since the cursor is left in a different position while in the
# weird state (concept at beginning of next line, vt100 at end
# of this line) so all versions of vi before 3.7 don't handle
# xenl right on vt100. The correct way to handle xenl is when
# you output the char in column 80, immediately output CR LF
# and then assume you are in column 1 of the next line. If xenl
# is on, am should be on too.
# 
# I assume you have smooth scroll off or are at a slow enough baud
# rate that it doesn't matter (1200? or less). Also this assumes
# that you set auto-nl to "on", if you set it off use vt100-nam 
# below.
# 
# The padding requirements listed here are guesses. It is strongly
# recommended that xon/xoff be enabled, as this is assumed here.
# 
# The vt100 uses rs2 and rf rather than is2/tbc/hts because the 
# tab settings are in non-volatile memory and don't need to be 
# reset upon login. Also setting the number of columns glitches 
# the screen annoyingly. You can type "reset" to get them set.
#
# This is how the keypad gets assigned in Application Keypad mode.
#	PF1 = kf1	  PF2 = kf2	    PF3   = kf3	      PF4 = kf4
#	7   = kf9	  8   = kf10	    9     = kf0	      - 
#	4   = kf5	  5   = kf6	    6     = kf7	      ,   = kf8
#	1   = ka1	  2   = kb2	    3     = ka3
#	0   = kc1	  .   = kc3	    ENTER = kent
#
vt100|vt100-am|dec vt100 (w/advanced video):\
	:am:mi:ms:xn:xo:\
	:co#80:it#8:li#24:vt#3:\
	:@8=\EOM:DO=\E[%dB:K1=\EOq:K2=\EOr:K3=\EOs:K4=\EOp:\
	:K5=\EOn:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:as=^N:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:do=^J:eA=\E(B\E)0:ho=\E[H:k0=\EOy:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\EOt:k6=\EOu:k7=\EOv:\
	:k8=\EOl:k9=\EOw:k;=\EOx:kb=^H:kd=\EOB:ke=\E[?1l\E>:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m\017:mr=\E[7m:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:..sa=\E[0%?%p1%p6%|%t;1%;%?%p2%t;4%;%?%p1%p3%|%t;7%;%?%p4%t;5%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[1;7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:

vt100nam|vt100-nam|vt100 w/no am (w/advanced video):\
	:am@:xn@:\
	:tc=vt100-am:

# Ordinary vt100 in 132 column ("wide") mode.
vt100-w|vt100-w-am|dec vt100 132 cols (w/advanced video):\
	:co#132:li#24:\
	:r2=\E>\E[?3h\E[?4l\E[?5l\E[?8h:tc=vt100-am:
vt100-w-nam|vt100-nam-w|dec vt100 132 cols (w/advanced video):\
	:co#132:li#14:vt@:\
	:r2=\E>\E[?3h\E[?4l\E[?5l\E[?8h:tc=vt100-nam:

# vt100 with no advanced video.
vt100-nav|vt100 without advanced video option:\
	:sg#1:\
	:mb@:md@:me@:mr@:sa@:se=\E[m:so=\E[7m:ue@:us@:tc=vt100:
vt100-nav-w|vt100-w-nav|dec vt100 132 cols 14 lines (no advanced video option):\
	:co#132:li#14:\
	:tc=vt100-nav:

# vt100 with one of the 24 lines used as a status line.
# We put the status line on the top.
vt100-s|vt100-s-top|vt100-top-s|vt100 for use with sysline:\
	:es:hs:\
	:li#23:\
	:cl=\E[2;1H\E[J:cm=\E[%i%+^A;%dH:cs=\E[%i%i%d;%dr:\
	:ds=\E7\E[1;24r\E8:fs=\E8:ho=\E[2;1H:\
	:is=\E7\E[2;24r\E8:ts=\E7\E[1;%p1%dH\E[1K:tc=vt100-am:

# Status line at bottom. 
# Clearing the screen will clobber status line.
vt100-s-bot|vt100-bot-s|vt100 for use with sysline:\
	:es:hs:\
	:li#23:\
	:ds=\E7\E[1;24r\E8:fs=\E8:is=\E[1;23r\E[23;1H:\
	:ts=\E7\E[24;%p1%dH\E[1K:tc=vt100-am:

# DEC VT100 with Advanced Video Option -- NOT DEC'S ENTRY!!!
# This may be used as an alternate vt102 entry; it's probably better than the
# stock one if you can live with XON/XOFF.  All the AVO gave you was smul/rmul.
# From: Doug Gwyn <gwyn@smoke.brl.mil> 25 Jan 93
# The following SET-UP modes are assumed for normal operation:
#	ANSI_MODE	AUTO_XON/XOFF_ON	NEWLINE_OFF	80_COLUMNS
#	WRAP_AROUND_ON
# Other SET-UP modes may be set for operator convenience or communication
# requirements; I recommend
#	SMOOTH_SCROLL	AUTOREPEAT_ON	BLOCK_CURSOR	MARGIN_BELL_OFF
#	SHIFTED_3_#
# Unless you have a graphics add-on such as Digital Engineering's VT640
# (and even then, whenever it can be arranged!) you should set
#	INTERLACE_OFF
# Hardware tabs are assumed to be set every 8 columns; they can be set up
# by the "reset", "tset", or "tabs" utilities (use vt100-x, 132 columns, for
# this).  I have included some compatible code in "rs" for the VT640 if you
# have one.  No delays are specified; use "stty ixon -ixany" to enable DC3/DC1
# flow control!
# Thanks to elsie!ado (Arthur David Olson) for numerous improvements.
vt100-avo|DEC VT100 with AVO:\
	:ms:xo:\
	:co#80:it#8:li#24:vt#3:\
	:DO=\E[%dB:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:ae=^O:as=^N:\
	:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=\E[%i%d;%dr:ct=\E[3g:do=^J:ho=\E[H:\
	:is=\E<\E)0:k0=\EOP:k1=\EOQ:k2=\EOR:k3=\EOS:kb=^H:\
	:kd=\EOB:ke=\E[?1l\E>:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:\
	:ku=\EOA:l0=PF1:l1=PF2:l2=PF3:l3=PF4:le=^H:ll=\E[24H:\
	:mb=\E[5m:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:nw=\EE:\
	:rc=\E8:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:\
	:ta=^I:te=150\E[?7h:ti=\E[?7l:ue=\E[m:up=\EM:\
	:us=\E[4m:

# Most of the `vt100' emulators out there actually emulate a vt102
# This entry (or vt102-nsgr) is probably the right thing to use for
# these.  
vt102|dec vt102:\
	:mi:\
	:al=\E[L:dc=\E[P:dl=\E[M:ei=\E[4l:im=\E[4h:tc=vt100:

# Many brain-dead PC comm programs that pretend to be `vt100-compatible'
# fail to interpret the ^O and ^N escapes properly.  Symptom: the sgr0
# string in the canonical vt100 entry above leaves the screen littered
# with little  snowflake or star characters (IBM PC ROM character \017 = ^O)
# after highlight turnoffs.  This entry should fix that, and even leave
# ACS support working, at the cost of making multiple-highlight changes 
# slightly more expensive.
# From: Eric S. Raymond <esr@snark.thyrsus.com> July 22 1995
vt102-nsgr|dec vt102 with ACS support disabled:\
	:me=\E[m:sa@:tc=vt102:

# VT125 Graphics CRT.  Clear screen also erases graphics
vt125|vt125 graphics terminal:\
	:cl=\E[;H\E[2J\EPpS(E)\E\\:tc=vt100:

# vt132 - like vt100 but slower and has ins/del line and such.
# I'm told that smir/rmir are backwards in the terminal from the
# manual and from the ANSI standard, this describes the actual 
# terminal. I've never actually used a vt132 myself, so this 
# is untested.
#
vt132|DEC vt132:\
	:xn:\
	:al=\E[L:dc=\E[P:dl=\E[M:ei=\E[4h:im=\E[4l:ip=:sf=\n:tc=vt100:

# vt220:
# This vt220 description maps F5--F9 to the second block of function keys
# at the top of the keyboard.  The "DO" key is used as F10 to avoid conflict
# with the key marked (ESC) on the vt220.  See vt220d for an alternate mapping.
# PF1--PF4 are used as F1--F4.
#
vt220|DEC VT220 in vt100 emulation mode:\
	:am:mi:xn:xo:\
	:co#80:li#24:vt#3:\
	:@7=\E[4~:ac=kkllmmjjnnwwqquuttvvxx:ae=\E(B:al=\E[L:\
	:as=\E(0:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[M:\
	:do=\E[B:ei=\E[4l:ho=\E[H:if=/usr/lib/tabset/vt100:\
	:im=\E[4h:is=\E[1;24r\E[24;1H:k1=\EOP:k2=\EOQ:\
	:k3=\EOR:k4=\EOS:k5=\E[17~:k6=\E[18~:k7=\E[19~:\
	:k8=\E[20~:k9=\E[21~:k;=\E[29~:kD=\E[3~:kI=\E[2~:\
	:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:kh=\E[1~:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[m:\
	:mr=\E[7m:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:rf=/usr/lib/tabset/vt100:\
	:..sa=\E[0%?%p6%t;1%;%?%p2%t;4%;%?%p4%t;5%;%?%p1%p3%|%t;7%;m%?%p9%t\E(0%e\E(B%;:\
	:sc=\E7:se=\E[m:sf=20\ED:so=\E[7m:sr=14\EM:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:ve=\E[?25h:vi=\E[?25l:
#
# vt220d:
# This vt220 description regards F6--F10 as the second block of function keys
# at the top of the keyboard.  This mapping follows the description given
# in the VT220 Programmer Reference Manual and agrees with the labeling
# on some terminals that emulate the vt220.  There is no support for an F5.
# See vt220 for an alternate mapping. 
#
vt220d|DEC VT220 in vt100 mode with DEC function key labeling:\
	:F1=\E[23~:F2=\E[24~:F3=\E[25~:F4=\E[26~:F5=\E[28~:\
	:F6=\E[29~:F7=\E[31~:F8=\E[32~:F9=\E[33~:FA=\E[34~:\
	:k5@:k6=\E[17~:k7=\E[18~:k8=\E[19~:k9=\E[20~:\
	:k;=\E[21~:tc=vt220:

vt220nam|vt220-nam|v220n|VT220 in vt100 mode with no auto margins:\
	:am@:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7l\E[?8h:tc=vt220:

vt220-8|dec vt220 8 bit terminal:\
	:5i:am:mi:ms:xn:xo:\
	:co#80:it#8:li#24:\
	:%0=\E[29~:%1=\E[28~:*6=\E[4~:@0=\E[1~:AL=\E[%dL:\
	:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[23~:F2=\E[24~:\
	:F3=\E[25~:F4=\E[26~:F7=\E[31~:F8=\E[32~:F9=\E[33~:\
	:FA=\E[34~:IC=\E[%d@:LE=\E[%dD:RA=\E[?7l:RI=\E[%dC:\
	:SA=\E[?7h:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:eA=\E)0:ec=\E[%dX:\
	:ei=\E[4l:ho=\E[H:if=/usr/lib/tabset/vt100:im=\E[4h:\
	:is=\E[?7h\E[>\E[?1h\E F\E[?4l:k1=\EOP:k2=\EOQ:\
	:k3=\EOR:k4=\EOS:k6=\E[17~:k7=\E[18~:k8=\E[19~:\
	:k9=\E[20~:k;=\E[21~:kI=\E[2~:kN=\E[6~:kP=\E[5~:\
	:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:\
	:l1=pf1:l2=pf2:l3=pf3:l4=pf4:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[0m:mr=\E[7m:nd=\E[C:nw=\EE:pf=\E[4i:po=\E[5i:\
	:ps=\E[i:r1=\E[?3l:rc=\E8:sc=\E7:se=\E[27m:sf=\ED:\
	:so=\E[7m:sr=\EM:st=\EH:ta=^I:ue=\E[24m:up=\E[A:\
	:us=\E[4m:vb=\E[?5h\E[?5l:

vt320|DEC VT320 in vt100 emulation mode:\
	:tc=vt220:
#
#  Use v320n for LYRIX
#
vt320nam|vt320-nam|v320n|DEC VT320 in vt100 emul. mode with NO AUTO WRAP mode:\
	:am@:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7l\E[?8h:tc=vt220:

vt420|DEC VT420:\
	:am:mi:xn:xo:\
	:co#80:li#24:vt#3:\
	:*6=\E[4~:@0=\E[1~:\
	:S5=\E[?0;0r\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=\E(B:al=\E[L:as=\E(0:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[;H\E[2J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:ho=\E[H:\
	:i2=\E[?67h\E[64;1"p:if=/usr/lib/tabset/vt100:\
	:im=\E[4h:is=\E[1;24r\E[24;1H:k0=\E[29~:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\E[17~:k6=\E[18~:\
	:k7=\E[19~:k8=\E[20~:k9=\E[21~:k;=\E[29~:kD=\E[3~:\
	:kI=\E[2~:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:ke=\E>:\
	:kl=\E[D:kr=\E[C:ks=\E=:ku=\E[A:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:\
	:r3=\E[?67h\E[64;1"p:rc=\E8:rf=/usr/lib/tabset/vt100:\
	:..sa=\E[0%?%p6%t;1%;%?%p2%t;4%;%?%p4%t;5%;%?%p1%p3%|%t;7%;m%?%p9%t\E(0%e\E(B%;:\
	:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:ue=\E[m:\
	:up=\E[A:us=\E[4m:

vt420nam|vt420-nam|v420n|DEC VT420 in vt100 emul. mode with NO AUTO WRAP mode:\
	:am@:\
	:tc=vt420:

#
#  DECUDK   
#               if (key < 16) then  value = key;
#               else if (key < 21) then value = key + 1; 
#               else if (key < 25) then value = key + 2;
#               else if (key < 27) then value = key + 3;
#               else if (key < 30) then value = key + 4;
#               else value = key + 5;
#
vt420pc|DEC VT420 w/PC keyboard:\
	:@7=\E[4~:F1=\E[23~:F2=\E[24~:F3=\E[11;2~:\
	:F4=\E[12;2~:F5=\E[13;2~:F6=\E[14;2~:F7=\E[15;2~:\
	:F8=\E[17;2~:F9=\E[18;2~:FA=\E[19;2~:FB=\E[20;2~:\
	:FC=\E[21;2~:FD=\E[23;2~:FE=\E[24;2~:FF=\E[23~:\
	:FG=\E[24~:FH=\E[25~:FI=\E[26~:FJ=\E[28~:FK=\E[29~:\
	:FL=\E[31~:FM=\E[32~:FN=\E[33~:FO=\E[34~:FP=\E[35~:\
	:FQ=\E[36~:FR=\E[23;2~:FS=\E[24;2~:FT=\E[25;2~:\
	:FU=\E[26;2~:FV=\E[28;2~:FW=\E[29;2~:FX=\E[31;2~:\
	:FY=\E[32;2~:FZ=\E[33;2~:Fa=\E[34;2~:Fb=\E[35;2~:\
	:Fc=\E[36;2~:S6=USR_TERM\072vt420pcdos\072:k1=\E[11~:\
	:k2=\E[12~:k3=\E[13~:k4=\E[14~:k5=\E[15~:k6=\E[17~:\
	:k7=\E[18~:k8=\E[19~:k9=\E[20~:k;=\E[21~:kD=^_:\
	:kh=\E[H:\
	:..px=\EP1;1|%?%{16}%p1%>%t%{0}%e%{21}%p1%>%t%{1}%e%{25}%p1%>%t%{2}%e%{27}%p1%>%t%{3}%e%{30}%p1%>%t%{4}%e%{5}%;%p1%+%d/%p2%s\E\\:tc=vt420:

vt420pcdos|DEC VT420 w/PC for DOS Merge:\
	:li#25:\
	:S1=%?%p2%{19}%=%t\E\023\021%e%p2%{32}%<%t\E%p2%c%e%p2%{127}%=%t\E\177%e%p2%c%;:\
	:S4=\E[?1;2r\E[34h:\
	:S5=\E[?0;0r\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:S6@:\
	:me=\E[0m:sa@:tc=vt420pc:

vt420f|DEC VT420 with VT kbd; VT400 mode; F1-F5 used as Fkeys:\
	:F1=\E[23~:F2=\E[24~:F3=\E[25~:F4=\E[26~:F5=\E[28~:\
	:F6=\E[29~:F7=\E[31~:F8=\E[32~:F9=\E[33~:FA=\E[34~:\
	:k1=\E[11~:k2=\E[12~:k3=\E[13~:k4=\E[14~:k5=\E[15~:\
	:k6=\E[17~:k7=\E[18~:k8=\E[19~:k9=\E[20~:k;=\E[21~:\
	:kD=^_:kh=\E[H:l1=\EOP:l2=\EOQ:l3=\EOR:l4=\EOS:tc=vt420:

vt420f-nam|v420fn|DEC VT420 no auto margins:\
	:am@:\
	:tc=vt420f:
vt420pc-nam|v420pcn|DEC VT420 PC keyboard no auto margins:\
	:am@:\
	:tc=vt420pc:

vt510|DEC VT510:\
	:tc=vt420:
vt510nam|vt510-nam|v510n|DEC VT510 in vt100 emul. mode with NO AUTO WRAP mode:\
	:tc=vt420nam:
vt510pc|DEC VT510 w/PC keyboard:\
	:tc=vt420pc:
vt510pc-nam|v510pcn|DEC VT510 PC keyboard no auto margins:\
	:am@:\
	:tc=vt420pc:
vt510pcdos|DEC VT510 w/PC for DOS Merge:\
	:tc=vt420pcdos:

# VT520/VT525
#
# The VT520 is a monochrome text terminal capable of managing up to
# four independent sessions in the terminal.  It has multiple ANSI
# emulations (VT520, VT420, VT320, VT220, VT100, VT PCTerm, SCO Console)
# and ASCII emulations (WY160/60, PCTerm, 50/50+, 150/120, TVI 950,
# 925 910+, ADDS A2).  This terminfo data is for the ANSI emulations only.
#
# Terminal Set-Up is entered by pressing [F3], [Caps Lock]/[F3] or
# [Alt]/[Print Screen] depending upon which keyboard and which
# terminal mode is being used.  If Set-Up has been disabled or
# assigned to an unknown key, Set-Up may be entered by pressing
# [F3] as the first key after power up, regardless of keyboard type.
vt520|DEC VT520:\
	:am:mi:xn:xo:\
	:co#80:li#24:vt#3:\
	:*6=\E[4~:@0=\E[1~:\
	:S5=\E[?0;0r\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=\E(B:al=\E[L:as=\E(0:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[;H\E[2J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:ho=\E[H:\
	:i2=\E[?67h\E[64;1"p:if=/usr/lib/tabset/vt100:\
	:im=\E[4h:is=\E[1;24r\E[24;1H:k0=\E[29~:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\E[17~:k6=\E[18~:\
	:k7=\E[19~:k8=\E[20~:k9=\E[21~:k;=\E[29~:kD=\E[3~:\
	:kI=\E[2~:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[m:\
	:mr=\E[7m:nd=\E[C:\
	:..px=\EP1;1|%?%{16}%p1%>%t%{0}%e%{21}%p1%>%t%{1}%e%{25}%p1%>%t%{2}%e%{27}%p1%>%t%{3}%e%{30}%p1%>%t%{4}%e%{5}%;%p1%+%d/%p2%s\E\\:\
	:r3=\E[?67h\E[64;1"p:rc=\E8:rf=/usr/lib/tabset/vt100:\
	:..sa=\E[0%?%p6%t;1%;%?%p2%t;4%;%?%p4%t;5%;%?%p1%p3%|%t;7%;m%?%p9%t\E(0%e\E(B%;:\
	:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:ue=\E[m:\
	:up=\E[A:us=\E[4m:

vt520nam|vt520-nam|v520n|DEC VT520 with NO AUTO WRAP:\
	:am@:\
	:tc=vt520:

vt525|DEC VT525:\
	:am:mi:xn:xo:\
	:co#80:li#24:vt#3:\
	:*6=\E[4~:@0=\E[1~:\
	:S5=\E[?0;0r\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=\E(B:al=\E[L:as=\E(0:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[;H\E[2J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:ho=\E[H:\
	:i2=\E[?67h\E[64;1"p:if=/usr/lib/tabset/vt100:\
	:im=\E[4h:is=\E[1;24r\E[24;1H:k0=\E[29~:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\E[17~:k6=\E[18~:\
	:k7=\E[19~:k8=\E[20~:k9=\E[21~:k;=\E[29~:kD=\E[3~:\
	:kI=\E[2~:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[m:\
	:mr=\E[7m:nd=\E[C:\
	:..px=\EP1;1|%?%{16}%p1%>%t%{0}%e%{21}%p1%>%t%{1}%e%{25}%p1%>%t%{2}%e%{27}%p1%>%t%{3}%e%{30}%p1%>%t%{4}%e%{5}%;%p1%+%d/%p2%s\E\\:\
	:r3=\E[?67h\E[64;1"p:rc=\E8:rf=/usr/lib/tabset/vt100:\
	:..sa=\E[0%?%p6%t;1%;%?%p2%t;4%;%?%p4%t;5%;%?%p1%p3%|%t;7%;m%?%p9%t\E(0%e\E(B%;:\
	:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:ue=\E[m:\
	:up=\E[A:us=\E[4m:

vt525nam|vt525-nam|v525n|DEC VT525 with NO AUTO WRAP:\
	:am@:\
	:tc=vt525:

#### Xterm variants
#

# X10/6.6	11/7/86, minus alternate screen, plus (csr)
# (xterm: ":MT:" changed to ":km:"; mapped ":pt:" to ":it#8:";
# removed (hs, eslok, tsl=\E[?E\E[?%i%dT, fsl=\E[?F, dsl=\E[?E)
# as these seem not to work -- esr)
x10term|vs100-x10|xterm terminal emulator (X10 window system):\
	:am:bs:km:mi:ms:pt:xn:xo:\
	:co#80:it#8:li#65:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:al=\E[L:cd=\E[J:\
	:ce=\E[K:cl=\E[H\E[2J:cm=\E[%i%d;%dH:cs=\E[%i%d;%dr:\
	:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:ho=\E[H:im=\E[4h:\
	:is=\E\E[m\E[?7h\E[?1;4l:k1=\EOP:k2=\EOQ:k3=\EOR:\
	:k4=\EOS:kb=^H:kd=\EOB:ke=\E[?1l\E>:kl=\EOD:kr=\EOC:\
	:ks=\E[?1h\E=:ku=\EOA:le=^H:md=\E[1m:me=\E[m:\
	:mr=\E[7m:nd=\E[C:\
	:rs=\E[r\E<\E[m\E[H\E[2J\E[?7h\E[?1;3;4;6l:se=\E[m:\
	:sf=^J:so=\E[7m:sr=\EM:ue=\E[m:up=\E[A:us=\E[4m:
# X11R6 xterm.  This is known good for the XFree86 version under Linux.
# From: Eric S. Raymond <esr@snark.thyrsus.com> 9 Jul 1995
# Note: If you use the line-drawing character set, the disable afterwards
# will leave you in US-ASCII.  If you live somewhere that wants a pound sign
# at 2/3, change rmacs to "\E(A".  Further note: cuf and cub don't seem
# to be reliable under my xterm, so they're commented out.  Final note:
# Older versions of this entry set/reset application keypad mode (\EO-prefix
# cursor keys) in the [sr]mkx caps, but it wasn't necessary, and doesn't
# actually fit the terminfo model properly.
xterm|vs100|xterm terminal emulator (X11R6 Window System):\
	:am:bs:km:mi:ms:pt:xn:xo:\
	:co#80:it#8:li#65:\
	:@7=\E[[:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:F1=\E[23~:\
	:F2=\E[24~:IC=\E[%d@:LE=\E[%dD:UP=\E[%dA:\
	:ac=++\054\054..00II--``aaffgghhjjkkllmmnnooqqssttuuvvwwxx~~:\
	:ae=\E(B:al=\E[L:as=\E(0:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[2J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3k:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:ho=\E[H:\
	:ic=\E[@:im=\E[4h:\
	:is=\E[r\E[m\E[2J\E[H\E[?7h\E[?1;3;4;6l\E[4l:\
	:k1=\E[11~:k2=\E[12~:k3=\E[13~:k4=\E[14~:k5=\E[15~:\
	:k6=\E[17~:k7=\E[18~:k8=\E[19~:k9=\E[20~:k;=\E[21~:\
	:kI=\E[2~:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:kh=\E[@:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:md=\E[1m:me=\E[m:\
	:mr=\E[7m:nd=\E[C:\
	:r2=\E[r\E[m\E[2J\E[H\E[?7h\E[?1;3;4;6l\E[4l\E<:\
	:rc=\E8:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:ta=^I:\
	:te=\E[2J\E[?47l\E8:ti=\E7\E[?47h:u6=\E[%d;%dR:\
	:u7=\E[6n:u8=\E[?1;2c:u9=\E[c:ue=\E[m:up=\E[A:\
	:us=\E[4m:
xterm24|vs100-24|xterm terminal emulator (24 lines) (X11R6 window system):\
	:co#80:li#24:\
	:tc=xterm:
xterm25|vs100-25|xterm terminal emulator (25 lines) (X11R6 window system):\
	:co#80:li#25:\
	:tc=xterm:
xterm50|vs100-50|xterm terminal emulator (50 lines) (X11R6 window system):\
	:co#80:li#50:\
	:tc=xterm:
xterms|vs100s|xterm terminal emulator (small) (X11R6 window system):\
	:tc=xterm24:
# (kterm: this had unknown capabilities ":KJ:TY=ascii:" -- esr)
kterm|kterm kanji terminal emulator (X window system):\
	:es:hs:\
	:cs=\E[%i%d;%dr:ds=\E[?H:fs=\E[?F:rc=\E8:sc=\E7:\
	:ts=\E[?E\E[?%i%dT:tc=xterm:

# See the note on ICH/ICH1 VERSUS RMIR/SMIR near the end of file
xterm-nic|xterm with ich/ich1 suppressed for non-curses programs:\
	:IC@:ei=:ic@:im=:tc=xterm:

# From: Eric S. Raymond <esr@snark.thyrsus.com> May 4 1995
# Should work with the color xterm on the X11R6 contrib tape.
xterm-color|xterm with color support:\
	:tc=xterm:tc=ansi-pc-color:

# From: David J. MacKenzie <djm@va.pubnix.com> 20 Apr 1995
# Here's a termcap entry I've been using for xterm_color, which comes
# with BSD/OS 2.0, and the X11R6 contrib tape too I think.  Besides the
# color stuff, I also have a status line defined as the window manager
# title bar. [I have translated it to terminfo -- ESR]
xterm-pcolor|xterm with color used for highlights and status line:\
	:hs:\
	:ws#40:\
	:ds=\E]0;\007:fs=^G:md=\E[1m\E[43m:mr=\E[7m\E[34m:\
	:so=\E[7m\E[31m:ts=\E]0;:us=\E[4m\E[42m:tc=xterm:

######## UNIX VIRTUAL TERMINALS AND VIRTUAL CONSOLES
#

# Columbus UNIX virtual terminal. This terminal also appears in 
# UNIX 4.0 and successors as line discipline 1 (?), but is 
# undocumented and does not really work quite right.
cbunix|cb unix virtual terminal:\
	:am:bs:da:db:\
	:co#80:li#24:lm#0:\
	:al=\EP:bl=^G:cd=\EL:ce=\EK:cl=\EL:cm=\EG%r%.%.:\
	:cr=^M:dc=\EM:dl=\EN:do=^J:ei=:ic=\EO:im=:kd=\EB:\
	:kh=\EE:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:se=\Eb^D:\
	:sf=^J:so=\Ea^D:ue=\Eb^A:up=\EA:us=\Ea^A:
# (vremote: removed obsolete ":nl@:" -- esr)
vremote|virtual remote terminal:\
	:am@:\
	:co#79:\
	:tc=cbunix:
pty|4bsd pseudo teletype:\
	:cm=\EG%+ %+ :se=\Eb$:so=\Ea$:ue=\Eb!:us=\Ea!:tc=cbunix:

# Entries for use by the FSF's `screen' program.  These came with version 3.6.2
screen|VT 100/ANSI X3.64 virtual terminal:\
	:am:km:mi:ms:xn:\
	:co#80:it#8:li#24:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[23~:\
	:F2=\E[24~:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~..--++\054\054hhII00:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:ho=\E[H:\
	:im=\E[4h:is=\E)0:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:\
	:k5=\E[15~:k6=\E[17~:k7=\E[18~:k8=\E[19~:k9=\E[20~:\
	:k;=\E[21~:kD=\E[3~:kH=\E[4~:kI=\E[2~:kN=\E[6~:\
	:kP=\E[5~:kb=^H:kd=\EOB:ke=\E[?1l\E>:kh=\E[1~:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:nw=\EE:r2=\Ec:\
	:rc=\E8:sc=\E7:se=\E[23m:sf=^J:so=\E[3m:sr=\EM:\
	:st=\EH:ta=^I:ue=\E[24m:up=\EM:us=\E[4m:
screen-w|VT 100/ANSI X3.64 virtual terminal with 132 cols:\
	:am:km:mi:ms:xn:\
	:co#132:it#8:li#24:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[23~:\
	:F2=\E[24~:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~..--++\054\054hhII00:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:ho=\E[H:\
	:im=\E[4h:is=\E)0:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:\
	:k5=\E[15~:k6=\E[17~:k7=\E[18~:k8=\E[19~:k9=\E[20~:\
	:k;=\E[21~:kD=\E[3~:kH=\E[4~:kI=\E[2~:kN=\E[6~:\
	:kP=\E[5~:kb=^H:kd=\EOB:ke=\E[?1l\E>:kh=\E[1~:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:nw=\EE:r2=\Ec:\
	:rc=\E8:sc=\E7:se=\E[23m:sf=^J:so=\E[3m:sr=\EM:\
	:st=\EH:ta=^I:ue=\E[24m:up=\EM:us=\E[4m:

######## WORKSTATION CONSOLES
#

#### Sun consoles
#

# :is: resets scrolling region in case a previous user had used "tset vt100"
# (sun: mapped ":pt:" to ":it#8:" -- esr)
oldsun|Sun Microsystems Workstation console:\
	:am:bs:km:mi:ms:pt:\
	:co#80:it#8:li#34:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:IC=\E[%d@:al=\E[L:\
	:bl=^G:cd=\E[J:ce=\E[K:cl=^L:cm=\E[%i%d;%dH:cr=^M:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=:ic=\E[@:im=:is=\E[1r:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:nd=\E[C:rs=\E[1r:\
	:se=\E[m:sf=^J:so=\E[7m:ta=^I:up=\E[A:
# New entry from vendor
sun|sun1|sun2|Sun Microsystems Inc. workstation:\
	:am:km:ms:\
	:co#80:li#34:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:IC=\E[%d@:al=\E[L:\
	:bl=^G:cd=\E[J:ce=\E[K:cl=^L:cm=\E[%i%d;%dH:cr=^M:\
	:dc=\E[P:dl=\E[M:do=^J:ei=:ho=\E[H:ic=\E[@:im=:\
	:k1=\E[224z:k2=\E[225z:k3=\E[226z:k4=\E[227z:\
	:k5=\E[228z:k6=\E[229z:k7=\E[230z:k8=\E[231z:\
	:k9=\E[232z:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:r2=\E[s:\
	:..sa=\E[0%?%p6%t;1%;%?%p2%t;4%;%?%p1%p3%|%t;7%;m:\
	:se=\E[m:sf=^J:so=\E[7m:ta=^I:ue=\E[m:up=\E[A:\
	:us=\E[4m:
# From: <john@ucbrenoir>  Tue Sep 24 13:14:44 1985
sun-s|Sun Microsystems Workstation window with status line:\
	:hs:\
	:ds=\E]l\E\\:fs=\E\\:ts=\E]l:tc=sun:
sun-e-s|sun-s-e|Sun Microsystems Workstation with status hacked for emacs:\
	:hs:\
	:ds=\E]l\E\\:fs=\E\\:ts=\E]l:tc=sun-e:
sun-48|Sun 48-line window:\
	:co#80:li#48:\
	:tc=sun:
sun-34|Sun 34-line window:\
	:co#80:li#34:\
	:tc=sun:
sun-24|Sun 24-line window:\
	:co#80:li#24:\
	:tc=sun:
sun-17|Sun 17-line window:\
	:co#80:li#17:\
	:tc=sun:
sun-12|Sun 12-line window:\
	:co#80:li#12:\
	:tc=sun:
sun-1|Sun 1-line window for sysline:\
	:es:hs:\
	:co#80:li#1:\
	:ds=^L:fs=\E[K:ts=^M:tc=sun:
sun-e|sun-nic|sune|Sun Microsystems Workstation without insert character:\
	:ei@:ic@:im@:tc=sun:
sun-c|sun-cmd|Sun Microsystems Workstation console with scrollable history:\
	:te=\E[>4h:ti=\E[>4l:tc=sun:

#### Iris consoles
#

# (wsiris: this had unknown capabilities
#	:HS=\E7F2:HE=\E7F7:\
#	:CT#2:CZ=*Bblack,red,green,yellow,blue,magenta,cyan,*Fwhite:
# I mapped ":pt:" to ":it#8:", removed incorrect ":cl=\Ev:" -- esr)
wsiris|iris40|iris emulating a 40 line visual 50 (approximately):\
	:am:bs:pt:\
	:co#80:it#8:li#40:\
	:al=\EL:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :dl=\EM:\
	:ho=\EH:is=\E7B0\E7F7\E7C2\E7R3:k0=\E0:k1=\E1:k2=\E2:\
	:k3=\E3:k4=\E4:k5=\E5:k6=\E6:k7=\E7:k8=\E8:k9=\E9:\
	:kd=\EB:kl=\ED:kr=\EC:ku=\EA:nd=\EC:se=\E0@:so=\E9P:\
	:sr=\EI:ue=\E7R3\E0@:up=\EA:us=\E7R2\E9P:ve=\E>:\
	:vs=\E;:

#### Masscomp consoles
#

masscomp2:\
	:co#64:li#21:\
	:tc=masscomp:
masscomp1:\
	:co#104:li#36:\
	:tc=masscomp:
# (masscomp: ":MT:" changed to ":km:"; mapped ":pt:" to ":it#8:" -- esr)
masscomp:\
	:bs:km:mi:pt:\
	:co#80:it#8:li#24:sg#0:\
	:al=\E[L:cd=\E[J:ce=\E[K:cl=\E[2J:cm=\E[%i%d;%dH:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:im=\E[4h:\
	:is=\EGc\EGb\EGw:kb=^H:kd=\EOB:kl=\EOD:kr=\EOC:\
	:ku=\EOA:nd=\E[C:se=\E[0m:so=\E[7m:ue=\EGau:up=\E[A:\
	:us=\EGu:

#### NeWS consoles
#
# Console terminal windows under the NeWS (Sun's Display Postscript windowing
# environment).   Note: these have nothing to do with Sony's News workstation
# line.
#

# Entry for NeWS's psterm from Eric Messick & Hugh Daniel
# (psterm: unknown ":sl=\EOl:el=\ENl:" removed;
# mapped ":pt:" to ":it#8:" -- esr)
psterm|psterm-basic|psterm-80x34:\
	:am:bs:hs:km:pt:ul:\
	:co#80:it#8:li#34:\
	:al=\EA:cd=\EB:ce=\EC:cl=^L:cm=\E%d;%d;:cs=\EE%d;%d;:\
	:dc=\EF:dl=\EK:do=\EP:ei=\ENi:fs=\ENl:ho=\ER:im=\EOi:\
	:is=\EN*:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:le=\ET:\
	:ll=\EU:mb=\EOb:md=\EOd:me=\EN*:mr=\EOr:nd=\EV:rc=^\:\
	:rs=\EN*:sc=^]:se=\ENo:sf=\EW:so=\EOo:sr=\EX:te=\ENt:\
	:ti=\EOt:ts=\EOl:ue=\ENu:up=\EY:us=\EOu:vb=\EZ:
psterm-96x48:\
	:co#96:li#48:\
	:tc=psterm:
psterm-90x28:\
	:co#90:li#28:\
	:tc=psterm:
psterm-80x24:\
	:co#80:li#24:\
	:tc=psterm:
# This is a faster termcap for psterm.  Warning:  if you use this termcap,
# some control characters you type will do strange things to the screen.
# (psterm-fast: unknown ":sl=^Ol:el=^Nl:";
# removed; mapped ":pt:" to ":it#8:" -- esr)
psterm-fast:\
	:am:bs:hs:km:pt:ul:\
	:co#80:it#8:li#34:\
	:al=^A:cd=^B:ce=^C:cl=^L:cm=\004%d;%d;:cs=\005%d;%d;:\
	:dc=^F:dl=^K:do=^P:ei=^Ni:fs=^Nl:ho=^R:im=^Oi:is=^N*:\
	:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:le=^T:ll=^U:mb=^Ob:\
	:md=^Od:me=^N*:mr=^Or:nd=^V:rc=^\:rs=^N*:sc=^]:\
	:se=^No:sf=^W:so=^Oo:sr=^X:te=^Nt:ti=^Ot:ts=^Ol:\
	:ue=^Nu:up=^Y:us=^Ou:vb=^Z:

#### Apollo consoles
#
# Apollo got bought by Hewlett-Packard.  The Apollo workstations are 
# labeled HP700s now.
#

# From: Gary Darland <goodmanc@garnet.berkeley.edu>
apollo:\
	:am:bs:mi:\
	:co#88:li#53:\
	:al=\EI:cd=\EJ:ce=\EK:ch=\EN%d:cl=^L:cm=\EM%+ %d):\
	:cv=\EO+ :dc=\EP:dl=\EL:do=\EB:ei=\ER:im=\EQ:nd=\EC:\
	:se=\ET:sf=\EE:so=\ES:sr=\ED:te=\EX:ti=\EW:ue=\EV:\
	:up=\EA:us=\EU:
apollo_15P|apollo 15 inch display:\
	:dN@:\
	:tc=vt132:
apollo_19L|apollo 19 inch display:\
	:dN@:\
	:tc=vt132:
apollo_color|apollo color display:\
	:dN@:\
	:tc=vt132:

#### Fortune Systems consoles
#

# From: Robert Nathanson <c160-3bp@Coral> via tut   Wed Oct 5, 1983
# (This had unknown capabilities
#	:rv=\EH:re=\EI:rg=0:\
#	:GG=0:GV=-:GH=&:GU=%:GD=#:G1=(:G2= :G3=":G4=*:CF=\E]:\
#	:CO=\E\\:WL=^Aa\r:WR=^Ab\r:CL=^Ac\r:CR=^Ad\r:DL=^Ae\r:RF=^Af\r:\
#	:RC=^Ag\r:CW=^Ah\r:NU=^Aj\r:EN=^Ak\r:HM=^Al:PL=^Am\r:\
#	:PU=^An\r:PD=^Ao\r:PR=^Ap\r:HP=^A@\r:RT=^Aq\r:TB=\r:CN=\177:MP=\E+F:
# It had both ":bs:" and ":bs=^H:"; I removed the latter.  Also, it had
# ":sg=0:" and ":ug=0:"; evidently the composer was trying (unnecessarily)
# to force both magic cookie glitches off.  Once upon a time, I
# used a Fortune myself, so I know the capabilities of the form ^A[a-z]\r are
# function keys; thus the "Al" value for HM was certainly an error.  I renamed
# EN/PD/PU/CO/CF according to the XENIX/TC mappings, but not HM/DL/RF/RC/RT.  
# I think rv and re are start and end reverse video and rg is a nonexistent
# "reverse-video-glitch" capability; I have put rv and re in with standard
# names below.  I've removed obsolete ":nl=5^J:" as there is a :do: -- esr)
fos|fortune|Fortune system:\
	:am:bs:bw:\
	:co#80:li#25:\
	:@7=^Ak\r:ae=^O:al=\034E:as=\Eo:bl=^G:cd=\034Y:\
	:ce=^\Z:cl=\014:cm=\034C%+ %+ :cr=^M:dc=\034W:\
	:dl=\034R:do=\n:ei=:ho=\036:ic=\034Q:im=:is=^_..:\
	:k1=^Aa\r:k2=^Ab\r:k3=^Ac\r:k4=^Ad\r:k5=^Ae\r:\
	:k6=^Af\r:k7=^Ag\r:k8=^Ah\r:kN=^Ao\r:kP=^An\r:kb=^H:\
	:kd=^Ay\r:kh=^A?\r:kl=^Aw\r:kr=^Az\r:ku=^Ax\r:le=^H:\
	:mb=\EN:me=\EI:mr=\EH:nw=^M^J:se=^\I`:sf=^J:so=^\H`:\
	:ta=^Z:ue=^\IP:up=\013:us=^\HP:ve=\E\\:vi=\E]:\
	:vs=\E\072:

######## COMMON TERMINAL TYPES
#
# This section describes terminal classes and maker brands that are still
# quite common, but have proprietary command sets not blessed by ANSI.

#### Altos
#
# Altos descriptions from Ted Mittelstaedt <tedm@agora.rain.com> 4 Sep 1993
# His comments suggest they were shipped with the system.
#

# (altos2: had unknown capabilities
#	:c0=^A`\r:c1=^Aa\r:c2=^Ab\r:c3=^Ac\r:\
#	:c4=^Ad\r:c5=^Ae\r:c6=^Af\r:c7=^Ag\r:\
#	:c8=^Ah\r:c9=^Ai\r:cA=^Aj\r:cB=^Ak\r:\
#	:cC=^Al\r:cD=^Am\r:cE=^An\r:cF=^Ao\r:
#	:XU=^Aq\r:XD=^Ar\r:XR=^As\r:XL=^At\r:\
#	:YU=^AQ\r:YD=^AR\r:YR=^AS\r:YL=^AT\r:\
#	:HL=^AP\r:SP=\E[i:\
#	:IS=\E[@:DE=\E[P:IL=\E[L:NS=\E[S:PS=\E[T:\
#	:LO=\E[0q:LC=\E[5q:LL=\E[6q:\
# Comparison with the k* capabilities makes it obvious that the c* things are
# shift keys.  I have renamed them to keys 32 and up accordingly.  Also,
# :sr: was given as a boolean-- esr)
altos2|alt2|altos-2|altos II:\
	:co#80:it#8:li#24:sg#0:\
	:*5=^Am\r:*8=^An\r:DL=\E[M:FM=^A`\r:FN=^Aa\r:\
	:FO=^Ab\r:FP=^Ac\r:FQ=^Ad\r:FR=^Ae\r:FS=^Af\r:\
	:FT=^Ag\r:FU=^Ah\r:FV=^Ai\r:FW=^Aj\r:FX=^Ak\r:\
	:al=\E[L:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:do=\E[1B:ei=:ho=\E[H:\
	:ic=\E[@:if=/usr/share/lib/tabset/vt100:im=:\
	:is=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=^AJ\r:\
	:kB=^AK\r:kC=^AL\r:kD=^AM\r:kE=^AN\r:kF=^AO\r:kb=^H:\
	:kd=\E[B:kh=\E[f:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:nd=\E[1C:nw=^M^J:se=\E[m:sf=^J:so=\E[7m:ta=^I:\
	:ue=\E[m:up=\E[1A:us=\E[4m:
# (altos3: had unknown capabilities
#	:c0=^A`\r:c1=^Aa\r:c2=^Ab\r:c3=^Ac\r:\
#	:c4=^Ad\r:c5=^Ae\r:c6=^Af\r:c7=^Ag\r:\
#	:c8=^Ah\r:c9=^Ai\r:cA=^Aj\r:cB=^Ak\r:\
#	:cC=^Al\r:cD=^Am\r:cE=^An\r:cF=^Ao\r:
#	:XU=^Aq\r:XD=^Ar\r:XR=^As\r:XL=^At\r:\
#	:HL=^AP\r:SP=\E[i:\
#	:IS=\E[@:DE=\E[P:IL=\E[L:NS=\E[S:PS=\E[T:\
# Comparison with the k* capabilities makes it obvious that the c* things are
# shift keys.  I have renamed them to keys 32 and up accordingly -- esr)
altos3|alt3|altos-3|altos III:\
	:co#80:it#8:li#24:sg#0:\
	:*5=^Am\r:*8=^An\r:DL=\E[M:FM=^A`\r:FN=^Aa\r:\
	:FO=^Ab\r:FP=^Ac\r:FQ=^Ad\r:FR=^Ae\r:FS=^Af\r:\
	:FT=^Ag\r:FU=^Ah\r:FV=^Ai\r:FW=^Aj\r:FX=^Ak\r:\
	:al=\E[L:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:do=\E[1B:ei=:ho=\E[H:\
	:ic=\E[@:if=/usr/share/lib/tabset/vt100:im=:\
	:is=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=^AJ\r:\
	:kB=^AK\r:kC=^AL\r:kD=^AM\r:kE=^AN\r:kF=^AO\r:kb=^H:\
	:kd=\E[B:kh=\E[f:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:mb=\E[5p:me=\E[p:nd=\E[1C:nw=^M^J:se=\E[m:sf=^J:\
	:so=\E[7m:sr=\EM:ta=^I:ue=\E[m:up=\E[1A:us=\E[4m:
altos4|alt4|altos-4|altos IV:\
	:tc=wy50:
altos5|alt5|altos-5|altos V:\
	:tc=altos3:
# (altos7: had unknown capabilities:
#	:GG#0:GS=\EH^B:GE=\EH^C:\
#	:G1=3:G2=2:G3=1:G4=5:GD=0:GU==:GH=\072:\
#	:GV=6:GR=4:GL=9:GC=8:GI=\EH8:GF=\EH7:\
#	:c0=^A`\r:c1=^Aa\r:c2=^Ab\r:c3=^Ac\r:\
#	:c4=^Ad\r:c5=^Ae\r:c6=^Af\r:c7=^Ag\r:\
#	:c8=^Ah\r:c9=^Ai\r:cA=^Aj\r:cB=^Ak\r:\
#	:cC=^Al\r:cD=^Am\r:cE=^An\r:cF=^Ao\r:
#	:PD=\EK:PU=\EJ:PN=\Ed#:PS=\EJ:DL=\ER:\
# Comparison with the k* capabilities makes it obvious that the c* things are
# shift keys.  I have renamed them to keys 32 and up accordingly -- esr)
altos7|alt7|altos VII:\
	:am:mi:\
	:co#80:li#24:sg#0:\
	:*5=^Am\r:*8=^An\r:DL=\ER:FM=^A`\r:FN=^Aa\r:FO=^Ab\r:\
	:FP=^Ac\r:FQ=^Ad\r:FR=^Ae\r:FS=^Af\r:FT=^Ag\r:\
	:FU=^Ah\r:FV=^Ai\r:FW=^Aj\r:FX=^Ak\r:al=\EE:cd=\EY:\
	:ce=\ET:cl=\E+^^:cm=\E=%+ %+ :cr=^M:dc=\EW:do=^J:\
	:ei=\Er:ho=^^:im=\Eq:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Eu\E~2:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=^AJ\r:\
	:kB=^AK\r:kC=^AL\r:kD=^AM\r:kE=^AN\r:kF=^AO\r:kb=^H:\
	:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:mb=\EG2:md=\EGt:\
	:me=\EG0:mh=\EGp:mk=\EG1:mr=\EG4:nd=^L:nw=^M^J:\
	:se=\EG0:sf=^J:so=\EG4:sr=\Ej:ta=^I:ue=\EG0:up=^K:\
	:us=\EG8:
altos7pc|alt7pc|altos PC VII:\
	:@7=\ET:tc=altos7:

#### Hewlett-Packard (hp)
#
#	Hewlett-Packard
#	8000 Foothills Blvd 
#	Roseville, CA 95747
#	Vox: 1-(916)-785-4363	(Technical response line for VDTs)
#	     1-(800)-633-3600	(General customer support)
#

# Generic HP terminal - this should (hopefully) work on any HP terminal.
hpgeneric|hewlett-packar|hewlettpackard:\
	:am:da:db:mi:xs:\
	:co#80:li#24:lm#0:vt#6:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EK:ch=\E&a%dC:cl=\EH\EJ:\
	:cm=\E&a%r%dc%dY:cr=^M:ct=\E3:cv=\E&a%dY:dc=\EP:\
	:dl=\EM:do=^J:ei=\ER:im=\EQ:kB=\Ei:kb=^H:le=^H:\
	:nd=\EC:se=\E&d@:sf=^J:so=\E&dJ:st=\E1:ta=^I:\
	:ue=\E&d@:up=\EA:us=\E&dD:

hp110|hewlett-packard model 110 portable:\
	:li#16:\
	:tc=hpgeneric:

hp+pfk+cr|hp function keys with CR:\
	:k1=\Ep\r:k2=\Eq\r:k3=\Er\r:k4=\Es\r:k5=\Et\r:\
	:k6=\Eu\r:k7=\Ev\r:k8=\Ew\r:

hp+pfk-cr|hp function keys w/o CR:\
	:k1=\Ep:k2=\Eq:k3=\Er:k4=\Es:k5=\Et:k6=\Eu:k7=\Ev:\
	:k8=\Ew:

# The 2621s use the same keys for the arrows and function keys, 
# but not separate escape sequences. These definitions allow the 
# user to use those keys as arrow keys rather than as function 
# keys.
hp+pfk+arrows|hp alternate arrow definitions:\
	:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:kF=\Er\r:kH=\Eq\r:\
	:kR=\Es\r:kd=\Ew\r:kh=\Ep\r:kl=\Eu\r:kr=\Ev\r:\
	:ku=\Et\r:

hp+arrows|hp arrow definitions:\
	:kF=\ES:kH=\EF:kR=\ET:kd=\EB:kh=\Eh:kl=\ED:kr=\EC:\
	:ku=\EA:

# Generic stuff from the HP 262x series
#
hp262x:\
	:xs:\
	:cd=\EJ:dc=\EP:ip=:kA=\EL:kD=\EP:kE=\EK:kF=\ES:\
	:kI=\EQ:kL=\EM:kM=\ER:kN=\EU:kP=\EV:kR=\ET:kS=\EJ:\
	:kd=\EB:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:ks=\E&s1A:\
	:ku=\EA:mb=\E&dA:me=\E&d@:mk=\E&dS:mr=\E&dB:\
	:..sa=\E&d%'@'%?%p1%t%'B'%|%;%?%p2%t%'D'%|%;%?%p3%t%'B'%|%;%?%p4%t%'A'%|%;%c:\
	:se=\E&d@:sf=\ES:so=\E&dB:ta=\011:ue=\E&d@:us=\E&dD:
# Note: no "home" on HP's since that homes to top of memory, not screen.
# Due to severe 2621 braindamage, the only way to get the arrow keys to
# transmit anything at all is to turn on the function key labels
# with smkx, and even then the user has to hold down shift!
# The default 2621 turns off the labels except when it has to to 
# enable the function keys. If your installation prefers labels 
# on all the time, or off all the time (at the "expense" of the 
# function keys) move the # 2621-nl or 2621-wl labels to the 
# front using reorder.
# Note: there are newer ROMs for 2621's that allow you to set 
# strap A so the regular arrow keys xmit \EA, etc, as with the 
# 2645. However, even with this strap set, the terminal stops 
# xmitting if you reset it, until you unset and reset the strap!
# Since there is no way to set/unset the strap with an escape 
# sequence, we don't use it in the default.
# If you like, you can use 2621-ba (braindmaged arrow keys).
hp2621-ba|2621-ba|2621 w/new rom and strap A set:\
	:ke@:ks@:tc=hp+arrows:tc=hp2621:

# 2621 with function labels. Most of the time they are off,
# but inside vi, the function key labels appear. You have to
# hold down shift to get them to xmit.
hp2621|hp2621a|hp2621A|2621|2621a|2621A|hp2621-wl|2621-wl|hp 2621 w/labels:\
	:is=\E&jA\r:ke=\E&jA:tc=hp2621-fl:

# 2621 with function labels.  Most of the time they are off,
# but inside vi, the function key labels appear.  You have to
# hold down shift to get them to xmit.
hp2621-fl|2621-fl|hp 2621:\
	:xo:xs@:\
	:pb#19200:\
	:bt=\Ei:cm=\E&a%r%dc%dY:dc=\EP:ip=:is=\E&j@\r:\
	:ke=\E&j@:ks=\E&jB:me=\E&d@:se=\E&d@:so=\E&dD:\
	:ta=\011:ue=\E&d@:us=\E&dD:tc=hp+pfk+cr:tc=hpgeneric:

# To use 2621p printer, setenv TERM=2621p, PRINTER=2612p
hp2621p|2621p|2621P|hp 2621 with printer:\
	:pf=\E&p13C:po=\E&p11C:tc=hp2621:

hp2621p-a|2621p-a|hp2621p with fn as arrows:\
	:tc=hp+pfk+arrows:tc=hp2621p:

# hp2621 with k45 keyboard
hp2621-k45|hp2621k45|2621k45|k45|hp 2621 with 45 keyboard:\
	:kb=^H:kd=\EB:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:\
	:ks=\E&s1A:ku=\EA:tc=hp2621:

# This terminal should be used at 4800 baud or less. It needs padding for
# plain characters at 9600, I guessed at an appropriate cr delay.  It really
# wants ^E/^F handshaking, but that doesn't work well even if you write
# software to support it.
hp2645|hp45|hp 264x series:\
	:pb#9600:\
	:cr=\r:kA=\EL:kD=\EP:kE=\EK:kF=\ES:kI=\EQ:kL=\EM:\
	:kM=\ER:kN=\EU:kP=\EV:kR=\ET:kS=\EJ:kT=\E1:kd=\EB:\
	:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:ks=\E&s1A:kt=\E2:\
	:ku=\EA:mb=\E&dA:me=\E&d@:mh=\E&dH:mr=\E&dB:\
	:..sa=\E&d%'@'%?%p1%t%'B'%|%;%?%p2%t%'D'%|%;%?%p3%t%'B'%|%;%?%p4%t%'A'%|%;%?%p5%t%'H'%|%;%?%p6%t%'B'%|%;%c:\
	:us=\E&dD:tc=hpgeneric:

# Hp 2624 B with 4 or 10 pages of memory.
# 
# Some assumptions are made with this entry. These settings are 
# NOT set up by the initialization strings.
# 
# Port Configuration
# 	RecvPace=Xon/Xoff
# 	XmitPace=Xon/Xoff
# 	StripNulDel=Yes
# 
# Terminal Configuration
# 	InhHndShk=Yes
# 	InhDC2=Yes
# 	XmitFnctn(A)=No
# 	InhEolWrp=No
# 
# Note: the 2624 DOES have a true "home," believe it or not!
# 
# The 2624 has an "error line" to which messages can be sent. 
# This is CLOSE to what is expected for a "status line". However,
# after a message is sent to the "error line", the next carriage 
# return is EATEN and the "error line" is turned back off again! 
# So I guess we can't define hs, eslok, wsl, dsl, fsl, tsl
# 
# This entry supports emacs (and any other program that uses raw 
# mode) at 4800 baud and less. I couldn't get the padding right 
# for 9.6.
#
hp2624|hp2624a|hp2624b|hp2624b-4p|2624-4p|2624|2624a|2624b|Hewlett Packard 2624 B:\
	:da:db:\
	:lm#96:\
	:vb=\E&w13F\200\200\200\200\E&w12F\200\200\200\200\E&w13F\200\200\200\200\E&w12F:tc=hp+labels:tc=scrhp:

# These attributes are not set above:
# 
# civis, cmdch, cnorm, csr, cub, cud, cuf, cuu, cvvis, dch, dl, 
# ech, eo, eslok, fsl, gn, hc, hd, hu, hz, ich, ich1, if, il, in,
# indn, iprog, is2, is3, it, ka1, ka3, kb2, kc1, kc3, kclr, kf0, 
# kf10, khts, km, ktbc, lf0, lf1, lf10, lf2, lf3, lf4, lf5, lf6, 
# lf7, lf8, lf9, mc5p, os, pad, pfkey*, pfloc*, pfx*, prot, rc, 
# rep, rin, rmcup, rmdc, rmm, rs2, rs3, sc, smcup, smdc, smm, tsl,
# uc, ul, vt, wind, wsl, xenl, xmc, xsb, xt
# 
# not needed if tset is used:
# 	if=/usr/lib/tabset/std,
# 
# This hp2626 entry does not use any of the fancy windowing stuff 
# of the 2626.
# 
# Indeed, terminfo does not yet handle such stuff. Since changing 
# any window clears memory, it is probably not possible to use 
# this for screen opt.
# 
# ed is incredibly slow most of the time - I am guessing at the 
# exact padding. Since the terminal uses xoff/xon this is intended 
# only for cost computation, so that the terminal will prefer el 
# or even dl1 which is probably faster!
# 
# \ED\EJ\EC hack for ed from Ed Bradford - apparently ed is only 
# extra slow # on the last line of the window. 
# 
# The padding probably should be changed.
#
hp2626|hp2626a|hp2626p|2626|2626a|2626p|2626A|2626P|hp 2626:\
	:da:db:\
	:lm#0:pb#19200:\
	:SF=\E&r%dD:SR=\E&r%dU:cd=\ED\EJ\EC:ip=:is=\E&j@\r:tc=hp+pfk+cr:tc=hp+labels:tc=scrhp:

# This entry is for sysline. It allocates a 23 line window with 
# a 115 line workspace for regular use, and a 1 line window for 
# the status line.
# 
# This assumes port 2 is being used.
# Turn off horizontal line, Create ws #1 with 115 lines,
# Create ws #2 with 1 line, Create window #1 lines 1-23,
# Create window #2 lines 24-24, Attach cursor to workspace #1.
# Note that this clears the tabs so it must be done by tset before
# it sets the tabs.
#
hp2626-s|2626-s|hp 2626 using only 23 lines:\
	:es:hs:\
	:li#23:\
	:fs=\E&d@\E&w7f2p1I\E&w4f1I:\
	:i1=\E&q3t0{0H \E&w0f115n1I \E&w0f1n2I\n\E&w2f1i0d0u22l0S \E&w2f2i0d23u23l0S \E&w7f2p1I \r:\
	:ts=\E&w7f2p2I\E&w4f2I\r\EK\E&a%p1%dC:tc=hp2626:
# Force terminal back to 24 lines after being 23.
#
hp2626-ns|2626-ns|hp 2626 using all 24 lines:\
	:i1=\E&q3t0{0H \E&w0f118n1I \E&w0f1n2I\n\E&w2f1i0d0u23l0S \E&w3f2I \E&w7f2p1I \r:tc=hp2626:
# Various entries useful for small windows on 2626.
#
hp2626-12|2626-12:\
	:li#12:\
	:tc=hp2626:
hp2626-12x40|2626-12x40:\
	:co#40:li#12:\
	:tc=hp2626:
hp2626-x40|2626-x40:\
	:co#40:\
	:tc=hp2626:
hp2626-12-s|2626-12-s:\
	:li#11:\
	:tc=hp2626-s:
# You should use this terminal at 4800 baud or less.
#
hp2648|hp2648a|2648a|2648A|2648|HP 2648a graphics terminal:\
	:cl=\EH\EJ:cm=\E&a%r%dc%dY:dc=\EP:ip=:tc=hp2645:

# 2640a doesn't have the Y cursor addressing feature, and C is 
# memory relative instead of screen relative, as we need.
#
hp2640a|2640a|hp 2640a:\
	:cm@:ke@:ks@:tc=hp2645:

hp2640b|hp2644a|hp 264x series:\
	:ke@:ks@:tc=hp2645:

# 2621 using all 48 lines of memory, only 24 visible at any time.  
#
hp2621-48|48 line 2621:\
	:li#48:\
	:cm=\E&a%r%dc%dR:cv=\E&a%dR:ho=\EH:tc=hp2621:

# 2621 with no labels ever. Also prevents vi delays on escape.
#
hp2621-nl|hp 2621 with no labels:\
	:kd@:ke@:kh@:kl@:kr@:ks@:ku@:tc=hp2621-fl:

# Needed for UCB ARPAVAX console, since lsi-11 expands tabs 
# (wrong).
#
hp2621-nt|hp 2621 w/no tabs:\
	:ta@:tc=hp2621:

# The HP 150 terminal is a fairly vanilla HP terminal, with the 
# clreol standout problem. It also has graphics capabilities and 
# a touch screen, which we don't describe here.
hp150|hewlett packard Model 150:\
	:tc=hp2622:

# Hp 2382a terminals, "the little ones." They don't have any 
# alternate character set support and sending out ^N/^O will 
# leave the screen blank.
hp2382a|hp2382|hewlett packard 2382a:\
	:da:db:\
	:lh#1:lm#48:\
	:ac@:ae@:as@:me=\E&d@:\
	:..pn=\E&f0a%p1%dk%p2%l%Pa%?%ga%t%ga%d%e1%;d0L%?%ga%!%t %;%p2%s:\
	:..sa=\E&d%{0}%Pa%?%p4%t%{1}%ga%+%Pa%;%?%p1%p3%|%p6%|%t%{2}%ga%+%Pa%;%?%p2%p6%|%t%{4}%ga%+%Pa%;%?%p1%p5%|%t%{8}%ga%+%Pa%;%?%p7%t%?%ga%ts%ga%'@'%+%e%'S'%;%e%?%ga%t%ga%'@'%+%e%'@'%;%;%c:tc=hp+labels:tc=scrhp:

hp2621-a|hp2621a-a|2621-a|hp2621 with fn as arrows:\
	:tc=hp+pfk+arrows:tc=hp2621-fl:

# newer hewlett packard terminals

newhpkeyboard|generic entry for HP extended keyboard:\
	:kA=\EL:kB=\Ei:kC=\EJ:kD=\EP:kE=\EK:kF=\ET:kH=\EF:\
	:kI=\EQ:kL=\EM:kM=\ER:kN=\EU:kP=\EV:kR=\ES:kS=\EJ:\
	:kb=^H:kd=\EB:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:\
	:ks=\E&s1A:ku=\EA:tc=hp+pfk-cr:

newhp|generic entry for new hewlett packard terminals:\
	:am:bw:mi:xo:xs:\
	:co#80:li#24:pb#4800:\
	:ac=T1R!U2S"W3O#V4P$t5u6w7v8\072'9(LQKWlRkT5I3@2[MAJSmFjGdHQ;Y+Z*X\0724>q\\\054x.n/:\
	:ae=^O:al=\EL:as=^N:bl=^G:bt=\Ei:cd=\EJ:ce=\EK:cr=^M:\
	:ct=\E3:dc=\EP:dl=\EM:do=^J:ei=\ER:i1=\E&jB:im=\EQ:\
	:ip=:le=^H:mb=\E&dA:md=\E&dF:me=\E&d@\017:mh=\E&dH:\
	:mk=\E&dS:mr=\E&dB:nd=\EC:nw=^M^J:\
	:..pk=\E&f0a%p1%dk0d%p2%l%dL%p2%s:\
	:..pl=\E&f1a%p1%dk0d%p2%l%dL%p2%s:\
	:..px=\E&f2a%p1%dk0d%p2%l%dL%p2%s:r1=\Eg:\
	:..sa=\E&d%{0}%Pa%?%p4%t%{1}%ga%+%Pa%;%?%p1%p3%|%p6%|%t%{2}%ga%+%Pa%;%?%p2%p6%|%t%{4}%ga%+%Pa%;%?%p1%p5%|%t%{8}%ga%+%Pa%;%?%p7%t%?%ga%ts%ga%'@'%+%e%'S'%;%e%?%ga%t%ga%'@'%+%e%'@'%;%;%c%?%p9%t\016%e\017%;:\
	:se=\E&d@:sf=^J:so=\E&dJ:sr=\ET:st=\E1:ta=\011:\
	:ue=\E&d@:up=\EA:us=\E&dD:tc=newhpkeyboard:

memhp|memory relative addressing for new HP ttys:\
	:vt#6:\
	:CM=\E&a%p1%dr%p2%dC:DO=\E&a+%dR:LE=\E&a-%dC:\
	:RI=\E&a+%dC:UP=\E&a-%dR:ch=\E&a%dC:cl=\EH\EJ:\
	:cm=\E&a%dr%dC:cv=\E&a%dR:ho=\EH:ll=\E&a23R\r:tc=newhp:

scrhp|screen relative addressing for new HP ttys:\
	:CM=\E&a%p1%dr%p2%dC:DO=\E&a+%dR:LE=\E&a-%dC:\
	:RI=\E&a+%dC:UP=\E&a-%dR:ch=\E&a%dC:cl=\E&a0c0Y\EJ:\
	:cm=\E&a%dy%dC:cv=\E&a%dY:ho=\E&a0y0C:ll=\E&a0y0C\EA:tc=newhp:

hp+labels|"standard" label info for new HP ttys:\
	:Nl#8:lh#2:lw#8:\
	:LO=\E&jB:\
	:..pn=\E&f2a%p1%dk%p2%l%Pa%?%ga%t%ga%d%e1%;d0L%?%ga%!%t %;%p2%s:

hp+printer| "standard" printer info for HP ttys:\
	:ff=\E&p4u0C:pf=\E&p13C:po=\E&p11C:ps=\EH\E&p4dF:


# The new hp2621b is kind of a cross between the old 2621 and the
# new 262x series of machines. It has dip-switched options. 
# The firmware has a bug in it such that if you give it a null 
# length label, the following character is eaten!
hp2621b|2621b|hp 2621b with old style keyboard:\
	:Nl#8:lh#1:lm#48:lw#8:\
	:LO=\E&jB:kF=\ET:kH=\EF:kR=\ES:kd=\EB:kh=\Eh:kl=\ED:\
	:kr=\EC:ku=\EA:\
	:..pn=\E&f0a%p1%dk%p2%l%Pa%?%ga%t%ga%d%e1%;d3L%?%ga%!%t%{32}%c%;%p2%s\E%'o'%p1%+%c\r:tc=hp2621:

hp2621b-p|2621b-p|hp 2621b with printer:\
	:tc=hp+printer:tc=hp2621b:

# hp2621b - new 2621b with new extended keyboard
# these are closer to the new 26xx series than the other 2621b
hp2621b-kx|2621b-kx|hp 2621b with extended keyboard:\
	:tc=newhpkeyboard:tc=hp2621b:

hp2621b-kx-p|2621b-kx-p|hp 2621b with new keyboard & printer:\
	:tc=hp+printer:tc=hp2621b-kx:

# Some assumptions are made in the following entries.
# These settings are NOT set up by the initialization strings.
# 
#    Port Configuration
# RecvPace=Xon/Xoff	XmitPace=Xon/Xoff	StripNulDel=Yes
# 
#    Terminal Configuration
# InhHndShk(G)=Yes	InhDC2(H)=Yes
# XmitFnctn(A)=No		InhEolWrp=No
#
# 
# Hp 2622a & hp2623a display and graphics terminals
#
hp2622|hp2622a|2622|2622a|hp 2622:\
	:da:db:\
	:lm#0:pb#19200:\
	:is=\E&dj@\r:tc=hp+pfk+cr:tc=hp+labels:tc=scrhp:

# The 2623 is a 2622 with extra graphics hardware.
hp2623|hp2623a|2623|2623a|hp 2623:\
	:tc=hp2622:


hp2624b-p|hp2624b-4p-p|hewlett packard 2624 B with printer:\
	:tc=hp+printer:tc=hp2624:

# The hewlett packard B can have an optional extra 6 pages of 
# memory.
hp2624-10p|hp2624a-10p|hp2624b-10p|2624-10p|2624a-10p|2624b-10p|hewlett packard 2624 B w/ 10 pages of memory:\
	:lm#240:\
	:tc=hp2624:

hp2624b-10p-p|hewlett packard 2624 B w/ extra memory & printer:\
	:lm#240:\
	:tc=hp2624b-p:

# Color manipulations for HP terminals

hp+color|hp with colors:\
	:cc:\
	:Co#16:NC#17:pa#7:\
	:..Ip=\E&v%?%p2%{1000}%=%t1%e.%p2%d%;a\n%?%p3%{1000}%=%t1%e.%p3%d%;b\n%?%p4%{1000}%=%t1%e.%p4%d%;c\n%?%p5%{1000}%=%t1%e.%p5%d%;x\n%?%p6%{1000}%=%t1%e.%p6%d%;y\n%?%p7%{1000}%=%t1%e.%p7%d%;z\n%p1%dI:\
	:oc=\E&v0m1a1b1c0I\E&v1a1I\E&v1b2I\E&v1a1b3I\E&v1c4I\E&v1a1c5I\E&v1b1c6I\E&v1x1y7I:\
	:op=\E&v0S:sp=\E&v%dS:

# is2 set screen to be 80 columns wide
hp2397a|2397a|hp2397|2397|hewlett packard 2397A color terminal:\
	:is=\E&w6f80X:tc=memhp:tc=hp+labels:tc=hp+color:

#  HP 700/44 Setup parameters:  
# Terminal Mode		HP-PCterm
# Inhibit Auto Wrap	NO
# Status Line		Host Writable
# PC Character Set	YES
# Twenty-Five Line Mode	YES
# XON/XOFF		@128 or 64 (sc)
# Keycode Mode 		NO   or YES (sc)
# Backspace Key		BS or BS/DEL
#
# is2	sets pcterm; autowrap; 25 lines; pc char set; prog DEL key; \E\\?
# does not turn off keycode mode
# smsc	sets alternate start/stop; keycode on
#
hpansi|hp700|hewlett packard 700/44 in HP-PCterm mode:\
	:am:eo:xn:xo:\
	:co#80:li#25:\
	:@7=\E[4~:S4=\E[>11h\EPO**x0/65;1/67\E\\:\
	:S5=\E[>11l\EP1**x0/11;1/13\E[0m\E\\:XF=g:XN=e:\
	:ac=k\277l\332m\300j\331n\305w\302q\304u\264t\303v\301x\263:\
	:al=\E[L:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:cl=\E[2J\E[H:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:do=\E[B:ei=:\
	:ho=\E[H:ic=\E[@:im=:\
	:is=\E[44"p\E[?7h\E[>10h\E[>12h\EP1;1|3/7F\E\\:\
	:k1=\E[17~:k2=\E[18~:k3=\E[19~:k4=\E[20~:k5=\E[21~:\
	:k6=\E[23~:k7=\E[24~:k8=\E[25~:k9=\E[26~:k;=\E[28~:\
	:kB=\E[Z:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:kh=\E[1~:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=\E[D:nd=\E[C:se=\E[m:\
	:sf=^J:so=\E[7m:ta=^I:ue=\E[m:up=\E[A:us=\E[4m:\
	:ve=\E[?25h:vi=\E[?25l:
#
hp2392|2392|2393|239x series:\
	:co#80:\
	:bt=\Ei:cm=\E&a%dy%dC:cv=\E&a%dY:im=\EQ:k1=\Ep\r:\
	:k2=\Eq\r:k3=\Er\r:k4=\Es\r:k5=\Et\r:k6=\Eu\r:\
	:k7=\Ev\r:k8=\Ew\r:kF=\EU:kN=\Eu:kP=\Ev:kR=\EV:\
	:kh=\Eh:ue=\E&d@:us=\E&dD:tc=hpsub:

2392nam|hp2392nam|HP 239x series with no auto margins:\
	:am@:\
	:tc=hp2392:

hpsub|hp terminals -- capability subset:\
	:am:da:db:mi:xo:xs:\
	:li#24:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EK:ch=\E&a%dC:cl=\EH\EJ:\
	:cr=^M:dc=\EP:dl=\EM:do=\EB:ei=\ER:\
	:if=/usr/lib/tabset/stdcrt:is=\E&s1A\E<\E&k0\\:kb=^H:\
	:kd=\EB:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:ks=\E&s1A:\
	:ku=\EA:le=^H:nd=\EC:se=\E&d@:sf=^J:so=\E&dB:ta=^I:\
	:up=\EA:

# HP 236 console
# From: <ddavis@ic.berkeley.edu>
hp236|hp236 internal terminal emulator:\
	:am:bs:\
	:co#80:li#24:\
	:al=\EG:ce=\EK:cl=\EF:cm=\EE%+ %+ :dc=\EJ:dl=\EH:ei=:\
	:ic=\EI:im=:se=\ECI:so=\EBI:up=^K:ve=\EDE:vs=\EDB:

# This works on a hp300 console running Utah 4.3 BSD
# From: Craig Leres <leres@okeeffe.berkeley.edu>
hp300h|HP Catseye console:\
	:am:bs:da:db:mi:xs:\
	:co#128:li#51:lm#0:sg#0:\
	:al=\EL:bl=^G:bt=\Ei:cd=\EJ:ce=\EK:ch=\E&a%dC:\
	:cl=\E&a0y0C\EJ:cm=\E&a%dy%dC:cr=^M:ct=\E3:\
	:cv=\E&a%dY:dc=\EP:dl=\EM:do=\EB:ei=\ER:\
	:if=/usr/share/tabset/stdcrt:im=\EQ:kb=^H:kd=\EB:\
	:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:ks=\E&s1A:ku=\EA:\
	:le=^H:me=\E&d@:nd=\EC:se=\E&d@:sf=^J:so=\E&dB:ta=^I:\
	:ue=\E&d@:up=\EA:us=\E&dD:
# From: Greg Couch <gregc@ernie.berkeley.edu>
# (hp9837: removed obsolete ":ko=ce,cd,al,im,dl,dc:";
# mapped ":pt:" to ":it#8:" -- esr)
hp9837|hp98720|hp98721|HP 9000/300 workstations:\
	:am:bs:da:db:mi:pt:xs:\
	:co#128:it#8:li#46:lm#0:\
	:al=\EL:bl=^G:bt=\Ei:cd=\EJ:ce=\EK:ch=\E&a%dC:\
	:cl=\E&a0y0C\EJ:cm=\E&a%dy%dC:ct=\E3:cv=\E&a%dY:\
	:dc=\EP:dl=\EM:do=\EB:ei=\ER:im=\EQ:is=\E&v0m1b0i&j@:\
	:kN=\EU:kP=\EV:kb=^H:kd=\EB:ke=\E&s0A:kh=\Eh:kl=\ED:\
	:kr=\EC:ks=\E&s1A:ku=\EA:le=^H:me=\E&d@:nd=\EC:\
	:se=\E&v0S:sf=^J:so=\E&v5S:st=\E1:ue=\E&d@:up=\EA:\
	:us=\E&dD:
# From: Charles A. Finnell of MITRE <finnell@mitre.org>, developed 07SEP90
# (hp98550: removed obsolete ":kn#12:ko=al,cd,ce,ct,dc,dl,do,ei,im,nd,st,up:";
# mapped ":pt:" to ":it#8:" -- esr)
hp98550|hp98550a|HP 9000 Series 300 color console:\
	:am:bs:da:db:mi:pt:xs:\
	:co#128:it#8:li#49:lm#0:\
	:ae=^O:al=\EL:as=^N:bl=^G:bt=\Ei:cd=\EJ:ce=\EK:\
	:ch=\E&a%dC:cl=\EH\EJ:cm=\E&a%dy%dC:cr=^M:ct=\E3:\
	:cv=\E&a%dY:dc=\EP:dl=\EM:do=^J:ei=\ER:\
	:if=/usr/share/tabset/9837:im=\EQ:k1=\Ep:k2=\Eq:\
	:k3=\Er:k4=\Es:k5=\Et:k6=\Eu:k7=\Ev:k8=\Ew:kA=\EL:\
	:kC=\EJ:kD=\EP:kE=\EK:kF=\ES:kH=\EF:kI=\EQ:kL=\EM:\
	:kM=\ER:kN=\EU:kP=\EV:kR=\ET:kS=\EJ:kT=\E1:ka=\E3:\
	:kb=^H:kd=\EB:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:\
	:ks=\E&s1A:kt=\E2:ku=\EA:le=^H:mb=\E&dA:md=\E&dJ:\
	:me=\E&d@:mh=\E&dH:mk=\E&ds:mr=\E&dJ:nd=\EC:se=\E&d@:\
	:sf=^J:so=\E&dJ:st=\E1:ta=^I:ue=\E&d@:up=\EA:\
	:us=\E&dD:ve=\E*dQ:vi=\E*dR:
# From: Victor Duchovni <vic@fine.princeton.edu>
# (hp700-wy: removed obsolete ":ko=cl,ho,ce,bt,ta,im,ei,ce,cd:nl=^J:";
# mapped ":pt:" to ":it#8:" -- esr)
hp700-wy|HP700/41 emulating wyse30:\
	:am:bs:bw:mi:ms:pt:\
	:co#80:it#8:li#24:sg#1:ug#1:\
	:al=0.7*\EE:bl=^G:bt=\EI:cd=\EY:ce=10\ET:cl=^Z:\
	:cm=\E=%+ %+ :cr=^M:ct=\E0:cv=\E[%+ :dc=\EW:dl=\ER:\
	:do=^V:ei=\Er:ho=^^:if=/usr/share/tabset/hp700-wy:\
	:im=\Eq:is=\E~"\EC\Er\E(\EG0\003\E`9\E`1:kb=\177:\
	:kd=^V:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:ll=^^^K:nd=^L:\
	:rs=\E~"\EC\Er\E(\EG0\003\E`9\E`1:se=10\EG0:\
	:so=10\EG4:sr=\Ej:st=\E1:ue=10\EG0:up=^K:us=10\EG8:
hp70092|70092a|70092A|hp70092a|hp70092A|Hewlett-Packard 70092:\
	:am:da:db:xs:\
	:Nl#8:co#80:lh#2:li#24:lm#0:lw#8:\
	:LF=\E&j@:LO=\E&jB:ae=^O:al=\EL:as=^N:bl=^G:bt=\Ei:\
	:ce=\EK:ch=\E&a%dC:cl=\E&a0y0C\EJ:cm=\E&a%dy%dC:\
	:cr=^M:ct=\E3:cv=\E&a%dY:dc=\EP:dl=\EM:do=\EB:ei=\ER:\
	:im=\EQ:k1=\Ep:k2=\Eq:k3=\Er:k4=\Es:k5=\Et:k6=\Eu:\
	:k7=\Ev:k8=\Ew:kA=\EL:kC=\EJ:kD=\EP:kE=\EK:kF=\ES:\
	:kH=\EF:kI=\EQ:kL=\EM:kM=\ER:kN=\EU:kP=\EV:kR=\ET:\
	:kS=\EJ:kT=\E1:ka=\E3:kb=^H:kd=\EB:ke=\E&s0A:kh=\Eh:\
	:kl=\ED:kr=\EC:ks=\E&s1A:kt=\E2:ku=\EA:le=^H:\
	:mb=\E&dA:md=\E&dB:me=\E&d@:mh=\E&dH:mr=\E&dB:nd=\EC:\
	:se=\E&d@:so=\E&dJ:sr=\ET:st=\E1:ta=^I:ue=\E&d@:\
	:up=\EA:us=\E&dD:

bobcat|sbobcat|HP 9000 model 300 console:\
	:am:da:db:mi:xs:\
	:co#128:it#8:li#47:sg#0:\
	:al=10*\EL:bt=\Ei:cd=\EJ:ce=\EK:ch=6\E&a%dC:\
	:cl=\EH\EJ:cm=6\E&a%dy%dC:cr=^M:cv=6\E&a%dY:dc=\EP:\
	:dl=10*\EM:do=\EB:ei=\ER:im=\EQ:kb=^H:kd=\EB:\
	:ke=\E&s0A:kh=\Eh:kl=\ED:kr=\EC:ks=\E&s1A:ku=\EA:\
	:le=^H:nd=\EC:nw=^M^J:se=\E&d@:sf=^J:so=\E&dB:ta=^I:\
	:ue=\E&d@:up=\EA:us=\E&dD:
gator-t|HP 9000 model 237 emulating extra-tall AAA:\
	:bw:km:mi:ul:\
	:co#128:it#8:li#94:\
	:AL=1*\E[%dL:DC=4\E[%dP:DL=1*\E[%dM:IC=4\E[%d@:\
	:al=\E[L:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:ch=\E[%i%d`:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:\
	:do=^J:ei=:ho=\E[H:ic=\E[@:im=:kb=^H:kd=^J:kl=^H:\
	:le=^H:me=\E[m:mr=\E[7m:nd=\E[C:nw=^M^J:\
	:..rp=%.\E[%db:se=\E[m:so=\E[7m:ta=^I:ue=\E[m:up=\EM:\
	:us=\E[4m:
gator|HP 9000 model 237 emulating AAA:\
	:bw:km:mi:ul:\
	:co#128:it#8:li#47:\
	:AL=1*\E[%dL:DC=4\E[%dP:DL=1*\E[%dM:IC=4\E[%d@:\
	:al=\E[L:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:ch=\E[%i%d`:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:\
	:do=^J:ei=:ho=\E[H:ic=\E[@:im=:kb=^H:kd=^J:kl=^H:\
	:le=^H:me=\E[m:mr=\E[7m:nd=\E[C:nw=^M^J:\
	:..rp=%.\E[%db:se=\E[m:so=\E[7m:ta=^I:ue=\E[m:up=\EM:\
	:us=\E[4m:
gator-52|HP 9000 model 237 emulating VT52:\
	:co#128:it#8:li#47:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:..cm=\EY%+ %+ :cr=^M:\
	:do=^J:ho=\EH:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:\
	:le=^H:nd=\EC:nw=^M^J:sr=\EI:ta=^I:up=\EA:
gator-52t|HP 9000 model 237 emulating extra-tall VT52:\
	:co#128:it#8:li#94:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:..cm=\EY%+ %+ :cr=^M:\
	:do=^J:ho=\EH:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:\
	:le=^H:nd=\EC:nw=^M^J:sr=\EI:ta=^I:up=\EA:

#### Honeywell-Bull
#
# From: Michael Haardt <michael@gandalf.moria> 11 Jan 93
#

# Honeywell Bull terminal.  Its cursor and function keys send single
# control characters and it has standout/underline glitch.  Most programs
# do not like these features/bugs.  This is a dumb mode for this terminal.
# Visual bell is realized by flashing the "keyboard locked" LED.
dku7003-dumb|Honeywell Bull DKU 7003, dumb mode:\
	:co#80:li#25:\
	:cd=^_:ce=\E[K:cl=^]^_:cm=\E[%i%d;%dH:cr=^M:do=^K:\
	:ho=^]:kb=^H:kd=^K:kh=^]:kl=^Y:kr=^X:ku=^Z:le=^Y:\
	:nd=^X:nw=^M^J:sf=^J:ta=^I:up=^Z:vb=\E[2h\E[2l:
# Honeywell Bull terminal.  Its cursor and function keys send single
# control characters and it has standout/underline glitch.  Most programs
# do not like these features/bugs.  The following entry may cause problems
# with some programs.  Visual bell is realized by flashing the "keyboard 
# locked" LED.
dku7003|Honeywell Bull DKU 7003, all features described:\
	:ms:\
	:co#80:li#25:sg#1:ug#1:\
	:cd=^_:ce=\E[K:cl=^]^_:cm=\E[%i%d;%dH:cr=^M:do=^K:\
	:ho=^]:kb=^H:kd=^K:kh=^]:kl=^Y:kr=^X:ku=^Z:le=^Y:\
	:mb=\E[5m:md=\E[7m:me=\E[0m:mh=\E[2m:mr=\E[7m:nd=^X:\
	:nw=^M^J:se=\E[0m:sf=^J:so=\E[7m:ta=^I:ue=\E[0m:\
	:up=^Z:us=\E[4m:vb=\E[2h\E[2l:

#### Lear-Siegler (adm)
#
# These guys are long since out of the terminals business, but
# in 1995 many current terminals still have an adm type as one of their
# emulations (usually their stupidest, and usually labelled adm3, though
# these `adm3' emulations normally have adm3a+ capabilities).
#

adm1a|adm1|lsi adm1a:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cl=\E;:cm=\E=%+ %+ :cr=^M:do=^J:ho=^^:le=^H:\
	:nd=^L:sf=^J:up=^K:
adm2|lsi adm2:\
	:am:bs:\
	:co#80:li#24:\
	:al=\EE:bl=^G:cd=\EY:ce=\ET:cl=\E;:cm=\E=%+ %+ :\
	:cr=^M:dc=\EW:dl=\ER:do=^J:ei=:ho=^^:ic=\EQ:im=:\
	:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:sf=^J:\
	:up=^K:
# (adm3: removed obsolete ":ma=^K^P:" -- esr)
adm3|lsi adm3:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cl=^Z:cr=^M:do=^J:le=^H:sf=^J:
# The following ADM-3A switch settings are assumed for normal operation:
#	SPACE		U/L_DISP	CLR_SCRN	24_LINE
#	CUR_CTL		LC_EN		AUTO_NL		FDX
# Other switches may be set for operator convenience or communication
# requirements.  I recommend
#	DISABLE_KB_LOCK	LOCAL_OFF	103		202_OFF
#	ETX_OFF		EOT_OFF
# (adm3a: removed obsolete ":ma=^K^P:" -- esr)
adm3a|lsi adm3a:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cl=\032:cm=\E=%+ %+ :cr=^M:do=^J:ho=^^:le=^H:\
	:nd=^L:sf=^J:up=^K:
adm3a+|adm3aplus:\
	:kd=^J:kl=^H:kr=^L:ku=^K:tc=adm3a:
# (adm5: removed obsolete ":ma=^Hh^Jj^Kk^Ll^^H:" & duplicate ":do+^J:" -- esr)
adm5|lsi adm5:\
	:sg#1:\
	:bl=^G:cd=\EY:ce=\ET:cr=^M:do=^J:kb=^H:kh=^^:se=\EG:\
	:so=\EG:tc=adm3a+:
# From: <stephen%comp.lancs.ac.uk@ucl-cs.arpa>
# (adm11: removed obsolete ":ma=^Hh^Jj^Kk^Ll^^H:" -- esr)
adm11|lsi adm11:\
	:am:bs:hs:\
	:co#80:li#24:\
	:bl=^G:cd=\EY:ce=\ET:cl=^Z:cm=\E=%+ %+ :cr=^M:do=^J:\
	:ds=\Eh:fs=\E(\r:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:\
	:nd=^L:se=\E(:so=\E):ts=\EF\E):up=^K:
# From: Andrew Scott Beals <bandy@lll-crg.ARPA>
# Corrected by Olaf Siebert <rhialto@polder.ubc.kun.nl>, 11 May 1995
# (adm12: removed obsolete ":kn:ma=j^Jk^P^K^Pl ^R^L^L :" -- esr)
adm12|lsi adm12:\
	:am:bs:mi:\
	:co#80:li#24:\
	:al=\EE:bl=^G:cd=\EY:ce=\ET:cl=^Z:cm=\E=%+ %+ :cr=^M:\
	:dc=\EW:dl=\ER:do=^J:ei=\Er:ho=^^:im=\Eq:is=\Eq:\
	:k0=^A0\r:k1=^A1\r:k2=^A2\r:k3=^A3\r:k4=^A4\r:\
	:k5=^A5\r:k6=^A6\r:k7=^A7\r:k8=^A8\r:k9=^A9\r:kd=^J:\
	:kl=^H:kr=^L:ku=^K:le=^H:mk=\EG1:nd=^L:se=\EG0:\
	:so=\EG4:ue=\EG0:up=^K:us=\EG8:
# (adm20: removed obsolete ":kn#7:"; mapped ":pt:" to ":it#8:" -- esr)
adm20|lear siegler adm20:\
	:am:bs:pt:\
	:co#80:it#8:li#24:\
	:al=\EE:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=^Z:\
	:cm=\E=%i%r%+^_%+^_:cr=^M:dc=\EW:dl=\ER:ei=:ho=^^:\
	:ic=\EQ:im=:k1=^A:k2=^B:k3=^W:k4=^D:k5=^E:k6=^X:\
	:k7=^Z:nd=^L:se=\E(:so=\E):up=^K:
adm21|lear siegler adm21:\
	:sg#1:ug#1:\
	:al=30*\EE:bl=^G:cd=\EY:ce=\ET:cr=^M:dc=\EW:\
	:dl=30*\ER:do=^J:ei=:ic=\EQ:im=:kb=^H:kd=^J:kh=^^:\
	:kl=^H:kr=^L:ku=^K:se=\EG0:sf=^J:so=\EG4:ue=\EG0:\
	:us=\EG8:tc=adm3a:
# (adm22: ":em=:" was an obvious typo for ":ei=:"; also,
# removed obsolete ":kn#7:ko=ho:ma=j^Jk^P^K^Pl ^R^L^L :" -- esr)
adm22|lsi adm22:\
	:am:bs:\
	:co#80:li#24:\
	:al=\EE:bl=^G:bt=\EI:cd=\Ey:ce=\Et:cl=\E+:\
	:cm=\200\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=^J:ei=:\
	:ho=^^:ic=\EQ:im=:\
	:is=\E%\014\014\014\016\003\200\003\002\003\002\200\200\200\200\200\200\200\200\200\200\200:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:\
	:ku=^K:l1=F1:l2=F2:l3=F3:l4=F4:l5=F5:l6=F6:l7=F7:\
	:nd=^L:se=\E(:so=\E):ta=\Ei:up=^K:
# If the adm31 gives you trouble with standout mode, check the DIP switch in
# position 6, bank @c11, 25% from back end of the circuit board.  Should be
# OFF.  If there is no such switch, you have an old adm31 and must use oadm31.
# (adm31: removed obsolete ":ma=j^Jk^P^K^Pl ^R^L^L :" -- esr)
adm31|lsi adm31:\
	:am:bs:mi:\
	:co#80:li#24:\
	:al=\EE:bl=^G:cd=\EY:ce=\ET:cl=\E*:cm=\E=%+ %+ :\
	:cr=^M:dc=\EW:dl=\ER:do=^J:ei=\Er:ho=^^:im=\Eq:\
	:is=\Eu\E0:k0=^A0\r:k1=^A1\r:k2=^A2\r:k3=^A3\r:\
	:k4=^A4\r:k5=^A5\r:k6=^A6\r:k7=^A7\r:k8=^A8\r:\
	:k9=^A9\r:kd=^J:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:\
	:se=\EG0:sf=^J:so=\EG1:ue=\EG0:up=^K:us=\EG1:
oadm31|o31|old adm31:\
	:so=\EG4:ue@:us@:tc=adm31:
# ADM36 in native mode (not VT52 emulation mode)
adm36|lsi adm36:\
	:am:mi:\
	:co#80:li#24:\
	:al=\E[1L:cd=\E[0J:ce=\E[0K:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:dl=\E[1M:ei=\E[4l:im=\E[4h:\
	:is=\E[6;?7h\E[4;20;?1;?3;?6;?4l\E(B\E)B\E>:kd=\EB:\
	:kl=\ED:kr=\EC:ku=\E[A:le=^H:nd=\E[D:up=\E[A:
# (adm42: removed obsolete ":ma=^K^P:" -- esr)
adm42|lsi adm42:\
	:am:bs:\
	:co#80:li#24:\
	:al=\EE:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=\E;:\
	:cm=\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=^J:ei=\Er:\
	:im=\Eq:ip=:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:\
	:nd=^L:pc=\177:se=\EG0:sf=^J:so=\EG4:ta=^I:up=^K:\
	:vs=\EC\E3 \E3(:
# The following termcap for the Lear Siegler ADM-42 leaves the 
# "system line" at the bottom of the screen blank (for those who 
# find it distracting otherwise)
adm42-nl|lsi adm-42 with no system line:\
	:al=\EE\EF \011:bt=\EI\EF \011:cd=\EY\EF \011:\
	:ce=\ET\EF \011:cl=\E;\EF \011:cm=\E=%+ %+ \EF \011:\
	:dc=\EW\EF \011:dl=\ER\EF \011:ei=\Er\EF \011:\
	:im=\Eq\EF \011:tc=adm42:

#### Prime
#
# Yes, Prime makes terminals.  These entries were posted by Kevin J. Cummings
# <cummings@primerd.Prime.COM> on 14 Dec 1992 and lightly edited by esr.

pt100|pt200|wren|fenix|prime pt100/pt200:\
	:am:bw:mi:ms:\
	:co#80:it#8:li#24:\
	:DC=\E[%dP:DL=\E[M:DO=\E[%dB:LE=\E[%dD:RI=\E[%dC:\
	:UP=\E[%dA:al=\E[L\E[t:bt=\E[Z:cd=\E[J\E[r:\
	:ce=\E[K\E[t:cl=\E?:cm=\E0%+!%+!:cr=^M:dc=\E[P:\
	:do=\ED:ei=\E[4l:ho=\E$B:im=\E[4h:kb=^H:kd=\E[B:\
	:ke=\E[>13l:kh=\E$A:kl=\E[D:kr=\E[C:ks=\E[>13h:\
	:ku=\E[A:le=^H:nd=\E[C:nw=^M^J:se=\E[m:sf=^J:\
	:so=\E[2;7m:ta=^I:\
	:ti=\E[>1l\E[>2l\E[>16l\E[4l\E[>9l\E[20l\E[>3l\E[>7h\E[>12l\E[1Q:\
	:ue=\E[m:up=\EM:us=\E[4m:\
	:vb=\E$E\200\200\200\200\200\200\200\200\200\200\200\200\200\200\E$P:
pt100w|pt200w|wrenw|fenixw|prime pt100/pt200 in 132-column mode:\
	:co#132:\
	:cm=\E[%i%d;%dH:tc=pt100:
pt250|Prime PT250:\
	:so@:tc=pt100:
pt250w|Prime PT250 in 132-column mode:\
	:so@:tc=pt100w:

#### Qume (qvt)
#
#	Qume, Inc.
#	3475-A North 1st Street
#	San Jose CA 95134
#	Vox: (800)-457-4447
#	Fax: (408)-473-1510
#	Net: josed@techsupp.wyse.com (Jose D'Oliveira)
#
# Qume was bought by Wyse, but still (as of early 1995) has its own support
# group and production division.
#
# Discontinued Qume models:
#
# The qvt101 and qvt102 listed here are long obsolete; so is the qvt101+
# built to replace them, and a qvt119+ which was a 101+ with available wide
# mode (132 columns).  There was a qvt103 which added vt100/vt131 emulations
# and an ANSI-compatible qvt203 that replaced it.  Qume started producing
# ANSI-compatible terminals with the qvt323 and qvt61.
#
# Current Qume models (as of February 1995):
#
# All current Qume terminals have ANSI-compatible operation modes.
# Qume is still producing the qvt62, which features emulations for other
# popular lines such as ADDS, and dual-host capabilities.  The qvt82 is
# designed for use as a SCO ANSI terminal.  The qvt70 is a color terminal
# with many emulatioms including Wyse370, Wyse 325, etc.  Their newest
# model is the qvt520, which is vt420-compatible.
#
# There are some ancient printing Qume terminals under `Daisy Wheel Printers'

qvt101|qvt108|qume qvt 101 and QVT 108:\
	:sg#1:\
	:se=\EG0:so=\EG4:tc=qvt101+:
qvt101+|qvt101p|qume qvt 101 PLUS product:\
	:am:bw:hs:ul:\
	:co#80:li#24:sg#0:\
	:al=\EE:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=^Z:\
	:cm=\E=%+ %+ :cr=^M:ct=\E3:dc=\EW:dl=\ER:do=^J:\
	:ds=\Eg\Ef\r:ei=:fs=^M:ho=^^:ic=\EQ:im=:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kA=\EE:kB=\EI:\
	:kE=\ET:kI=\EQ:kL=\ER:kS=\EY:kb=^H:kd=^J:kh=^^:kl=^H:\
	:kr=^L:ku=^K:le=^H:nd=^L:pf=\EA:po=\E@:se=\E(:sf=^J:\
	:so=\E0P\E):st=\E1:ta=^I:ts=\Eg\Ef:ue=\EG0:up=^K:\
	:us=\EG8:vb=\Eb\Ed:ve=\E.4:vs=\E.2:
qvt102|qume qvt 102 product:\
	:ve=\E.:tc=qvt101:
qvt103|qume qvt 103:\
	:am:xn:xo:\
	:co#80:it#8:li#24:vt#3:\
	:DO=\E[%dB:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:bl=^G:\
	:cd=\E[J:ce=\E[K:cl=\E[H\E[2J:cm=\E[%i%d;%dH:cr=^M:\
	:cs=\E[%i%d;%dr:ct=\E[3g:do=^J:ho=\E[H:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:kb=^H:kd=\EOB:ke=\E[?1l\E>:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:..sa=\E[%?%p1%t;7%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p6%t;1%;m:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:
qvt103-w|qume qvt103 132 cols:\
	:co#132:li#24:\
	:r2=\E>\E[?3h\E[?4l\E[?5l\E[?8h:tc=qvt103:
qvt119+|qvt119p|qvt119|qume qvt 119 and 119PLUS terminals:\
	:am:hs:mi:ms:\
	:co#80:li#24:sg#0:\
	:al=\EE:bl=^G:bt=\EI:cd=\Ey:ce=\Et:cl=\E*1:\
	:cm=\E=%+ %+ :cr=^M:ct=\E3:dc=\EW:dl=\ER:do=^J:\
	:ds=\Eg\Ef\r:ei=\Er:fs=^M:ho=^^:im=\Eq:\
	:is=\EDF\EC\EG0\Er\E(\E%EX:k0=^AI\r:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=^H:kd=^J:kh=^^:kl=^H:\
	:kr=^L:ku=^K:le=^H:nd=^L:pf=\EA:po=\E@:se=\EG0:sf=^J:\
	:so=\EG4:sr=\EJ:st=\E1:ta=^I:ts=\Eg\Ef:ue=\EG0:up=^K:\
	:us=\EG8:vb=\En0\En1:ve=\E.4:vs=\E.2:
qvt119+-25|qvt119p-25|QVT 119 PLUS with 25 data lines:\
	:li#25:\
	:tc=qvt119+:
qvt119+-w|qvt119p-w|qvt119-w|QVT 119 and 119 PLUS in 132 column mode:\
	:co#132:\
	:is=\EDF\EC\EG0\Er\E(\E%\EX\En4:tc=qvt119+:
qvt119+-25-w|qvt119p-25-w|qvt119-25-w|QVT 119 and 119 PLUS 132 by 25:\
	:li#25:\
	:tc=qvt119+:
qvt203|qvt203+|qume qvt 203 Plus:\
	:am:xn:xo:\
	:co#80:it#8:li#24:vt#3:\
	:DO=\E[%dB:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:al=\E[L:\
	:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[2J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=\E[%i%d;%dr:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:\
	:ei=\E[4l:ho=\E[H:im=\E[4h:ip=:k0=\E[29~:k1=\E[17~:\
	:k2=\E[18~:k3=\E[19~:k4=\E[20~:k5=\E[21~:k6=\E[23~:\
	:k7=\E[24~:k8=\E[25~:k9=\E[28~:kb=^H:kd=\EOB:\
	:ke=\E[?1l\E>:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:\
	:le=^H:mb=\E[5m:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:..sa=\E[%?%p1%t;7%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p6%t;1%;m:\
	:sc=\E7:se=\E[m:sf=\n:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:
qvt203-w|qvt203-w-am|qume qvt 203 PLUS in 132 cols (w/advanced video):\
	:co#132:li#24:\
	:r2=\E>\E[?3h\E[?4l\E[?5l\E[?8h:tc=qvt203:
#
#	Since a command is present for enabling 25 data lines,
#	a specific terminfo entry may be generated for the 203.
#	If one is desired for the QVT 119 PLUS then 25 lines must
#	be selected in the status line (setup line 9).
#
qvt203-25|QVT 203 PLUS with 25 by 80 column mode:\
	:co#80:li#25:\
	:is=\E[=40h\E[?3l:tc=qvt203:
qvt203-25-w|QVT 203 PLUS with 25 by 132 columns:\
	:co#132:li#25:\
	:r2=\E[?3h\E[=40h:tc=qvt203:

#### Televideo (tvi)
#
#	TeleVideo
#	550 East Brokaw Road
#	PO Box 49048    95161
#	San Jose CA 95112
#	Vox: (408)-954-8333
#	Fax: (408)-954-0623
#
#
# There are some tvi terminals that require incredible amounts of padding and
# some that don't.  I'm assuming 912 and 920 are the old slow ones,
# and 912b, 912c, 920b, 920c are the new ones that don't need padding.
#
# All of these terminals (912 to 970 and the tvipt) are discontinued.  Newer
# Televideo terminals are ANSI and PC-ANSI compatible.

tvi803|televideo 803:\
	:cl=\E*:tc=tvi950:

# Vanilla tvi910 -- W. Gish <cswarren@violet> 10/29/86
# (tvi910: removed obsolete ":ma=^Kk^Ll^R^L:";
# mapped ":pt:" to ":it#8:"; added ":ug#0:" for terminfo translation;
# added khome, cub1, cud1, ind, hpa, vpa, am, msgr from SCO entry -- esr)
tvi910|televideo model 910:\
	:am:bs:ms:pt:\
	:co#80:it#8:li#24:sg#1:ug#0:\
	:bl=^G:bt=\EI:cd=\EY:ce=\ET:ch=\E]%+ :cl=^Z:\
	:cm=\E=%+ %+ :cr=^M:cv=\E[%+ :do=^J:ho=\E=\001\001:\
	:if=/usr/share/tabset/stdcrt:k0=^AI\r:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=^H:kd=^J:kh=^^:kl=^H:\
	:kr=^L:ku=^K:le=^H:nd=^L:se=\EG0:sf=^J:so=\EG4:\
	:ue=\EG0:up=^K:us=\EG8:
# From: Alan R. Rogers <rogers%albany@csnet-relay>
# as subsequently hacked over by someone at SCO
# (tvi910+: removed obsolete ":ma=^K^P^L :"; mapped ":pt:" to ":it#8:";
# added ":ug#0:" for terminfo translation -- esr)
tvi910+|910+|televideo 910+:\
	:am:bs:ms:pt:\
	:co#80:it#8:li#24:sg#1:ug#0:\
	:al=\EE:bl=^G:bt=\EI:cd=\EY:ce=\ET:ch=\E]%+ :cl=^Z:\
	:cm=\E=%+ %+ :cr=^M:cv=\E[%+ :dc=\EW:dl=\ER:do=^J:\
	:ei=:ho=^^:ic=\EQ:if=/usr/share/tabset/stdcrt:im=:\
	:k0=^A@\r:k1=^AA\r:k2=^AB\r:k3=^AC\r:k4=^AD\r:\
	:k5=^AE\r:k6=^AF\r:k7=^AG\r:k8=^AH\r:k9=^AI\r:kb=^H:\
	:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^M:ll=\E=7 :nd=^L:\
	:se=\EG0:sf=^J:so=\EG4:ue=\EG0:up=^K:us=\EG8:

# (tvi912: removed obsolete ":ma=^K^P^L :";
# mapped ":pt:" to default tabs -- esr)
tvi912|tvi920|old televideo 912:\
	:am:bs:pt:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EE:bl=^G:cd=\Ey:ce=\ET:cl=^Z:cm=\E=%+ %+ :cr=^M:\
	:ct=\E3:dc=\EW:dl=\ER:do=^J:ei=:ho=^^:ic=\EQ:\
	:if=/usr/share/tabset/stdcrt:im=:k0=^AI\r:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=^H:kd=^J:kl=^H:kr=^L:\
	:ku=^K:le=^H:nd=^L:se=\Ek:sf=^J:so=\Ej:st=\E1:ta=^I:\
	:ue=\Em:up=^K:us=\El:
# the 912 has a <funct> key that's like shift: <funct>8 xmits "^A8\r".
# The 920 has this plus real function keys that xmit different things.
# Terminfo makes you use the funct key on the 912 but the real keys on the 920.
tvi912c|tvi912b|912c|912b|tvi|new televideo 912:\
	:al=\EE:dl=\ER:tc=tvi912:
# set to page 1 when entering ex (\E-17 )
# reset to page 0 when exiting ex (\E-07 )
tvi912-2p|tvi920-2p|912-2p|920-2p|tvi-2p|televideo w/2 pages:\
	:te=\E-07 :ti=\E-17 :tc=tvi912:
# We got some new tvi912c terminals that act really weird on the regular 
# termcap, so one of our gurus worked this up. Seems that cursor 
# addressing is broken.
tvi912cc|tvi912 at cowell college:\
	:cm@:tc=tvi912c:

tvi920b|tvi920c|new televideo 920:\
	:al=\EE:dl=\ER:k0=^AI\r:k1=^A@\r:k2=^AA\r:k3=^AB\r:\
	:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:k8=^AG\r:\
	:k9=^AH\r:tc=tvi912:

tvi924|televideo tvi924:\
	:am:bw:hs:in:mi:ms:xn:xo:\
	:co#80:it#8:li#24:sg#0:ws#80:\
	:F1=^AK\r:F2=^AL\r:F3=^AM\r:F4=^AN\r:F5=^AO\r:al=\EE:\
	:bl=^G:bt=\EI:cd=\Ey:ce=\Et:cl=\E*0:cm=\E=%+ %+ :\
	:cr=^M:cs=\E_%+ %+ :ct=\E3:dc=\EW:dl=\ER:do=^V:\
	:ds=\Es0:ei=:fs=^Y:ho=^^:\
	:i1=\017\E%\E'\E(\EDF\EC\EG0\EN0\Es0\Ev0:ic=\EQ:\
	:if=/usr/lib/tabset/stdcrt:im=:k0=^A@\r:k1=^AA\r:\
	:k2=^AB\r:k3=^AC\r:k4=^AD\r:k5=^AE\r:k6=^AF\r:\
	:k7=^AG\r:k8=^AH\r:k9=^AI\r:k;=^AJ\r:kA=\EE:kC=\E*0:\
	:kD=\EW:kE=\Et:kI=\EQ:kL=\ER:kS=\Ey:kb=^H:kd=^V:\
	:kh=^^:kl=^H:kr=^L:ku=^K:l0=F1:l1=F2:l2=F3:l3=F4:\
	:l4=F5:l5=F6:l6=F7:l7=F8:l8=F9:l9=F10:la=F11:le=^H:\
	:mb=\EG2:me=\EG0:mk=\EG1:nd=^L:pk=\E|%+1%s\031:\
	:se=\EG0:sf=^J:so=\EG4:sr=\Ej:st=\E1:ta=^I:ts=\Ef:\
	:ue=\EG0:up=^K:us=\EG8:vb=\Eb\Ed:ve=\E.3:vi=\E.0:\
	:vs=\E.1:
tvi924vb|924vb|televideo model 924 visual bells:\
	:vb=\Eb\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Ed:tc=tvi924:

tvi925|925|televideo 925:\
	:am:bw:hs:ul:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EE:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=^Z:\
	:cm=\E=%+ %+ :cr=^M:ct=\E3:dc=\EW:dl=\ER:do=^V:\
	:ds=\Eh:ei=:fs=^M\Eg:ho=^^:ic=\EQ:im=:k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=\EE:kC=^Z:\
	:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kS=\EY:kb=^H:kd=^V:\
	:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:se=\EG0:sf=^J:so=\EG4:\
	:st=\E1:ta=^I:ts=\Eh\Ef:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eb\Ed:ve=\E.4:vs=\E.2:
tvi925vb|925vb|televideo model 925 visual bells:\
	:vb=\Eb\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Ed:tc=tvi925:
# Since the 925 uses a character position to store the escape sequences to go
# in and out of both stand out and underline modes, screen positioning is
# difficult.  The following 925 entries don't use these modes.
tvi925n|925n|televideo model 925 no standout or underline:\
	:se@:so@:ue@:us@:tc=tvi925:
tvi925vbn|925vbn|televideo model 925 visual bells no so or ul:\
	:vb=\Eb\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Ed:tc=tvi925n:

# From: Tim Curry, Univ. of Central Fla. <duke!ucf-cs!tim> 5/21/82 
# (tvi925a: removed obsolete ":kn#12:"; mapped ":pt:" to ":it#8:" --esr)
tvi925a|925a|TeleVideo Model 925:\
	:am:bs:bw:pt:\
	:co#80:it#8:li#24:sg#1:ug#1:\
	:al=\EE:bt=\EI:cd=\EY:ce=\ET:cl=^Z:cm=\E=%+ %+ :\
	:dc=\EW:dl=\ER:do=^V:ei=:ic=\EQ:\
	:if=/usr/share/tabset/std:im=:is=\El:kb=^H:kd=^V:\
	:kh=^^:kl=^H:kr=^L:ku=^K:nd=^L:se=\EG0:so=\EG4:\
	:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eb\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Ed:\
	:ve=\E.4:vs=\E.2:

# From: Todd Litwin <litwin@litwin.jpl.nasa.gov> 28 May 1993
# Originally Tim Curry, Univ. of Central Fla., <duke!ucf-cs!tim> 5/21/82
# for additional capabilities, 
# The following tvi descriptions from B:pjphar and virus!mike
# is for all 950s.  It sets the following attributes:
# full duplex (\EDF)		write protect off (\E()
# conversation mode (\EC)	graphics mode off (\E%)
# white on black (\Ed)		auto page flip off (\Ew)
# turn off status line (\Eg)	clear status line (\Ef\r)
# normal video (\E0)		monitor mode off (\EX or \Eu)
# edit mode (\Er)		load blank char to space (\Ee\040)
# line edit mode (\EO)		enable buffer control (^O)
# protect mode off (\E\047)	duplex edit keys (\El)
# program unshifted send key to send line all (\E016)
# program shifted send key to send line unprotected (\E004)
# set the following to nulls:
#	field delimiter (\Ex0\200\200)
#	line delimiter (\Ex1\200\200)
#	start-protected field delimiter (\Ex2\200\200)
#	end-protected field delimiter (\Ex3\200\200)
# set end of text delimiter to carriage return/null (\Ex4\r\200)
# (tvi950: early versions had ":ko=ic,dc,al,dl,cl,bt,ce,cd:"
# and ":ma=^Vj^Kk^Hh^Ll^^H:". I mapped ":pt:" to ":it#8:";
#
tvi950|950|televideo950:\
	:am:bs:hs:mi:ms:pt:xn:xo:\
	:co#80:li#24:sg#1:ug#1:\
	:ac=d\rc\014e\nb\011i\013:ae=^X:al=\EE:as=^U:bl=^G:\
	:bt=\EI:cd=\Ey:ce=\Et:cl=\E*:cm=\E=%+ %+ :cr=^M:\
	:ct=\E3:dc=\EW:dl=\ER:do=^J:ds=\Eg\Ef\r:ei=\Er:fs=^M:\
	:ho=^^:im=\Eq:\
	:is=\EDF\EC\Ed\EG0\Eg\Er\EO\E'\E(\E%\Ew\EX\Ee \017\011\El\E016\E004\Ex0\200\200\Ex1\200\200\Ex2\200\200\011\Ex3\200\200\Ex4\r\200\Ef\r:\
	:k0=^A0\r:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:\
	:k5=^AD\r:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=\EE:\
	:kB=\EI:kC=\E*:kD=\EW:kE=\Et:kL=\ER:kS=\Ey:kb=^H:\
	:kd=^V:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:pf=\Ea:\
	:po=\E`:se=\EG0:sf=^J:so=\EG4:sr=\Ej:st=\E1:ta=^I:\
	:ts=\Eg\Ef:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eb\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Ed:
#
# is for 950 with two pages adds the following:
#	set 48 line page (\E\\2)
#	place cursor at page 0, line 24, column 1 (\E-07 )
#	set local (no send) edit keys (\Ek)
#
# two page 950 adds the following:
#	when entering ex, set 24 line page (\E\\1)
#	when exiting ex, reset 48 line page (\E\\2)
#			 place cursor at 0,24,1 (\E-07 )
#	set duplex (send) edit keys (\El) when entering vi
#	set local (no send) edit keys (\Ek) when exiting vi
#
tvi950-2p|950-2p|televideo950 w/2 pages:\
	:is=\EDF\EC\Ed\EG0\Eg\Er\EO\E'\E(\E%\Ew\EX\Ee \017\011\Ek\E016\E004\Ex0\200\200\Ex1\200\200\Ex2\200\200\011\Ex3\200\200\Ex4\r\200\E\\2\E-07 \011:\
	:ke=\Ek:ks=\El:te=\E\\2\E-07 :ti=\E\\1\E-07 :tc=tvi950:
#
# is for 950 with four pages adds the following:
#	set 96 line page (\E\\3)
#	place cursor at page 0, line 24, column 1 (\E-07 )
#
# four page 950 adds the following:
#	when entering ex, set 24 line page (\E\\1)
#	when exiting ex, reset 96 line page (\E\\3)
#			 place cursor at 0,24,1 (\E-07 )
#
tvi950-4p|950-4p|televideo950 w/4 pages:\
	:is=\EDF\EC\Ed\EG0\Eg\Er\EO\E'\E(\E%\Ew\EX\Ee \017\011\Ek\E016\E004\Ex0\200\200\Ex1\200\200\Ex2\200\200\011\Ex3\200\200\Ex4\r\200\E\\3\E-07 \011:\
	:ke=\Ek:ks=\El:te=\E\\3\E-07 :ti=\E\\1\E-07 :tc=tvi950:
#
# is for reverse video 950 changes the following:
#	set reverse video (\Ed)
#
# set vb accordingly (\Ed ...nulls... \Eb)
#
tvi950-rv|950-rv|televideo950 rev video:\
	:is=\EDF\EC\Eb\EG0\Eg\Er\EO\E'\E(\E%\Ew\EX\Ee \017\011\El\E016\E004\Ex0\200\200\Ex1\200\200\Ex2\200\200\011\Ex3\200\200\Ex4\r\200:\
	:vb=\Ed\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Eb:tc=tvi950:
#
# uses the appropriate entries from 950-2p and 950-rv
#
tvi950-rv-2p|950-rv-2p|televideo950 rev video w/2 pages:\
	:is=\EDF\EC\Eb\EG0\Eg\Er\EO\E'\E(\E%\Ew\EX\Ee \017\011\Ek\E016\E004\Ex0\200\200\Ex1\200\200\Ex2\200\200\011\Ex3\200\200\Ex4\r\200\E\\2\E-07 :\
	:ke=\Ek:ks=\El:te=\E\\2\E-07 :ti=\E\\1\E-07 :\
	:vb=\Ed\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Eb:tc=tvi950:
#
# uses the appropriate entries from 950-4p and 950-rv
#
tvi950-rv-4p|950-rv-4p|televideo950 rev video w/4 pages:\
	:is=\EDF\EC\Eb\EG0\Er\EO\E'\E(\E%\Ew\EX\Ee \017\011\Ek\E016\E004\Ex0\200\200\Ex1\200\200\Ex2\200\200\011\Ex3\200\200\Ex4\r\200\E\\3\E-07 :\
	:ke=\Ek:ks=\El:te=\E\\3\E-07 :ti=\E\\1\E-07 :\
	:vb=\Ed\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Eb:tc=tvi950:
# From: Andreas Stolcke <stolcke@icsi.berkeley.edu>
# (tvi955: removed obsolete ":ko=ic,dc,al,dl,cl,bt,ce,cd:ma:=^Vj^Kk^Hh^Ll^^H";
# mapped ":pt:" to ":it#8:"; removed incorrect (and overridden) ":do=^J:";
# fixed broken continuations in the :rs: string -- esr)
tvi955|televideo955:\
	:5i:am:bs:hs:mi:pt:xn:xo:\
	:co#80:it#8:li#24:\
	:RA=\E[=7l:RX=^N:SA=\E[=7h:SX=^O:\
	:ac=0_`RjHkGlFmEnIoPqKsQtMuLvOwNxJ:ae=\E%:al=\EE:\
	:as=\E$:bt=\EI:cd=\Ey:ce=\Et:cl=\E*:cm=\E=%+ %+ :\
	:ct=\E3:dc=\EW:dl=\ER:do=^V:ds=\Eg\Ef\r:ei=\Er:fs=^M:\
	:ho=^^:im=\Eq:is=\E[=3l\EF1\Ed\EG0\E[=5l\E%\El:\
	:k0=^A0\r:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:\
	:k5=^AD\r:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=\EE:\
	:kB=\EI:kC=\EY:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kM=\EQ:\
	:kN=\EK:kP=\EJ:kT=\E1:ka=\E3:kb=^H:kd=^V:kh=^^:kl=^H:\
	:kr=^L:kt=\E2:ku=^K:le=^H:mb=\EG2:me=\EG0\E[=5l:\
	:mh=\E[=5h:mk=\EG1:mr=\EG4:nd=^L:pf=\Ea:po=\E`:\
	:ps=\EP:\
	:rs=\EDF\EC\Eg\Er\EO\E'\E(\Ew\EX\Ee \017\E0P\E6\200\E0p\E4\200\Ef\r:\
	:se=\EG0:so=\EG4:sr=\Ej:st=\E1:ts=\Eg\Ef:ue=\EG0:\
	:up=^K:us=\EG8:\
	:vb=\Eb\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Ed:\
	:ve=\E.2:vi=\E.0:vs=\E.1:
tvi955-w|955-w|televideo955 w/132 cols:\
	:co#132:\
	:cm=\E[%i%d;%dH:is=\E[=3h\EF1\Ed\EG0\E[=5l\E%\El:tc=tvi955:
# use half-intensity as normal mode, full intensity as bold (md)
tvi955-hb|955-hb|televideo955 half-bright:\
	:is=\E[=3l\EF1\Ed\EG0\E[=5h\E%\El:md=\E[=5l:\
	:me=\EG0\E[=5h:mh@:tc=tvi955:
# From: Humberto Appleton <beto@cs.utexas.edu>, 880521 UT Austin
# (tvi970: removed ":sg#0:"; mapped ":pt:" to ":it#8:" -- esr)
tvi970|televideo970:\
	:bs:da:db:mi:ms:pt:\
	:co#80:it#8:li#24:\
	:ae=\E(B:al=\E[L:as=\E(B:bt=\E[Z:cd=\E[0J:ce=\E[0K:\
	:cl=\E[H\E[2J:cm=\E[%i%d;%df:dc=\E[P:dl=\E[M:do=\ED:\
	:ei=\E[4l:im=\E[4h:\
	:is=\E<\E[?21l\E[19h\E[1Q\E[10l\E[7l\E[H\E[2J:\
	:k1=\E?a:k2=\E?b:k3=\E?c:k4=\E?d:k5=\E?e:k6=\E?f:\
	:k7=\E?g:k8=\E?h:k9=\E?i:kb=^H:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:nd=\E[C:se=\E[0m:so=\E[7m:\
	:sr=\EM:ue=\E[0m:up=\EM:us=\E[4m:\
	:vb=\E[5;m\200\200\200\200\200\200\200\200\200\E[0;m:\
	:vs=\E[1Q:
# From Gene Rochlin <armsis@amber> 9/19/84. 
# Works with vi and rogue.  NOTE: Esc v sets autowrap on, Esc u sets 80 chars
# per line (rather than 40), Esc K chooses the normal character set.  Not sure
# padding is needed, but adapted from the tvi920c termcap.  The :so: and :us:
# strings are klutzy, but at least use no screen space.
# (tvipt: removed obsolete ":ma=^Kk^Ll^R^L:" -- esr)
tvipt|televideopt:\
	:am:bs:\
	:co#80:li#24:\
	:al=\EE<5*>:bt=\EI:ce=\ET:cl=^Z:cm=\E=%+ %+ :\
	:dl=\ER<5*>:ho=^^:if=/usr/share/tabset/stdcrt:\
	:is=\Ev\Eu\EK:kb=^H:kd=^J:kl=^H:kr=^L:ku=^K:nd=^L:\
	:se=\EF:so=\EG1@A\EH:ue=\EF:up=^K:us=\EG1B@\EH:

#### Visual (vi)
#

# (vi50: mapped ":pt:" to default 8-char tabs -- esr)
vi50|visual 50:\
	:am:bs:ms:pt:\
	:co#80:li#24:\
	:al=\EL:bl=^G:cd=\Ek:ce=\EK:cl=^Z:cm=\E=%+ %+ :cr=^M:\
	:dl=\EM:do=^J:ho=\EH:kb=^H:kd=\EB:kh=\EH:kl=\ED:\
	:kr=\EC:ku=\EA:le=^H:nd=^L:se=\ET:sf=^J:so=\EU:ta=^I:\
	:up=^K:
# From: Jeff Siegal <jbs@athena.mit.edu>
# (vi55: mapped ":pt:" to ":it#8:" -- esr)
vi55|Visual 55:\
	:am:bs:mi:ms:pt:\
	:co#80:it#8:li#24:\
	:al=\EL:cd=\EJ:ce=\EK:cl=\Ev:cm=\EY%+ %+ :\
	:cs=\E_%+A%+A:dc=\Ew:dl=\EM:do=^J:ei=\Eb:ho=\EH:\
	:im=\Ea:is=\Ev\E_AX\Eb\EW\E9P\ET:kb=^H:kd=\EB:kl=\ED:\
	:kr=\EC:ku=\EA:le=^H:nd=\EC:se=\ET:so=\EU:sr=\EI:\
	:up=\EA:

# The Visual 200 beeps when you type a character in insert mode.
# This is a horribly obnoxious misfeature, and some of the entries
# below try to get around the problem by ignoring the feature or
# turning it off when inputting a character.  They are said not to
# work well at 300 baud.  (You could always cut the wire to the bell!)
# From: <mike@brl-vgr> Mon Nov 14 08:34:29 1983
# (vi200: mapped ":pt:" to default 8-char tabbing -- esr)
vi200|vis200|visual 200 with function keys:\
	:am:bs:pt:\
	:co#80:li#24:\
	:al=\EL:bl=^G:cd=\Ey:ce=\Ex:cl=\Ev:cm=\EY%+ %+ :\
	:cr=^M:dc=\EO:dl=\EM:do=^J:ei=:ho=\EH:ic=\Ei \010\Ej:\
	:im=:is=\E3\Eb\Ej\E\\\El\EG\Ec\Ek:k0=\EP:k1=\EQ:\
	:k2=\ER:k3=\E :k4=\E!:k5=\E":k6=\E#:k7=\E$:k8=\E%:\
	:k9=\E&:kd=\EB:kh=\EH:kl=\ED:kr=\EC:ku=\EA:le=^H:\
	:nd=\EC:se=\E3:sf=^J:so=\E4:sr=\EI:ta=^I:up=\EA:\
	:ve=\Ec:vs=\Ed:
vi200-rv-ic|visual 200 reverse video using insert char:\
	:ei=\Ej:ic@:im=\Ei:tc=vi200-rv:
# The older Visuals didn't come with function keys. This entry uses
# ks and ke so that the keypad keys can be used as function keys.
# If your version of vi doesn't support function keys you may want
# to use vi200-f.
# (vi200: mapped ":pt:" to ":it#8:" -- esr)
vi200-f|visual|visual 200 no function keys:\
	:am:bs:pt:\
	:co#80:it#8:li#24:\
	:al=\EL:bl=^G:cd=\Ey:ce=\Ex:cl=\Ev:cm=\EY%+ %+ :\
	:cr=^M:dc=\EO:dl=\EM:do=^J:ei=:ho=\EH:ic=\Ei \010\Ej:\
	:im=:is=\E3\Eb\Ej\E\\\El\EG\Ed\Ek:k0=\E?p:k1=\E?q:\
	:k2=\E?r:k3=\E?s:k4=\E?t:k5=\E?u:k6=\E?v:k7=\E?w:\
	:k8=\E?x:k9=\E?y:kd=\EB:ke=\E>:kh=\EH:kl=\ED:kr=\EC:\
	:ks=\E=:ku=\EA:le=^H:nd=\EC:sf=^J:sr=\EI:ta=^I:\
	:up=\EA:ve=\Ec:vs=\Ed:
vi200-rv|visual 200 reverse video:\
	:se=\E3:so=\E4:sr@:ve@:vs@:tc=vi200:
vi200-ic|visual 200 using insert char:\
	:ei=\Ej:ic@:im=\Ei:tc=vi200:

# the function keys are programmable but we don't reprogram
# them to their default values with "is" because programming
# them is very verbose. maybe an "if" file should be made for
# the 300 and they could be stuck in it.
vi300|visual 300 ansi x3.64:\
	:am:bw:mi:xn:\
	:co#80:li#24:\
	:al=\E[L:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:do=\E[B:\
	:ei=\E[4l:ho=\E[H:im=\E[4h:\
	:is=\E[7s\E[2;3;4;20;?5;?6l\E[12;?7h\E[1Q\E[0;1(D\E[8s:\
	:k1=\E_A\E\\:k2=\E_B\E\\:k3=\E_C\E\\:k4=\E_D\E\\:\
	:k5=\E_E\E\\:k6=\E_F\E\\:k7=\E_G\E\\:k8=\E_H\E\\:\
	:k9=\E_I\E\\:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:\
	:le=^H:nd=\E[C:se=\E[m:sf=^J:so=\E[1m:sr=\EM:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:
vi300-rv|visual 300 reverse video:\
	:bl=^G:cr=^M:do=^J:\
	:is=\E[7s\E[2;3;4;20;?6l\E[12;?5;?7h\E[1Q\E[0;1(D\E[8s:\
	:sf=^J:tc=vi300:
# slow scroll doesn't work that well; if you type on the
# keyboard while the terminal is scrolling it drops characters
vi300-ss|visual 300 slow scroll:\
	:bl=^G:cr=^M:do=^J:sf=^J:ve=\E[?4h:vs=\E[?4l:tc=vi300:
# some of the vi300s have older firmware that has the command
# sequence for setting editing extent reversed.
ovi300|visual 300 old:\
	:bl=^G:cr=^M:do=^J:\
	:is=\E[7s\E[2;3;4;20;?5;?6l\E[12;?7h\E[2Q\E[0;1(D\E[8s:\
	:sf=^J:tc=vi300:
# if your version of ex/vi doesn't correctly implement xn
# use this termcap for the vi300
vi300-aw|visual 300 no autowrap:\
	:am@:xn@:\
	:ve=\E[?7h:vs=\E[?7l:tc=vi300:

# the visual 550 is a visual 300 with tektronix graphics,
# and with 33 lines. clear screen is modified here to
# also clear the graphics.
vi550|visual 550 ansi x3.64:\
	:li#33:\
	:bl=^G:cl=\030\E[H\E[2J:cr=^M:do=^J:sf=^J:tc=vi300:

# (vi603: this had ":sb=\EM:"; sb is undefined, prob. an error for sr -- esr)
vi603|visual603|visual 603:\
	:hs:mi:\
	:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[J:\
	:cm=\E[%i%d;%dH:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[M:\
	:ds=\EP2;1~\E\\:ei=\E[4l:fs=\E\\:im=\E[4h:\
	:is=\E>\E[?3l\E[?4l\E[?7h\E[?8h\E[1;24r\E[24;1H:\
	:mb=\E[5m:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:\
	:rs=\E>\E[?3l\E[?4l\E[?7h\E[?8h:se=\E[27m:sf=\ED:\
	:so=\E[7m:sr=\EM:ts=\EP2~:ue=\E[24m:up=\E[A:us=\E[4m:tc=vt100:

#### Wyse (wy)
#
#	Wyse Technology
#	3471 North First Street
#	San Jose, CA 95134
#	Vox: (408)-473-1200
#	Fax: (408) 473-1222
#
# Wyse sales can be reached by phone at 1-800-GET-WYSE.  Tech support is at
# (800)-800-WYSE (option 5 gets you a human).
#
# All the following entries until (but not including) wy100q are direct from
# Wyse technical support and represent their best knowledge as of January 1995.
# I made two trivial syntax fixes in the wyse30 entry, added OTbs everywhere
# needed, and merged in OTug#1 entries (as indicated by the termcap version of
# their descriptions).
#
# Note: The wyse75, wyse85, and wyse99 have been discontinued.

#	   Although the Wyse 30 can support more than one attribute
#	it requires magic cookies to do so.  Many applications do not
#	function well with magic cookies.  The following terminfo uses
#	the protect mode to support one attribute (dim) without cookies.
#	If more than one attribute is needed then the wy30-mc terminfo
#	should be used.
#
wy30|wyse30|Wyse 30:\
	:5i:am:bs:bw:hs:mi:ms:xo:\
	:Nl#8:co#80:lh#1:li#24:lw#8:ma#1:ug#1:ws#45:\
	:#2=\E{:&3=\Er:@8=\E7:LF=\EA11:LO=\EA10:\
	:ac=0wa_h[jukslrmqnxqzttuyv]wpxv:ae=\EH^C:al=\EE:\
	:as=\EH^B:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=\E+:\
	:cm=\E=%+ %+ :cr=^M:ct=\E0:dc=\EW:dl=\ER:do=^J:\
	:ds=\EF\r:ei=\Er:fs=^M:ho=^^:im=\Eq:ip=:\
	:is=\E'\E(\E^3\E`9\016\024:k1=^A@\r:k2=^AA\r:\
	:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:kA=\EE:kB=\EI:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:\
	:kN=\EK:kP=\EJ:kS=\EY:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:\
	:ku=^K:le=^H:ll=^^^K:me=\E(\EH\003:mh=\E`7\E):\
	:mp=\E`7\E):nd=^L:nw=^M^J:pf=^T:pn=\Ez%+/%s\r:po=^X:\
	:ps=\EP:px=\Ez%+?%s\177:\
	:..sa=%?%p1%p5%p8%|%|%t\E`7\E)%e\E(%;%?%p9%t\EH\002%e\EH\003%;:\
	:se=\E(:sf=\n:so=\E`7\E):sr=\Ej:st=\E1:ta=\011:\
	:ts=\EF:up=^K:ve=\E`1:vi=\E`0:
#
#	This terminal description uses the non-hidden attribute mode
#	(with magic cookie).
#
wy30-mc|wyse30-mc|wyse 30 with magic cookies:\
	:ms@:\
	:ma@:sg#1:ug#1:\
	:ae=\EG0\EH\003:as=\EG0\EH\002:mb=\EG2:\
	:me=\EG0\E(\EH\003:mh=\EGp:mk=\EG1:mp=\EG0\E):\
	:mr=\EG4:\
	:..sa=\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c%?%p8%t\E)%e\E(%;%?%p9%t\EH\002%e\EH\003%;:\
	:se=\EG0:so=\EG4:te=\EG0:ue=\EG0:us=\EG8:tc=wy30:
#	The manditorary pause used by flash does not work with
#	older versions of terminfo.  If you see this effect then
#	unset xon and delete the / from the delay.
#	i.e. change $<100/> to $<100>
wy30-vb|wyse30-vb|wyse 30 visible bell:\
	:vb=\E`8\E`9:tc=wy30:
#
#	   The Wyse 50 can support one attribute (e.g. Dim, Inverse,
#	Normal) without magic cookies by using the protect mode.
#	The following description uses this feature, but when more
#	than one attribute is put on the screen at once, all attributes
#	will be changed to be the same as the last attribute given.
#	   The Wyse 50 can support more attributes when used with magic
#	cookies.  The wy50-mc terminal description uses magic cookies
#	to correctly handle multiple attributes on a screen.
#
wy50|wyse50|Wyse 50:\
	:5i:am:bs:bw:hs:mi:ms:xo:\
	:Nl#8:co#80:lh#1:li#24:lw#8:ma#1:ws#45:\
	:#2=\E{:%9=\EP:&3=\Er:@8=\E7:F1=^AJ\r:F2=^AK\r:\
	:F3=^AL\r:F4=^AM\r:F5=^AN\r:F6=^AO\r:LF=\EA11:\
	:LO=\EA10:ac=0wa_h[jukslrmqnxqzttuyv]wpxv:ae=\EH^C:\
	:al=\EE:as=\EH^B:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=\E+:\
	:cm=\E=%+ %+ :cr=^M:ct=\E0:dc=\EW:dl=\ER:do=^J:\
	:ds=\EF\r:ei=\Er:fs=^M:ho=^^:i1=\E`\072\E`9:im=\Eq:\
	:ip=:is=\016\024\E'\E(:k1=^A@\r:k2=^AA\r:k3=^AB\r:\
	:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:k8=^AG\r:\
	:k9=^AH\r:k;=^AI\r:kA=\EE:kB=\EI:kD=\EW:kE=\ET:\
	:kI=\EQ:kL=\ER:kN=\EK:kP=\EJ:kS=\EY:kb=^H:kd=^J:\
	:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:ll=^^^K:me=\E(\EH\003:\
	:mh=\E`7\E):mp=\E`7\E):mr=\E`6\E):nd=^L:nw=^M^J:\
	:pf=^T:pn=\Ez%+/%s\r:po=^X:ps=\EP:px=\Ez%+?%s\177:\
	:..sa=%?%p1%p3%|%t\E`6\E)\n%e%p5%p8%|%t\E`7\E)%e\E(%;\n%?%p9%t\EH\002%e\EH\003%;:\
	:se=\E(:sf=\n:so=\E`6\E):sr=\Ej:st=\E1:ta=^I:ts=\EF:\
	:up=^K:ve=\E`1:vi=\E`0:
#
#	This terminal description uses the non-hidden attribute mode
#	(with magic cookie).
#
wy50-mc|wyse50-mc|wyse 50 with magic cookies:\
	:ms@:\
	:ma@:sg#1:ug#1:\
	:ae=\EG0\EH\003:as=\EG0\EH\002:mb=\EG2:\
	:me=\EG0\E(\EH\003:mh=\EGp:mk=\EG1:mp=\EG0\E):\
	:mr=\EG4:\
	:..sa=\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c%?%p8%t\E)%e\E(%;%?%p9%t\EH\002%e\EH\003%;:\
	:se=\EG0:so=\EGt:te=\EG0:ue=\EG0:us=\EG8:tc=wy50:
#	The mandatory pause used by flash does not work with
#	older versions of terminfo.  If you see this effect then
#	unset xon and delete the / from the delay.
#	i.e. change $<100/> to $<100>
wy50-vb|wyse50-vb|wyse 50 visible bell:\
	:vb=\E`8\E`9:tc=wy50:
wy50-w|wyse50-w|wyse 50 132-column:\
	:Nl#16:co#132:lw#7:ws#97:\
	:cm=\Ea%i%dR%dC:dc=\EW:i1=\E`;\E`9:tc=wy50:
wy50-wvb|wyse50-wvb|wyse 50 132-column visible bell:\
	:vb=\E`8\E`9:tc=wy50-w:
#
#	The Wyse 350 is a Wyse 50 with color.
#	Unfortunately this means that it has magic cookies.
#	The color attributes are designed to overlap the reverse, dim and
#	underline attributes.  This is nice for monochrome applications
#	because you can make underline stuff green (or any other color)
#	but for true color applications it's not so hot because you cannot
#	mix color with reverse, dim or underline.
#	    To further complicate things one of the attributes must be
#	black (either the foreground or the background).  In reverse video
#	the background changes color with black letters.  In normal video
#	the foreground changes colors on a black background.  
#	    This terminfo uses some of the more advanced features of curses
#	to display both color and blink.  In the final analysis I am not
#	sure that the wy350 runs better with this terminfo than it does
#	with the wy50 terminfo (with user adjusted colors).
#
wy350|wyse350|Wyse 350:\
	:5i:am:bs:bw:hs:mi:xo:\
	:Co#8:NC#55:Nl#8:co#80:lh#1:li#24:lw#8:pa#8:sg#1:\
	:ug#1:ws#45:\
	:#2=\E{:%9=\EP:&3=\Er:@8=\E7:F1=^AJ\r:F2=^AK\r:\
	:F3=^AL\r:F4=^AM\r:F5=^AN\r:F6=^AO\r:LF=\EA11:\
	:LO=\EA10:Sb= :\
	:..Sf=%?%p1%{0}%=%t%{76}\n%e%p1%{1}%=%t%{64}\n%e%p1%{2}%=%t%{8}\n%e%p1%{3}%=%t%{72}\n%e%p1%{4}%=%t%{4}\n%e%p1%{5}%=%t%{68}\n%e%p1%{6}%=%t%{12}\n%e%p1%{7}%=%t%{0}\n%;%PC\n\EG%gC%gA%+%'0'%+%c:\
	:ac=0wa_h[jukslrmqnxqzttuyv]wpxv:ae=\EG0\EH\003:\
	:al=\EE:as=\EG0\EH\002:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:cl=\E+:cm=\E=%+ %+ :cr=^M:ct=\E0:dc=\EW:dl=\ER:\
	:do=^J:ds=\EF\r:ei=\Er:fs=^M:ho=^^:i1=\E`\072\E`9:\
	:i2=\E%?:im=\Eq:ip=:is=\016\024\E'\E(:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kA=\EE:kB=\EI:\
	:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kN=\EK:kP=\EJ:kS=\EY:\
	:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:ll=^^^K:\
	:mb=\EG2:me=\EG0\E(\EH\003%{0}%PA%{0}%PC:mh=\EGp:\
	:mk=\EG1:mp=\EG0\E):mr=\EG4:nd=^L:nw=^M^J:oc=\E%?:\
	:op=\EG0:pf=^T:pn=\Ez%+/%s\r:po=^X:ps=\EP:\
	:px=\Ez%+?%s\177:\
	:..sa=%{0}%?%p4%t%{2}%|%;\n%?%p7%t%{1}%|%;%PA\n\EG%?%gC%t%gC%e\n%{0}%?%p1%t%{4}%|%;\n%?%p2%t%{8}%|%;\n%?%p3%t%{4}%|%;\n%?%p5%t%{64}%|%;\n%;%gA%+%'0'%+%c\n%?%p8%t\E)%e\E(%;%?%p9%t\EH\002%e\EH\003%;:\
	:se=\EG0:sf=\n:so=\EG4:sr=\Ej:st=\E1:ta=^I:ts=\EF:\
	:ue=\EG0:up=^K:us=\EG8:ve=\E`1:vi=\E`0:
#	The manditorary pause used by flash does not work with
#	older versions of terminfo.  If you see this effect then
#	unset xon and delete the / from the delay.
#	i.e. change $<100/> to $<100>
wy350-vb|wyse350-vb|wyse 350 visible bell:\
	:vb=\E`8\E`9:tc=wy350:
wy350-w|wyse350-w|wyse 350 132-column:\
	:Nl#16:co#132:lw#7:ws#97:\
	:cm=\Ea%i%dR%dC:dc=\EW:i1=\E`;\E`9:tc=wy350:
wy350-wvb|wyse350-wvb|wyse 350 132-column visible bell:\
	:vb=\E`8\E`9:tc=wy350-w:
#
#	This terminfo description is untested.
#
wy100|wyse 100:\
	:hs:mi:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EE:bl=^G:cd=\EY:ce=\ET:cl=\E;:cm=\E=%+ %+ :\
	:cr=^M:dc=\EW:dl=\ER:do=^J:ds=\EA31:ei=\Er:fs=^M:\
	:im=\Eq:is=\Eu\E0:k1=^A@\r:k2=^AA\r:k3=^AB\r:\
	:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:k8=^AG\r:kb=^H:\
	:kd=^J:kh=\E{:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:se=\EG0:\
	:sf=^J:so=\EG4:ts=\EF:ue=\EG0:up=^K:us=\EG8:
#
#	The Wyse 120/150 has most of the features of the Wyse 60.
#
#	This terminal does not need padding up to 9600 baud!
#
#	(msgr) should be set but the clear screen fails when in
#	alt-charset mode.  Try \EcE  \E+  if the screen is really clear
#	then set msgr.
#
wy120|wyse120|wy150|wyse150|Wyse 120/150:\
	:5i:am:bs:bw:hs:km:mi:ms:xo:\
	:Nl#8:co#80:it#8:lh#1:li#24:lw#8:pb#9601:ws#45:\
	:#2=\E{:%9=\EP:&3=\Er:@8=\E7:F1=^AJ\r:F2=^AK\r:\
	:F3=^AL\r:F4=^AM\r:F5=^AN\r:F6=^AO\r:LF=\EA11:\
	:LO=\EA10:RA=\Ed.:RX=\Ec20:SA=\Ed/:SX=\Ec21\ntbc=\E0:\
	:ac=+/\\\054.0[Iha2fxgqh1jYk?lZm@nEqDtCu4vAwBx3yszr{c~~:\
	:ae=\EcD:al=\EE:as=\EcE:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:cl=\E+:cm=\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=^J:\
	:ds=\EF\r:ei=\Er:fs=^M:ho=^^:i1=\EcB0\EcC1:\
	:i2=\EwJ\Ew1:im=\Eq:ip=:\
	:is=\Ed$\EcD\E'\Er\EH\003\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1\016\024\El:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kA=\EE:\
	:kB=\EI:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kN=\EK:kP=\EJ:\
	:kS=\EY:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:\
	:ll=^^^K:mb=\EG2:me=\E(\EH\003\EG0\EcD:mh=\EGp:\
	:mk=\EG1:mp=\E):mr=\EG4:nd=^L:nw=\r\n:pf=^T:\
	:pl=\EZ2%+?%s\177:pn=\Ez%+/%s\r:po=\Ed#:ps=\EP:\
	:px=\EZ1%+?%s\177:r1=\E~!\E~4:r2=\EeF\E`\072:\
	:r3=\EwG\Ee(:\
	:..sa=%?%p8%t\E)%e\E(%;%?%p9%t\EcE%e\EcD%;\EG%'0'%?%p2%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c:\
	:se=\EG0:sf=\n:so=\EGt:sr=\Ej:st=\E1:ta=\011:te=\Ew1:\
	:ti=\Ew0:ts=\EF:ue=\EG0:up=^K:us=\EG8:ve=\E`1:\
	:vi=\E`0:
#
wy120-w|wyse120-w|wy150-w|wyse150-w|wyse 120/150 132-column:\
	:Nl#16:co#132:lw#7:ws#97:\
	:cm=\Ea%i%dR%dC:dc=\EW:ip=:r2=\E`;:tc=wy120:
#
wy120-25|wyse120-25|wy150-25|wyse150-25|wyse 120/150 80-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy120:
#
wy120-25-w|wyse120-25-w|wy150-25-w|wyse150-25-w|wyse 120/150 132-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy120-w:
#
wy120-vb|wyse120-vb|wy150-vb|wyse150-vb|Wyse 120/150 visible bell:\
	:vb=\E`8\E`9:tc=wy120:
#
wy120-w-vb|wy120-wvb|wyse120-wvb|wy150-w-vb|wyse150-w-vb|Wyse 120/150 132-column visible bell:\
	:vb=\E`8\E`9:tc=wy120-w:
#
#	The Wyse 60 is like the Wyse 50 but with more padding.
#	The reset strings are slow and the pad times very depending
#	on other parameters such as font loading.  I have tried
#	to follow the following outline:
#		rs1 -> set personality
#		rs2 -> set number of columns
#		rs3 -> set number of lines
#		is1 -> select the proper font
#		is2 -> do the initialization
#		is3 -> set up display memory (2 pages)
#
#	The Wyse 60's that have vt100 emulation are slower than the
#	older Wyse 60's.  This change happened mid-1987.
#	The capabilities effected are (dch1) (dl1) (il1) (ind) (ri)
#
#	The meta key is only half right.  This terminal will return the
#	high order bit set when you hit CTRL-function_key
#
#	It may be useful to assign two function keys with the
#	values  \E=(\s  look at old data in page 1
#	        \E=W,   look at bottem of page 1
#	where \s is a space ( ).
#
#	Note:
#	   The Wyse 60 runs faster when the XON/XOFF
#	   handshake is turned off.
#
wy60|wyse60|Wyse 60:\
	:5i:am:bs:bw:hs:km:mi:ms:\
	:Nl#8:co#80:lh#1:li#24:lw#8:ws#45:\
	:#2=\E{:%9=\EP:&3=\Er:@8=\E7:DK=\E`b:F1=^AJ\r:\
	:F2=^AK\r:F3=^AL\r:F4=^AM\r:F5=^AN\r:F6=^AO\r:\
	:LF=\EA11:LO=\EA10:RA=\Ed.:RC=\E`c:RX=\Ec20:SA=\Ed/:\
	:SX=\Ec21:\
	:ac=+/\\\054.0[Iha2fxgqh1jYk?lZm@nEqDtCu4vAwBx3yszr{c~~:\
	:ae=\EcD:al=\EE:as=\EcE:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:cl=\E+:cm=\E=%+ %+ :cr=^M:ct=\E0:dc=\EW:dl=\ER:\
	:do=^J:ds=\EF\r:ei=\Er:fs=^M:ho=^^:i1=\EcB0\EcC1:\
	:i2=\EwJ\Ew1:im=\Eq:ip=:\
	:is=\Ed$\EcD\E'\Er\EH\003\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1\016\024\El:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kA=\EE:\
	:kB=\EI:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kN=\EK:kP=\EJ:\
	:kS=\EY:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:\
	:ll=^^^K:mb=\EG2:me=\E(\EH\003\EG0\EcD:mh=\EGp:\
	:mk=\EG1:mp=\E):mr=\EG4:nd=^L:nw=\r\n:pf=^T:\
	:pl=\EZ2%+?%s\177:pn=\Ez%+/%s\r:po=\Ed#:ps=\EP:\
	:px=\EZ1%+?%s\177:r1=\E~!\E~4:r2=\EeG:r3=\EwG\Ee(:\
	:..sa=%?%p8%t\E)%e\E(%;%?%p9%t\EcE%e\EcD%;\EG%'0'%?%p2%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c:\
	:se=\EG0:sf=\n:so=\EGt:sr=\Ej:st=\E1:ta=\011:te=\Ew1:\
	:ti=\Ew0:ts=\EF:ue=\EG0:up=^K:us=\EG8:ve=\E`1:\
	:vi=\E`0:
#
wy60-w|wyse60-w|wyse 60 132-column:\
	:Nl#16:co#132:lw#7:ws#97:\
	:cm=\Ea%i%dR%dC:dc=\EW:ip=:r2=\EeF\E`;:tc=wy60:
#
wy60-25|wyse60-25|wyse 60 80-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy60:
wy60-25-w|wyse60-25-w|wyse 60 132-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy60-w:
#
wy60-42|wyse60-42|wyse 60 80-column 42-lines:\
	:li#42:\
	:al=\EE:cd=\Ey:cl=\E+:cm=\E=%+ %+ :dc=\EW:dl=\ER:\
	:i1=\EcB2\EcC3:ip=:nw=\r\n:r3=\Ee*:sf=\n:sr=\Ej:tc=wy60:
wy60-42-w|wyse60-42-w|wyse 60 132-column 42-lines:\
	:Nl#16:co#132:lw#7:ws#97:\
	:cd=\Ey:cl=\E+:cm=\Ea%i%dR%dC:dc=\EW:ho=\036:ip=:\
	:nw=\r\n:r2=\EeF\E`;:tc=wy60-42:
#
wy60-43|wyse60-43|wyse 60 80-column 43-lines:\
	:Nl@:lh@:li#43:lw@:\
	:pn@:r3=\Ee+:tc=wy60-42:
wy60-43-w|wyse60-43-w|wyse 60 132-column 43-lines:\
	:Nl@:lh@:li#43:lw@:\
	:pn@:r3=\Ee+:tc=wy60-42-w:
#
wy60-vb|wyse60-vb|Wyse 60 visible bell:\
	:vb=\E`8\E`9:tc=wy60:
wy60-w-vb|wy60-wvb|wyse60-wvb|Wyse 60 132-column visible bell:\
	:vb=\E`8\E`9:tc=wy60-w:

#	The Wyse-99GT looks at lot like the Wyse 60 except that it
#	does not have the 42/43 line mode.  In the Wyse-60 the "lines"
#	setup parameter controls the number of lines on the screen.
#	For the Wyse 99GT the "lines" setup parameter controls the
#	number of lines in a page.  The screen can display 25 lines max.
#	    The Wyse-99GT also has personalities for the VT220 and
#	Tektronix 4014.  But this has no bearing on the native mode.
#
#	(msgr) should be set but the clear screen fails when in
#	alt-charset mode.  Try \EcE  \E+  if the screen is really clear
#	then set msgr, else use msgr@.
#
#	u0 -> enter Tektronix mode
#	u1 -> exit Tektronix mode
#
wy99gt|wyse99gt|Wyse 99gt:\
	:ms@:\
	:al=\EE:cd=\Ey:ce=\Et:cl=\E+:dc=\EW:dl=\ER:i2=\Ew0:\
	:ip=:nw@:r2=\E`\072:sf=\n:sr=\Ej:ta=\011:te=\Ew0:\
	:ti=\Ew1:u0=\E~>\E8:u1=\E[42h:tc=wy60:
#
wy99gt-w|wyse99gt-w|wyse 99gt 132-column:\
	:Nl#16:co#132:lw#7:ws#97:\
	:cd=\Ey:cl=\E+:cm=\Ea%i%dR%dC:dc=\EW:ip=:r2=\E`;:tc=wy99gt:
#
wy99gt-25|wyse99gt-25|wyse 99gt 80-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r2=\E`\072:r3=\EwG\Ee):tc=wy99gt:
#
wy99gt-25-w|wyse99gt-25-w|wyse 99gt 132-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r2=\E`;:tc=wy99gt-w:
#
wy99gt-vb|wyse99gt-vb|Wyse 99gt visible bell:\
	:vb=\E`8\E`9:tc=wy99gt:
#
wy99gt-w-vb|wy99gt-wvb|wyse99gt-wvb|Wyse 99gt 132-column visible bell:\
	:vb=\E`8\E`9:tc=wy99gt-w:
#
#	The Wyse 160 is combination of the WY-60 and the WY-99gt.
#	The reset strings are slow and the pad times very depending
#	on other parameters such as font loading.  I have tried
#	to follow the following outline:
#		rs1 -> set personality
#		rs2 -> set number of columns
#		rs3 -> set number of lines
#		is1 -> select the proper font
#		is2 -> do the initialization
#		is3 -> set up display memory (2 pages)
#
#	The display memory may be used for either text or graphics.
#	When "Display Memory = Shared" the terminal will have more pages
#	but garbage may be left on the screen when you switch from
#	graphics to text.  If "Display Memory = Unshared" then the
#	text area will be only one page long.
#
wy160|wyse160|Wyse 160:\
	:5i:am:bs:bw:hs:km:mi:ms:\
	:Nl#8:co#80:lh#1:li#24:lw#8:ws#38:\
	:#2=\E{:%9=\EP:&3=\Er:@8=\E7:DK=\E`b:F1=^AJ\r:\
	:F2=^AK\r:F3=^AL\r:F4=^AM\r:F5=^AN\r:F6=^AO\r:\
	:LF=\EA11:LO=\EA10:RA=\Ed.:RC=\E`c:RX=\Ec20:SA=\Ed/:\
	:SX=\Ec21:\
	:ac=+/\\\054.0[Iha2fxgqh1jYk?lZm@nEqDtCu4vAwBx3yszr{c~~:\
	:ae=\EcD:al=\EE:as=\EcE:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:cl=\E+:cm=\E=%+ %+ :cr=^M:ct=\E0:dc=\EW:dl=\ER:\
	:do=^J:ds=\EF\r:ei=\Er:fs=^M:ho=^^:i1=\EcB0\EcC1:\
	:i2=\Ew0:im=\Eq:ip=:\
	:is=\Ed$\EcD\E'\Er\EH\003\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1\016\024\El:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kA=\EE:\
	:kB=\EI:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kN=\EK:kP=\EJ:\
	:kS=\EY:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:\
	:ll=^^^K:mb=\EG2:me=\E(\EH\003\EG0\EcD:mh=\EGp:\
	:mk=\EG1:mp=\E):mr=\EG4:nd=^L:nw=\r\n:pf=^T:\
	:pl=\EZ2%+?%s\177:pn=\Ez%+/%s\r:po=\Ed#:ps=\EP:\
	:px=\EZ1%+?%s\177:r1=\E~!\E~4:r2=\E`\072:r3=\EwG\Ee(:\
	:..sa=%?%p8%t\E)%e\E(%;%?%p9%t\EcE%e\EcD%;\EG%'0'%?%p2%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c:\
	:se=\EG0:sf=\n:so=\EGt:sr=\Ej:st=\E1:ta=^I:te=\Ew0:\
	:ti=\Ew1:ts=\EF:ue=\EG0:up=^K:us=\EG8:ve=\E`1:\
	:vi=\E`0:
#
wy160-w|wyse160-w|wyse 160 132-column:\
	:Nl#16:co#132:lw#7:ws#90:\
	:cm=\Ea%i%dR%dC:dc=\EW:r2=\EeF\E`;:tc=wy160:
#
wy160-25|wyse160-25|wyse 160 80-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy160:
wy160-25-w|wyse160-25-w|wyse 160 132-column 25-lines:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy160-w:
#
wy160-42|wyse160-42|wyse 160 80-column 42-lines:\
	:li#42:\
	:al=\EE:cd=\Ey:cl=\E+:dl=\ER:i1=\EcB2\EcC3:nw=\r\n:\
	:r3=\Ee*:sf=\n:sr=\Ej:tc=wy160:
wy160-42-w|wyse160-42-w|wyse 160 132-column 42-lines:\
	:Nl#16:co#132:lw#7:ws#90:\
	:cm=\Ea%i%dR%dC:dc=\EW:ip=:r2=\EeF\E`;:tc=wy160-42:
#
wy160-43|wyse160-43|wyse 160 80-column 43-lines:\
	:Nl@:lh@:li#43:lw@:\
	:pn@:r3=\Ee+:tc=wy160-42:
wy160-43-w|wyse160-43-w|wyse 160 132-column 43-lines:\
	:Nl@:lh@:li#43:lw@:\
	:pn@:r3=\Ee+:tc=wy160-42-w:
#
wy160-vb|wyse160-vb|Wyse 160 visible bell:\
	:vb=\E`8\E`9:tc=wy160:
wy160-w-vb|wy160-wvb|wyse160-wvb|Wyse 160 132-column visible bell:\
	:vb=\E`8\E`9:tc=wy160-w:
#
#	The Wyse 75 is a vt100 lookalike without advanced video.
#
#	   The Wyse 75 can support one attribute (e.g. Dim, Inverse,
#	Underline) without magic cookies.  The following description
#	uses this capability, but when more than one attribute is
#	put on the screen at once, all attributes will be changed
#	to be the same as the last attribute given.
#	   The Wyse 75 can support more attributes when used with magic
#	cookies.  The wy75-mc terminal description uses magic cookies
#	to correctly handle multiple attributes on a screen.
#
wy75|wyse75|wyse 75:\
	:5i:am:bs:hs:mi:ms:xn:xo:\
	:co#80:li#24:ma#1:pb#1201:ug#1:ws#78:\
	:%1=\E[28~:%9=\E[?5i:*6=\E[4~:@0=\E[1~:@8=\EOM:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[23~:\
	:F2=\E[24~:F3=\E[25~:F4=\E[26~:F5=\E[28~:F6=\E[29~:\
	:F7=\E[31~:F8=\E[32~:F9=\E[33~:FA=\E[34~:FB=\E[35~:\
	:IC=\E[%d@:K1=\EOw:K2=\EOu:K3=\EOy:K4=\EOq:K5=\EOs:\
	:LE=\E[%dD:RA=\E[?7l:RI=\E[%dC:SA=\E[?7h:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:ch=\E[%i%dG:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=\E[%i%d;%dr:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:\
	:ds=\E[>\\\054\001\001\E[>-\001\001:eA=\E)0:\
	:ec=\E[%dX:ei=\E[4l:fs=^A:ho=\E[H:\
	:i1=\E[2;4;20;30l\E[?1;10l\E[12h\E[?7;8;25h:i2=\E[m:\
	:im=\E[4h:ip=:is=\E>\E(B\E)0\017:k1=\E[?5i:k2=\E[?3i:\
	:k3=\E[2i:k4=\E[@:k5=\E[M:k6=\E[17~:k7=\E[18~:\
	:k8=\E[19~:k9=\E[20~:k;=\E[21~:kA=\E[L:kE=\E[K:\
	:kI=\E[@:kL=\E[M:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:\
	:ke=\E>:kh=\E[H:kl=\E[D:kr=\E[C:ks=\E[?1l\E[?7h\E=:\
	:ku=\E[A:le=^H:me=\E[m\017:mh=\E[0t\E[2m:\
	:mr=\E[1t\E[7m:nd=\E[C:pf=\E[4i:po=\E[5i:ps=\E[0i:\
	:r1=\E[13l\E[3l\E!p:r2=\E[35h\E[?3l:r3=\E[?5l:rc=\E8:\
	:..sa=%?%p5%t\E[0t%;%?%p3%p1%|%t\E[1t%;%?%p2%t\E[2t%;%?%p4%t\E[3t%;%?%p1%p2%p3%p4%p5%|%|%|%|%t\E[7m%e\E[m%;%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=\n:so=\E[1t\E[7m:sr=\EM:st=\EH:\
	:ta=^I:ts=\E[>\\\054\001:ue=\E[m:up=\E[A:\
	:us=\E[2t\E[4m:ve=\E[?25h:vi=\E[?25l:
#
#	This terminal description uses the non-hidden attribute mode
#	(with magic cookie).
#
wy75-mc|wyse75-mc|wyse 75 with magic cookies:\
	:ms@:\
	:ma@:sg#1:ug#1:\
	:ae=\E[0p\017:as=\E[0p\016:i2=\E[m\E[p:mb=\E[2p:\
	:me=\E[0p\017:mh=\E[1p:mk=\E[4p:mr=\E[16p:\
	:..sa=\E[%{0}%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{16}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{1}%|%;%?%p7%t%{4}%|%;%dp%?%p9%t\016%e\017%;:\
	:se=\E[0p:so=\E[17p:ue=\E[0p:us=\E[8p:tc=wy75:
wy75-vb|wyse75-vb|wyse 75 with visible bell:\
	:pb@:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy75:
wy75-w|wyse75-w|wyse 75 in 132 column mode:\
	:co#132:ws#130:\
	:r2=\E[35h\E[?3h:tc=wy75:
wy75-wvb|wyse75-wvb|wyse 75 with visible bell 132 columns:\
	:pb@:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy75-w:
#
#	Wyse 85 emulating a vt220 7 bit mode.
#		24 line screen with status line.
#
#	The vt220 mode permits more function keys but it wipes out
#	the escape key.  I strongly reccomend that f11 be set to
#	escape (esc).
#	The terminal may have to be set for 8 data bits and 2 stop
#	bits for the arrow keys to work.
#	The Wyse 85 runs faster with XON/XOFF enabled.  Also the
#	(dch) and (ich) work best when XON/XOFF is set.  (ich) and
#	(dch) leave trash on the screen when used without XON/XOFF.
#
wy85|wyse85|wyse 85:\
	:5i:am:bs:hs:mi:ms:xn:xo:\
	:co#80:it#8:li#24:ws#80:\
	:%1=\E[28~:*6=\E[4~:@0=\E[1~:@8=\EOM:AL=\E[%dL:\
	:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[23~:F2=\E[24~:\
	:F3=\E[25~:F4=\E[26~:F5=\E[28~:F6=\E[29~:F7=\E[31~:\
	:F8=\E[32~:F9=\E[33~:FA=\E[34~:IC=\E[%d@:K1=\EOw:\
	:K2=\EOu:K3=\EOy:K4=\EOq:K5=\EOs:LE=\E[%dD:RA=\E[?7l:\
	:RI=\E[%dC:SA=\E[?7h:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:\
	:cs=\E[%i%d;%dr:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:\
	:ds=\E[40l:eA=\E)0:ec=\E[%dX:ei=\E[4l:fs=\E[1;24r\E8:\
	:ho=\E[H:i1=\E[62;1"p\E[?5W:i2=\E>\E(B\E)0\017\E[m:\
	:im=\E[4h:ip=:\
	:is=\E[2;4;20;30l\E[?1;4;10;16l\E[12h\E[?7;8;25h:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:k6=\E[17~:k7=\E[18~:\
	:k8=\E[19~:k9=\E[20~:k;=\E[21~:kD=\E[3~:kI=\E[2~:\
	:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:ke=\E>:kh=\E[26~:\
	:kl=\E[D:kr=\E[C:ks=\E[?1l\E=:ku=\E[A:l1=PF1:l2=PF2:\
	:l3=PF3:l4=PF4:le=^H:mb=\E[5m:md=\E[1m:me=\E[m\017:\
	:mh=\E[2m:mk=\E[8m:mr=\E[7m:nd=\E[C:pf=\E[4i:\
	:po=\E[5i:ps=\E[0i:r1=\E[13l\E[3l\E!p:\
	:r2=\E[35h\E[?3l:r3=\E[?5l:rc=\E8:\
	:..sa=\E[0%?%p2%t;4%;%?%p3%p1%|%t;7%;%?%p4%t;5%;%?%p5%t;2%;%?%p6%t;1%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=\n:so=\E[7m:sr=\EM:st=\EH:ta=\011:\
	:ts=\E[40h\E7\E[25;%i%p1%dH:ue=\E[m:up=\E[A:us=\E[4m:\
	:ve=\E[?25h:vi=\E[?25l:
#
#	Wyse 85 with visual bell.
wy85-vb|wyse85-vb|wyse 85 with visible bell:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy85:
#
#	Wyse 85 in 132-column mode.
wy85-w|wyse85-w|wyse 85 in 132-column mode:\
	:co#132:ws#132:\
	:r2=\E[35h\E[?3h:tc=wy85:
#
#	Wyse 85 in 132-column mode with visual bell.
wy85-wvb|wyse85-wvb|wyse 85 with visible bell 132-columns:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy85-w:
#
#	Wyse 185 emulating a vt320 7 bit mode.
#
#	This terminal always displays 25 lines.  These lines may be used
#	as 24 data lines and a terminal status line (top or bottom) or
#	25 data lines.  The 48 and 50 line modes change the page size
#	and not the number of lines on the screen.
#
#	The Compose Character key can be used as a meta key if changed
#	by set-up.
#
wy185|wyse185|wyse 185:\
	:5i:am:bs:hs:km:mi:ms:xn:xo:\
	:co#80:it#8:li#24:ws#80:\
	:%1=\E[28~:*6=\E[4~:@0=\E[1~:@8=\EOM:AL=\E[%dL:\
	:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[23~:F2=\E[24~:\
	:F3=\E[25~:F4=\E[26~:F5=\E[28~:F6=\E[29~:F7=\E[31~:\
	:F8=\E[32~:F9=\E[33~:FA=\E[34~:IC=\E[%d@:K1=\EOw:\
	:K2=\EOu:K3=\EOy:K4=\EOq:K5=\EOs:LE=\E[%dD:RA=\E[?7l:\
	:RI=\E[%dC:SA=\E[?7h:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:ch=\E[%i%d`:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=\E[%i%d;%dr:ct=\E[3g:cv=\E[%i%dd:dc=\E[P:\
	:dl=\E[M:do=^J:ds=\E7\E[99;0H\E[K\E8:eA=\E)0:\
	:ec=\E[%dX:ei=\E[4l:fs=\E[1;24r\E8:ho=\E[H:i1=\E[?5W:\
	:i2=\E>\E(B\E)0\017\E[m:im=\E[4h:ip=:\
	:is=\E[2;4;20;30l\E[?1;4;10;16l\E[12h\E[?7;8;25h:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:k6=\E[17~:k7=\E[18~:\
	:k8=\E[19~:k9=\E[20~:k;=\E[21~:kB=\E[Z:kD=\E[3~:\
	:kI=\E[2~:kN=\E[6~:kP=\E[5~:kb=^H:kd=\E[B:ke=\E>:\
	:kh=\E[26~:kl=\E[D:kr=\E[C:ks=\E[?1l\E=:ku=\E[A:\
	:l1=PF1:l2=PF2:l3=PF3:l4=PF4:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[m\017:mh=\E[2m:mk=\E[8m:mr=\E[7m:nd=\E[C:\
	:pf=\E[4i:po=\E[5i:ps=\E[0i:\
	:r1=\E[13l\E[3l\E\\\E[63;1"p\E[!p:r2=\E[35h\E[?3l:\
	:r3=\E[?5l\E[47h\E[40l\E[r:rc=\E8:\
	:..sa=\E[0%?%p2%t;4%;%?%p3%p1%|%t;7%;%?%p4%t;5%;%?%p5%t;2%;%?%p6%t;1%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[27m:sf=\n:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:te=\E[ R:ti=\E[ Q:ts=\E7\E[99;%i%p1%dH:ue=\E[24m:\
	:up=\E[A:us=\E[4m:ve=\E[34h\E[?25h:vi=\E[?25l:\
	:vs=\E[?25h\E[34l:
#
#	Wyse 185 with 24 data lines and top status (terminal status)
wy185-24|wyse185-24|wyse 185 with 24 data lines:\
	:hs@:\
	:ds@:fs@:r3=\E[?5l\E[47h\E[40l\E[1;24r:ts@:tc=wy185:
#
#	Wyse 185 with visual bell.
wy185-vb|wyse185-vb|wyse 185 with visible bell:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy185:
#
#	Wyse 185 in 132-column mode.
wy185-w|wyse185-w|wyse 185 in 132-column mode:\
	:co#132:ws#132:\
	:DC=\E[%dP:IC=\E[%d@:dc=\E[P:ei=:im=:ip=:\
	:r2=\E[35h\E[?3h:tc=wy185:
#
#	Wyse 185 in 132-column mode with visual bell.
wy185-wvb|wyse185-wvb|wyse 185 with visible bell 132-columns:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy185-w:

# wy325 terminfo entries
# Done by Joe H. Davis        3-9-92

# lines 25  columns 80
#
wy325|wyse325|Wyse-epc:\
	:5i:am:bs:bw:hs:mi:\
	:Nl#8:co#80:lh#1:li#24:lw#8:pb#9601:ws#45:\
	:#2=\E{:%9=\EP:&3=\Er:@8=\E7:F1=^AJ\r:F2=^AK\r:\
	:F3=^AL\r:F4=^AM\r:F5=^AN\r:F6=^AO\r:LF=\EA11:\
	:LO=\EA10:RA=\Ed.:SA=\Ed/:\
	:ac=+/\\\054.0[Iha2fxgqh1jYk?lZm@nEqDtCu4vAwBx3yszr{c~~:\
	:ae=\EcD:al=\EE:as=\EcE:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:cl=\E+:cm=\E=%+ %+ :cr=^M:ct=\E0:dc=\EW:dl=\ER:\
	:do=^J:ds=\EF\r:ei=\Er:fs=^M:ho=^^:i1=\EcB0\EcC1:\
	:i2=\Ew0:im=\Eq:ip=:\
	:is=\EcD\E'\Er\EH\003\Ed/\EO\Ee1\Ed*\E`@\E`9\E`1\016\024\El:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kA=\EE:\
	:kB=\EI:kD=\EW:kE=\ET:kI=\Eq:kL=\ER:kN=\EK:kP=\EJ:\
	:kS=\EY:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:\
	:ll=^^^K:mb=\EG2:me=\E(\EH\003\EG0\EcD:mh=\EGp:\
	:mk=\EG1:mp=\E):mr=\EG4:nd=^L:pf=^T:pl=\EZ2%+?%s\177:\
	:pn=\Ez%+/%s\r:po=\Ed#:ps=\EP:px=\EZ1%+?%s\177:\
	:r1=\E~!\E~4:r2=\EeF\E`\072:r3=\EwG\Ee(:\
	:..sa=%?%p8%t\E)%e\E(%;%?%p9%t\EcE%e\EcD%;\EG%'0'%?%p2%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c:\
	:se=\EG0:sf=\n:so=\EGt:sr=\Ej:st=\E1:ta=^I:te=\Ew0:\
	:ti=\Ew1:ts=\EF:ue=\EG0:up=^K:us=\EG8:ve=\E`1:\
	:vi=\E`0:

#
# lines 24  columns 80  vb 
#
wy325-vb|wyse325-vb|wy150-vb:\
	:vb=\E`8\E`9:tc=wy325:

#
# lines 24  columns 132
#
wy325-w|wyse325-w|wy325w-24:\
	:Nl#16:co#132:lw#7:ws#97:\
	:cm=\Ea%i%dR%dC:dc=\EW:ip=:r2=\E`;:tc=wy325:
#
# lines 25  columns 80
#
wy325-25|wyse325-25|wy325-80:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy325:
#
# lines 25  columns 132
#
wy325-25w|wyse325-25w|wy325 132 columns:\
	:Nl@:lh@:li#25:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy325-w:
#
# lines 25  columns 132  vb 
#
wy325-w-vb|wy325-wvb|wyse325-wvb:\
	:vb=\E`8\E`9:tc=wy325-w:

#
# lines 42  columns 80
#
wy325-42|wyse325-42:\
	:Nl@:lh@:li#42:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy325:
#
# lines 42  columns 132
#
wy325-42w|wyse325-42w:\
	:Nl@:lh@:li#42:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy325-w:
#
# lines 42  columns 132  vb 
#
wy325-42w-vb|wy325-42wvb:\
	:vb=\E`8\E`9:tc=wy325-w:
#
# lines 43  columns 80
#
wy325-43|wyse325-43:\
	:Nl@:lh@:li#43:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy325:
#
# lines 43  columns 132
#
wy325-43w|wyse325-43w:\
	:Nl@:lh@:li#43:lw@:\
	:pn@:r3=\EwG\Ee):tc=wy325-w:
#
# lines 43  columns 132  vb 
#
wy325-43w-vb|wy325-43wvb:\
	:vb=\E`8\E`9:tc=wy325-w:
#	Wyse 370
#
#		24 line screen with status line.
#
#	The terminal may have to be set for 8 data bits and 2 stop
#	bits for the arrow keys to work.
#
#	If you change keyboards the terminal will send different
#	escape sequences.
#	The following definition is for the basic terminal without
#	function keys.
#
#	u0 -> enter Tektronix 4010/4014 mode
#	u1 -> exit  Tektronix 4010/4014 mode
#	u2 -> enter ASCII mode (from any ANSI mode)
#	u3 -> exit  ASCII mode (goto native ANSI mode)
#	u4 -> enter Tek 4207 ANSI mode (from any ANSI mode)
#	u5 -> exit  Tek 4207 mode (goto native ANSI mode)
#
# (untranslatable capabilities removed to fit entry within 1023 bytes)
# WARNING: this entry, 1201 bytes long, may core-dump older termcap libraries!
wy370-nk|wyse 370 without function keys:\
	:5i:am:bs:cc:hs:mi:ms:xn:xo:\
	:Co#64:NC#48:co#80:it#8:li#24:pa#64:ws#80:\
	:AL=\E[%dL:DC=\E[%dP:DK=\E[31h:DL=\E[%dM:DO=\E[%dB:\
	:IC=\E[%d@::LE=\E[%dD:RA=\E[?7l:RC=\E[31l:RI=\E[%dC:\
	:SA=\E[?7h:Sb=\E[62;%dw:Sf=\E[61;%dw:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:ch=\E[%i%d`:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=\E[%i%d;%dr:ct=\E[3g:cv=\E[%i%dd:dc=\E[P:\
	:dl=\E[M:do=^J:ds=\E[40l:eA=\E)0:ec=\E[%dX:ei=\E[4l:\
	:fs=\E[1;24r\E8:ho=\E[H:i1=\E[90;1"p\E[?5W:\
	:i2=\E>\017\E)0\E(B\E[63;0w\E[m:im=\E[4h:ip=:\
	:is=\E[2;4;20;30;40l\E[?1;10;16l\E[12h\E[?7;8;25h:\
	:ke=\E>:ks=\E[?1l\E=:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[m\017:mh=\E[2m:mk=\E[8m:mr=\E[7m:nd=\E[C:\
	:oc=\E[60w\E[63;0w\n\E[66;1;4w\n\E[66;2;13w\n\E[66;3;16w\n\E[66;4;49w\n\E[66;5;51w\n\E[66;6;61w\n\E[66;7;64w:\
	:op=\E[m:pf=\E[4i:po=\E[5i:ps=\E[0i:\
	:r1=\E[13l\E[3l\E!p\E[?4i:r2=\E[35h\E[?3l:r3=\E[?5l:\
	:rc=\E8::sc=\E7:se=\E[27m:sf=\n:so=\E[7m:sr=\EM:\
	:st=\EH:ta=\011:te=\E[ R:ti=\E[ Q:\
	:ts=\E[40l\E[40h\E7\E[99;%i%p1%dH:u0=\E[?38h\E8:\
	:u1=\E[?38l\E)0:u2=\E[92;52"p:u3=\E~B:u4=\E[92;76"p::\
	:ue=\E[24m:up=\E[A:us=\E[4m:ve=\E[34h\E[?25h:\
	:vi=\E[?25l:vs=\E[?25h\E[34l:
#
#	Function key set for the ASCII (wy-50 compatable) keyboard
#
wy370-101k|Wyse 370 with 101 key keyboard:\
	:@8=\EOM:F1=\E[23~:F2=\E[24~:F3=\E[25~:F4=\E[26~:\
	:F5=\E[28~:F6=\E[29~:k1=\E[?4i:k2=\E[?3i:k3=\E[2i:\
	:k4=\E[@:k5=\E[M:k6=\E[17~:k7=\E[18~:k8=\E[19~:\
	:k9=\E[20~:k;=\E[21~:kA=\EOP:kB=\E[Z:kD=\EOQ:kI=\EOP:\
	:kL=\EOQ:kN=\E[U:kP=\E[V:kb=^H:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:tc=wy370-nk:
#
#	Function key set for the VT-320 (and wy85) compatable keyboard
#
wy370-105k|Wyse 370 with 105 key keyboard:\
	:%1=\E[28~:*6=\E[4~:@0=\E[1~:@8=\EOM:F1=\E[23~:\
	:F2=\E[24~:F3=\E[25~:F4=\E[26~:F5=\E[28~:F6=\E[29~:\
	:F7=\E[31~:F8=\E[32~:F9=\E[33~:FA=\E[34~:K1=\EOw:\
	:K2=\EOu:K3=\EOy:K4=\EOq:K5=\EOs:k1=\EOP:k2=\EOQ:\
	:k3=\EOR:k4=\EOS:k6=\E[17~:k7=\E[18~:k8=\E[19~:\
	:k9=\E[20~:k;=\E[21~:kD=\E[3~:kI=\E[2~:kN=\E[6~:\
	:kP=\E[5~:kb=^H:kd=\E[B:kh=\E[26~:kl=\E[D:kr=\E[C:\
	:ku=\E[A:l1=PF1:l2=PF2:l3=PF3:l4=PF4:tc=wy370-nk:
#
#	Function key set for the PC compatable keyboard
#
wy370-EPC|Wyse 370 with 102 key keyboard:\
	:@7=\E[1~:@8=\EOM:F1=\E[23~:F2=\E[24~:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\E[M:k6=\E[17~:k7=\E[18~:\
	:k8=\E[19~:k9=\E[20~:k;=\E[21~:kB=\E[Z:kI=\E[2~:\
	:kN=\E[U:kP=\E[V:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:\
	:kr=\E[C:ku=\E[A:tc=wy370-nk:
#
#	Set up the default WY-370.
#
wy370|wyse370|Wyse 370:\
	:tc=wy370-101k:
#
#	Wyse 370 with visual bell.
wy370-vb|Wyse 370 with visible bell:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy370:
#
#	Wyse 370 in 132-column mode.
wy370-w|Wyse 370 in 132-column mode:\
	:co#132:ws#132:\
	:r2=\E[35h\E[?3h:tc=wy370:
#
#	Wyse 370 in 132-column mode with visual bell.
wy370-wvb|Wyse 370 with visible bell 132-columns:\
	:vb=\E[30h\E\\\054\E[30l:tc=wy370-w:
wy370-rv|Wyse 370 reverse video:\
	:r3=\E[32h\E[?5h:tc=wy370:
#
#	Wyse 99gt Tektronix 4010/4014 emulator,
#
wy99gt-tek|Wyse 99gt Tektronix 4010/4014 emulator:\
	:am:bs:os:\
	:co#74:li#35:\
	:bl=^G:cl=\E^L:\
	:..cm=\035%{3040}%{89}%p1%*%-%Py\n%p2%{55}%*%Px\n%gy%{128}%/%{31}%&%{32}%+%c\n%gy%{3}%&%{4}%*%gx%{3}%&%+%{96}%+%c\n%gy%{004}%/%{31}%&%{96}%+%c\n%gx%{128}%/%{31}%&%{32}%+%c\n%gx%{004}%/%{31}%&%{64}%+%c\037:\
	:cr=^M:do=^J:ff=^L:\
	:hd=\036HHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHH\037:\
	:ho=^]7`x @\037:\
	:hu=\036DDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDD\037:\
	:is=\E8:le=^H:nd= :nw=^M^J:u0=\E~>\E8:u1=\E[42h:\
	:up=^K:
#
#	Wyse 160 Tektronix 4010/4014 emulator,
#
wy160-tek|Wyse 160 Tektronix 4010/4014 emulator:\
	:..cm=\035%{3103}%{91}%p1%*%-%Py\n%p2%{55}%*%Px\n%gy%{128}%/%{31}%&%{32}%+%c\n%gy%{3}%&%{4}%*%gx%{3}%&%+%{96}%+%c\n%gy%{004}%/%{31}%&%{96}%+%c\n%gx%{128}%/%{31}%&%{32}%+%c\n%gx%{004}%/%{31}%&%{64}%+%c\037:\
	:ho=^]8`g @\037:tc=wy99gt-tek:
#
#	Wyse 370 Tektronix 4010/4014 emulator,
#
wy370-tek|Wyse 370 Tektronix 4010/4014 emulator:\
	:am:bs:os:\
	:co#80:li#36:\
	:bl=^G:cl=\E^L:\
	:..cm=\035%{775}%{108}%p1%*%{5}%/%-%Py\n%p2%{64}%*%{4}%+%{5}%/%Px\n%gy%{32}%/%{31}%&%{32}%+%c\n%gy%{31}%&%{96}%+%c\n%gx%{32}%/%{31}%&%{32}%+%c\n%gx%{31}%&%{64}%+%c\037:\
	:cr=^M:do=^J:ff=^L:\
	:hd=\036HHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHHH\037:\
	:ho=^]8g @\037:\
	:hu=\036DDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDDD\037:\
	:is=\E8:kb=^H:kd=^J:kl=^H:kr=^I:ku=^K:le=^H:nd= :\
	:nw=^M^J:u0=\E[?38h\E8:u1=\E[?38l\E)0:up=^K:

# Vendor-supplied Wyse entries end here.

# From: Eric Freudenthal <freudent@eric.ultra.nyu.edu>
wy100q|Wyse 100 for Quotron:\
	:bs:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EE:bt=\EI:cd=\EY:ce=\ET:cl=^Z:cm=\E=%+ %+ :\
	:dc=\EW:dl=\ER:do=^J:ei=\Er:ho=^^:im=\Eq:\
	:is=\E`\072\200\EC\EDF\E0\E'\E(\EA21:kd=^J:kl=^H:\
	:kr=^L:ku=^K:nd=^L:se=\EG0:so=\EG4:sr=\Ej:ue=\EG0:\
	:up=^K:us=\EG8:

#### Kermit terminal emulations
#
# Obsolete Kermit versions may be listed in the section describing obsolete
# non-ANSI terminal emulators later in the file.
#

# KERMIT standard all versions.
# Straight ascii keyboard. :sr=\EI: not avail. many versions + bug prone in vi.
# (kermit: removed obsolete ":ma=^Hh^Jj^Kk^Ll^^H:" -- esr)
# From: greg small <gts@populi.berkeley.edu> 9-25-84
kermit|standard kermit:\
	:bs:\
	:co#80:li#24:\
	:cd=\EJ:ce=\EK:cl=\EE:cm=\EY%+ %+ :ho=\EH:\
	:is=K0 Standard Kermit  9-25-84\n:kd=^J:kh=^^:kl=^H:\
	:kr=^L:ku=^K:nd=\EC:up=\EA:
kermitam|standard kermit plus auto-margin:\
	:am:\
	:is=K1 Standard Kermit plus Automatic Margins\n:tc=kermit:
# IBMPC Kermit 1.2.
# Bugs :cd:ce: do not work except at beginning of line!  :cl: does not work,
# but fake with :cl=\EH\EJ (since :cd=\EJ: works at beginning of line).
# From: greg small <gts@populi.berkeley.edu> 8-30-84
pckermit|pckermit12|UCB IBMPC Kermit 1.2:\
	:am:\
	:li#25:\
	:cd@:ce@:cl=\EH\EJ:\
	:is=K2 UCB IBMPC Kermit 1.2  8-30-84\n:tc=kermit:
# IBMPC Kermit 1.20
# Cannot use line 25, now acts funny like ansi special scrolling region.
# Initialization must escape from that region by cursor position to line 24.
# Cannot use character insert because 1.20 goes crazy if insert at col 80.
# Does not use am: because autowrap mode lost when kermit dropped and restarted.
# (pckermit: mapped ":pt:" to ":it#8:" -- esr)
# From: greg small <gts@populi.berkeley.edu> 12-19-84
pckermit120|UCB IBMPC Kermit 1.20:\
	:am@:pt:\
	:it#8:li#24:\
	:al=\EL:dc=\EN:dl=\EM:do=\EB:ei@:im@:\
	:is=\EO\Eq\EJ\EY7 K3 UCB IBMPC Kermit 1.20  12-19-84\n:\
	:se=\Eq:so=\Ep:vs=\EO\Eq\EEK3:tc=kermit:
# MS-DOS Kermit 2.27 for the IBMPC
# Straight ascii keyboard. :sr=\EI: not avail. many versions + bug prone in vi.
# Cannot use line 25, now acts funny like ansi special scrolling region.
# Initialization must escape from that region by cursor position to line 24.
# Does not use am: because autowrap mode lost when kermit dropped and restarted.
# Reverse video for standout like H19.
# (msk227: removed obsolete ":ma=^Hh^Jj^Kk^Ll^^H:";
# mapped ":pt:" to ":it#8:" -- esr)
# From: greg small <gts@populi.berkeley.edu> 3-17-85
msk227|mskermit227|MS-DOS Kermit 2.27 for the IBMPC:\
	:am@:bs:pt:\
	:co#80:it#8:li#24:\
	:al=\EL:cd=\EJ:ce=\EK:cl=\EE:cm=\EY%+ %+ :dc=\EN:\
	:dl=\EM:do=\EB:ei=\EO:ho=\EH:im=\E@:\
	:is=\EO\Eq\EG\Ew\EJ\EY7 K4 MS Kermit 2.27 for the IBMPC 3-17-85\n:\
	:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:nd=\EC:rc=\Ek:sc=\Ej:\
	:se=\Eq:so=\Ep:up=\EA:vs=\EO\Eq\EG\EwK4:
# MS-DOS Kermit 2.27 with automatic margins
# From:	greg small <gts@populi.berkeley.edu> 3-17-85
msk227am|mskermit227am|UCB MS-DOS Kermit 2.27 with automatic margins:\
	:am:\
	:is=\EO\Eq\EG\Ev\EJ\EY7 K5 MS Kermit 2.27 +automatic margins 3-17-85\n:\
	:vs=\EO\Eq\EG\EvK5:tc=msk227:
# MS-DOS Kermit 2.27 UCB 227.14 for the IBM PC
# Automatic margins now default.  Use ansi set graphic rendition for standout,
# underline and ul codes (:md:,:me:,:mr:).  Define function keys.
# (msk22714: removed obsolete ":kn#10:" -- esr)
# From: greg small <gts@populi.berkeley.edu> 3-17-85
msk22714|mskermit22714|UCB MS-DOS Kermit 2.27 UCB 227.14 IBM PC:\
	:am:\
	:is=\EO\Eq\EG\Ev\EJ\EY7 K6 MS Kermit 2.27 UCB 227.14 IBM PC 3-17-85\n:\
	:k0=\E0:k1=\E1:k2=\E2:k3=\E3:k4=\E4:k5=\E5:k6=\E6:\
	:k7=\E7:k8=\E8:k9=\E9:md=\E[1m:me=\E[m:mr=\E[7m:\
	:se=\E[m:so=\E[1m:ue=\E[m:us=\E[4m:vs=\EO\Eq\EG\EvK6:tc=mskermit227:
# This was designed for a VT320 emulator, but it is probably a good start
# at support for the VT320 itself.
# Please send changes with explanations to bug-gnu-emacs@prep.ai.mit.edu.
vt320-k3|MS-Kermit 3.00's vt320 emulation:\
	:am:es:hs:km:mi:ms:xn:\
	:co#80:it#8:li#49:pb#9600:vt#3:\
	:AL=\E[%dL:CC=\E:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:\
	:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:SR=\E[%dL:UP=\E[%dA:\
	:ae=\E(B:al=\E[L:as=\E(0:bl=^G:cd=\E[J:ce=\E[K:\
	:ch=\E[%i%dG:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:\
	:cs=\E[%i%d;%dr:ct=\E[3g:cv=\E[%i%dd:dc=\E[P:dl=\E[M:\
	:do=^J:ds=\E[0$~:ec=\E[%dX:ei=\E[4l:fs=\E[0$}:\
	:ho=\E[H:im=\E[4h:is=\E>\E F\E[?1l\E[?7h\E[r\E[2$~:\
	:k0=\E[21~:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:k6=\E[17~:\
	:k7=\E[18~:k8=\E[19~:k9=\E[20~:kI=\E[2~:kL=\E[3~:\
	:kN=\E[6~:kP=\E[5~:kb=^H:kd=\EOB:ke=\E[?1l\E>:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:nw=^M^J:pf=\E[4i:\
	:po=\E[5i:ps=\E[0i:\
	:r1=\E(B\E)B\E>\E F\E[4;20l\E[12h\E[?1;5;6;38;42l\E[?7;25h\E4i\E?4i\E[m\E[r\E[2$~:\
	:rc=\E8:sc=\E7:se=\E[27m:sf=^J:so=\E[7m:sr=\EM:\
	:st=\EH:ta=^I:ts=\E[1$}\r\E[K:ue=\E[24m:up=\E[A:\
	:us=\E[4m:vb=\E[?5h\E[?5l\E[?5h\E[?5l\E[?5h\E[?5l:\
	:ve=\E[?25h:vi=\E[?25l:

######## OLDER TERMINAL TYPES
#
# This section is devoted to older commercial terminal brands that are now
# discontinued, but known to be still in use or represented by emulations.
#

#### AT&T (att, tty)
#
# This section also includes Teletype-branded VDTs.
#
# The AT&T/Teletype terminals group was sold to SunRiver Data Systems; for
# details, see the header comment on the ADDS section.
#
# These are AT&T's official terminfo entries
#
att2300|ATT2300|sv80|AT&T 2300 Video Information Terminal 80 column mode:\
	:am:eo:mi:ms:xo:\
	:co#80:it#8:li#24:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\E[11r:\
	:F2=\E[12r:F3=\E[13r:F4=\E[14r:F5=\E[15r:F6=\E[16r:\
	:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:al=\E[L:\
	:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:cl=\E[H\E[J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:\
	:ho=\E[H:im=\E[4h:k1=\E[1r:k2=\E[2r:k3=\E[3r:\
	:k4=\E[4r:k5=\E[5r:k6=\E[6r:k7=\E[7r:k8=\E[8r:\
	:k9=\E[9r:k;=\E[10r:kA=\E[L:kB=\E[Z:kC=\E[J:kD=\E[P:\
	:kI=\E[@:kL=\E[M:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=^H:me=\E[m:mr=\E[7m:nd=\E[C:\
	:pf=\E[4i:po=\E[5i:ps=\E[0i:se=\E[0m:sf=^J:so=\E[7m:\
	:ta=^I:up=\E[A:
att2350|AT&T 2350 Video Information Terminal 80 column mode:\
	:pf@:po@:ps@:tc=att2300:
att2300-x40|sv40|AT&T 2300 Video Information Terminal 40 column mode:\
	:co#40:it#5:li#23:\
	:AL@:al@:tc=att2300:
att2350-x40|ATT2350-x40|AT&T 2350 Video Information Terminal 40 column mode:\
	:co#40:it#5:li#23:\
	:AL@:al@:tc=att2350:

# Must setup RETURN KEY - CR, REC'VD LF - INDEX.
# Seems upward compatible with vt100, plus ins/del line/char.
# On sgr, the protection parameter is ignored.
# No check is made to make sure that only 3 parameters are output.
# 	standout= reverse + half-intensity = 3 | 5.
# 	bold= reverse + underline = 2 | 3.
# note that half-bright blinking doesn't look different from normal blinking.
# NOTE:you must program the function keys first, label second!
att5410v1|att4410v1|tty5410v1|AT&T 4410/5410 80 columns - version 1:\
	:am:hs:mi:ms:xo:\
	:Nl#8:co#80:it#8:lh#2:li#24:lw#8:ws#80:\
	:ac=``aaffhhggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~00++--\\\054\\\054..:\
	:ae=^O:al=\E[L:as=^N:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=:fs=\E8:ho=\E[H:\
	:i1=\E[?3l\E)0:\
	:i2=\E[1;03q   f1           \EOP\E[2;03q   f2           \EOQ\E[3;03q   f3           \EOR\E[4;03q   f4           \EOS\E[5;03q   f5           \EOT\E[6;03q   f6           \EOU\E[7;03q   f7           \EOV\E[8;03q   f8           \EOW:\
	:ic=\E[@:im=:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\EOT:\
	:k6=\EOU:k7=\EOV:k8=\EOW:kC=\E[2J:kH=\E[24;1H:kb=^H:\
	:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:ll=\E[24H:mb=\E[5m:md=\E[2;7m:me=\E[m\017:mh=\E[2m:\
	:mk=\E[8m:mr=\E[7m:nd=\E[C:nw=^M^J:\
	:..pn=\E[%p1%d;00q%p2%\072-16s:\
	:..px=\E[%p1%1d;%p2%l%2.2dq   f%p1%1d           %p2%s:\
	:r2=\Ec\E[?3l\E[2;0y:rc=\E8:\
	:..sa=\E[0%?%p1%p5%|%t;2%;%?%p2%p6%|%t;4%;%?%p4%t;5%;%?%p3%p1%|%p6%|%t;7%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:ta=^I:\
	:ts=\E7\E[25;%p1%{1}%+%dH:ue=\E[m:up=\E[A:us=\E[4m:

att4410v1-w|att5410v1-w|tty5410v1-w|AT&T 4410/5410 132 columns - version 1:\
	:co#132:ws#132:\
	:i1=\E[?3h\E)0:r2=\Ec\E[?3h\E[2;0y:tc=att5410v1:

att4410|att5410|tty5410|AT&T 4410/5410 80 columns - version 2:\
	:..px=\E[%p1%d;%p2%l%02dq   f%p1%d           %p2%s:tc=att5410v1:

att4410-nfk|att5410-nfk|4410-nfk|tty5410-nfk|5410-nfk|version 1 AT&T 4410/5410 entry without function keys:\
	:i3@:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:pn@:tc=att4410:

att5410-w|att4410-w|4410-w|tty5410-w|5410-w|AT&T 4410/5410 in 132 column mode:\
	:co#132:ws#132:\
	:i1=\E[?3h\E)0:r2=\Ec\E[?3h\E[2;0y:tc=att4410:

att5410-nsl|4410-nsl|att4410-nsl|ATT4410-nsl|tty5410-nsl|tty5410 entry without pln defined:\
	:pn@:tc=att4410:

otty5410|teletype 5410 for S5R2 curses:\
	:ts=\E7\E[25;%p1%{1}%+%dH:tc=att4410:

# 5410 in terms of a vt100
v5410|5410 in terms of a vt100:\
	:am:mi:ms:xo:\
	:co#80:it#8:li#24:vt#3:\
	:@8=\EOM:K1=\EOq:K2=\EOr:K3=\EOs:K4=\EOp:K5=\EOn:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:dc=\E[P:dl=\E[M:do=^J:eA=\E(B\E)0:ei=:\
	:ho=\E[H:ic=\E[@:im=:k0=\EOy:k1=\EOP:k2=\EOQ:k3=\EOR:\
	:k4=\EOS:k5=\EOt:k6=\EOu:k7=\EOv:k8=\EOl:k9=\EOw:\
	:k;=\EOx:kb=^H:kd=\EOB:ke=\E[?1l\E>:kl=\EOD:kr=\EOC:\
	:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[m\017:mr=\E[7m:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:..sa=\E[0%?%p1%p6%|%t;1%;%?%p2%t;4%;%?%p1%p3%|%t;7%;%?%p4%t;5%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[1;7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:

# 
# Teletype Model 5420 -- A souped up 5410, with multiple windows,
# even! the 5420 has three modes: scroll, window or page mode
# this terminfo should work in scroll or window mode, but doesn't
# take advantage of any of the differences between them.
#
# Has memory below (2 lines!)
# 3 pages of memory (plus some spare)
# The 5410 sequences for cup,cvvis,dch,dl,ech,flash,home,hpa,hts would work
# for these, but these work in both scroll and window mode...
# Unset insert character so insert mode works
# is1 sets 80 column mode,
# is2 escape sequence:
# 1) turn off all fonts
# 2) function keys off, keyboard lock off, control display off,
#    insert mode off, erasure mode off,
# 3) full duplex, monitor mode off, send graphics off, nl on lf off
# 4) reset origin mode
# 5) set line wraparound
# 6) exit erasure mode, positional attribute mode, and erasure extent mode
# 7) clear margins
# 8) program ENTER to transmit ^J,
# We use \212 to program the ^J because a bare ^J will get translated by
# UNIX into a CR/LF. The enter key is needed for AT&T uOMS.
#     1      2            3              4     5     6    7  8
# is3 set screen color to black,
# No representation in terminfo for the delete word key: kdw1=\Ed
# Key capabilities assume the power-up send sequence...
# This rmcup is not strictly necessary, but it helps maximize 
# memory usefulness: rmcup=\Ez,
# Alternate sgr0:	sgr0=\E[0m\EW^O,
# Alternate sgr:	sgr=\E[%?%p1%t2;7%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p5%t;2%;%?%p7%t;8%;m%?%p8%t\EV%;%?%p9%t^N%e^O%;,
# smkx programs the SYS PF keys to send a set sequence.
# It also sets up labels f1, f2, ..., f8, and sends edit keys.
# This string causes them to send the strings kf1-kf8
# when pressed in SYS PF mode.
att4415|tty5420|att5420|AT&T 4415/5420 80 columns:\
	:db:mi:xo:\
	:Nl#8:lh#2:lm#78:lw#8:ws#55:\
	:@1=\Et:@7=\Ez:@8=\Eent:AL=\E[%dL:\
	:CM=\E[%i%p1%d;%p2%dt:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:\
	:IC=\E[%d@:LE=\E[%dD:LF=\E|:LO=\E~:RI=\E[%dC:\
	:SF=\E[%dE:SR=\E[%dF:UP=\E[%dA:bt=\E[Z:ch=\E[%+^AG:\
	:cl=\E[x\E[J:cm=\E[%i%d;%dx:ct=\E[3g:cv=\E[%+^Ad:\
	:ec=\E[%ds\E[%dD:ei=\E[4l:ho=\E[x:i1=\E[?3l:\
	:i2=\E[?5l:ic@:im=\E[4h:\
	:is=\E[0m\017\E[1;2;3;4;6l\E[12;13;14;20l\E[?6;97;99l\E[?7h\E[4i\Ex\E[21;1j\212:\
	:k1=\EOc:k2=\EOd:k3=\EOe:k4=\EOf:k5=\EOg:k6=\EOh:\
	:k7=\EOi:k8=\EOj:kA=\E[L:kB=\E[Z:kD=\E[P:kE=\E[2K:\
	:kF=\E[T:kH=\Eu:kI=\E[4h:kL=\E[M:kN=\E[U:kP=\E[V:\
	:kR=\E[S:ke=\E[19;0j\E[21;1j\212:\
	:ks=\E[19;1j\E[21;4j\Eent:l1=F1:l2=F2:l3=F3:l4=F4:\
	:l5=F5:l6=F6:l7=F7:l8=F8:ll=\Ew:me=\E[0m\017:mp=\EV:\
	:pf=\E[?9i:..pn=\E[%p1%d;0;0;0q%p2%\072-16.16s:\
	:po=\E[?4i:ps=\E[?2i:\
	:..px=\E[%p1%d;%p2%l%02dq   F%p1%d           %p2%s:\
	:..sa=\E[0%?%p1%p5%|%t;2%;%?%p2%p6%|%t;4%;%?%p4%t;5%;%?%p3%p1%|%p6%|%t;7%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:st=\EH:ts=\E7\E[25;%p1%{8}%+%dH:vb=\E[?5h\E[?5l:\
	:ve=\E[11;0j:vs=\E[11;1j:tc=att4410:

att4415-w|tty5420-w|att5420-w|5420-w|AT&T model 4415/5420 in 132 column mode:\
	:co#132:lm#54:ws#97:\
	:i1=\E[?3h:tc=att4415:

att4415-rv|tty5420-rv|att5420-rv|AT&T model 4415/5420 80 columns in reverse video:\
	:i2=\E[?5h:vb=\E[?5l\E[?5h:tc=att4415:

att4415-w-rv|tty5420-w-rv|att5420-w-rv|AT&T model 4415/5420 132 columns in reverse video:\
	:co#132:lm#54:ws#97:\
	:i1=\E[?3h:i2=\E[?5h:vb=\E[?5l\E[?5h:tc=att4415:

# Note that this mode permits programming USER PF KEYS and labels
# However, when you program user pf labels you have to reselect
# user pf keys to make them appear! 
att4415+nl|4415+nl|tty5420+nl|att5420+nl|generic AT&T 4415/5420 changes for not changing labels:\
	:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:\
	:..pn=\E[%p1%d;0;0;1q%p2%\072-16.16s:\
	:..px=\E[%p1%d;%p2%l%02d;0;1q   F%p1%d           %p2%s:

att4415-nl|4415-nl|tty5420-nl|att5420-nl|AT&T 4415/5420 without changing labels:\
	:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:tc=att4415+nl:tc=att4415:

att4415-rv-nl|tty5420-rv-nl|att5420-rv-nl|AT&T 4415/5420 reverse video without changing labels:\
	:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:tc=att4415+nl:tc=att4415-rv:

att4415-w-nl|tty5420-w-nl|att5420-w-nl|AT&T 4415/5420 132 cols without changing labels:\
	:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:tc=att4415+nl:tc=att4415-w:

att4415-w-rv-n|tty5420-w-rv-n|att5420-w-rv-n|AT&T 4415/5420 132 cols reverse without changing labels:\
	:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:tc=att4415+nl:tc=att4415-w-rv:

otty5420|teletype 5420 for SVR2 curses on the 3B-20's:\
	:ch=\E[%+^AG:cv=\E[%+^Ad:tc=tty5420:

att5420_2|AT&T 5420 model 2 in 80 column mode:\
	:am:db:hs:mi:ms:xo:\
	:Nl#8:co#80:it#8:lh#2:li#24:lm#78:lw#8:ws#55:\
	:@1=\Et:@7=\Ez:@8=^J:AL=\E[%dL:CM=\E[%i%p1%d;%p2%dt:\
	:DC=\E[%dP:DL=\E[%dM:IC=\E[%d@:LE=\E[%dD:LF=\E|:\
	:LO=\E~:RI=\E[%dC:SF=\E[%dE:SR=\E[%dF:UP=\E[%dA:\
	:ae=^O:al=\E[L:as=^N:bt=\E[1Z:cb=\E[1K:cd=\E[0J:\
	:ce=\E[0K:ch=\E[%+^AG:cl=\EH\EJ:cm=\E[%i%d;%dH:\
	:cr=\EG:cs=\E[%i%d;%dr:ct=\E[3g:cv=\E[%+^Ad:dc=\E[P:\
	:dl=\E[M:do=\E[1B:ec=\E[%ds\E[%dD:ei=:fs=\E8:ho=\E[H:\
	:i1=\E[0;23r\Ex\Ey\E[2;0j\E[3;3j\E[4;0j\E[5;0j\E[6;0j\E[7;0j\E[8;0j\E[9;1j\E[10;0j\E[15;0j\E[16;1j\E[19;0j\E[20;1j\E[29;0j\E[1;24r:\
	:ic=\E[@:im=:k1=\EOc:k2=\EOd:k3=\EOe:k4=\EOf:k5=\EOg:\
	:k6=\EOh:k7=\EOi:k8=\EOj:kA=\E[L:kB=\E[Z:kC=\E[2J:\
	:kD=\E[P:kE=\E[2K:kF=\E[T:kH=\Eu:kI=\E[4h:kL=\E[M:\
	:kN=\E[U:kP=\E[V:kR=\E[S:kb=^H:kd=\E[B:ke=\E[19;0j:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ks=\E[19;1j:ku=\E[A:l1=F1:\
	:l2=F2:l3=F3:l4=F4:l5=F5:l6=F6:l7=F7:l8=F8:le=^H:\
	:ll=\Ew:mb=\E[5m:me=\E[0m\017:mh=\E[2m:mk=\E[8m:\
	:mp=\EV:mr=\E[7m:nd=\E[1C:nw=^M^J:pf=\E[4i:\
	:..pn=\E[%p1%d;0;0;0q%p2%\072-16.16s\E~:po=\E[5i:\
	:ps=\E[?;2i:\
	:..px=\E[%p1%d;%p2%l%02dq   F%p1%d           %p2%s\E~:\
	:r2=\Ec\E[?3l\E[2;0y:rc=\E8:\
	:..sa=\E[0%?%p1%p5%|%t;2%;%?%p2%p6%|%t;4%;%?%p4%t;5%;%?%p3%p1%|%p6%|%t;7%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:ts=\E7\E[25;%p1%{8}%+%dH:ue=\E[m:us=\E[4m:\
	:vb=\E[?5h\E[?5l:ve=\E[11;0j:vs=\E[11;1j:
att5420_2-w|AT&T 5420 model 2 in 132 column mode:\
	:co#132:\
	:i1=\E[0;23r\Ex\Ey\E[2;0j\E[3;3j\E[4;0j\E[5;1j\E[6;0j\E[7;0j\E[8;0j\E[9;1j\E[10;0j\E[15;0j\E[16;1j\E[19;0j\E[20;1j\E[29;0j\E[1;24r:tc=att5420_2:

att4418|att5418|ATT5418|AT&T 5418 in 80 column mode:\
	:am:xo:\
	:co#80:li#24:\
	:@8=\E[:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:\
	:F1=\E[n:F2=\E[o:F3=\E[H:F4=\E[I:F5=\E[J:F8=\E[K:\
	:F9=\E[L:FA=\E[E:FB=\E[_:FC=\E[M:FD=\E[N:FE=\E[O:\
	:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:ae=^O:\
	:al=\E[1L:as=^N:bl=^G:cd=\E[0J:ce=\E[0K:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[1P:dl=\E[M:do=\E[B:ei=:\
	:ho=\E[H:i1=\E[?3l:ic=\E[1@:im=:is=\E)0\E?6l\E?5l:\
	:k1=\E[h:k2=\E[i:k3=\E[j:k6=\E[k:k7=\E[l:k8=\E[f:\
	:k9=\E[w:k;=\E[m:kC=\E[%:kd=\EU:kh=\Ec:kl=\E@:kr=\EA:\
	:ku=\ES:le=\E[D:mb=\E[5m:me=\E[0m\017:mh=\E[2m:\
	:mr=\E[7m:nd=\E[C:rc=\E8:sc=\E7:se=\E[0m:sf=^J:\
	:so=\E[7m:ue=\E[0m:up=\E[A:us=\E[4m:
att4418-w|att5418-w|AT&T 5418 in 132 column mode:\
	:co#132:\
	:i1=\E[?3h:tc=att5418:

tty4420|teletype 4420:\
	:da:db:eo:ms:ul:xo:\
	:co#80:li#24:lm#72:\
	:al=\EL:bl=^G:cd=\EJ:ce=\Ez:cl=\EH\EJ:cm=\EY%+ %+ :\
	:cr=\EG:dc=\EP:dl=\EM:dm@:do=\EB:ed@:ho=\EH:k0=\EU:\
	:k3=\E@:kA=\EL:kB=\EO:kC=\EJ:kD=\EP:kF=\ES:kI=\E^:\
	:kL=\EM:kR=\ET:kd=\EB:kh=\EH:kl=^H:kr=\EC:ku=\EA:\
	:l0=segment advance:l3=cursor tab:le=\ED:nd=\EC:\
	:se=\E~:sf=\EH\EM\EY7 :so=\E}:ue=\EZ:up=\EA:us=\E\\:

#  The following is a termcap entry for the Teletype 4424
#  asynchronous keyboard-display terminal.  It supports
#  the vi editor.  The terminal must be "set up" as follows,
# 	
# 	HIGHLIGHT DEFINITION	3-TONE
# 	DISPLAY FUNCTION	GROUP III
# 	
#  The second entry below provides limited (a la adm3a)
#  operation under GROUP II.
# 	
#  This must be used with DISPLAY FUNCTION GROUP I or III
# 	and HIGHLIGHT DEFINITION 3-TONE
# The terminal has either bold or blink, depending on options
#
att4424|tty4424|4424-3|teletype 4424:\
	:am:xo:\
	:co#80:li#24:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:\
	:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:ae=\E(B:al=\EL:\
	:as=\E(0:bl=^G:bt=\EO:cd=\EJ:ce=\Ez:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:ct=\EF:dc=\EP:\
	:dl=\EM:do=\EB:ei=:ho=\E[H:ic=\E^:im=:\
	:is=\E[20l\E[?7h:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:\
	:kC=\EJ:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:\
	:ku=\E[A:le=^H:mb=\E3:md=\E3:me=\EX\E~\EZ\E4\E(B:\
	:mh=\EW:mr=\E}:nd=\EC:nw=\EE:\
	:..sa=\E[%?%p1%t7%;%?%p2%t;4%;%?%p3%t;7%;%?%p6%t;1%;%?%p6%p4%|%t;5%;%?%p5%t;0%;m:\
	:se=\E~:sf=^J:so=\E}:sr=\ET:st=\EH:ta=^I:ti=\E[1m:\
	:ue=\EZ:up=\EA:us=\E\\:

att4424-1|tty4424-1|teletype 4424 in display function group I:\
	:kC@:kd=\EB:kh@:kl=\ED:kr=\EC:ku=\EA:tc=att4424:

# The Teletype 5425 is really version 2 of the Teletype 5420. It 
# is quite similar, except for some minor differences. No page 
# mode, for example, so all of the cup sequences used above have 
# to change back to what's being used for the 5410. Many of the 
# option settings have changed their numbering as well.
# 
# This has been tested on a preliminary model.
#
att5425|tty5425|att4425|AT&T 4425/5425:\
	:am:da:db:hs:mi:ms:xn:xo:\
	:Nl#8:co#80:it#8:lh#2:li#24:lm#78:lw#8:ws#55:\
	:@1=\Et:@7=\Ez:@8=\Eent:AL=\E[%dL:DC=\E[%dP:\
	:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:LE=\E[%dD:LF=\E|:\
	:LO=\E~:RI=\E[%dC:SF=\E[%dE:SR=\E[%dF:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:ch=\E[%+^AG:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=\E[%i%d;%dr:ct=\E[3g:cv=\E[%+^Ad:dc=\E[P:\
	:dl=\E[M:do=^J:eA=\E(B\E)0:ec=\E[%ds\E[%dD:ei=\E[4l:\
	:fs=\E8:ho=\E[H:i1=\E<\E[?3l:i2=\E[?5l:im=\E[4h:\
	:is=\E[0m\017\E[1;2;3;4;6l\E[12;13;14;20l\E[?6;97;99l\E[?7h\E[4i\Ex\E[25;1j\212:\
	:k1=\EOc:k2=\EOd:k3=\EOe:k4=\EOf:k5=\EOg:k6=\EOh:\
	:k7=\EOi:k8=\EOj:kA=\E[L:kB=\E[Z:kC=\E[J:kD=\E[P:\
	:kE=\E[2K:kF=\E[T:kI=\E[4h:kL=\E[M:kR=\E[S:kb=^H:\
	:kd=\E[B:ke=\E[21;0j\E[25;1j\212:kh=\E[H:kl=\E[D:\
	:kr=\E[C:ks=\E[21;1j\E[25;4j\Eent\E~:ku=\E[A:le=^H:\
	:ll=\E[24H:mb=\E[5m:md=\E[2;7m:me=\E[m\017:mh=\E[2m:\
	:mk=\E[8m:mp=\EV:mr=\E[7m:nd=\E[C:nw=^M^J:pf=\E[?9i:\
	:..pn=\E[%p1%d;0;0;0q%p2%\072-16.16s:po=\E[?4i:\
	:ps=\E[?2i:\
	:..px=\E[%p1%d;%p2%l%02dq   F%p1%1d           %p2%s:\
	:r2=\Ec\E[?3l\E[2;0y:rc=\E8:\
	:..sa=\E[0%?%p1%p5%|%t;2%;%?%p2%p6%|%t;4%;%?%p4%t;5%;%?%p3%p1%|%p6%|%t;7%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:ts=\E7\E[25;%p1%{8}%+%dH:ue=\E[m:up=\E[A:us=\E[4m:\
	:vb=\E[?5h\E[?5l:ve=\E[12;0j:vs=\E[12;1j:

att5425-nl|tty5425-nl|att4425-nl|AT&T 4425/5425 80 columns no labels:\
	:ks=\E[21;1j\E[25;4j\Eent:tc=att4425:

att5425-nl-w|tty5425-nl-w|att4425-nl-w|AT&T 4425/5425 132 columns no labels:\
	:ks=\E[21;1j\E[25;4j\Eent:tc=att4425-w:

tty5425-fk|att4425-fk|AT&T 4425/5425 without function keys:\
	:ke@:ks@:tc=att5425:

att5425-w|att4425-w|tty5425-w|teletype 4425/5425 in 132 column mode:\
	:co#132:lm#54:ws#97:\
	:i1=\E[?3h:tc=tty5425:

tty5425-w-fk|att4425-w-fk|att5425-w-fk|AT&T 4425/5425 without function keys in wide mode:\
	:ke@:ks@:tc=att5425-w:

	
# This had bogus capabilities: ri=\EM, ri=\E[1U, 
att4426|tty4426|teletype 4426S:\
	:am:da:db:xo:\
	:co#80:li#24:lm#48:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:\
	:LE=\E[%dD:RI=\E[%dC:SF=\E[%dS:SR=\E[%dT:UP=\E[%dA:\
	:ae=\E(B:al=\EL:as=\E(0:bl=^G:cd=\E[J:ce=\E[0K:\
	:ch=\E[%dG:cl=\E[H\E[2J\E[1U\E[H\E[2J\E[1V:\
	:cm=\E[%i%d;%dH:cr=^M:ct=\E[3g:cv=\E[%dd:dc=\EP:\
	:dl=\E[M:do=\E[B:ei=:ho=\E[H:i1=\Ec\E[?7h:ic=\E^:im=:\
	:is=\E[m\E[1;24r:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:\
	:k5=\EOT:k6=\EOU:k7=\EOV:k8=\EOW:kB=\EO:kC=\E[2J:\
	:kH=\E[24;1H:kb=^H:kd=\EB:kh=\E[H:kl=\ED:kr=\EC:\
	:ku=\EA:le=\E[D:ll=\E[24H:md=\E[5m:me=\E[0m\E(B:\
	:mr=\E[7m:nd=\E[C:nw=^M^J:r2=\Ec\E[?3l\E[2;0y:rc=\E8:\
	:sc=\E7:se=\E[0m:sf=^J:so=\E[5m:sr=\ET:st=\E1:ta=^I:\
	:ue=\E[m:up=\EA:us=\E[4m:


# Terminfo entry for the AT&T 510 A Personal Terminal
# Function keys 9 - 16 are available only after the 
# screen labeled (soft keys/action blocks) are labeled.  Function key
# 9 corresponds to the leftmost touch target on the screen,
# function key 16 corresponds to the rightmost.
#
# This entry is based on one done by Ernie Rice at Summit, NJ and
# changed by Anne Gallup, Skokie, IL, ttrdc!anne
att510a|510a|bct510a|510A|AT&T 510A Personal Terminal:\
	:am:mi:ms:xn:xo:\
	:Nl#8:co#80:lh#2:li#24:lw#7:\
	:#4=\E[u:%i=\E[v:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:\
	:DO=\E[%dB:F1=\EOe:F2=\EOf:F3=\EOg:F4=\EOh:F5=\EOi:\
	:F6=\EOj:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=hrisjjkkllmmnnqqttuuvvwwxx{{||}}~~-f\\\054h.e+g`b:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[0J:\
	:ce=\E[0K:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:ct=\E[3g:\
	:dc=\E[P:dl=\E[M:do=\E[1B:eA=\E(B\E)1:ff=^L:ho=\E[H:\
	:i1=\E(B\E)1\E[2l:i2=\E[21;1|\212:k1=\EOm:k2=\EOV:\
	:k3=\EOu:k4=\ENj:k5=\ENe:k6=\ENf:k7=\ENh:k8=\E[H:\
	:k9=\EOc:k;=\EOd:kB=\E[Z:kF=\E[S:kR=\E[T:kb=^H:\
	:kd=\E[B:ke=\E[19;0|:kl=\E[D:kr=\E[C:ks=\E[19;1|:\
	:ku=\E[A:le=^H:mb=\E[5m:md=\E[2;7m:me=\E[m\017:\
	:mh=\E[2m:mr=\E[7m:nd=\E[C:nw=\EE:pf=\E[?8i:\
	:..pn=\E[%p1%dp%p2%\072-16s:po=\E[?4i:ps=\E[0i:\
	:rc=\E8:\
	:..sa=\E[0%?%p5%p6%|%t;2%;%?%p2%t;4%;%?%p4%t;5%;%?%p3%p1%|%p6%|%t;7%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:ve=\E[11;3|:vi=\E[11;0|:\
	:vs=\E[11;2|:

# Terminfo entry for the AT&T 510 D Personal Terminal
# Function keys 9 through 16 are accessed by bringing up the
# system blocks.
# Function key 9 corresponds to the leftmost touch target on the screen,
# function key 16 corresponds to the rightmost.
#
# There are problems with soft key labeling.  These are due to 
# strangenesses in the native terminal that are impossible to
# describe in a terminfo.  
att510d|510d|bct510d|510D|AT&T 510D Personal Terminal:\
	:am:da:db:mi:ms:xn:xo:\
	:Nl#8:co#80:lh#2:li#24:lm#48:lw#7:\
	:#4=\E[u:%i=\E[v:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:\
	:DO=\E[%dB:F1=\EOe:F2=\EOf:F3=\EOg:F4=\EOh:F5=\EOi:\
	:F6=\EOj:IC=\E[%d@:LE=\E[%dD:LF=\E<:LO=\E?:MC=\E\072:\
	:ML=\E4:MR=\E5:RI=\E[%dC:RX=\E[29;1|:SF=\E[%dS:\
	:SR=\E[%dT:SX=\E[29;0|:UP=\E[%dA:\
	:ac=hrisjjkkllmmnnqqttuuvvwwxx{{||}}~~-f\\\054h.e+g`b:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[0J:\
	:ce=\E[0K:ch=\E[%+^AG:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:ct=\E[3g:cv=\E[%+^Ad:dc=\E[P:dl=\E[M:do=\E[1B:\
	:eA=\E(B\E)1:ei=\E[4l:ff=^L:ho=\E[H:\
	:i1=\E(B\E)1\E[5;0|:i2=\E[21;1|\212:im=\E[4h:k1=\EOm:\
	:k2=\EOV:k3=\EOu:k4=\ENj:k5=\ENe:k6=\ENf:k7=\ENh:\
	:k8=\E[H:k9=\EOc:k;=\EOd:kB=\E[Z:kF=\E[S:kR=\E[T:\
	:kb=^H:kd=\E[B:ke=\E[19;0|:kl=\E[D:kr=\E[C:\
	:ks=\E[19;1|:ku=\E[A:le=^H:ll=\E#2:mb=\E[5m:\
	:md=\E[2;7m:me=\E[m\017:mh=\E[2m:mk=\E[8m:mr=\E[7m:\
	:nd=\E[C:nw=\EE:pf=\E[?8i:..pn=\E[%p1%dp%p2%\072-16s:\
	:po=\E[?4i:ps=\E[0i:r2=\E[5;0|:rc=\E8:\
	:..rp=%p1%c\E[%p2%{1}%-%db:\
	:..sa=\E[0%?%p5%p6%|%t;2%;%?%p2%t;4%;%?%p4%t;5%;%?%p3%p1%|%p6%|%t;7%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:ve=\E[11;3|:vs=\E[11;2|:

# (untranslatable capabilities removed to fit entry within 1023 bytes)
# WARNING: this entry, 1245 bytes long, may core-dump older termcap libraries!
att513|att513-page|513-page|attis513-pfk|513bct|AT&T 513 Terminal using page mode:\
	:HC:am:mi:ms:xn:xo:\
	:Nl#8:co#80:lh#2:li#24:lw#8:\
	:!1=\EOO:!2=\EOP:!3=\EOS:#1=\EOM:#2=\ENM:#3=\ENJ:\
	:#4=\ENK:%0=\EOt:%1=\EOm:%2=\ENi:%3=\EOl:%4=\ENc:\
	:%5=\ENh:%6=\EOv:%7=\EOr:%8=\ENg:%9=\EOz:%a=\EOL:\
	:%b=\ENC:%c=\ENH:%d=\EOR:%e=\ENG:%f=\EOZ:%g=\EOT:\
	:%h=\EOY:%i=\ENL:%j=\EOQ:&0=\EOW:&1=\EOb:&2=\ENa:\
	:&3=\EOy:&4=\EOB:&5=\EOq:&6=\EOo:&7=\EOp:&8=\EOs:\
	:&9=\ENB:*0=\EOX:*1=\EOU:*2=\END:*3=\EON:*4=\ENF:\
	:*5=\ENE:*6=\ENI:*7=\ENN:*8=\EOA:*9=\EOK:@0=\EOx:\
	:@1=\E9:@2=\EOw:@3=\EOV:@4=\EOu:@5=\ENd:@6=\EOn:\
	:@7=\E0:@8=\Eent:@9=\EOk:AL=\E[%dL:DC=\E[%dP:\
	:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:LE=\E[%dD:LF=\E<:\
	:LO=\E?:RI=\E[%dC:SF=\E[%dE:SR=\E[%dF:UP=\E[%dA:\
	:ac=hrisjjkkllmmnnqqttuuvvwwxx{{||}}~~-f\\\054h.e+g`b:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:ch=\E[%+^AG:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=%i\E[%d;%dr:ct=\E[3g:cv=\E[%+^Ad:dc=\E[P:\
	:dl=\E[M:do=^J:eA=\E(B\E)1:ei=\E[4l:ho=\E[H:\
	:i1=\E?\E[3;3|\E[10;0|\E[21;1|\212\E[6;1|\E[1{\E[?99l:\
	:im=\E[4h:k1=\EOc:k2=\EOd:k3=\EOe:k4=\EOf:k5=\EOg:\
	:k6=\EOh:k7=\EOi:k8=\EOj:kB=\E[Z:kC=\E[J:kD=\ENf:\
	:kE=\EOa:kF=\E[S:kI=\ENj:kL=\ENe:kN=\E[U:kP=\E[V:\
	:kR=\E[T:kb=^H:kd=\E[B:ke=\E[19;0|\E[21;1|\212:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ks=\E[19;1|\E[21;4|\Eent:\
	:ku=\E[A:le=^H:ll=\E#2:mb=\E[5m:md=\E[2;7m:\
	:me=\E[m\017:mh=\E[2m:mk=\E[8m:mr=\E[7m:nd=\E[C:\
	:nw=\EE:pf=\E[?98l\E[?8i::::po=\E[?98l\E[?4i:\
	:ps=\E[?98l\E[0i::\
	:r1=\E?\E[3;3|\E[10;0|\E[21;1|\212\E[6;1|\E[1{\E[?99l\E[2;0|\E[6;1|\E[8;0|\E[19;0|\E[1{\E[?99l:\
	:r2=\E[5;0|:rc=\E8:::sc=\E7:se=\E[m:sf=^J:so=\E[7m:\
	:sr=\EM:st=\EH:ta=^I:ue=\E[m:up=\E[A:us=\E[4m:\
	:ve=\E[11;0|:vs=\E[11;1|:

att500|bct500|500|AT&T-IS 500 terminal:\
	:tc=att513:

# 01-07-88
# printer must be set to EMUL ANSI to accept ESC codes
# cuu1 stops at top margin
# is1 sets cpi 10,lpi 6,form 66,left 1,right 132,top 1,bottom 66,font
#	and alt font ascii,wrap on,tabs cleared
# is2 disables newline on LF,Emphasized off
# The u0 capability sets form length
# (untranslatable capabilities removed to fit entry within 1023 bytes)
# WARNING: this entry, 1034 bytes long, may core-dump older termcap libraries!
att5320|AT&T Model 5320 matrix printer:\
	:YA:YD:\
	:Ya#8192:Yi#10:Yj#12:Yk#100:Yl#72:Ym#120:co#132:it#8:\
	:li#66:\
	:DO=\E[%de:RI=\E[%da:\
	:ZA=%?%p1%{10}%=%t\E[w%e%p1%{12}%=%t\E[2w%e%p1%{5}%=%t\E[5w%e%p1%{13}%=%p1%{14}%=%O%t\E[3w%e%p1%{16}%=%p1%{17}%=%O%t\E[4w%e%p1%{6}%=%t\E[6w%e%p1%{7}%=%t\E[7w%e%p1%{8}%=%t\E[8w%;:\
	:ZB=%?%p1%{2}%=%t\E[4z%e%p1%{3}%=%t\E[5z%e%p1%{4}%=%t\E[6z%e%p1%{6}%=%t\E[z%e%p1%{8}%=%t\E[2z%e%p1%{12}%=%t\E[3z%;:\
	:ZM=\E[5m:ZU=\E[m:\
	:Zj=%?%p1%{0}%=%t\E(B%e%p1%{1}%=%t\E(A%e%p1%{2}%=%t\E(C%e%p1%{3}%=%t\E(D%e%p1%{4}%=%t\E(E%e%p1%{5}%=%t\E(H%e%p1%{6}%=%t\E(K%e%p1%{7}%=%t\E(R%e%p1%{8}%=%t\E(Q%e%p1%{9}%=%t\E(Y%e%p1%{10}%=%t\E(Z%e%p1%{11}%=%t\E(0%e%p1%{12}%=%t\E(1%e%p1%{13}%=%t\E(3%e%p1%{14}%=%ttM:\
	:Zl=\E[;%dr:Zm=\E[%+^As:Zn=\E[;%+^As:Zp=\E[%dr:\
	:Zy=%?%p1%{0}%=%tusascii%e%p1%{1}%=%tenglish%e%p1%{2}%=%tfinnish%e%p1%{3}%=%tjapanese%e%p1%{4}%=%tnorwegian%e%p1%{5}%=%tswedish%e%p1%{6}%=%tgermanic%e%p1%{7}%=%tfrench%e%p1%{8}%=%tcanadian_french%e%p1%{9}%=%titalian%e%p1%{10}%=%tspanish%e%p1%{11}%=%tline%e%p1%ÆM:\
	:ch=\E[%d`:cr=^M:cv=\E[%dd:do=^J:ff=^L:i1=\Ec:\
	:is=\E[20l\r:nd= :ta=^I:u0=\E[%dt:up=\EM:

att5310|AT&T 5310 matrix printer:\
	:co#80:\
	:tc=att5320:

# 5620 terminfo  (2.0 or later ROMS with char attributes)
# assumptions: ind (scroll forward one line) is only done at screen bottom
att5620|dmd|tty5620|ttydmd|5620|5620 terminal 88 columns:\
	:NL:NP:am:xo:\
	:co#88:it#8:li#70:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:IC=\E[%d@:SF=\E[%dS:\
	:SR=\E[%dT:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:do=\E[B:ei=:\
	:ho=\E[H:ic=\E[@:im=:kC=\E[2J:kH=\E[70;1H:kb=^H:\
	:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:md=\E[2m:me=\E[0m:mh=\E[2m:mr=\E[7m:nd=\E[C:nw=^J:\
	:..px=\E[%p1%d;%p2%l%dq%p2%s:r1=\Ec:rc=\E8:sc=\E7:\
	:se=\E[0m:sf=\E[S:so=\E[7m:sr=\E[T:ta=^I:ue=\E[0m:\
	:up=\E[A:us=\E[4m:

att5620-24|dmd-24|teletype dmd 5620 in a 24x80 layer:\
	:li#24:\
	:tc=att5620:

att5620-34|dmd-34|teletype dmd 5620 in a 34x80 layer:\
	:li#34:\
	:tc=att5620:

# Entries for kf15 thru kf28 refer to the shifted system pf keys.
#
# Entries for kf29 thru kf46 refer to the alternate keypad mode
# keys:  = * / + 7 8 9 - 4 5 6 , 1 2 3 0 . ENTER
att605|605bct|AT&T 605  80 column  102key keyboard:\
	:am:eo:xo:\
	:Nl#8:co#80:li#24:lw#8:ws#80:\
	:#4=\E[ A:%i=\E[ @:@7=\E[24;1H:DC=\E[%dP:DL=\E[%dM:\
	:F1=\ENq:F2=\ENr:F3=\ENs:F4=\ENt:F5=\EOC:F6=\EOD:\
	:F7=\EOE:F8=\EOF:F9=\EOG:FA=\EOH:FB=\EOI:FC=\EOJ:\
	:FD=\ENO:FE=\ENP:FF=\ENQ:FG=\ENR:FH=\ENS:FI=\ENT:\
	:FJ=\EOP:FK=\EOQ:FL=\EOR:FM=\EOS:FN=\EOw:FO=\EOx:\
	:FP=\EOy:FQ=\EOm:FR=\EOt:FS=\EOu:FT=\EOv:FU=\EOl:\
	:FV=\EOq:FW=\EOr:FX=\EOs:FY=\EOp:FZ=\EOn:Fa=\EOM:\
	:IC=\E[%d@:LF=\E[2p:LO=\E[p:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=\E)0\016:bl=^G:bt=\E[Z:cb=\E[1K:\
	:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:fs=\E8:\
	:i1=\E[8;0|\E[?\E[13;20l\E[?\E[12h:ic=\E[@:im=\E[4h:\
	:is=\E[0m\017:k1=\EOc:k2=\EOd:k3=\EOe:k4=\EOf:\
	:k5=\EOg:k6=\EOh:k7=\EOi:k8=\EOj:k9=\ENo:k;=\ENp:\
	:kA=\E[L:kB=\E[Z:kC=\E[2J:kD=\E[P:kF=\E[S:kI=\E[@:\
	:kL=\E[M:kN=\E[U:kP=\E[V:kb=^H:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:ll=\E[24H:mb=\E[5m:\
	:md=\E[1m:me=\E[m\017:mh=\E[2m:mk=\E[8m:mr=\E[7m:\
	:nd=\E[C:nw=\EE:pf=\E[?4i:\
	:..pn=\E[%p1%d;0;0;0q%p2%\072-16.16s:po=\E[?5i:\
	:..px=\E[%p1%d;%p2%l%02dq   F%p1%1d           %p2%s:\
	:r2=\Ec\E[?3l:rc=\E8:sc=\E7:se=\E[m:sf=^J:so=\E[7m:\
	:ta=^I:ts=\E7\E[25;%i%p1%dx:ue=\E[m:up=\E[A:us=\E[4m:
att605-pc|605bct-pc|ATT 605 in pc term mode:\
	:@7=\E[F:AL=\E[L:S4=250\E[?11l\E[50;1|:\
	:S5=400\E[50;0|:XF=g:XN=e:\
	:ac=k\277l\332m\300j\331n\305w\302q\304u\264t\303v\301x\263:\
	:al=\E[L:bt=\E[Z:dc=\E[P:dl=\E[M:do=\E[B:ei=:ic=\E[@:\
	:im=:k1=\E[M:k2=\E[N:k3=\E[O:k4=\E[P:k5=\E[Q:k6=\E[R:\
	:k7=\E[S:k8=\E[T:k9=\E[U:k;=\E[V:kB=\E[Z:kD=\E[P:\
	:kI=\E[@:kL=\E[M:kN=\E[G:kP=\E[I:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=\E[D:nd=\E[C:up=\E[A:tc=att605:
att605-w|605bct-w|AT&T 605-w 132 column 102 key keyboard:\
	:co#132:ws#132:\
	:i1=\E[8;0|\E[?4;5;13;15l\E[13;20l\E[?3;7h\E[12h\E(B\E)0:tc=att605:
att610|610bct|AT&T 610; 80 column; 98key keyboard:\
	:am:es:hs:mi:ms:xn:xo:\
	:Nl#8:co#80:it#8:lh#2:li#24:lw#8:ws#80:\
	:#4=\E[ @:%i=\E[ A:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:\
	:DO=\E[%dB:F1=\ENq:F2=\ENr:F3=\ENs:F4=\ENt:IC=\E[%d@:\
	:LE=\E[%dD:LF=\E[2p:LO=\E[p:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:\
	:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:\
	:fs=\E8:ho=\E[H:\
	:i1=\E[8;0|\E[?3;4;5;13;15l\E[13;20l\E[?7h\E[12h\E(B\E)0:\
	:i2=\E(B\E)0:im=\E[4h:is=\E[0m\017:k1=\EOc:k2=\EOd:\
	:k3=\EOe:k4=\EOf:k5=\EOg:k6=\EOh:k7=\EOi:k8=\EOj:\
	:k9=\ENo:k;=\ENp:kB=\E[Z:kC=\E[2J:kF=\E[S:kR=\E[T:\
	:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:ll=\E[24H:mb=\E[5m:md=\E[1m:me=\E[m\017:mh=\E[2m:\
	:mk=\E[8m:mr=\E[7m:nd=\E[C:nw=\EE:pf=\E[?4i:\
	:..pn=\E[%p1%d;0;0;0q%p2%\072-16.16s:po=\E[?5i:\
	:..px=\E[%p1%d;%p2%l%02dq   F%p1%1d           %p2%s:\
	:r2=\Ec\E[?3l:rc=\E8:\
	:..sa=\E[0%?%p6%t;1%;%?%p5%t;2%;%?%p2%t;4%;%?%p4%t;5%;%?%p3%p1%|%t;7%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:\
	:ts=\E7\E[25;%i%p1%dx:ue=\E[m:up=\E[A:us=\E[4m:\
	:vb=\E[?5h\E[?5l:ve=\E[?25h\E[?12l:vi=\E[?25l:\
	:vs=\E[?12;25h:
att610-w|610bct-w|AT&T 610; 132 column; 98key keyboard:\
	:co#132:ws#132:\
	:i1=\E[8;0|\E[?4;5;13;15l\E[13;20l\E[?3;7h\E[12h:tc=att610:

att610-103k|610-103k|610bct-103k|AT&T 610; 80 column; 103key keyboard:\
	:!1=\EOO:!2=\EOP:!3=\EOS:#1=\EOM:%0=\EOt:%1=\EOm:\
	:%2=\ENi:%3=\EOl:%4=\ENc:%5=\ENh:%6=\EOv:%7=\EOr:\
	:%8=\ENg:%9=\EOz:%a=\EOL:%b=\ENC:%c=\ENH:%d=\EOR:\
	:%e=\ENG:%f=\EOZ:%g=\EOT:%h=\EOY:%j=\EOQ:&0=\EOW:\
	:&1=\EOb:&2=\ENa:&3=\EOy:&4=\EOB:&5=\EOq:&6=\EOo:\
	:&7=\EOp:&8=\EOs:&9=\ENB:*0=\EOX:*1=\EOU:*2=\END:\
	:*3=\EON:*4=\ENF:*5=\ENE:*6=\ENI:*7=\ENN:*8=\EOA:\
	:*9=\EOK:@0=\EOx:@1=\E9:@2=\EOw:@3=\EOV:@4=\EOu:\
	:@5=\ENd:@6=\EOn:@7=\E0:@8=^M:@9=\EOk:F1@:F2@:F3@:\
	:F4@:k9@:k;@:kD=\ENf:kE=\EOa:kI=\ENj:kL=\ENe:kM=\ENj:\
	:kN=\E[U:kP=\E[V:tc=att610:
att610-103k-w|610-103k-w|610bct-103k-w|AT&T 610; 132 column; 103key keyboard:\
	:co#132:ws#132:\
	:i1=\E[8;0|\E[?4;5;13;15l\E[13;20l\E[?3;7h\E[12h:tc=att610-103k:
att615|615mt|AT&T 615; 80 column; 98key keyboard:\
	:#4=\E[ A:%i=\E[ @:F5=\EOC:F6=\EOD:F7=\EOE:F8=\EOF:\
	:F9=\EOG:FA=\EOH:FB=\EOI:FC=\EOJ:FD=\ENO:FE=\ENP:\
	:FF=\ENQ:FG=\ENR:FH=\ENS:FI=\ENT:FJ=\EOP:FK=\EOQ:\
	:FL=\EOR:FM=\EOS:FN=\EOw:FO=\EOx:FP=\EOy:FQ=\EOm:\
	:FR=\EOt:FS=\EOu:FT=\EOv:FU=\EOl:FV=\EOq:FW=\EOr:\
	:FX=\EOs:FY=\EOp:FZ=\EOn:Fa=\EOM:tc=att610:
att615-w|615-w|615mt-w|AT&T 615; 132 column; 98key keyboard:\
	:#4=\E[ A:%i=\E[ @:F5=\EOC:F6=\EOD:F7=\EOE:F8=\EOF:\
	:F9=\EOG:FA=\EOH:FB=\EOI:FC=\EOJ:FD=\ENO:FE=\ENP:\
	:FF=\ENQ:FG=\ENR:FH=\ENS:FI=\ENT:FJ=\EOP:FK=\EOQ:\
	:FL=\EOR:FM=\EOS:FN=\EOw:FO=\EOx:FP=\EOy:FQ=\EOm:\
	:FR=\EOt:FS=\EOu:FT=\EOv:FU=\EOl:FV=\EOq:FW=\EOr:\
	:FX=\EOs:FY=\EOp:FZ=\EOn:Fa=\EOM:tc=att610-w:
att615-103k|615-103k|615mt-103k|AT&T 615; 80 column; 103key keyboard:\
	:#4=\E[ A:%i=\E[ @:tc=att610-103k:
att615-103k-w|615-103k-w|615mt-103k-w|AT&T 615; 132 column; 103key keyboard:\
	:#4=\E[ A:%i=\E[ @:tc=att610-103k-w:
att620|620mtg|AT&T 620; 80 column; 98key keyboard:\
	:am:es:hs:mi:ms:xn:xo:\
	:Nl#8:co#80:it#8:lh#2:li#24:lw#8:ws#80:\
	:#4=\E[ A:%i=\E[ @:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:\
	:DO=\E[%dB:F1=\ENq:F2=\ENr:F3=\ENs:F4=\ENt:F5=\EOC:\
	:F6=\EOD:F7=\EOE:F8=\EOF:F9=\EOG:FA=\EOH:FB=\EOI:\
	:FC=\EOJ:FD=\ENO:FE=\ENP:FF=\ENQ:FG=\ENR:FH=\ENS:\
	:FI=\ENT:FJ=\EOP:FK=\EOQ:FL=\EOR:FM=\EOS:FN=\EOw:\
	:FO=\EOx:FP=\EOy:FQ=\EOm:FR=\EOt:FS=\EOu:FT=\EOv:\
	:FU=\EOl:FV=\EOq:FW=\EOr:FX=\EOs:FY=\EOp:FZ=\EOn:\
	:Fa=\EOM:IC=\E[%d@:LE=\E[%dD:LF=\E[2p:LO=\E[p:\
	:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=\E(B\017:al=\E[L:as=\E)0\016:bl=^G:bt=\E[Z:\
	:cb=\E[1K:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[M:do=\E[B:\
	:ei=\E[4l:fs=\E8:ho=\E[H:\
	:i1=\E[8;0|\E[?3;4;5;13;15l\E[13;20l\E[?7h\E[12h:\
	:i2=\E(B\E)0:im=\E[4h:is=\E[0m\017:k1=\EOc:k2=\EOd:\
	:k3=\EOe:k4=\EOf:k5=\EOg:k6=\EOh:k7=\EOi:k8=\EOj:\
	:k9=\ENo:k;=\ENp:kB=\E[Z:kC=\E[2J:kF=\E[S:kR=\E[T:\
	:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:ll=\E[24H:mb=\E[5m:md=\E[1m:me=\E[m\E(B\017:\
	:mh=\E[2m:mk=\E[8m:mr=\E[7m:nd=\E[C:nw=\EE:pf=\E[?4i:\
	:..pn=\E[%p1%d;0;0;0q%p2%\072-16.16s:po=\E[?5i:\
	:..px=\E[%p1%d;%p2%l%02dq   F%p1%1d           %p2%s:\
	:r2=\Ec\E[?3l:rc=\E8:\
	:..sa=\E[0%?%p6%t;1%;%?%p2%t;4%;%?%p4%t;5%;%?%p3%p1%|%t;7%;%?%p7%t;8%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:\
	:ts=\E7\E[25;%i%p1%dx:ue=\E[m:up=\E[A:us=\E[4m:\
	:vb=\E[?5h\E[?5l:ve=\E[?25h\E[?12l:vi=\E[?25l:\
	:vs=\E[?12;25h:
att620-w|620-w|620mtg-w|AT&T 620; 132 column; 98key keyboard:\
	:co#132:ws#132:\
	:i1=\E[8;0|\E[?4;5;13;15l\E[13;20l\E[?3;7h\E[12h:tc=att620:
att620-103k|620-103k|620mtg-103k|AT&T 620; 80 column; 103key keyboard:\
	:!1=\EOO:!2=\EOP:!3=\EOS:#1=\EOM:%0=\EOt:%1=\EOm:\
	:%2=\ENi:%3=\EOl:%4=\ENc:%5=\ENh:%6=\EOv:%7=\EOr:\
	:%8=\ENg:%9=\EOz:%a=\EOL:%b=\ENC:%c=\ENH:%d=\EOR:\
	:%e=\ENG:%f=\EOZ:%g=\EOT:%h=\EOY:%j=\EOQ:&0=\EOW:\
	:&1=\EOb:&2=\ENa:&3=\EOy:&4=\EOB:&5=\EOq:&6=\EOo:\
	:&7=\EOp:&8=\EOs:&9=\ENB:*0=\EOX:*1=\EOU:*2=\END:\
	:*3=\EON:*4=\ENF:*5=\ENE:*6=\ENI:*7=\ENN:*8=\EOA:\
	:*9=\EOK:@0=\EOx:@1=\E9:@2=\EOw:@3=\EOV:@4=\EOu:\
	:@5=\ENd:@6=\EOn:@7=\E0:@8=^M:@9=\EOk:F1@:F2@:F3@:\
	:F4@:F5@:F6@:F7@:F8@:F9@:FA@:FB@:FC@:FD@:FE@:FF@:FG@:\
	:FH@:FI@:FJ@:FK@:FL@:FM@:FN@:FO@:FP@:FQ@:FR@:FS@:FT@:\
	:FU@:FV@:FW@:FX@:FY@:FZ@:Fa@:k9@:k;@:kD=\ENf:kE=\EOa:\
	:kI=\ENj:kL=\ENe:kM=\ENj:kN=\E[U:kP=\E[V:tc=att620:

att620-103k-w|620-103k-w|620mtg-103k-w|AT&T 620; 132 column; 103key keyboard:\
	:co#132:ws#132:\
	:i1=\E[8;0|\E[?4;5;13;15l\E[13;20l\E[?3;7h\E[12h:tc=att620-103k:

# 630 short descriptions without \E
att630|5630|5630DMD|630MTG|AT&T 630 windowing terminal:\
	:NP:am:da:db:mi:ms:xo:\
	:co#80:it#8:li#60:lm#0:\
	:@8=^M:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:\
	:F1=\ENq:F2=\ENr:F3=\ENs:F4=\ENt:F5=\ENu:F6=\ENv:\
	:F7=\ENw:F8=\ENx:F9=\ENy:FA=\ENz:FB=\EN{:FC=\EN|:\
	:FD=\EN}:FE=\EN~:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:\
	:SF=\E[%dS:SR=\E[%dT:UP=\E[%dA:al=\E[L:bl=^G:bt=\E[Z:\
	:cb=\E[1K:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:ho=\E[H:\
	:im=\E[4h:is=\E[m:k9=\ENo:k;=\ENp:kA=\E[L:kB=\E[Z:\
	:kC=\E[2J:kD=\E[P:kI=\E[@:kL=\E[M:kb=^H:kd=\E[B:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:me=\E[m:\
	:mr=\E[7m:nd=\E[C:nw=^M^J:pf=\E[?4i:po=\E[?5i:\
	:..px=\E[%p1%d;%p2%l%dq%p2%s:r2=\Ec:rc=\E8:\
	:..sa=\E[0%?%p2%t;4%;%?%p1%p3%|%p4%|%p5%|%t;7%;m:\
	:sc=\E7:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:ue=\E[m:\
	:up=\E[A:us=\E[4m:


att630-24|5630-24|5630DMD-24|630MTG-24|AT&T 630 windowing terminal 24 lines:\
	:li#24:\
	:tc=att630:

# This entry was modified 3/13/90 by JWE.
# fixes include additions of enacs, correcting rep, and modification
# of kHOM.  (See comments below)
# has status line of 80 chars
# These were commented out: indn=\E[%p1%dS, rin=\E[%p1%dT,
# the k25 and up keys are used for shifted system Fkeys
# NOTE: JWE 3/13/90 The 98 key keyboard translation for shift/HOME is 
# currently the same as khome (unshifted HOME or \E[H).  On the 102, 102+1
# and 122 key keyboards, the 730's translation is \E[2J.  For consistency
# kHOM has been commented out.  The user can uncomment kHOM if using the
# 102, 102+1, or 122 key keyboards
#       kHOM=\E[2J,
# (untranslatable capabilities removed to fit entry within 1023 bytes)
# WARNING: this entry, 1063 bytes long, may core-dump older termcap libraries!
att730|730MTG|AT&T 730 windowing terminal Version:\
	:NP:am:da:db:es:hs:mi:ms:xn:xo:\
	:Nl#24:co#80:it#8:lh#2:li#60:lm#0:lw#8:ws#80:\
	:#4=\E[ @:%i=\E[ A:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:\
	:DO=\E[%dB:F1=\ENq:F2=\ENr:F3=\ENs:F4=\ENt:F5=\ENu:\
	:F6=\ENv:F7=\ENw:F8=\ENx:F9=\ENy:FA=\ENz:FB=\EN{:\
	:FC=\EN|:FD=\EN}:FE=\EN~:FF=\EOC:FG=\EOD:FH=\EOE:\
	:FI=\EOF:FJ=\EOG:FK=\EOH:FL=\EOI:FM=\EOJ:FN=\ENO:\
	:FO=\ENP:FP=\ENQ:FQ=\ENR:FR=\ENS:FS=\ENT:FT=\EOU:\
	:FU=\EOV:FV=\EOW:FW=\EOX:FX=\EOY:FY=\EOZ:FZ=\EO[:\
	:Fa=\EO :Fb=\EO]:Fc=\EO^:IC=\E[%d@:LE=\E[%dD:\
	:LF=\E[?13h:LO=\E[?13l:RI=\E[%dC:RX=\E[?21l:\
	:SX=\E[?21h:UP=\E[%dA:ZF=\E#6:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:\
	:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[M:do=\E[B:eA=\E(B\E)0:\
	:ei=\E[4l:fs=\E8:ho=\E[H:\
	:i1=\E[8;0|\E[?3;4;5;13;15l\E[13;20l\E[?7h\E[12h\E(B\E)B:\
	:i2=\E(B\E)0:im=\E[4h:is=\E[0m\017:k1=\EOc:k2=\EOd:\
	:k3=\EOe:k4=\EOf:k5=\EOg:k6=\EOh:k7=\EOi:k8=\EOj:\
	:k9=\ENo:k;=\ENp:kA=\E[L:kB=\E[Z:kC=\E[2J:kF=\E[S:\
	:kI=\E[@:kR=\E[T:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[m\017:\
	:mh=\E[2m:mk=\E[8m:mr=\E[7m:nd=\E[C:nw=\EE:pf=\E[?4i:\
	::po=\E[?5i:ps=\E[?19h\E[0i::r2=\Ec\E[?3l:rc=\E8:::\
	:sc=\E7:se=\E[27m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:\
	:ts=\E7\E[;%i%p1%dx:ue=\E[24m:up=\E[A:us=\E[4m:\
	:vb=\E[?5h\E[?5l:ve=\E[?25h\E[?12l:vi=\E[?25l:\
	:vs=\E[?12;25h::

att730-41|730MTG-41|AT&T 730-41 windowing terminal Version:\
	:li#41:\
	:tc=att730:

att730-24|730MTG-24|AT&T 730-24 windowing terminal Version:\
	:li#24:\
	:tc=att730:

att730r|730MTGr|AT&T 730 rev video windowing terminal Version:\
	:i1=\E[8;0|\E[?3;4;13;15l\E[?5h\E[13;20l\E[?7h\E[12h\E(B\E)B:\
	:vb=\E[?5l\E[?5h:tc=att730:

att730r-41|730MTG-41r|AT&T 730r-41 rev video windowing terminal Version:\
	:li#41:\
	:tc=att730r:

att730r-24|730MTGr-24|AT&T 730r-24 rev video windowing terminal Version:\
	:li#24:\
	:tc=att730r:


# 05-Aug-86:
# The following Terminfo entry describes functions which are supported by
# the AT&T 5430/pt505 terminal software version 2 and later.
#
# The following represents the screen layout along with the associated
# bezel buttons for the 5430/pt505 terminal. The "kf" designations do
# not appear on the screen but are shown to reference the bezel buttons.
# The "CMD", "MAIL", and "REDRAW" buttons are shown in their approximate
# position relative to the screen.
#
#
#
#      +----------------------------------------------------------------+
#      |                                                                |
# XXXX | kf0                                                       kf24 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf1                                                       kf23 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf2                                                       kf22 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf3                                                       kf21 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf4                                                       kf20 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf5                                                       kf19 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf6                                                       kf18 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX |                                                                | XXXX
#      |                                                                |
#      |                                                                |
#      +----------------------------------------------------------------+
#
#          XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX
#
# Note: XXXX represents the screen buttons
#                                                          CMD   REDRAW
#
#                                                          MAIL
#
# Depression of the "CMD" key sends    \E!    (kcmd)
# Depression of the "MAIL" key sends   \E[26s (kf26)
# "REDRAW" same as "REFRESH" (krfr)
#
# "kf" functions adds carriage return to output string if terminal is in
# 'new line' mode.
#
# The following are functions not covered in the table above:
#
#       Set keyboard character (SKC): \EPn1;Pn2w
#                       Pn1= 0 Back Space key
#                       Pn1= 1 Break key
#                       Pn2=   Program char (hex)
#
#       Screen Definition (SDF): \E[Pn1;Pn2;Pn3;Pn4;Pn5t
#                       Pn1=     Window number (1-39)
#                       Pn2-Pn5= Y;X;Y;X coordinates
#
#       Screen Selection (SSL): \E[Pnu
#                       Pn= Window number
#
#       Set Terminal Modes (SM): \E[Pnh
#                       Pn= 3 Graphics mode
#                       Pn= > Cursor blink
#                       Pn= < Enter new line mode
#                       Pn= = Enter reverse insert/replace mode
#                       Pn= ? Enter no scroll mode
#
#       Reset Terminal Mode (RM): \E[Pnl
#                       Pn= 3 Exit graphics mode
#                       Pn= > Exit cursor blink
#                       Pn= < Exit new line mode
#                       Pn= = Exit reverse insert/replace mode
#                       Pn= ? Exit no scroll mode
#
#       Screen Status Report (SSR): \E[Pnp
#                       Pn= 0 Request current window number
#                       Pn= 1 Request current window dimensions
#
#       Device Status Report (DSR): \E[6n    Request cursor position
#
#       Call Status Report (CSR): \E[Pnv
#                       Pn= 0 Call failed
#                       Pn= 1 Call successful
#
#       Transparent Button String (TBS): \E[Pn1;Pn2;Pn3;{string
#                       Pn1= Button number to be loaded
#                       Pn2= Character count of "string"
#                       Pn3= Key mode being loaded:
#                               0= Unshifted
#                               1= Shifted
#                               2= Control
#                       String= Text string (15 chars max)
#
#       Screen Number Report (SNR): \E[Pnp
#                       Pn= Screen number
#
#       Screen Dimension Report (SDR): \E[Pn1;Pn2r
#                       Pn1= Number of rows available in window
#                       Pn2= Number of columns available in window
#
#       Cursor Position Report (CPR): \E[Pn1;Pn2R
#                       Pn1= "Y" Position of cousor
#                       Pn2= "X" Position of cursor
#
#       Request Answer Back (RAB): \E[c
#
#       Answer Back Response (ABR): \E[?;*;30;VSV
#                       *=  0 No printer available
#                       *=  2 Printer available
#                       V=  Software version number
#                       SV= Software sub version number
#
#       Screen Alingment Aid: \En
#
#       Bell (lower pitch): \E[x
#
#       Dial Phone Number: \EPdstring\
#                       string= Phone number to be dialed
#
#       Set Phone Labels: \EPpstring\
#                       string= Label for phone buttons
#
#       Set Clock: \EPchour;minute;second\
#
#       Position Clock: \EPsY;X\
#                       Y= "Y" coordinate
#                       X= "X" coordinate
#
#       Delete Clock: \Epr\
#
#       Programming The Function Buttons: \EPfPn;string\
#                       Pn= Button number (00-06, 18-24)
#                                         (kf00-kf06, kf18-kf24)
#                       string= Text to sent on button depression
#
#       Request For Local Directory Data: \EPp12;\
#
#       Local Directory Data to host: \EPp11;LOCAL...DIRECTORY...DATA\
#
#	Request for Local Directory Data in print format: \EPp13;\
#
#	Enable 'Prt on Line' mode: \022 (DC2)
#
#	Disable 'Prt on Line' mode: \024 (DC4)
#
att505|pt505|att5430|gs5430|AT&T Personal Terminal 505 or 5430 GETSET terminal:\
	:am:xo:\
	:co#80:it#8:li#24:\
	:&2=\E[27s:@4=\E!:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:\
	:DO=\E[%dB:F8=\E[18s:F9=\E[19s:FA=\E[20s:FB=\E[21s:\
	:FC=\E[22s:FD=\E[23s:FE=\E24s:FG=\E26s:LE=\E[%dD:\
	:RA=\E[11;1j:RI=\E[%dC:SA=\E[11;0j:UP=\E[%dA:\
	:ae=\E[10m:al=\E[L:as=\E[11m:bl=^G:cb=\E2K:cd=\E[0J:\
	:ce=\E[0K:cl=\E[2J\E[H:cm=\E[%d;%dH:cr=^M:dc=\E[P:\
	:dl=\E[M:do=\E[B:ei=\E[4l:ho=\E[H:\
	:i1=\EPr\\E[0u\E[2J\E[0;0H\E[0m\E[3l\E[<l\E[4l\E[>l\E[=l\E[?l:\
	:im=\E[4h:k0=\E[00s:k1=\E[01s:k2=\E[02s:k3=\E[03s:\
	:k4=\E[04s:k5=\E[05s:k6=\E[06s:kb=^H:kd=\E[B:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=\E[D:mb=\E[5m:md=\E[1m:me=\E[0m:\
	:mr=\E[7m:nd=\E[C:pf=\E[4i:po=\E[5i:r1=\Ec:rc=\E8:\
	:sc=\E7:se=\E[0m:sf=^J:so=\E[1m:ta=^I:ue=\E[0m:\
	:up=\E[A:us=\E[4m:ve=\E[>l:vs=\E[>h:

#
# The following Terminfo entry describes functions which are supported by
# the AT&T 5430/pt505 terminal software version 1.
#
# The following represents the screen layout along with the associated
# bezel buttons for the 5430/pt505 terminal. The "kf" designations do
# not appear on the screen but are shown to reference the bezel buttons.
# The "CMD", "MAIL", and "REDRAW" buttons are shown in their approximate
# position relative to the screen.
#
#
#
#      +----------------------------------------------------------------+
#      |                                                                |
# XXXX | kf0                                                       kf24 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf1                                                       kf23 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf2                                                       kf22 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf3                                                       kf21 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf4                                                       kf20 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf5                                                       kf19 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX | kf6                                                       kf18 | XXXX
#      |                                                                |
#      |                                                                |
# XXXX |                                                                | XXXX
#      |                                                                |
#      |                                                                |
#      +----------------------------------------------------------------+
#
#          XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX  XXXX
#
# Note: XXXX represents the screen buttons
#                                                          CMD   REDRAW
#
#                                                          MAIL
#
#       Depression of the "CMD" key sends    \E!    (kcmd)
# Depression of the "MAIL" key sends   (note) (kf26)
# "REDRAW" same as "REFRESH" (krfr)    (note)
#
# note: The character string sent by key 'kf26' may be user programmable
#       to send either \E[16s, or \E[26s.
#       The character string sent by key 'krfr' may be user programmable
#       to send either \E[17s, or \E[27s.
#
# "kf" functions adds carriage return to output string if terminal is in
# 'new line' mode.
#
# The following are functions not covered in the table above:
#
#       Set keyboard character (SKC):
#
#               \EPn1;Pn2w
#
#                       Pn1= 0 Back Space key
#                       Pn1= 1 Break key
#                       Pn2=   Program char (hex)
#
#       Screen Definition (SDF):
#
#               \E[Pn1;Pn2;Pn3;Pn4;Pn5t
#
#                       Pn1=     Window number (1-39)
#                       Pn2-Pn5= Y;X;Y;X coordinates
#
#       Screen Selection (SSL):
#
#               \E[Pnu
#
#                       Pn= Window number
#
#       Set Terminal Modes (SM):
#
#               \E[Pnh
#
#                       Pn= 3 Graphics mode
#                       Pn= > Cursor blink
#                       Pn= < Enter new line mode
#                       Pn= = Enter reverse insert/replace mode
#                       Pn= ? Enter no scroll mode
#
#       Reset Terminal Mode (RM):
#
#               \E[Pnl
#
#                       Pn= 3 Exit graphics mode
#                       Pn= > Exit cursor blink
#                       Pn= < Exit new line mode
#                       Pn= = Exit reverse insert/replace mode
#                       Pn= ? Exit no scroll mode
#
#       Screen Status Report (SSR):
#
#               \E[Pnp
#
#                       Pn= 0 Request current window number
#                       Pn= 1 Request current window dimensions
#
#       Device Status Report (DSR):
#
#               \E[6n    Request cursor position
#
#       Call Status Report (CSR):
#
#               \E[Pnv
#
#                       Pn= 0 Call failed
#                       Pn= 1 Call successful
#
#       Transparent Button String (TBS):
#
#               \E[Pn1;Pn2;Pn3;{string
#
#                       Pn1= Button number to be loaded
#                       Pn2= Character count of "string"
#                       Pn3= Key mode being loaded:
#                               0= Unshifted
#                               1= Shifted
#                               2= Control
#                       String= Text string (15 chars max)
#
#       Screen Number Report (SNR):
#
#               \E[Pnp
#
#                       Pn= Screen number
#
#       Screen Dimension Report (SDR):
#
#               \E[Pn1;Pn2r
#
#                       Pn1= Number of rows available in window
#                       Pn2= Number of columns available in window
#
#       Cursor Position Report (CPR):
#
#               \E[Pn1;Pn2R
#
#                       Pn1= "Y" Position of cousor
#                       Pn2= "X" Position of cursor
#
#       Request Answer Back (RAB):
#
#               \E[c
#
#       Answer Back Response (ABR):
#
#               \E[?;0;30;VSV
#
#                       V=  Software version number
#                       SV= Software sub version number
#
#       Screen Alignment Aid:
#
#               \En
#
#       Bell (lower pitch):
#
#               \E[x
#
#       Dial Phone Number:
#
#               \EPdstring\
#
#                       string= Phone number to be dialed
#
#       Set Phone Labels:
#
#               \EPpstring\
#
#                       string= Label for phone buttons
#
#       Set Clock:
#
#               \EPchour;minute;second\
#
#       Position Clock:
#
#               \EPsY;X\
#
#                       Y= "Y" coordinate
#                       X= "X" coordinate
#
#       Delete Clock:
#
#               \Epr\
#
#       Programming The Function Buttons:
#
#               \EPfPn;string\
#
#                       Pn= Button number (00-06, 18-24)
#                                         (kf00-kf06, kf18-kf24)
#
#                       string= Text to sent on button depression
#
#
#
# 							05-Aug-86
#
# 
att505-24|pt505-24|gs5430-24| AT&T PT505 or 5430 GETSET version 1 24 lines:\
	:am:xo:\
	:co#80:it#8:li#24:\
	:&2=\E[27s:@4=\E!:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:\
	:DO=\E[%dB:F8=\E[18s:F9=\E[19s:FA=\E[20s:FB=\E[21s:\
	:FC=\E[22s:FD=\E[23s:FE=\E24s:FG=\E26s:LE=\E[%dD:\
	:RI=\E[%dC:UP=\E[%dA:ae=\E[10m:al=\E[L:as=\E[11m:\
	:bl=^G:cb=\E2K:cd=\E[0J:ce=\E[0K:cl=\E[2J\E[H:\
	:cm=\E[%d;%dH:cr=^M:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:\
	:ho=\E[H:\
	:i1=\EPr\\E[0u\E[2J\E[0;0H\E[0m\E[3l\E[<l\E[4l\E[>l\E[=l\E[?l:\
	:im=\E[4h:k0=\E[00s:k1=\E[01s:k2=\E[02s:k3=\E[03s:\
	:k4=\E[04s:k5=\E[05s:k6=\E[06s:kb=^H:kd=\E[B:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=\E[D:mb=\E[5m:md=\E[1m:me=\E[0m:\
	:mr=\E[7m:nd=\E[C:r1=\Ec:se=\E[0m:sf=^J:so=\E[1m:\
	:ta=^I:ue=\E[0m:up=\E[A:us=\E[4m:ve=\E[>l:vs=\E[>h:
att505-22|pt505-22|gs5430-22| AT&T PT505 or 5430 GETSET version 1 22 lines:\
	:li#22:\
	:tc=att505-24:
#
# -------------------- TERMINFO FILE CAN BE SPLIT HERE -----------------------
# This cut mark helps make life less painful for people running ncurses tic
# on machines with relatively little RAM.  The file can be broken in half here
# cleanly and compiled in sections -- no `use' references cross this cut
# going forward.
#

#### Ampex (Dialogue)
#
# Yes, these are the same people who are better-known for making audio- and
# videotape.  I'm told they are located in Redwood City, CA.

# From: <cbosg!ucbvax!SRC:george> Fri Sep 11 22:38:32 1981
# (ampex80: mapped ":pt:" to default tabs; some capabilities merged in from
# SCO's entry -- esr)
ampex80|a80|d80|dialogue|dialogue80|ampex dialogue 80:\
	:am:bs:bw:pt:ul:\
	:co#80:li#24:\
	:al=\EE:bl=^G:bt=\EI:cd=\Ey:ce=\Et:cl=\E*:\
	:cm=\E=%+ %+ :cr=^M:ct=\E3:dc=\EW:dl=\ER:do=^J:ei=:\
	:ic=\EQ:im=:is=\EA:le=^H:nd=^L:se=\Ek:sf=^J:so=\Ej:\
	:st=\E1:ta=^I:ue=\Em:up=^K:us=\El:
# This entry was from somebody anonymous, Tue Aug  9 20:11:37 1983, who wrote:
ampex175|ampex d175:\
	:am:\
	:co#80:li#24:\
	:al=\EE:bl=^G:cd=\Ey:ce=\Et:cl=\E+:cm=\E=%+ %+ :\
	:cr=^M:dc=\EW:dl=\ER:do=^J:ei=:ho=^^:ic=\EQ:im=:\
	:is=\EX\EA\EF:kA=\EE:kD=\EW:kI=\EQ:kL=\ER:kd=^J:\
	:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:ll=^^^K:nd=^L:se=\Ek:\
	:sf=^J:so=\Ej:te=\EF:ti=\EN:ue=\Em:up=^K:us=\El:
# No backspace key in the main QWERTY cluster. Fortunately, it has a
# NEWLINE/PAGE key just above RETURN that sends a strange single-character
# code.  Given a suitable Unix (one that lets you set an echo-erase-as-BS-SP-BS
# mode), this key can be used as the erase key; I find I like this. Because
# some people and some systems may not, there is another termcap ("ampex175")
# that suppresses this little eccentricity by omitting the relevant capability.
ampex175-b|ampex d175 using left arrow for erase:\
	:kb=^_:tc=ampex175:
# From: Richard Bascove <atd!dsd!rcb@ucbvax.berkeley.edu>
# (ampex210: removed obsolete ":kn#10:"; mapped ":pt:" to default tabs -- esr)
ampex210|a210|ampex a210:\
	:am:bs:hs:pt:xn:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EE:bt=\EI:cd=\Ey:ce=\Et:cl=\E*:cm=\E=%+ %+ :\
	:dc=\EW:dl=\ER:ei=:fs=\E.2:ho=^^:ic=\EQ:\
	:if=/usr/share/tabset/std:im=:\
	:is=\EC\Eu\E'\E(\El\EA\E%\E{\E.2\EG0\Ed\En:k0=^A0\r:\
	:k1=^A1\r:k2=^A2\r:k3=^A3\r:k4=^A4\r:k5=^A5\r:\
	:k6=^A6\r:k7=^A7\r:k8=^A8\r:k9=^A9\r:kd=^V:kh=^^:\
	:kl=^H:kr=^L:ku=^K:nd=^L:se=\EG0:so=\EG4:\
	:ts=\E.0\Eg\E}\Ef:ue=\EG0:up=^K:us=\EG8:\
	:vb=\EU\EX\EU\EX\EU\EX\EU\EX:
ampex219|ampex-219|amp219|Ampex with Automargins:\
	:hs:xn:\
	:co#80:it#8:li#24:\
	:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:cs=%i\E[%2;%2r:do=\E[B:ho=\E[H:\
	:is=\E>\E[?1l\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:\
	:k0=\E[21~:k1=\E[7~:k2=\E[8~:k3=\E[9~:k4=\E[10~:\
	:k5=\E[11~:k6=\E[17~:k7=\E[18~:k8=\E[19~:k9=\E[20~:\
	:kd=\E[B:ke=\E>:kh=\E[H:kl=\E[D:kr=\E[C:ks=\E=:\
	:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[0m:mh=\E[1m:\
	:mr=\E[7m:nd=\E[C:se=\E[0m:sf=^J:so=\E[7m:sr=\EM:\
	:ta=^I:ue=\E[0m:up=\E[A:us=\E[4m:
ampex219w|ampex-219w|amp219w|Ampex 132 cols:\
	:co#132:li#24:\
	:bl=^G:cr=^M:do=^J:\
	:is=\E>\E[?3h\E[?4l\E[?5l\E[?7h\E[?8h:sf=^J:\
	:vs=\E[?3h:tc=ampex219:
ampex232|ampex-232|Ampex Model 232:\
	:am:\
	:co#80:li#24:sg#1:ug#1:\
	:al=5*\EE:bt=\EI:cd=\EY:ce=\ET:cl=\E+:cm=\E=%+ %+ :\
	:dc=\EW:dl=5*\ER:do=^V:ei=:ic=\EQ:\
	:if=/usr/lib/tabset/ampex:im=:is=\Eg\El:k0=^A@\r:\
	:k1=^AA\r:k2=^AB\r:k3=^AC\r:k4=^AD\r:k5=^AE\r:\
	:k6=^AF\r:k7=^AG\r:k8=^AH\r:k9=^AI\r:kb=^H:kd=^V:\
	:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:se=\EG0:so=\EG4:\
	:ta=^I:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eb\200\200\200\200\200\200\200\200\200\200\200\200\200\200\Ed:\
	:ve=\E.4:vi=\E.0:
ampex232w|Ampex Model 232 / 132 columns:\
	:co#132:li#24:\
	:if=/usr/lib/tabset/amp-132:is=\E\034Eg\El:tc=ampex232:

#### Ann Arbor (aa)
#

# Originally from Mike O'Brien@Rand and Howard Katseff at Bell Labs.
# Highly modified 6/22 by Mike O'Brien.
# split out into several for the various screen sizes by dave-yost@rand
# Modifications made 3/82 by Mark Horton
# Modified by Tom Quarles at UCB for greater efficiency and more diversity
# status line moved to top of screen, :vb: removed 5/82
# Some unknown person at SCO then hacked the init strings to make them more
# efficient.
#
# assumes the following setup:
#   A menu: 0000 1010  0001 0000
#   B menu: 9600  0100 1000  0000 0000  1000 0000  17  19
#   C menu: 56   66   0    0    9600  0110 1100
#   D menu: 0110 1001   1   0
#
#	Briefly, the settings are for the following modes:
#	   (values are for bit set/clear with * indicating our preference
#	    and the value used to test these termcaps)
#	Note that many of these settings are irelevent to the termcap
#	and are just set to the default mode of the terminal as shipped
#	by the factory.
#
# A menu: 0000 1010  0001 0000
#	Block/underline cursor*
#	blinking/nonblinking cursor*
#	key click/no key click*
#	bell/no bell at column 72*
#
#	key pad is cursor control*/key pad is numeric
#	return and line feed/return for <cr> key *
#	repeat after .5 sec*/no repeat
#	repeat at 25/15 chars per sec. *
#
#	hold data until pause pressed/process data unless pause pressed*
#	slow scroll/no slow scroll*
#	Hold in area/don't hold in area*
#	functions keys have default*/function keys disabled on powerup
#
#	show/don't show position of cursor during page transmit*
#	unused
#	unused
#	unused
#
# B menu: 9600  0100 1000  0000 0000  1000 0000  17  19
#	Baud rate (9600*)
#
#	2 bits of parity - 00=odd,01=even*,10=space,11=mark
#	1 stop bit*/2 stop bits
#	parity error detection off*/on
#
#	keyboard local/on line*
#	half/full duplex*
#	disable/do not disable keyboard after data transmission*
#
#	transmit entire page/stop transmission at cursor*
#	transfer/do not transfer protected characters*
#	transmit all characters/transmit only selected characters*
#	transmit all selected areas/transmit only 1 selected area*
#
#	transmit/do not transmit line seperators to host*
#	transmit/do not transmit page tab stops tabs to host*
#	transmit/do not transmit column tab stop tabs to host*
#	transmit/do not transmit graphics control (underline,inverse..)*
#
#	enable*/disable auto XON/XOFF control
#	require/do not require receipt of a DC1 from host after each LF*
#	pause key acts as a meta key/pause key is pause*
#	unused
#
#	unused
#	unused
#	unused
#	unused
#
#	XON character (17*)
#	XOFF character (19*)
#
# C menu: 56   66   0    0    9600  0110 1100
#	number of lines to print data on (printer) (56*)
#
#	number of lines on a sheet of paper (printer) (66*)
#
#	left margin (printer) (0*)
#
#	number of pad chars on new line to printer (0*)
#
#	printer baud rate (9600*)
#
#	printer parity: 00=odd,01=even*,10=space,11=mark
#	printer stop bits: 2*/1
#	print/do not print guarded areas*
#
#	new line is: 01=LF,10=CR,11=CRLF*
#	unused
#	unused
#
# D menu: 0110 1001   1   0
#	LF is newline/LF is down one line, same column*
#	wrap to preceeding line if move left from col 1*/don't wrap
#	wrap to next line if move right from col 80*/don't wrap
#	backspace is/is not destructive*
#
#	display*/ignore DEL character
#	display will not/will scroll*
#	page/column tab stops*
#	erase everything*/erase unprotected only
#
#	editing extent: 0=display,1=line*,2=field,3=area
#
#	unused
#

annarbor|4080|ann arbor 4080:\
	:am:\
	:co#80:li#40:\
	:bl=^G:cl=\014:\
	:..cm=\017%p2%{10}%/%{16}%*%p2%{10}%m%+%c%p1%?%p1%{19}%>%t%{12}%+%;%'@'%+%c:\
	:cr=^M:ct=^^P^P:do=^J:ho=^K:kb=^^:kd=^J:kh=^K:kl=^H:\
	:kr=^_:ku=^N:le=^H:nd=^_:sf=^J:st=^]^P1:ta=^I:up=^N:

# If you're using the GNU termcap library, add
#	:cS=\E[%d;%d;%d;%dp:
# to these capabilities.  This is the nonstandard GNU termcap scrolling
# capability, arguments are:
#   1. Total number of lines on the screen.
#   2. Number of lines above desired scroll region.
#   3. Number of lines below (outside of) desired scroll region.
#   4. Total number of lines on the screen, the same as the first parameter.
# The generic Ann Arbor entry is the only one that uses this.
aaa+unk|aaa-unk|ann arbor ambassador (internal - don't use this directly):\
	:5i:am:km:mi:xo:\
	:co#80:it#8:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:F1=\EOK:\
	:F2=\EOL:F3=\EOM:F4=\EON:F5=\EOO:F6=\EOP:F7=\EOQ:\
	:F8=\EOR:F9=\EOS:FA=\EOT:FB=\EOU:FC=\EOV:FD=\EOW:\
	:FE=\EOX:IC=\E[%d@:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:al=\E[L:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:ch=\E[%+^AG:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:ct=\E[2g:\
	:cv=\E[%+^Ad:dc=\E[P:dl=\E[M:do=^K:ei=:ho=\E[H:\
	:i1=\E[m\E7\E[H\E9\E8:i2=\E[1Q\E[>20;30l\EP`+x~M\E\\:\
	:ic=\E[@:im=:k1=\EOA:k2=\EOB:k3=\EOC:k4=\EOD:k5=\EOE:\
	:k6=\EOF:k7=\EOG:k8=\EOH:k9=\EOI:k;=\EOJ:kA=\E[L:\
	:kB=\E[Z:kC=\E[J:kD=\E[P:kI=\E[@:kL=\E[M:kM=\E6:\
	:kb=^H:kd=\E[B:\
	:ke=\EP`>y~[[J`8xy~[[A`4xy~[[D`6xy~[[C`2xy~[[B\E\\:\
	:kh=\E[H:kl=\E[D:kr=\E[C:\
	:ks=\EP`>z~[[J`8xz~[[A`4xz~[[D`6xz~[[C`2xz~[[B\E\\:\
	:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[0m:mk=\E[8m:\
	:mm=\E[>52h:mo=\E[>52l:mr=\E[7m:nd=\E[C:pO=\E[%dv:\
	:pf=^C:po=\E[v:ps=\E[0i:rc=\E8:\
	:..rp=%p1%c\E[%p2%{1}%-%db:\
	:..sa=\E[%?%p1%t7;%;%?%p2%t4;%;%?%p3%t7;%;%?%p4%t5;%;%?%p6%t1;%;m:\
	:sc=\E7:se=\E[m:sf=^K:so=\E[7m:st=\EH:ta=^I:ue=\E[m:\
	:up=\E[A:us=\E[4m:

aaa+rv:\
	:i1=\E[7m\E7\E[H\E9\E8:mb=\E[5;7m:md=\E[1;7m:\
	:me=\E[7m\016:mk=\E[7;8m:mr=\E[m:r1=\E[H\E[7m\E[J:\
	:..sa=\E[%?%p1%p3%|%!%t7;%;%?%p2%t4;%;%?%p4%t5;%;%?%p6%t1;%;%?%p7%t8;%;m:\
	:se=\E[7m:so=\E[m:ue=\E[7m:us=\E[4;7m:
# Ambassador with the DEC option, for partial vt100 compatibility.
aaa+dec:\
	:ac=aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz||}}:\
	:ae=^N:as=^O:cs=\E[%i%d;%dr:eA=\E(0:\
	:..sa=\E[%?%p1%p3%|%!%t7;%;%?%p2%t4;%;%?%p4%t5;%;%?%p6%t1;%;%?%p7%t8;%;m%?%p9%t\017%e\016%;:
aaa-18|ann arbor ambassador/18 lines:\
	:li#18:\
	:is=\E7\E[60;0;0;18p\E8:te=\E[60;0;0;18p\E[60;1H\E[K:\
	:ti=\E[18;0;0;18p:tc=aaa+unk:
aaa-18-rv|ann arbor ambassador/18 lines+reverse video:\
	:tc=aaa+rv:tc=aaa-18:
aaa-20|ann arbor ambassador/20 lines:\
	:li#20:\
	:is=\E7\E[60;0;0;20p\E8:te=\E[60;0;0;20p\E[60;1H\E[K:\
	:ti=\E[20;0;0;20p:tc=aaa+unk:
aaa-22|ann arbor ambassador/22 lines:\
	:li#22:\
	:is=\E7\E[60;0;0;22p\E8:te=\E[60;0;0;22p\E[60;1H\E[K:\
	:ti=\E[22;0;0;22p:tc=aaa+unk:
aaa-24|ann arbor ambassador/24 lines:\
	:li#24:\
	:is=\E7\E[60;0;0;24p\E8:te=\E[60;0;0;24p\E[60;1H\E[K:\
	:ti=\E[24;0;0;24p:tc=aaa+unk:
aaa-24-rv|ann arbor ambassador/24 lines+reverse video:\
	:tc=aaa+rv:tc=aaa-24:
aaa-26|ann arbor ambassador/26 lines:\
	:li#26:\
	:is=\E7\E[60;0;0;26p\E8:te=\E[60;0;0;26p\E[26;1H\E[K:\
	:ti=\E[H\E[J\E[26;0;0;26p:tc=aaa+unk:
aaa-28|ann arbor ambassador/28 lines:\
	:li#28:\
	:is=\E7\E[60;0;0;28p\E8:te=\E[60;0;0;28p\E[28;1H\E[K:\
	:ti=\E[H\E[J\E[28;0;0;28p:tc=aaa+unk:
aaa-30-s|aaa-s|ann arbor ambassador/30 lines w/status:\
	:es:hs:\
	:li#29:\
	:ds=\E7\E[60;0;0;30p\E[1;1H\E[K\E[H\E8\r\n\E[K:\
	:fs=\E[>51l:is=\r\n\E[A\E7\E[60;1;0;30p\E8:\
	:te=\E[60;1;0;30p\E[29;1H\E[K:\
	:ti=\E[H\E[J\E[30;1;0;30p\E[30;1H\E[K:\
	:ts=\E[>51h\E[1;%p1%dH\E[2K:tc=aaa+unk:
aaa-30-s-rv|aaa-s-rv|ann arbor ambassador/30 lines+status line+reverse video:\
	:tc=aaa+rv:tc=aaa-30-s:
aaa-s-ctxt|aaa-30-s-ctxt|ann arbor ambassador/30 lines+status line+save context:\
	:te=\E[60;1;0;30p\E[59;1H\E[K:\
	:ti=\E[30;1H\E[K\E[30;1;0;30p:tc=aaa-30-s:
aaa-s-rv-ctxt|aaa-30-s-rv-ct|aaa-30-srvctxt|ann arbor ambassador/30 lines; status line; saving context:\
	:te=\E[60;1;0;30p\E[59;1H\E[K:\
	:ti=\E[30;1H\E[K\E[30;1;0;30p:tc=aaa-30-s-rv:
aaa|aaa-30|ambas|ambassador|ann arbor ambassador/30 lines:\
	:li#30:\
	:is=\E7\E[60;0;0;30p\E8:te=\E[60;0;0;30p\E[30;1H\E[K:\
	:ti=\E[H\E[J\E[30;0;0;30p:tc=aaa+unk:
aaa-30-rv|aaa-rv|ann arbor ambassador/30 lines in reverse video:\
	:tc=aaa+rv:tc=aaa-30:
aaa-30-ctxt|aaa-ctxt|ann arbor ambassador/30 lines; saving context:\
	:te=\E[60;0;0;30p\E[60;1H\E[K:ti=\E[30;0;0;30p:tc=aaa-30:
aaa-30-rv-ctxt|aaa-rv-ctxt|ann arbor ambassador/30 lines; saving context:\
	:te=\E[60;0;0;30p\E[60;1H\E[K:ti=\E[30;0;0;30p:tc=aaa+rv:tc=aaa-30:
aaa-36|ann arbor ambassador/36 lines:\
	:li#36:\
	:is=\E7\E[60;0;0;36p\E8:te=\E[60;0;0;36p\E[36;1H\E[K:\
	:ti=\E[H\E[J\E[36;0;0;36p:tc=aaa+unk:
aaa-36-rv|ann arbor ambassador/36 lines+reverse video:\
	:tc=aaa+rv:tc=aaa-36:
aaa-40|ann arbor ambassador/40 lines:\
	:li#40:\
	:is=\E7\E[60;0;0;40p\E8:te=\E[60;0;0;40p\E[40;1H\E[K:\
	:ti=\E[H\E[J\E[40;0;0;40p:tc=aaa+unk:
aaa-40-rv|ann arbor ambassador/40 lines+reverse video:\
	:tc=aaa+rv:tc=aaa-40:
aaa-48|ann arbor ambassador/48 lines:\
	:li#48:\
	:is=\E7\E[60;0;0;48p\E8:te=\E[60;0;0;48p\E[48;1H\E[K:\
	:ti=\E[H\E[J\E[48;0;0;48p:tc=aaa+unk:
aaa-48-rv|ann arbor ambassador/48 lines+reverse video:\
	:tc=aaa+rv:tc=aaa-48:
aaa-60-s|ann arbor ambassador/59 lines plus status line:\
	:es:hs:\
	:li#59:\
	:ds=\E7\E[60;0;0;60p\E[1;1H\E[K\E[H\E8\r\n\E[K:\
	:fs=\E[>51l:is=\r\n\E[A\E7\E[60;1;0;60p\E8:\
	:ts=\E[>51h\E[1;%p1%dH\E[2K:tc=aaa+unk:
aaa-60-s-rv|ann arbor ambassador/59 lines+status line+reverse video:\
	:tc=aaa+rv:tc=aaa-60-s:
aaa-60-s-rv-dec|ann arbor ambassador/dec mode+59 lines+status line+rev video:\
	:tc=aaa+dec:tc=aaa+rv:tc=aaa-60-s:
aaa-60|ann arbor ambassador/60 lines:\
	:li#60:\
	:is=\E7\E[60;0;0;60p\E[1Q\E[m\E[>20;30l\E8:tc=aaa+unk:
aaa-60-rv|ann arbor ambassador/60 lines+reverse video:\
	:tc=aaa+rv:tc=aaa-60:
aaa-db|ann arbor ambassador 30/destructive backspace:\
	:i2=\E[1Q\E[m\E[>20l\E[>30h:le=\E[D:tc=aaa-30:

guru|guru-33|guru+unk|ann arbor guru/33 lines 80 cols:\
	:li#33:\
	:i2=\E[>59l:is=\E7\E[255;0;0;33;80;80p\E8\E[J:\
	:te=\E[255p\E[255;1H\E[K:ti=\E[33p:vb=\E[>59h\E[>59l:tc=aaa+unk:
guru+rv|guru changes for reverse video:\
	:i2=\E[>59h:vb=\E[>59l\E[>59h:
guru-rv|guru-33-rv|ann arbor guru/33 lines+reverse video:\
	:tc=guru+rv:tc=guru-33:
guru+s|changes for status line:\
	:es:hs:\
	:ds=\E7\E[;0p\E[1;1H\E[K\E[H\E8\r\n\E[K:fs=\E[>51l:\
	:te=\E[255;1p\E[255;1H\E[K:\
	:ts=\E[>51h\E[1;%p1%dH\E[2K:
guru-nctxt:\
	:ti=\E[H\E[J\E[33p\E[255;1H\E[K:tc=guru:
guru-s|guru-33-s|ann arbor guru/33 lines w/status line:\
	:li#32:\
	:is=\r\n\E[A\E7\E[255;1;0;33;80;80p\E8\E[J:\
	:ti=\E[33;1p\E[255;1H\E[K:tc=guru+s:tc=guru+unk:
guru-24:\
	:co#80:li#24:\
	:is=\E7\E[255;0;0;24;80;80p\E8\E[J:ti=\E[24p:tc=guru+unk:
guru-44:\
	:co#97:li#44:\
	:is=\E7\E[255;0;0;44;97;100p\E8\E[J:ti=\E[44p:tc=guru+unk:
guru-44-s|ann arbor guru/44 lines w/status line:\
	:li#43:\
	:is=\r\n\E[A\E7\E[255;1;0;44;80;80p\E8\E[J:\
	:ti=\E[44;1p\E[255;1H\E[K:tc=guru+s:tc=guru+unk:
guru-76|guru with 76 lines by 89 cols:\
	:co#89:li#76:\
	:is=\E7\E[255;0;0;76;89;100p\E8\E[J:ti=\E[76p:tc=guru+unk:
guru-76-s|ann arbor guru/76 lines w/status line:\
	:co#89:li#75:\
	:is=\r\n\E[A\E7\E[255;1;0;76;89;100p\E8\E[J:\
	:ti=\E[76;1p\E[255;1H\E[K:tc=guru+s:tc=guru+unk:
guru-76-lp|guru-lp|guru with page bigger than line printer:\
	:co#134:li#76:\
	:is=\E7\E[255;0;0;76;134;134p\E8\E[J:ti=\E[76p:tc=guru+unk:
guru-76-w|guru 76 lines by 178 cols:\
	:co#178:li#76:\
	:is=\E7\E[255;0;0;76;178;178p\E8\E[J:ti=\E[76p:tc=guru+unk:
guru-76-w-s|ann arbor guru/76 lines w/status line:\
	:co#178:li#75:\
	:is=\r\n\E[A\E7\E[255;1;0;76;178;178p\E8\E[J:\
	:ti=\E[76;1p\E[255;1H\E[K:tc=guru+s:tc=guru+unk:
guru-76-wm|guru 76 lines by 178 cols with 255 cols memory:\
	:co#178:li#76:\
	:is=\E7\E[255;0;0;76;178;255p\E8\E[J:ti=\E[76p:tc=guru+unk:
aaa-rv-unk:\
	:Nl#0:lh#0:lw#0:\
	:i1=\E[7m\E7\E[H\E9\E8:mb=\E[5;7m:md=\E[1;7m:\
	:me=\E[7m:mk=\E[7;8m:mr=\E[m:r1=\E[H\E[7m\E[J:\
	:..sa=\E[%?%p1%!%t7;%;%?%p2%t4;%;%?%p3%t7;%;%?%p4%t5;%;%?%p6%t1;%;%?%p7%t8;%;m:\
	:se=\E[7m:so=\E[m:ue=\E[7m:us=\E[4;7m:

#### Applied Digital Data Systems (adds)
#
# ADDS itself is long gone.  ADDS was bought by NCR, and the same group made
# ADDS and NCR terminals.  When AT&T and NCR merged, the engineering for
# terminals was merged again.  Then AT&T sold the terminal business to
# SunRiver.  The engineers from Teletype, AT&T terminals, ADDS,
# and NCR (who are still there) are at:
#
#	SunRiver Data Systems
#	100 Marcus Boulevard
#	Hauppauge, NY 117883-762
#	Vox: (800)-231-5445
#	Fax: (516)-342-7378
#
# Their voice mail describes the place as "SunRiver (formerly ADDS)". 

# Regent: lowest common denominator, works on all regents.
# (regent: renamed ":bc:" to ":le:" -- esr)
regent|Adds Regent Series:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cl=^L:cr=^M:do=^J:ho=\EY  :le=^U:ll=^A:nd=^F:\
	:sf=^J:up=^Z:
# Regent 100 has a bug where if computer sends escape when user is holding
# down shift key it gets confused, so we avoid escape.
regent100|Adds Regent 100:\
	:sg#1:ug#1:\
	:bl=^G:cm=\013%+ %B\020%.:k0=^B1\r:k1=^B2\r:k2=^B3\r:\
	:k3=^B4\r:k4=^B5\r:k5=^B6\r:k6=^B7\r:k7=^B8\r:l0=F1:\
	:l1=F2:l2=F3:l3=F4:l4=F5:l5=F6:l6=F7:l7=F8:se=\E0@:\
	:so=\E0P:ue=\E0@:us=\E0`:tc=regent:
regent20|Adds Regent 20:\
	:bl=^G:cd=\Ek:ce=\EK:cm=\EY%+ %+ :tc=regent:
regent25|Adds Regent 25:\
	:bl=^G:kd=^J:kh=^A:kl=^U:kr=^F:ku=^Z:tc=regent20:
regent40|Adds Regent 40:\
	:sg#1:ug#1:\
	:al=\EM:bl=^G:dl=\El:k0=^B1\r:k1=^B2\r:k2=^B3\r:\
	:k3=^B4\r:k4=^B5\r:k5=^B6\r:k6=^B7\r:k7=^B8\r:l0=F1:\
	:l1=F2:l2=F3:l3=F4:l4=F5:l5=F6:l6=F7:l7=F8:se=\E0@:\
	:so=\E0P:ue=\E0@:us=\E0`:tc=regent25:
regent40+|Adds Regent 40+:\
	:is=\EB:tc=regent40:
# (regent60: removed obsolete ":ko=dc,im,ei:" -- esr)
regent60|regent200|Adds Regent 60:\
	:dc=\EE:ei=\EF:im=\EF:is=\EV\EB:kD=\EE:kI=\EF:kM=\EF:\
	:se=\ER\E0@\EV:so=\ER\E0P\EV:tc=regent40+:
regent60na|regent 60 w/no arrow keys:\
	:kd@:kl@:kr@:ku@:tc=regent60:
# From: <edward@onyx.berkeley.edu> Thu Jul  9 09:27:33 1981
# (viewpoint: added kcuf1, kf* and dl1 capabilities -- esr)
viewpoint|addsviewpoint|adds viewpoint:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cd=\Ek:ce=\EK:cl=^L:cm=\EY%+ %+ :cr=^M:dl=\El:\
	:do=^J:is=\017\E0`:k0=^B1:k2=^B2:k3=^B!:k4=^B":\
	:k5=^B#:kd=^J:kh=^A:kl=^U:kr=^F:ku=^Z:le=^H:ll=^A:\
	:nd=^F:se=^O:sf=^J:so=^N:ue=^O:up=^Z:us=^N:\
	:ve=\017\E0`:vs=\017\E0P:
screwpoint|adds viewpoint with ^O bug:\
	:am:bs:\
	:Nl#0:co#80:lh#0:li#24:lw#0:\
	:bl=^G:cd=\Ek:ce=\EK:cl=\014:cm=\EY%+ %+ :cr=^M:\
	:dl=\El:do=^J:is=^G:kd=^J:kh=^A:kl=^U:kr=^F:ku=^Z:\
	:le=^H:ll=^A:nd=^F:sf=^J:up=^Z:
fviewpoint|flaky adds viewpoint with ^O bug:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cd=\Ek:ce=\EK:cl=\014:cm=\EY%+ %+ :cr=^M:\
	:dl=\El:do=^J:is=^G:kd=^J:kh=^A:kl=^U:kr=^F:ku=^Z:\
	:le=^H:ll=^A:nd=^F:sf=^J:up=^Z:
# From: Jay S. Rouman <jsr@dexter.mi.org> 5 Jul 92
# The civis/cnorm/sgr/sgr0 strings were added by ESR from specs.  
# Theory; the 3a+ wants \E0%c to set highlights, where normal=01000000,
# underline=01100000, rev=01010000, blink=01000010,dim=01000001,
# invis=01000100 and %c is the logical or of desired attributes.
# There is also a `tag bit' enabling attributes, set by \E) and unset by \E(.
vp3a+|viewpoint3a+|adds viewpoint 3a+:\
	:am:bw:\
	:co#80:it#8:li#24:\
	:cd=\EY:ce=\ET:cl=\E*:cm=\E=%+ %+ :cr=^M:do=^J:ho=^^:\
	:kb=^H:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:le=^H:me=\E(:\
	:nd=^L:nw=^M^J:\
	:..sa=\E0%'@'%?%p1%tQ%|%;%?%p2%t%'`'%|%;%?%p3%tP%|%;%?%p4%t%{2}%|%;%?%p5%t%{1}%|%;%?%p7%tD%|%;%c\E):\
	:se=\E(:sf=^J:so=\E0Q\E):ta=^I:up=^K:ve=^X:vi=^W:
vp60|viewpoint60|addsviewpoint60|adds viewpoint60:\
	:tc=regent40:
#
# adds viewpoint 90 - from cornell
# Note:  emacs sends ei occasionally to insure the terminal is out of
#        insert mode. This unfortunately puts the viewpoint90 IN insert
#        mode.  A hack to get around this is :ic=\EF \EF^U:.  (Also,
#   -    :ei=:im=: must be present in the termcap translation.)
#   -    :xs: indicates glitch that attributes stick to location
#   -    :ms: means it's safe to move in standout mode
#   -    :cl=\EG\Ek: clears screen and visual attributes without affecting
#               the status line
# Function key and label capabilities merged in from SCO.
vp90|viewpoint90|adds viewpoint 90:\
	:bs:bw:ms:xs:\
	:co#80:li#24:\
	:cd=\Ek:ce=\EK:cl=\EG\Ek:cm=\EY%+ %+ :dc=\EE:dl=\El:\
	:do=^J:ei=:ho=\EY  :ic=\EF \EF\025:im=:k0=^B1\r:\
	:k1=^B2\r:k2=^B3\r:k3=^B4\r:k4=^B5\r:k5=^B6\r:\
	:k6=^B7\r:k7=^B8\r:k8=^B9\r:k9=^B\072\r:k;=^B;\r:\
	:kb=^H:kd=^J:kh=^A:kl=^U:kr=^F:ku=^Z:l0=F1:l1=F2:\
	:l2=F3:l3=F4:l4=F5:l5=F6:l6=F7:l7=F8:l8=F9:l9=F10:\
	:la=F11:ll=^A:nd=^F:se=\ER\E0@\EV:sf=^J:\
	:so=\ER\E0Q\EV:ta=^I:ue=\ER\E0@\EV:up=^Z:\
	:us=\ER\E0`\EV:
# Note: if return acts weird on a980, check internal switch #2
# on the top chip on the CONTROL pc board.
adds980|a980|adds consul 980:\
	:am:bs:\
	:co#80:li#24:\
	:al=\E\016:bl=^G:cl=\014\013@:cm=\013%+@\E\005%2:\
	:cr=^M:dl=\E\017:do=^J:k0=\E0:k1=\E1:k2=\E2:k3=\E3:\
	:k4=\E4:k5=\E5:k6=\E6:k7=\E7:k8=\E8:k9=\E9:le=^H:\
	:nd=\E^E01:se=^O:sf=^J:so=^Y^^^N:

#### C. Itoh Electronics
#
# As of 1995 these people no longer make terminals (they're still in the
# printer business).  Their terminals were all clones of the DEC VT series.
# They're located in Orange County, CA.
#

# CIT 80  - vt-52 emulator, the termcap has been modified to remove
#           the delay times and do an auto tab set rather than the indirect
#           file used in vt100.
cit80|cit-80|citoh 80:\
	:am:bs:\
	:co#80:li#24:\
	:cd=\EJ:ce=\EK:cl=\E[;H\EJ:cm=\E[%i%2;%2H:cr=^M:\
	:ff=^L:is=\E>:kd=\EOB:ke=\E[?1l\E>:kl=\EOD:kr=\EOC:\
	:ks=\E[?1h\E=:ku=\EOA:nd=\E[C:sf=^J:up=\E[A:
# Alternate cit101 (vt100 em) file used in vt100.
#	    Uses 23 lines so can run citsys (like h19sys).
#	24 May 85 (mtxinu!sybase!tim) - removed 2-byte limit on :cm: cursor
#	  coordinates otherwise there is garbling on long lines in 
#	  co#132 mode; also added support for multipage	memory on the Itoh.
# From: Tim Wood <mtxinu!sybase!tim> Fri Sep 27 09:39:12 PDT 1985
citc|Citoh fast vt100:\
	:am:bs:xn:\
	:co#80:li#23:\
	:al=\E[L:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:\
	:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:ei=:ic=\E[@:im=:\
	:is=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h\E[3g\E[>5g:\
	:kd=\EOB:ke=\E[?1l\E>:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:\
	:ku=\EOA:nd=\E[C:se=\E[m:so=\E[7m:ue=\E[m:up=\E[A:\
	:us=\E[4m:\
	:vb=\E[?5h\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\E[?5l:\
	:ve=\E[V\E8:vs=\E7\E[U:
cita:\
	:am:bs:xn:\
	:co#80:li#23:\
	:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:cm=\E[%i%d;%dH:\
	:is=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h\E[3g\E[>5g:\
	:kd=\EOB:ke=\E[?1l\E>:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:\
	:ku=\EOA:nd=\E[C:se=\E[m:so=\E[7m:ue=\E[m:up=\E[A:\
	:us=\E[4m:\
	:vb=\E[?5h\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\E[?5l:\
	:ve=\E[V\E8:vs=\E7\E[U:
cit101:\
	:li#24:\
	:vb@:tc=citc:
cit101b:\
	:li#24:\
	:tc=citc:
# The CIT-500 was unusual in that it had a portrait-style display.
# (cit500: mapped ":pt:" to default tabs -- esr)
cit500|cit-500|cit 500:\
	:am:bs:pt:xn:\
	:co#80:li#40:\
	:al=\E[L:cd=50\E[J:ce=3\E[K:cl=50\E[;H\E[2J:\
	:cm=5\E[%i%2;%2H:dc=\E[P:dl=\E[M:do=\ED:\
	:is=\E(B\E)0\E>\E[?3l\E[?7h\E[?8h:k1=\EOP:k2=\EOQ:\
	:k3=\EOR:k4=\EOS:kd=\EOB:ke=\E[?1l\E>:kh=\E[H:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:nd=2\E[C:\
	:se=2\E[m:so=2\E[7m:sr=5\EM:ue=2\E[m:up=2\E[A:\
	:us=2\E[4m:

citoh|ci8510|8510|c.itoh 8510a:\
	:co#80:it#8:\
	:is=\E(009\054017\054025\054033\054041\054049\054057\054065\054073.:\
	:le@:md=\E!:me=\E"\EY:rp=\ER%r%03%.:sr=\Er:ue=\EY:\
	:us=\EX:tc=lpr:
citoh-pica|citoh in pica:\
	:i1=\EN:tc=citoh:
citoh-elite|citoh in elite:\
	:co#96:\
	:i1=\EE:\
	:is=\E(009\054017\054025\054033\054041\054049\054057\054065\054073\054081\054089.:tc=citoh:
citoh-comp|citoh in compressed:\
	:co#136:\
	:i1=\EQ:\
	:is=\E(009\054017\054025\054033\054041\054049\054057\054065\054073\054081\054089\054097\054105\054113\054121\054129.:tc=citoh:
# citoh has infinite cols because we don't want lp ever inserting \n\t**.
citoh-prop|citoh-ps|ips|citoh in proportional spacing mode:\
	:co#32767:\
	:i1=\EP:tc=citoh:
citoh-6lpi|citoh in 6 lines per inch mode:\
	:i2=\EA:tc=citoh:
citoh-8lpi|citoh in 8 lines per inch mode:\
	:li#88:\
	:i2=\EB:tc=citoh:

#### Control Data (cdc)
#

cdc456|cdc:\
	:am:bs:\
	:co#80:li#24:\
	:al=\EL:bl=^G:cd=^X:ce=^V:cl=^Y^X:cm=\E1%+ %+ :cr=^M:\
	:dl=\EJ:do=^J:ho=^Y:le=^H:nd=^L:sf=^J:up=^Z:
cdc456tst:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cl=^Y^X:cm=\E1%+ %+ :cr=^M:do=^J:le=^H:sf=^J:

#### Human Designed Systems (Concept)
#
#	Human Designed Systems
#	400 Fehley Drive
#	King of Prussia, PA 19406
#	Vox: (610)-277-8300
#	Fax: (610)-275-5739
#	Net: support@hds.com
# 
# John Martin <john@hds.com> is their termcap expert.  They're mostly out of
# the character-terminal business now (1995) and making X terminals.  In
# particular, the whole `Concept' line described here was discontinued long
# ago.

# From: <vax135!hpk>  Sat Jun 27 07:41:20 1981
# Extensive changes to c108 by arpavax:eric Feb 1982
# Some unknown person at SCO then translated it to terminfo.
#
# There seem to be a number of different versions of the C108 PROMS
# (with bug fixes in its Z-80 program).
# 
# The first one that we had would lock out the keyboard of you
# sent lots of short lines (like /usr/dict/words) at 9600 baud.
# Try that on your C108 and see if it sends a ^S when you type it.
# If so, you have an old version of the PROMs.
# 
# You should configure the C108 to send ^S/^Q before running this.
# It is much faster (at 9600 baud) than the c100 because the delays
# are not fixed.
# new status line display entries for c108-8p:
# is3 - init str #3 - setup term for status display - 
# set programmer mode, select window 2, define window at last 
# line of memory, set bkgnd stat mesg there, select window 0.
# 
# tsl - to status line - select window 2, home cursor, erase to 
# end-of-window, 1/2 bright on, goto(line#0, col#?)
# 
# fsl - from status line - 1/2 bright off, select window 0
# 
# dsl - disable status display - set bkgnd status mesg with 
# illegal window #
# 
# There are probably more function keys that should be added but 
# I don't know what they are.
#
c108|concept108|c108-8p|concept108-8p|concept 108 w/8 pages:\
	:i2=\EU\E z"\Ev\001\177 !p\E ;"\E z \Ev  \001\177p\Ep\n:\
	:te=\Ev  \001\177p\Ep\r\n:tc=c108-4p:
c108+acs|alternate charset defns for c108:\
	:ac=l\\qLkTxUmMjE:ae=\Ej :as=\Ej!:
c108-4p-acs|c108-4p w/ acs:\
	:tc=c108+acs:tc=c108-4p:
c108-8p-acs|c108-8p w/ acs:\
	:tc=c108+acs:tc=c108-8p:
c108-rv-8p-acs|c108-rv-8p w/ acs:\
	:tc=c108+acs:tc=c108-rv-8p:
c108-4p|concept108-4p|concept 108 w/4 pages:\
	:es:hs:xo:\
	:pb@:\
	:..cm=\Ea%p1%?%p1%{95}%>%t\001%{96}%-%;%{32}%+%c%p2%?%p2%{95}%>%t\001%{96}%-%;%{32}%+%c:\
	:cr=^M:dc=\E 1:ds=\E ;\177:fs=\Ee\E z :i1=\EK\E!\E F:\
	:i2=\EU\E z"\Ev\177 !p\E ;"\E z \Ev  \001 p\Ep\n:\
	:sf=^J:te=\Ev  \001 p\Ep\r\n:\
	:ti=\EU\Ev  8p\Ep\r\E\025:\
	:ts=\E z"\E?\E\005\EE\Ea %+ :ve=\Ew:vs=\EW:tc=c100:
c108-rv|c108-rv-8p|concept 108 w/8 pages in reverse video:\
	:te=\Ev  \002 p\Ep\r\n:ti=\EU\Ev  8p\Ep\r:tc=c108-rv-4p:
c108-rv-4p|concept108-rv-4p|concept108rv4p|concept 108 w/4 pages in reverse video:\
	:i1=\Ek:se=\Ee:so=\EE:vb=\EK\Ek:tc=c108-4p:
c108-rv-4p-acs|c108-rv-4p w/ acs:\
	:tc=c108+acs:tc=c108-rv-4p:
c108-na|c108-na-8p|c108-8p-na|concept108-na-|concept108na8p|concept 108 w/8 pages no arrows:\
	:k7=\E;:k8=\E<:k9=\E=:ke@:ks@:tc=c108-8p:
c108-na-acs|c108-na w/ acs:\
	:tc=c108+acs:tc=c108-na:
c108-rv-na|c108-rv-na-8p|c108-8p-rv-na|concept 108 8 pages no arrows rev video:\
	:k7=\E;:k8=\E<:k9=\E=:ke@:ks@:tc=c108-rv-8p:
c108-rv-na-acs|c108-na w/ acs:\
	:tc=c108+acs:tc=c108-rv-na:
c108-w|c108-w-8p|concept108-w-8|concept108-w8p|concept 108 w/8 pages in wide mode:\
	:co#132:\
	:i1=\E F\E":te=\Ev  ^A0\001D\Ep\r\n:\
	:ti=\EU\Ev  8\001D\Ep\r:tc=c108-8p:
c108-w-acs|c108-w w/ acs:\
	:tc=c108+acs:tc=c108-w:

# Concept 100:
# These have only window relative cursor addressing, not screen 
# relative. To get it to work right here, smcup/rmcup (which 
# were invented for the concept) lock you into a one page 
# window for screen style programs.
# 
# To get out of the one page window, we use a clever trick:
# we set the window size to zero ("\Ev    " in rmcup) which the 
# terminal recognizes as an error and resets the window to all 
# of memory.
# 
# This trick works on c100 but does not on c108, sigh.
# 
# Some tty drivers use cr3 for concept, others use nl3, hence 
# the delays on cr and ind below. This padding is only needed at 
# 9600 baud. One or the other is commented out depending on 
# local conventions.
# 
# 2 ms padding on rmcup isn't always enough. 6 works fine. Maybe 
# less than 6 but more than 2 will work.
# 
# Note: can't use function keys f7-f10 because they are 
# indistinguishable from arrow keys (!), also, del char and 
# clear eol use xon/xoff so they probably won't work very well.
# 
# Also note that we don't define insrt/del char/delline/eop/send 
# because they don't transmit unless we reset them - I figured 
# it was a bad idea to clobber their definitions.
# 
# The mc5 sequence changes the escape character to ^^ so that 
# escapes will be passed through to the printer. Only trouble 
# is that ^^ won't be - ^^ was chosen to be unlikely. 
# Unfortunately, if you're sending raster bits through to be 
# plotted, any character you choose will be likely, so we lose.
#
# \EQ"\EY(^W (send anything from printer to host, for xon/xoff) 
# cannot be # in is2 because it will hang a c100 with no printer 
# if sent twice.
c100|concept100|concept|c104|c100-4p|hds concept 100:\
	:am:eo:mi:ul:xn:\
	:co#80:li#24:pb#9600:vt#8:\
	:al=\E\022:bl=^G:cd=\E\005:ce=\E\025:cl=\E?\E\005:\
	:cm=\Ea%+ %+ :cr=\r:dc=\E\021:dl=\E\002:do=^J:\
	:ei=\E  :i1=\EK:i2=\Ev    \Ep\n:im=\E^P:ip=:\
	:is=\EU\Ef\E7\E5\E8\El\ENH\E\200\Eo&\200\Eo'\E\Eo!\200\E\007!\E\010A@ \E4#\072"\E\072a\E4#;"\E\072b\E4#<"\E\072c:\
	:k1=\E5:k2=\E6:k3=\E7:k4=\E8:k5=\E9:k6=\E\072a:\
	:k7=\E\072b:k8=\E\072c:kA=\E^R:kB=\E':kD=\E^Q:\
	:kE=\E^S:kF=\E[:kI=\E^P:kL=\E^B:kM=\E\200:kN=\E-:\
	:kP=\E.:kR=\E\\:kS=\E^C:kT=\E]:kb=^H:kd=\E<:ke=\Ex:\
	:kh=\E?:kl=\E>:kr=\E=:ks=\EX:kt=\E_:ku=\E;:le=^H:\
	:mb=\EC:me=\EN@:mh=\EE:mk=\EH:mp=\EI:mr=\ED:nd=\E=:\
	:pf=\036o \E\EQ!\EYP\027:po=\EQ"\EY(\027\EYD\Eo \036:\
	:rp=\Er%.%+ :se=\Ed:sf=^J:so=\ED:ta=\011:\
	:te=\Ev    \Ep\r\n:ti=\EU\Ev  8p\Ep\r\E\025:ue=\Eg:\
	:up=\E;:us=\EG:vb=\Ek\EK:
c100-rv|c100-rv-4p|concept100-rv|c100 rev video:\
	:i1=\Ek:se=\Ee:so=\EE:vb=\EK\Ek:ve@:vs@:tc=c100:
c100-rv-na|c100-rv-4p-na|c100 with no arrows:\
	:ke@:ks@:tc=c100-rv:
oc100|oconcept|c100-1p|old 1 page concept 100:\
	:in:\
	:i3@:tc=c100:

# ht through el included to specify padding needed in raw mode.
avt-ns|concept avt with status lins disabled:\
	:am:eo:mi:ul:xn:xo:\
	:co#80:it#8:li#24:lm#192:\
	:AL=\E[%dL:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:LE=\E[%dD:\
	:RI=\E[%dC:UP=\E[%dA:ae=\016:al=\E[L:as=\017:bl=^G:\
	:bt=\E[Z:cd=\E[J:ce=\E[K:ch=\E[%+^AG:cl=\E[H\E[J:\
	:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:ct=\E[2g:\
	:cv=\E[%+^Ad:dc=\E[P:dl=\E[M:do=^J:ei=\E4l:ho=\E[H:\
	:i1=\E[=103l\E[=205l:ic=\E[@:im=\E1:ip=:\
	:is=\E[1*q\E[2!t\E[7!t\E[=4;101;119;122l\E[=107;118;207h\E)1\E[1Q\EW\E[!y\E[!z\E>\E[0\0720\07232!r\E[0*w\E[w\E2\r\n\E[2;27!t:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:kA=\E^C\r:kD=\E^B\r:\
	:kI=\E^A\r:kS=\E^D\r:kb=^H:kd=\E[B:ke=\E[!z\E[0;2u:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ks=\E[1!z\E[0;3u:ku=\E[A:\
	:le=^H:ll=\E[24H:mb=\E[5m:md=\E[1m:me=\E[m:mh=\E[1!{:\
	:mk=\E8m:mp=\E[99m:mr=\E[7m:nd=\E[C:pf=\E[4i:\
	:pl=\E[%d;0u#%s#:po=\E[5i:ps=\E[0i:px=\E[%d;1u#%s#:\
	:rc=\E8:..rp=%p1%c\E[%p2%{1}%-%db:\
	:..sa=\E[%?%p1%t7;%;%?%p2%t4;%;%?%p3%t7;%;%?%p4%t5;%;%?%p6%t1;%;m:\
	:sc=\E7:se=\E[7!{:sf=\n:so=\E[7m:sr=\EM:st=\EH:\
	:ta=\011:te=\E[w\E2\r\n:ti=\E[=4l\E[1;24w\E2\r:\
	:ue=\E[4!{:up=\E[A:us=\E[4m:ve=\E[=119l:vs=\E[=119h:
avt-rv-ns|concept avt in reverse video mode/no status line:\
	:i1=\E[=103l\E[=205h:vb=\E[=205l\E[=205h:tc=avt-ns:
avt-w-ns|concept avt in 132 column mode/no status line:\
	:i1=\E[=103h\E[=205l:ti=\E[H\E[1;24;1;132w:tc=avt-ns:
avt-w-rv-ns|concept avt in 132 column mode/no status line:\
	:i1=\E[=103h\E[=205h:ti=\E[H\E[1;24;1;132w:\
	:vb=\E[=205l\E[=205h:tc=avt-ns:

# Concept AVT with status line. We get the status line using the
# "Background status line" feature of the terminal. We swipe the
# first line of memory in window 2 for the status line, keeping
# 191 lines of memory and 24 screen lines for regular use.
# The first line is used instead of the last so that this works
# on both 4 and 8 page AVTs. (Note the lm#191 or 192 - this
# assumes an 8 page AVT but lm isn't currently used anywhere.)
#
avt+s|concept avt status line changes:\
	:es:hs:\
	:lm#191:\
	:ds=\E[0*w:fs=\E[1;1!w:\
	:i2=\E[2w\E[2!w\E[1;1;1;80w\E[H\E[2*w\E[1!w\E2\r\n:\
	:te=\E[2w\E2\r\n:ti=\E[2;25w\E2\r:\
	:ts=\E[2;1!w\E[;%p1%dH\E[2K:
avt|avt-s|concept-avt|avt w/80 columns:\
	:tc=avt+s:tc=avt-ns:
avt-rv|avt-s-rv|avt-rv-s|concept avt in reverse video w/status line:\
	:i1=\E[=103l\E[=205h:vb=\E[=205l\E[=205h:tc=avt+s:tc=avt-ns:
avt-w|avt-w-s|concept avt in 132 column mode w/status line:\
	:i1=\E[=103h\E[=205l:ti=\E[H\E[1;24;1;132w:tc=avt+s:tc=avt-ns:
avt-w-rv|avt-rv-w|avt-w-s-rv|avt-w-rv-s|avt 132 cols w/status line:\
	:i1=\E[=103h\E[=205h:ti=\E[H\E[1;24;1;132w:\
	:vb=\E[=205l\E[=205h:tc=avt+s:tc=avt-ns:

#### Contel Business Systems. 
#

# Contel c300 and c320 terminals. 
contel300|contel320|c300|Contel Business Systems C-300 or C-320:\
	:am:in:xo:\
	:co#80:li#24:sg#1:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EI:cl=\EK:cm=\EX%+ \EY%+ :\
	:cr=^M:ct=\E3:dc=\EO:dl=\EM:do=^J:ei=:ho=\EH:ic=\EN:\
	:im=:ip=:k0=\ERJ:k1=\ERA:k2=\ERB:k3=\ERC:k4=\ERD:\
	:k5=\ERE:k6=\ERF:k7=\ERG:k8=\ERH:k9=\ERI:kb=^H:le=^H:\
	:ll=\EH\EA:nd=\EC:se=\E!\200:sf=^J:so=\E!\r:st=\E1:\
	:up=\EA:vb=\020\002\020\003:
# Contel c301 and c321 terminals.
contel301|contel321|c301|c321|Contel Business Systems C-301 or C-321:\
	:am:in:xo:\
	:co#80:li#24:sg#1:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EI:cl=\EK:cm=\EX%+ \EY%+ :\
	:cr=^M:ct=\E3:dc=\EO:dl=\EM:do=^J:ho=\EH:k0=\ERJ:\
	:k1=\ERA:k2=\ERB:k3=\ERC:k4=\ERD:k5=\ERE:k6=\ERF:\
	:k7=\ERG:k8=\ERH:k9=\ERI:kb=^H:le=^H:ll=\EH\EA:\
	:nd=\EC:se=\E!\200:sf=^J:so=\E!\r:st=\E1:up=\EA:

#### Data General (dg)
#
# According to James Carlson <carlson@xylogics.com> writing in January 1995,
# the terminals group at Data General was shut down in 1991; all these
# terminals have thus been discontinued.
#

dg200|data general dasher 200:\
	:NL:am:bw:\
	:co#80:li#24:\
	:bl=^G:ce=^K:cl=^L:cm=\020%r%.%.:cr=^M:do=^Z:ho=^H:\
	:k0=^^z:k1=^^q:k2=^^r:k3=^^s:k4=^^t:k5=^^u:k6=^^v:\
	:k7=^^w:k8=^^x:k9=^^y:kd=^Z:kh=^H:kl=^Y:kr=^X:ku=^W:\
	:l0=f10:le=^Y:nd=^X:nw=^J:se=^^E:sf=^J:so=^^D:ue=^U:\
	:up=^W:us=^T:
#
# dg450 and dg200 from cornell
dg450|dg6134|data general 6134:\
	:bs@:\
	:nd=^X:tc=dg200:
# Note: lesser Dasher terminals will not work with vi because vi insists upon
# having a command to move straight down from any position on the bottom line
# and scroll the screen up, or a direct vertical scroll command.  The 460 and
# above have both, the D210/211, for instance, has neither.  We must use ANSI
# mode rather than DG mode because standard UNIX tty drivers assume that ^H is
# backspace on all terminals.  This is not so in DG mode.
# (dg460-ansi: removed obsolete ":kn#6:"; also removed ":mu=\EW:", on the
# grounds that there is no matching ":ml:"; mapped ":pt:" to default tabs; 
# fixed garbled ":k9=\E[00\:z:" capability -- esr)
dg460-ansi|Data General Dasher 460, ANSI-mode:\
	:am:bs:ms:pt:ul:\
	:co#80:li#24:\
	:al=\E[L:cd=\E[J:ce=\E[K:cl=\E[2J:cm=\E[%i%2;%2H:\
	:dc=\E[P:dl=\E[M:do=\E[B:ei=:ho=\E[H:ic=\E[@:im=:\
	:is=^^F@:k0=\E[001z:k1=\E[002z:k2=\E[003z:k3=\E[004z:\
	:k4=\E[005z:k5=\E[006z:k6=\E[007z:k7=\E[008z:\
	:k8=\E[009z:k9=\E[010z:kb=\E[D:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:l0=f1:l1=f2:l2=f3:l3=f4:\
	:l4=f5:l5=f6:l6=f7:l7=f8:l9=f10:le=^H:mb=\E[5m:\
	:me=\E[0m:mh=\E[2m:mr=\E[7m:nd=\E[C:nl=\ED:se=\E[0m:\
	:sf=\E[S:so=\E[7m:sr=\E[T:ue=\E[05:up=\E[A:us=\E[4m:
# From: Wayne Throop <mcnc!rti-sel!rtp47!throopw>
# Data General 605x     
# Ought to work for a Model 6242, Type D210 as well as a 605x.
# Note that the cursor-down key transmits ^Z.  Job control users, beware!
dg6053|data general 6053:\
	:am:bs:bw:pt:ul:\
	:co#80:li#24:\
	:bl=^G:ce=^K:cl=^L:cm=\020%r%.%.:cr=^M:do=^Z:ho=^H:\
	:is=^R:k0=^^q:k1=^^r:k2=^^s:k3=^^t:k4=^^u:k5=^^v:\
	:k6=^^w:k7=^^x:k8=^^y:kb=^Y:kd=^Z:kh=^H:kl=^Y:kr=^X:\
	:ku=^W:le=^Y:nd=^X:nw=^M^Z:se=\200^^E:\
	:so=\200\200\200\200\200\036D:ta=^I:te=^L:ti=^L^R:\
	:ue=^U:up=^W:us=^T:ve=^L:vs=^L^R:
# From: Peter N. Wan <ihnp4!gatech!gacsr!wan>
# courtesy of Carlos Rucalde of Vantage Software, Inc.
dgd211|Data General d211:\
	:am:bw:\
	:co#80:li#24:\
	:ce=^K:cl=^L:..cm=\020%r%.%.:cr=^M:do=^Z:ho=^H:kb=^Y:\
	:kd=^Z:kh=^H:kl=^Y:kr=^X:ku=^W:le=^Y:nd=^X:nw=^M^Z:\
	:se=00\036E\200/>:so=00\036D\200\200\200\200\200/>:\
	:ta=^I:te=^L:ti=^L^R:ue=^U:up=^W:us=^T:ve=^L:vs=^L^R:
# From: Joan Walter <joanw@BRL.ARPA>
# Data General/One
#  David Holub got the dg1 to work with jove with this termcap
#   by making li#23 and co#78 to comply with obvious terminal
#   capabilities.  Still waiting for documentation.
# Data General/One from  modified DG Dasher DG210/211 (bw removed)
# From: Peter N. Wan <ihnp4!gatech!gacsr!wan>
# courtesy of Carlos Rucalde of Vantage Software, Inc.
dg1|Data General/One:\
	:am:\
	:co#78:li#23:\
	:ce=^K:cl=^L:cm=\020%r%.%.:cr=^M:do=^Z:ho=^H:kb=^Y:\
	:kd=^Z:kh=^H:kl=^Y:kr=^X:ku=^W:le=^Y:nd=^X:nw=^M^Z:\
	:ta=^I:up=^W:

#### Datamedia (dm)
#

cs10|colorscan|Datamedia Color Scan 10:\
	:ms:\
	:co#80:li#24:\
	:bl=^G:cd=\E[J:ce=\E[K:cl=\E[;H\E[J:cm=\E[%i%02;%02H:\
	:cr=^M:do=^J:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:kd=\E[B:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:nd=\E[C:se=\E[m:sf=^J:\
	:so=\E[7m:ue=\E[m:up=\E[A:us=\E[4m:
cs10-w|Datamedia Color Scan 10 with 132 columns:\
	:co#132:\
	:cm=\E[%i%02;%03H:tc=cs10:

# (dm1520: removed obsolete ":ma=^\ ^_^P^YH:";
# mapped ":pt:" to default tabs -- esr)
dm1520|dm1521|datamedia 1520:\
	:am:bs:pt:xn:\
	:co#80:li#24:\
	:bl=^G:cd=^K:ce=^]:cl=^L:cm=\036%r%+ %+ :cr=^M:do=^J:\
	:ho=^Y:kd=^J:kh=^Y:kl=^H:kr=^\:ku=^_:le=^H:nd=^\:\
	:sf=^J:ta=^I:up=^_:
dm2500|datamedia2500|datamedia 2500:\
	:bs:nc:\
	:co#80:li#24:\
	:al=\020\n\030\035\030\035:bl=^G:ce=^W:cl=^^^^\177:\
	:cm=\014%r%n%.%.:dc=\020\010\030\035:\
	:dl=\020\032\030\035:dm=^P:do=^J:ed=^X^]:\
	:ei=\377\377\030\035:ho=^B:ic=\020\034\030\035:im=^P:\
	:le=^H:nd=^\:pc=\377:se=^X^]:sf=^J:so=^N:up=^Z:
# dmchat is like DM2500, but DOES need "all that padding" (jcm 1/31/82)
# also, has a meta-key (:km:)
# From: <goldberger@su-csli.arpa>
# (dmchat: ":MT:" changed to ":km:" -- esr)
dmchat|dmchat version of datamedia 2500:\
	:km:\
	:al=1*\020\n\030\035\030\035:dl=2\020\032\030\035:tc=dm2500:
# (dm3025: ":MT:" changed to ":km:"; mapped ":pt:" to default tabs -- esr)
dm3025|datamedia 3025a:\
	:bs:km:pt:\
	:co#80:li#24:\
	:al=\EP\n\EQ:bl=^G:cd=\EJ:ce=\EK:cl=\EM:\
	:cm=\EY%r%+ %+ :cr=^M:dc=\010:dl=\EP\EA\EQ:dm=\EP:\
	:do=^J:ed=\EQ:ei=\EQ:ho=\EH:im=\EP:ip=:is=\EQ\EU\EV:\
	:le=^H:nd=\EC:se=\EO0:sf=^J:so=\EO1:ta=^I:up=\EA:
# (dm3045: mapped ":pt:" to default tabs -- esr)
dm3045|datamedia 3045a:\
	:am:bs:eo:pt:ul:xn:\
	:co#80:li#24:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EM:cm=\EY%r%+ %+ :cr=^M:\
	:dc=\EB:do=^J:ei=\EP:ho=\EH:im=\EP:ip=:is=\EU\EV:\
	:k0=\Ey\r:k1=\Ep\r:k2=\Eq\r:k3=\Er\r:k4=\Es\r:\
	:k5=\Et\r:k6=\Eu\r:k7=\Ev\r:k8=\Ew\r:k9=\Ex\r:kh=\EH:\
	:kr=\EC:ku=\EA:le=^H:nd=\EC:pc=\177:sf=^J:ta=^I:\
	:up=\EA:
# dm80/1 is a vt100 lookalike, but it doesn't seem to need any padding.
dm80|dmdt80|dt80|datamedia dt80/1:\
	:cd=\E[J:ce=\E[K:cl=\E[2J\E[H:cm=%i\E[%d;%dH:do=^J:\
	:ho=\E[H:nd=\E[C:pf=\E[4i:po=\E[5i:ps=\E[0i:se=\E[m:\
	:so=\E[7m:sr=\EM:ue=\E[m:up=\E[A:us=\E[4m:tc=vt100:
# except in 132 column mode, where it needs a little padding.
# This is still less padding than the vt100, and you can always turn on
# the ^S/^Q handshaking, so you can use vt100 flavors for things like
# reverse video.
dm80w|dmdt80w|dt80w|datamedia dt80/1 in 132 char mode:\
	:co#132:\
	:cd=20\E[0J:ce=20\E[0K:cl=50\E[H\E[2J:\
	:cm=5\E[%i%d;%dH:do=^J:up=5\E[A:tc=dm80:

#### Falco
#
#	Falco Data Products
#	440 Potrero Avenue
#	Sunnyvale, CA 940864-196
#	Vox: (800)-325-2648
#	Fax: (408)-745-7860
#	Net: techsup@charm.sys.falco.com
#
# Current Falco models as of 1995 are generally ANSI-compatible and support
# emulations of DEC VT-series, Wyse, and Televideo types.

# Test version for Falco ts-1. See "arpavax.hickman@ucb" for info
# (falco: mapped ":pt:" to default tabs -- esr)
# This terminal was released around 1983 and was discontinued long ago.
falco|ts1|ts-1|falco ts-1:\
	:am:bs:pt:\
	:co#80:li#24:\
	:al=\EE:bl=^G:cd=\EY:ce=\ET\EG0\010:cl=\E*:\
	:cm=\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=^J:ei=\Er:ho=^^:\
	:im=\Eq:is=\Eu\E3:k0=^A0\r:kd=^J:kl=^H:kr=^L:ku=^K:\
	:le=^H:nd=^L:se=\Eg0:sf=^J:so=\Eg1:ta=^I:ue=\Eg0:\
	:up=^K:us=\Eg1:
# (falco-p: mapped ":pt:" to default tabs -- esr)
falco-p|ts1p|ts-1p|falco ts-1 with paging option:\
	:am:bs:da:db:mi:ms:pt:ul:\
	:co#80:li#24:\
	:al=\EE:bl=^G:bt=\EI:cd=\EY:ce=\ET\EG0\010\Eg0:\
	:cl=\E*:cm=\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=\E[B:\
	:ei=\Er:im=\Eq:is=\EZ\E3\E_c:kd=\E[B:kh=\E[H:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=^H:nd=\E[C:se=\Eg0:sf=^J:so=\Eg4:\
	:ta=^I:te=\E_b:ti=\E_d:ue=\Eg0:up=\E[A:us=\Eg1:
ts100|ts100-sp|falco ts100-sp:\
	:am:mi:ms:xn:xo:\
	:co#80:it#8:li#24:vt#3:\
	:@8=\EOM:DO=\E[%dB:K1=\EOq:K2=\EOr:K3=\EOs:K4=\EOp:\
	:K5=\EOn:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E~E:as=^N:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:dc=\E~W:dl=\E~R:do=^J:eA=\E(B\E)0:ei=:\
	:ho=\E[H:i1=\E~)\E~ea:ic=\E~Q:im=:k0=\EOy:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\EOt:k6=\EOu:k7=\EOv:\
	:k8=\EOl:k9=\EOw:k;=\EOx:kb=^H:kd=\EOB:ke=\E[?1l\E>:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m\017:mr=\E[7m:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:..sa=\E[0%?%p1%p6%|%t;1%;%?%p2%t;4%;%?%p1%p3%|%t;7%;%?%p4%t;5%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[1;7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:
ts100-ctxt|falco ts-100 saving context:\
	:te=\E~_b:ti=\E~_d\E[2J:tc=ts100:

#### Florida Computer Graphics
#

#	Florida Computer Graphics Beacon System, using terminal emulator
#	program "host.com", as provided by FCG.  Entry provided by
#	David Bryant (cbosg!djb) 1/7/83.
#	This description is for an early release of the "host" program.
#	Known bug: ed clears the whole screen, so it's commented out.
#
beacon|FCG Beacon System:\
	:am:da:db:\
	:co#80:li#32:\
	:al=\EE:bl=\ESTART\r\E37\r\EEND\r:ce=\ET:cl=\EZ:\
	:cm=\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=^J:ei=:ho=\EH:\
	:ic=\EQ:im=:le=^H:mb=\ESTART\r\E61\0541\r\EEND\r:\
	:me=\ESTART\r\E78\r\E70\0540\r\EEND\r:\
	:mr=\ESTART\r\E59\0541\r\EEND\r:nd=\EV:\
	:se=\ESTART\r\E70\0540\r\EEND\r:sf=^J:\
	:so=\ESTART\r\E70\0546\r\EEND\r:\
	:ti=\ESTART\r\E2\0540\r\E12\r\EEND\r:\
	:ue=\ESTART\r\E60\0540\r\EEND\r:up=\EU:\
	:us=\ESTART\r\E60\0541\r\EEND\r:

#### Fluke
#

# The 1720a differences from ANSI: no auto margin, destructive 
# tabs, # of lines, funny highlighting and underlining
f1720|f1720a|fluke 1720A:\
	:xt:\
	:co#80:li#16:sg#1:ug#1:\
	:bl=^G:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:cm=\E[%i%d;%dH:\
	:cr=^M:do=\E[B:is=\E[;H\E[2J:kd=^]:kl=^_:kr=^^:ku=^\:\
	:le=^H:nd=\E[C:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:\
	:ue=\E[m:up=\E[A:us=\E[4m:

#### Liberty Electronics (Freedom)
#
#	Liberty Electronics
#	48089 Fremont Blvd
#	Fremont CA 94538
#	Vox: (510)-623-6000
#	Fax: (510)-623-7021

# From: <faletti@berkeley.edu>
f100|freedom|freedom100|freedom model 100:\
	:am:bw:hs:mi:ms:xo:\
	:co#80:li#24:\
	:ae=\E$:al=\EE:as=\E%:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:ch=\E]%+ :cl=^Z:cm=\E=%+ %+ :cr=^M:ct=\E3:cv=\E[%+ :\
	:dc=\EW:dl=\ER:do=^J:ds=\Eg\Ef\r:ei=\Er:fs=^M:ho=^^:\
	:im=\Eq:ip=:is=\Eg\Ef\r\Ed:k1=^A@\r:k2=^AA\r:\
	:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:k7=^AF\r:\
	:k8=^AG\r:k9=^AH\r:k;=^AI\r:kB=\EI:kb=^H:kd=^V:kh=^^:\
	:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:se=\EG0:sf=^J:so=\EG4:\
	:sr=\Ej:st=\E1:ta=^I:ts=\Eg\Ef:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eb\Ed:
f100-rv|freedom-rv|freedom 100 in reverse video:\
	:is=\Eg\Ef\r\Eb:vb=\Ed\Eb:tc=f100:
# The f110 and f200 have problems with vi(1).  They use the ^V
# code for the down cursor key. When kcud1 is defined in terminfo
# as ^V, the Control Character Quoting capability (^V in insert mode)
# is lost! It cannot be remapped in vi because it is necessary to enter
# a ^V to to quote the ^V that is being remapped!!!
# 
# f110 users will have to decide whether
# to lose the down cursor key or the quoting capability. We will opt
# initially for leaving the quoting capability out, since use of VI
# is not generally applicable to most interactive applications
# 
# The same applies to f200 users, except that another option exists.
# This option has been chosen locally. It will not be distributed unless
# a user runs into this problem and requests assistance. Very few users,
# if any, should run into this problem. The local solution is in
# vifix.local.ti. The f200 has the ability to reprogram the down cursor
# key. The key is reprogrammed to ^J (linefeed). This value is remembered
# in non-volatile RAM, so powering the terminal off and on will not cause
# the change to be lost. The terminfo definition for the f200 is changed
# to identify kcud1 as ^J instead of ^V.
f110|freedom110|Liberty Freedom 110:\
	:am:es:hs:mi:ms:xo:\
	:co#80:it#8:li#24:ws#80:\
	:ae=\E%%:al=\EE:as=\E$:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:ch=\E]%+ :cl=^Z:cm=\E=%+ %+ :cr=^M:ct=\E3:cv=\E[%+ :\
	:dc=\EW:dl=\ER:do=^V:ds=\Ef\r:ei=\Er\EO:fs=^M:ho=^^:\
	:k0=^AI\r:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:\
	:k5=^AD\r:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=\EE:\
	:kC=^^:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kS=\EY:kb=^H:\
	:kd=^V:kl=^H:kr=^L:ku=^K:le=^H:mb=\EG2:md=\EG0:\
	:me=\EG0:mh=\EG@:mk=\EG1:mr=\EG4:nd=^L:pf=\Ea:po=\E`:\
	:se=\EG0:sf=^J:so=\EG<:sr=\EJ\nsmir=\EO\Eq:st=\E1:\
	:ts=\Ef:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eb\200\200\200\200\Ed:ve=\E.2:vi=\E.1:vs=\E.2:
f110-14|Liberty Freedom 110 14inch:\
	:dc@:tc=f110:
f110-w|Liberty Freedom 110 - 132 cols:\
	:co#132:\
	:tc=f110:
f110-14w|Liberty Freedom 110 14in/132 cols:\
	:co#132:\
	:dc@:tc=f110:
f200|freedom200|Liberty Freedom 200:\
	:am:es:hs:mi:ms:xo:\
	:co#80:it#8:li#24:ws#80:\
	:ae=\E%%:al=\EE:as=\E$:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:ch=\E]%+ :cl=^Z:cm=\E=%+ %+ :cr=^M:cs=\Em0%+ %+ :\
	:ct=\E3:cv=\E[%+ :dc=\EW:dl=\ER:do=^V:ds=\Ef\r:\
	:ei=\Er:fs=^M:ho=^^:im=\Eq:k0=^AI\r:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=\EE:kC=^^:kD=\EW:\
	:kE=\ET:kI=\EQ:kL=\ER:kS=\EY:kb=^H:kd=^V:kl=^H:kr=^L:\
	:ku=^K:le=^H:mb=\EG2:md=\EG0:me=\EG0:mh=\EG@:mk=\EG1:\
	:mr=\EG4:nd=^L:pf=\Ea:po=\E`:se=\EG0:sf=^J:so=\EG<:\
	:sr=\EJ:st=\E1:ts=\Ef:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eo\200\200\200\200\200\200\200\200\200\200\200\200\200\200\200\En:\
	:ve=\E.1:vi=\E.0:vs=\E.1:
f200-w|Liberty Freedom 200 - 132 cols:\
	:co#132:\
	:tc=f200:
f200vi|Liberty Freedom 200 for vi:\
	:am:es:hs:mi:ms:xo:\
	:co#80:it#8:li#24:ws#80:\
	:ae=\E%%:al=\EE:as=\E$:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:ch=\E]%+ :cl=^Z:cm=\E=%+ %+ :cr=^M:cs=\Em0%+ %+ :\
	:ct=\E3:cv=\E[%+ :dc=\EW:dl=\ER:do=^V:ds=\Ef\r:\
	:ei=\Er:fs=^M:ho=^^:im=\Eq:k0=^AI\r:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:kA=\EE:kC=^^:kD=\EW:\
	:kE=\ET:kI=\EQ:kL=\ER:kS=\EY:kb=^H:kd=^J:kl=^H:kr=^L:\
	:ku=^K:le=^H:mb=\EG2:md=\EG0:me=\EG0:mh=\EG@:mk=\EG1:\
	:mr=\EG4:nd=^L:pf=\Ea:po=\E`:se=\EG0:sf=^J:so=\EG<:\
	:sr=\EJ:st=\E1:ts=\Ef:ue=\EG0:up=^K:us=\EG8:\
	:vb=\Eb\200\200\200\200\Ed:ve=\E.1:vi=\E.0:vs=\E.1:
f200vi-w|Liberty Freedom 200 - 132 cols for vi:\
	:co#132:\
	:tc=f200vi:

#### GraphOn (go)
#
#	Graphon Corporation
#	544 Division Street
#	Campbell, CA 95008
#	Vox: (408)-370-4080
#	Fax: (408)-370-5047
#	Net: troy@graphon.com (Troy Morrison)
#
#
# The go140 and go225 have been discontinued.  GraphOn now makes X terminals,
# including one odd hybrid that starts out life on power-up as a character
# terminal, than can be switched to X graphics mode (driven over the serial
# line) by an escape sequence.  No info on this beast yet.

# (go140: mapped ":pt:" to default tabs -- esr)
go140|graphon go-140:\
	:bs:pt:\
	:co#80:li#24:\
	:al=\E[L:cd=10\E[J:ce=\E[K:cl=10\E[;H\E[2J:\
	:cm=\E[%i%2;%2H:dc=\E[P:dl=\E[M:ei=\E[4l:\
	:if=/usr/share/tabset/vt100:im=\E[4h:\
	:is=\E<\E=\E[?3l\E[?7l\E(B\E[J\E7\E[;r\E8\E[m\E[q:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:kd=\EOB:\
	:ke=\E[?1l\E>:kh=\E[H:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:\
	:ku=\EOA:nd=\E[C:se=\E[m:so=\E[7m:sr=\EM:ue=\E[m:\
	:up=\E[A:us=\E[4m:
go140w|graphon go-140 in 132 column mode:\
	:co#132:\
	:is=\E<\E=\E[?3h\E[?7h\E(B\E[J\E7\E[;r\E8\E[m\E[q:tc=go140:
# Hacked up vt200 termcap to handle GO-225/VT220
# From: <edm@nwnexus.WA.COM>
# (go225: mapped ":pt:" to default tabs -- esr)
go225|go-225|Graphon 225:\
	:am:bs:mi:pt:xn:\
	:co#80:li#25:vt#3:\
	:al=\E[L:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[M:do=^J:ei=\E[4l:\
	:ho=\E[H:im=\E[4h:\
	:is=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:kb=^H:kd=\E[B:ke=\E>:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ks=\E=:ku=\E[A:le=^H:\
	:mb=\E[5m:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:rc=\E8:\
	:rf=/usr/share/tabset/vt100:rs=\E[!p\E[?7h\E[2;1;1#w:\
	:sc=\E7:se=\E[27m:sf=\ED:so=\E[7m:sr=\EM:\
	:te=\E[!p\E[?7h\E[2;1;1#w:ti=\E[2;0#w\E[1;25r:\
	:ue=\E[24m:up=\E[A:us=\E[4m:

#### Harris (Beehive)
#
# Bletch.  These guys shared the Terminal Brain Damage laurels with Hazeltine.
# Their terminal group is ancient history now (1995) though the parent
# company is still in business.
#

# Beehive documentation is undated and marked Preliminary and has no figures
# so we must have early Superbee2 (Model 600, according to phone conversation
# with mfr.). It has proved reliable except for some missing padding
# (notably after \EK and nl at bottom of screen).
# 
# The key idea is that AEP mode is poison for cup & that US's in 
# the local memory should be avoided like the plague. That means 
# that the 2048 character local buffer is used as 25 lines of 80 
# characters, period. No scrolling local memory, folks. It also 
# appears that we cannot use naked INS LINE feature since it uses
# US. The sbi fakes il1 with an 80-space insert that may be too 
# slow at low speeds; also spaces get converted to \040 which is 
# too long for some programs (not vi).  DEL LINE is ok but slow.
# 
# The nl string is designed for last line of screen ONLY; cup to 
# 25th line corrects the motion inherent in scrolling to Page 1.
# 
# There is one understood bug. It is that the screen appears to
# pop to a new (blank) page after a nel, or leave a half-line 
# elipsis to a quad that is the extra 48 memory locations. The 
# data received is dumped into memory but not displayed.  Not to 
# worry if cup is being used; the lines not displayed will be, 
# whenever the cursor is moved up there. Since cup is addressed 
# relative to MEMORY of window, nothing is lost; but beware of 
# relative cursor motion (cuu1,cud1,cuf1,cub1). Recommended, therefore, 
# is setenv MORE -c .
# 
# WARNING: Not all features tested.
# 
# Timings are assembled from 3 sources. Some timings may reflect 
# SB2/Model 300 that were used if more conservative.
# Tested on a Model 600 at 1200 and 9600 bd.
# 
# The BACKSPACEkb option is cute. The NEWLINE key, so cleverly 
# placed on the keyboard and useless because of AEP, is made 
# into a backspace key. In use ESC must be pressed twice (to send)
# and sending ^C must be prefixed by ESC to avoid that wierd 
# transmit mode associated with ENTER key.
# 
# IF TERMINAL EVER GOES CATATONIC with the cursor buzzing across 
# the screen, then it has dropped into ENTER mode; hit 
# RESET--ONLINE--!tset.
# 
# As delivered this machine has a FATAL feature that will throw 
# it into that strange transmit state (SPOW) if the space bar is 
# hit after a CR is received, but before receiving a LF (or a 
# few others).
# 
# The circuits MUST be modified to eliminate the SPOW latch. 
# This is done by strapping on chip A46 of the I/O board; cut 
# the p.c. connection to Pin 5 and strap Pin 5 to Pin 8 of that 
# chip. This mod has been checked out on a Mod 600 of Superbee II.
# With this modification absurdly high timings on cr are 
# unnecessary.
# 
# NOTE WELL that the rear panel switch should be set to CR/LF, 
# not AEP!
#
sb1|beehive superbee:\
	:am:bw:da:db:mi:ul:xb:\
	:co#80:li#25:sg#1:ug#1:\
	:al=\EN\EL\EQ                                                                                \EP \EO\ER\EA:\
	:bl=^G:bt=\E`:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EF%r%03%03:\
	:cr=\r:ct=\E3:dc=\EP:dl=\EM:do=^J:ei=\ER:ho=\EH:\
	:im=\EQ\EO:is=\EE\EX\EZ\EO\Eb\Eg\ER:k0=\E2:k1=\Ep:\
	:k2=\Eq:k3=\Er:k4=\Es:k5=\Et:k6=\Eu:k7=\Ev:k8=\Ew:\
	:k9=\E1:kE=\EK:kI=\EQ\EO:kL=\EM:kM=\ER:kS=\EJ:kb=^_:\
	:kd=\EB:kh=\EH:kl=\ED:kr=\EC:ku=\EA:l0=TAB CLEAR:\
	:l9=TAB SET:le=^H:nd=\EC:se=\E_3:sf=^J:so=\E_1:\
	:st=\E1:ta=^I:ti=\EO:ue=\E_3:up=\EA:us=\E_0:
sbi|superbee|beehive superbee at Indiana U.:\
	:xb:\
	:al=1\EN\EL\EQ \EP \EO\ER\EA:cr=\r:tc=sb1:
# Alternate (older) description of Superbee - f1=escape, f2=^C.
# Note: there are at least 3 kinds of superbees in the world.  The sb1
# holds onto escapes and botches ^C's.  The sb2 is the best of the 3.
# The sb3 puts garbage on the bottom of the screen when you scroll with
# the switch in the back set to CRLF instead of AEP.  This description
# is tested on the sb2 but should work on all with either switch setting.
# The f1/f2 business is for the sb1 and the xsb can be taken out for
# the other two if you want to try to hit that tiny escape key.
# This description is tricky: being able to use cup depends on there being
# 2048 bytes of memory and the hairy nl string.
superbee-xsb|beehive super bee:\
	:am:bs:da:db:pt:xb:\
	:co#80:dC#10:it#8:li#25:\
	:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EF%r%3%3:cr=\r:ct=\E3:\
	:dc=\EP:dl=\EM:do=^J:ho=\EH:is=\EH\EJ:k1=\Ep:k2=\Eq:\
	:k3=\Er:k4=\Es:k5=\Et:k6=\Eu:k7=\Ev:k8=\Ew:kd=\EB:\
	:kh=\EH:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:\
	:nl=\n\200\200\200\n\200\200\200\EA\EK\200\200\200\ET\ET:\
	:se=\E_3:\
	:sf=\n\200\200\200\n\200\200\200\EA\EK\200\200\200\ET\ET:\
	:so=\E_1:st=\E1:up=\EA:ve=^J:
# This loses on lines > 80 chars long, use at your own risk
superbeeic|super bee with insert char:\
	:ei=\ER:ic=:im=\EQ:tc=superbee-xsb:
sb2|sb3|fixed superbee:\
	:xb@:\
	:tc=superbee:

# Reports are that most of these Beehive entries (except superbee) have not
# been tested and do not work right.  :se: is a trouble spot.  Be warned.

# (bee: removed obsolete ":ko=al,bt,ce,cl,dc,dl,ei,ho,ic,im:" -- esr)
beehive|bee|harris beehive:\
	:am:bs:mi:\
	:co#80:li#24:\
	:al=\EL:bt=\E>:cd=\EJ:ce=\EK:cl=\EE:cm=\EF%+ %+ :\
	:dc=\EP:dl=\EM:do=\EB:ei=\E@:ho=\EH:ic=:im=\EQ:kb=^H:\
	:kd=\EB:kh=\EH:kl=\ED:kr=\EC:ku=\EA:nd=\EC:se=\Ed@:\
	:so=\EdP:ue=\Ed@:up=\EA:us=\Ed`:
# set tab is ^F, clear (one) tab is ^V, no way to clear all tabs.
# good grief - does this entry make sg/ug when it doesn't have to?
# look at those spaces in se/so.  Seems strange to me...
# (bh3m: mapped ":pt:" to default tabs -- esr)
beehive3|bh3m|beehiveIIIm:\
	:am:bs:pt:\
	:co#80:li#20:\
	:al=\023:bl=^G:cd=^R:ce=^P:cl=^E^R:cr=^M:dl=\021:\
	:do=^J:ho=^E:if=/usr/share/tabset/beehive:le=^H:\
	:ll=^E^K:nd=^L:se= ^_:sf=^J:so=^] :ta=^I:up=^K:
beehive4|bh4|beehive 4:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EE:cr=^M:do=^J:ho=\EH:\
	:le=\ED:nd=\EC:sf=^J:up=\EA:
# (microb: mapped ":pt:" to default tabs -- esr)
microb|microbee|micro bee series:\
	:am:bs:pt:\
	:co#80:li#24:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EE:cm=\EF%+ %+ :cr=^M:do=^J:\
	:k1=\Ep:k2=\Eq:k3=\Er:k4=\Es:k5=\Et:k6=\Eu:k7=\Ev:\
	:k8=\Ew:k9=\Ex:kd=\EB:kh=\EH:kl=\ED:kr=\EC:ku=\EA:\
	:le=^H:nd=\EC:se=\Ed@ :sf=^J:so= \EdP:ta=^I:ue=\Ed@:\
	:up=\EA:us=\Ed`:

# 8675, 8686, and bee from Cyrus Rahman
# (8675: changed k10, k11...k16 to k;, F1...F6 -- esr)
ha8675|harris 8675:\
	:F1=^W:F2=\ER:F3=\EE:F4=\EI:F5=\Ei:F6=\Eg:\
	:is=\ES\E#\E*\Eh\Em\E?\E1\E9\E@\EX\EU:k1=^F:k2=^P:\
	:k3=^N:k4=^V:k5=^J:k6=^T:k7=^H:k8=\177:k9=\Ee:k;=\Ed:tc=bee:
# (8686: changed k10, k11...k16 to k;, F1...F6; fixed broken continuation
# in :is: -- esr)
ha8686|harris 8686:\
	:F1=\EW:F2=\002\E{\003:F3=\002\E|\003:F4=\002\E}\003:\
	:F5=\002\E~\003:F6=\002\E\177\003:\
	:is=\ES\E#\E*\Eh\Em\E?\E1\E9\E@\EX\EU\E"*Z01\E"8F35021B7C83#\E"8F45021B7D83#\E"8F55021B7E83#\E"8F65021B7F83#\E"8F75021B7383#\E"8F851BD7#\E"8F95021B7083#\E"8FA5021B7183#\E"8FB5021B7283#:\
	:k1=\002\Ep\003:k2=\002\Eq\003:k3=\002\Er\003:\
	:k4=\002\Es\003:k5=\E3:k6=\EI:k7=\ER:k8=\EJ:k9=\E(:\
	:k;=\Ej:tc=bee:

#### Hazeltine
#
# Hazeltine appears to be out of the business now (1995).  These guys were 
# co-owners of the Terminal Brain Damage Hall Of Fame along with Harris.
# Good riddance.
#
# The ony contact information I have dates from 1993 and is:
#
# Customer Service Division
# 15 Law Drive
# P.O. Box 2076
# Fairfield, NJ 07007-2078
#
# Since :nd: is blank, when you want to erase something you
# are out of luck.  You will have to do ^L's a lot to
# redraw the screen.  h1000 is untested.  It doesn't work in
# vi - this terminal is too dumb for even vi.  (The code is
# there but it isn't debugged for this case.)
h1000|hazeltine 1000:\
	:bs:\
	:co#80:li#12:\
	:bl=^G:cl=^L:cr=^M:do=^J:ho=^K:le=^H:nd= :sf=^J:
# From: <cbosg!ucbvax!pur-ee!cincy!chris> Thu Aug 20 09:09:18 1981
h1420|hazeltine 1420:\
	:am:bs:\
	:co#80:li#24:\
	:al=\E^Z:bl=^G:cd=\E^X:ce=\E^O:cl=\E^\:\
	:cm=\E\021%r%.%+ :cr=^M:dl=\E^S:do=^J:le=^H:nd=^P:\
	:se=\E^Y:sf=^J:so=\E^_:ta=^N:up=\E^L:
# New "safe" cursor movement (11/87) from cgs@umd5.umd.edu.  Prevents freakout
# with out-of-range args and tn3270.  No hz since it needs to receive ~'s.
h1500|hazeltine 1500:\
	:am:bs:hz:\
	:co#80:li#24:\
	:al=~\032:bl=^G:cd=~\030:ce=~^O:cl=~^\:\
	:cm=~\021%r%>^^ %+`%+`:cr=^M:dl=~\023:do=~^K:ho=~^R:\
	:kd=^J:kh=~^R:kl=^H:kr=^P:ku=~^L:le=^H:nd=^P:se=~^Y:\
	:sf=^J:so=~^_:up=~^L:
# h1510 assumed to be in sane escape mode.  Else use h1500.
# (h1510: early versions of this entry apparently had ":se=\E^_:so=\E^Y:",
# but these caps were commented out in 8.3; also, removed incorrect
# and overridden ":do=^J:" -- esr)
h1510|hazeltine 1510:\
	:am:bs:\
	:co#80:li#24:\
	:al=\E^Z:bl=^G:cd=\E^X:ce=\E^O:cl=\E^\:\
	:cm=\E\021%r%.%.:cr=^M:dl=\E^S:do=\E^K:le=^H:nd=^P:\
	:sf=^J:up=\E^L:
# (h1520: removed incorrect and overridden ":do=^J:" -- esr)
h1520|hazeltine 1520:\
	:am:bs:hz:\
	:co#80:li#24:\
	:al=~^Z:bl=^G:cd=~^X:ce=~^O:cl=~^\:cm=~\021%r%.%.:\
	:cr=^M:dl=~^S:do=~^K:ho=~^R:le=^H:nd=^P:se=~^Y:sf=^J:\
	:so=~^_:up=~^L:
# Note: the h1552 appears to be the first Hazeltine terminal which
# is not braindamaged.  It has tildes and backprimes and everything!
# Be sure the auto lf/cr switch is set to cr.
h1552|hazeltine 1552:\
	:al=\EE:dl=\EO:do=^J:k1=\EP:k2=\EQ:k3=\ER:l1=blue:\
	:l2=red:l3=green:tc=vt52:
h1552rv|hazeltine 1552 reverse video:\
	:do=^J:se=\ET:so=\ES:tc=h1552:
# Note: h2000 won't work well because of a clash between upper case and ~'s.
h2000|hazeltine 2000:\
	:am:bs:nc:\
	:co#74:li#27:\
	:al=~\032:bl=^G:cl=~\034:cm=~\021%r%.%.:dl=~\023:\
	:do=^J:ho=~^R:le=^H:pc=\177:sf=^J:
# Date: Fri Jul 23 10:27:53 1982.  Some unknown person wrote:
# I tested this termcap entry for the Hazeltine Esprit with vi. It seems
# to work ok. There is one problem though if one types a lot of garbage
# characters very fast vi seems not able to keep up and hangs while trying
# to insert. That's in insert mode while trying to insert in the middle of
# a line. It might be because the Esprit doesn't have insert char and delete
# char as a built in function. Vi has to delete to end of line and then 
# redraw the rest of the line.
esprit|Hazeltine Esprit I:\
	:am:bw:\
	:co#80:li#24:\
	:al=\E^Z:bl=^G:bt=\E^T:cd=\E^W:ce=\E^O:cl=\E^\:\
	:cm=\E\021%r%.%.:cr=^M:dl=\E^S:do=\E^K:ho=\E^R:\
	:is=\E?:k0=^B0^J:k1=^B1^J:k2=^B2^J:k3=^B3^J:k4=^B4^J:\
	:k5=^B5^J:k6=^B6^J:k7=^B7^J:k8=^B8^J:k9=^B9^J:kb=^H:\
	:kd=\E^K:ke=\E>:kh=\E^R:kl=^H:kr=^P:ks=\E<:ku=\E^L:\
	:l0=0:l1=1:l2=2:l3=3:l4=4:l5=5:l6=6:l7=7:l8=8:l9=9:\
	:le=^H:nd=^P:se=\E^Y:sf=^J:so=\E^_:up=\E^L:
esprit-am|hazeltine esprit auto-margin:\
	:am:\
	:tc=esprit:

#### IBM
#

ibm327x|line mode IBM 3270 style:\
	:gn:\
	:ce=^M:cl=^M^J:ho=^M:
# From: J.B. Nicholson-Owens <jeffo@uiuc.edu> 8 Mar 94
ibm3101|i3101|IBM 3101-10:\
	:am:bs:pt:xo:\
	:co#80:li#24:\
	:bl=^G:cd=\EJ:ce=\EI:cl=\EK:cm=\EY%+ %+ :cr=^M:\
	:ct=\E1:do=^J:ho=\EH:if=/usr/share/tabset/ibm3101:\
	:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:\
	:nw=^M^J:sf=^J:st=\E0:ta=^I:up=\EA:
#   Received from the IBM terminals division (given to DRB)
#   June 1988 for PS/2 OS 2.2.3 cut
ibm3151|i3151:\
	:me=\E4@:\
	:..sa=\E4%{64}%?%p1%{0}%>%p1%{4}%<%&%t%{8}%|%;%?%p1%{7}%=%t%{16}%|%;%?%p2%t%{1}%|%;%?%p3%t%{4}%|%;%?%p4%t%{2}%|%;%c:\
	:se=\E4@:so=\E4A:ue=\E4@:us=\E4B:tc=ibm3163:
# From: Mark Easter <marke@fsi-ssd.csg.ssd.fsi.com> 29 Oct 1992 
# I commented out some IBM extensions.
ibm3161|ibm3163|wy60-316X|wyse60-316X|IBM 3161/3163 display:\
	:am:mi:ms:\
	:co#80:it#8:li#24:\
	:F1=\Ek\r:F2=\El\r:F3=\E!a\r:F4=\E!b\r:F5=\E!c\r:\
	:F6=\E!d\r:F7=\E!e\r:F8=\E!f\r:F9=\E!g\r:FA=\E!h\r:\
	:FB=\E!i\r:FC=\E!j\r:FD=\E!k\r:FE=\E!l\r:bl=^G:\
	:cd=\EJ:ce=\EI:cl=\EH\EJ:cm=\EY%+ %+ :cr=^M:dc=\EQ:\
	:dl=\EO:do=\EB:ho=\EH:k1=\Ea\r:k2=\Eb\r:k3=\Ec\r:\
	:k4=\Ed\r:k5=\Ee\r:k6=\Ef\r:k7=\Eg\r:k8=\Eh\r:\
	:k9=\Ei\r:k;=\Ej\r:kA=\EN:kC=\EL\r:kD=\EQ:kE=\EI:\
	:kI=\EP \010:kL=\EO:kS=\EJ:kT=\E0:ka=\E 1:kb=^H:\
	:kd=\EB:kh=\EH:kl=\ED:kr=\EC:kt=\E1:ku=\EA:le=\ED:\
	:mb=\E4D:md=\E4H:me=\E4@\E<@:mk=\E4P:mr=\E4A:nd=\EC:\
	:..sa=\E4%'@'%?%p1%t%'A'%|%;\n%?%p2%t%'B'%|%;\n%?%p3%t%'A'%|%;\n%?%p4%t%'D'%|%;\n%?%p5%t%'@'%|%;\n%?%p6%t%'H'%|%;\n%?%p7%t%'P'%|%;%c\n%?%p9%t\E>A%e\E<@%;:\
	:se=\E4@:sf=^J:so=\E4A:te=\E>A:ti=\E>A:ue=\E4@:\
	:up=\EA:us=\E4B:

# How the 3164 sgr string works:
#	%{32}	        # push space for no special video characteristics
#	%?%p2%t%{1}%|%; # if p2 set, then OR the 1 bit for reverse
#	%?%p3%t%{4}%|%; # if p3 set, then OR the 4 bit for blink
#	%?%p4%t%{2}%|%; # if p4 set, then OR the 2 bit for underline
#	%c              # pop Pa1
#	%{39}%p1%-	# calculate 32 + (7 - p1) for foreground
#	%c		# pop Pa2 
#	%{64}		# use only black background for now
#	%c		# pop Pa3
ibm3164|i3164|3164:\
	:mb=\E4D:md=\E4H:me=\E4@:\
	:..sa=\E4%{32}%?%p2%t%{1}%|%;%?%p3%t%{4}%|%;%?%p4%t%{2}%|%;%c%{39}%p1%-%c%{64}%c:tc=ibm3163:

# (ibmaed: mapped ":pt:" to default tabs -- esr)
ibmaed|IBM Experimental display:\
	:am:bs:eo:ms:pt:\
	:co#80:li#52:\
	:al=\EN:cd=\EJ:ce=\EI:cl=\EH\EK:cm=\EY%+ %+ :dc=\EQ:\
	:dl=\EO:do=\EB:ei=:ho=\EH:ic=\EP:im=:kb=^H:kd=\EB:\
	:kl=\ED:kr=\EC:ku=\EA:nd=\EC:se=\E0:so=\E0:ue=:\
	:up=\EA:us=:vb=\EG:
ibm-apl|apl|IBM apl terminal simulator:\
	:li#25:\
	:tc=dm1520:
# (ibmmono: this had an unknown `sb' boolean, I changed it to `bs'.  
# Also it had ":I0=f10:" which pretty obviously should be "l0=f10" -- esr)
ibmmono|ibm5151|IBM workstation monochrome:\
	:bs:es:hs:\
	:al=\EL:dl=\EM:ds=\Ej\EY8 \EI\Ek:fs=\Ek:k0=\E<:\
	:k1=\ES:k2=\ET:k3=\EU:k4=\EV:k5=\EW:k6=\EP:k7=\EQ:\
	:k8=\ER:k9=\EY:kF=\EE:kI=\200:kN=\EE:kP=\Eg:kR=\EG:\
	:kb=^H:kh=\EH:l0=f10:md=\EZ:me=\Ew\Eq\Ez\EB:\
	:mk=\EF\Ef0;\Eb0;:mr=\Ep:se=\Ez:so=\EZ:sr=\EA:\
	:ts=\Ej\EY8%+ \Eo:ue=\Ew:us=\EW:tc=ibm3101:
ibmega-c|ibm5154-c|IBM Enhanced Color Display:\
	:se=\EB:so=\EF\Ef3;:ue=\EB:us=\EF\Ef2;:tc=ibmmono:
# ibmapa* and ibmmono entries come from ACIS 4.3 distribution
rtpc|ibmapa16|ibm6155|IBM 6155 Extended Monochrome Graphics Display:\
	:li#32:\
	:ds=\Ej\EY@ \EI\Ek:ts=\Ej\EY@%+ \Eo:tc=ibmmono:
# Advanced Monochrome (6153) and Color (6154) Graphics Display:
ibmapa8c|ibmapa8|ibm6154|ibm6153|IBM 6153/4 Advanced Graphics Display:\
	:li#31:\
	:ds=\Ej\EY? \EI\Ek:ts=\Ej\EY?%+ \Eo:tc=ibmmono:
ibmapa8c-c|ibm6154-c|IBM 6154 Advanced Color Graphics Display:\
	:li#31:\
	:ds=\Ej\EY? \EI\Ek:mh=\EF\Ef7;:ts=\Ej\EY?%+ \Eo:tc=ibmega-c:
# From: Marc Pawliger <marc@ibminet.awdpa.ibm.com>
# also in /usr/lpp/bos/bsdsysadmin.
# (hft-c: this entry had :kb=\E[D:kf=\E[C: on the line with ku/kd/kh; this was
# pretty obviously mislabeled for :le: and :nd:; also ":ul=\E[4m:" was clearly
# a typo for ":us=\E[4m:"; also ":el=\E[K:" was a typo for ":ce=\E[K:".
# There was an unknown boolean ":ht:" which I assume was meant to set 
# hardware tabs, so I have insrted it#8. Finally, "ac=^N" paired with the
# ae looked like a typo for ":as=^N:" -- esr)
ibm8512|ibm8513|hft-c|IBM High Function Terminal:\
	:am:mi:ms:\
	:co#80:it#8:li#25:\
	:AL=\E[%dL:DL=\E[%dM:ae=^O:al=\E[L:as=^N:cd=\E[J:\
	:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:dl=\E[M:dm=\E[4h:\
	:do=^J:ec=\E[%dX:ed=\E[4l:ei=\E[4l:ho=\E[H:im=\E[4h:\
	:is=\Eb\E[m\017\E[?7h:k0=\E[010q:k1=\E[001q:\
	:k2=\E[002q:k3=\E[003q:k4=\E[004q:k5=\E[005q:\
	:k6=\E[006q:k7=\E[007q:k8=\E[008q:k9=\E[009q:kd=\E[B:\
	:kh=\E[H:ku=\E[A:le=\E[D:mb=\E[5m:md=\E[1m:me=\E[m:\
	:mr=\E[7m:nd=\E[C:rc=\E[u:\
	:rs=\Eb\E[m\017\E[?7h\E[H\E[J:sc=\E[s:se=\E[m:\
	:so=\E[7m:te=\E[20h:ti=\E[20;4l\E[?7h\Eb:ue=\E[m:\
	:up=\E[A:us=\E[4m:
hft|AIWS High Function Terminal:\
	:am:xo:\
	:co#80:li#25:\
	:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:do=^J:ei=\E6:\
	:ho=\E[H:ic=\E[@:im=\E6:k1=\E[001q:k2=\E[002q:\
	:k3=\E[003q:k4=\E[004q:k5=\E[005q:k6=\E[006q:\
	:k7=\E[007q:k8=\E[008q:k9=\E[009q:kN=\E[153q:\
	:kP=\E[159q:ka=\E[010q:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[0m:\
	:mk=\E[8m:mr=\E[7m:nd=\E[C:se=\E[m:sf=^J:so=\E[7m:\
	:ta=^I:ue=\E[m:up=\E[A:us=\E[4m:
# From: <pryor@math.berkeley.edu>
ibm5081|ibmmpel|IBM 5081 1024x1024 256/4096 color display:\
	:es:hs:\
	:li#33:\
	:ds=\Ej\EYA \EI\Ek:fs=\Ek:ts=\Ej\EYA%+ \Eo:tc=ibmmono:
ibm5081-c|ibmmpel-c|IBM 5081 1024x1024 256/4096 enhanced color display:\
	:es:hs:\
	:li#33:\
	:ds=\Ej\EYA \EI\Ek:fs=\Ek:ts=\Ej\EYA%+ \Eo:tc=ibmega-c:
ibm-system1|system1|ibm system/1 computer:\
	:am:xt:\
	:co#80:li#24:\
	:bl=^G:cl=^Z:cm=\005%+ %+ :ho=^K:le=^H:nd=^\:sf=^J:\
	:up=^^:

#### Infoton/General Terminal Corp.
#

# gt100 sounds like something DEC would come out with.  Let's hope they don't.
i100|gt100|gt100a|General Terminal 100A (formerly Infoton 100):\
	:am:bs:\
	:co#80:li#24:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EK:cl=^L:cm=\Ef%r%+ %+ :\
	:cr=^M:dl=\EM:do=^J:ho=\EH:le=^H:nd=\EC:se=\Ea:sf=^J:\
	:so=\Eb:up=\EA:vb=\Eb\Ea:
i400|infoton 400:\
	:am:bs:\
	:co#80:li#25:\
	:al=\E[L:bl=^G:ce=\E[N:cl=\E[2J:cm=%i\E[%3;%3H:cr=^M:\
	:dc=\E[4h\E[2Q\E[P\E[4l\E[0Q:dl=\E[M:do=^J:\
	:ei=\E[4l\E[0Q:im=\E[4h\E[2Q:le=^H:nd=\E[C:sf=^J:\
	:up=\E[A:
# (addrinfo: removed obsolete ":bc=^Z:" -- esr)
addrinfo:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cd=^K:cl=^L:..cm=\037%p1%{1}%-%c%p2%{1}%-%c:\
	:cr=^M:do=^J:ho=^H:le=^Z:ll=^H^\:nd=^Y:sf=^J:up=^\:
infoton:\
	:am:\
	:Nl#0:co#80:lh#0:li#24:lw#0:\
	:bl=^G:cd=^K:cl=^L:cr=^M:do=^J:le=^Z:ll=^H^\:nd=^Y:\
	:sf=^J:up=^\:
# (infotonKAS: removed obsolete ":bc=^Z:" -- esr)
infotonKAS:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cd=^K:cl=^L:cr=^M:do=^J:le=^Z:ll=^H^\:nd=^Y:\
	:sf=^J:up=^\:

#### Interactive Systems Corp
#
# ISC used to sell OEMed and customized hardware to support ISC UNIX.
# ISC UNIX still exists in 1995, but ISC itself is no more; they got
# bought out by Sun.
#

# From: <cithep!eric>  Wed Sep 16 08:06:44 1981
# (intext: removed obsolete ":ma=^K^P^R^L^L :";
# mapped ":pt:" to default tabs, removed obsolete ":bc=^_:", also the
# ":le=^_:" later overridden -- esr)
intext|Interactive Systems Corporation modified owl 1200:\
	:am:\
	:co#80:li#24:sg#1:\
	:al=\020:bl=^G:bt=^Y:cd=\026J:ce=^Kp^R:cl=\014:\
	:cm=\017%+ %+ :cr=^M:dc=\022:dl=\021:do=^J:ei=^V<:\
	:im=^V;:ip=:k0=^VJ\r:k1=^VA\r:k2=^VB\r:k3=^VC\r:\
	:k4=^VD\r:k5=^VE\r:k6=^VF\r:k7=^VG\r:k8=^VH\r:\
	:k9=^VI\r:kb=^H:kd=^J:ke=^V9:kh=^Z:kl=^_:kr=^^:\
	:ks=\036\072\264\026%:ku=^\:le=^H:nd=^^:se=^V# :\
	:sf=^J:so=^V$\054:ta=^I:up=^\:
intext2|intextii|INTERACTIVE modified owl 1251:\
	:am:bw:ul:\
	:co#80:li#24:sg#0:\
	:al=\E[L:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:ch=\E[%+^AG:\
	:cl=\E[H\E[2J:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:\
	:do=\E[B:ei=:ic=\E[@:im=:k0=\E@\r:k1=\EP\r:k2=\EQ\r:\
	:k3=\ES\r:k4=\ET\r:k5=\EU\r:k6=\EV\r:k7=\EW\r:\
	:k8=\EX\r:k9=\EY\r:kb=^H:kd=\EB\r:kh=\ER\r:kl=\ED\r:\
	:kr=\EC\r:ku=\EA\r:l0=REFRSH:l1=DEL CH:l2=TABSET:\
	:l3=GOTO:l4=+PAGE:l5=+SRCH:l6=-PAGE:l7=-SRCH:l8=LEFT:\
	:l9=RIGHT:nd=\E[C:se=\E[2 D:sf=\E[S:so=\E[6 D:\
	:sr=\E[T:ta=^I:ue=\E[2 D:up=\E[A:us=\E[18 D:\
	:vb=\E[;;;;;;;;;2;;u\E[;;;;;;;;;1;;u:

#### Kimtron (abm, kt)
#
# Kimtron entries include (undocumented) codes for: enter dim mode (:mh:),
# enter bold mode (:md:), enter reverse mode (:mr:), turn off all attributes
# (:me:).

# Kimtron ABM 85 added by Dual Systems
# (abm85: mapped ":pt:" to default tabs; removed duplicated ":kd=^J:" -- esr)
abm85|Kimtron ABM 85:\
	:am:bs:bw:ms:pt:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EE:bt=\EI:cd=\Ey:ce=\Et:cl=\E*:cm=\E=%+ %+ :\
	:dc=\EW:dl=\ER:do=^J:ei=\Er:\
	:if=/usr/share/tabset/stdcrt:im=\EQ:\
	:is=\EC\EX\Eg\En\E%\Er\E(\Ek\Em\Eq:kb=^H:kd=^J:kh=^^:\
	:kl=^H:kr=^L:ku=^K:nd=^L:se=\Ek:so=\Ej:ue=\Em:up=^K:\
	:us=\El:
# Kimtron ABM 85H added by Dual Systems.
# Some notes about the 85h entries:
# 1) there are several firmware revs of 85H in the world. Use o85h for
#    firmware revs prior to SP51
# 2) Make sure to use 85h entry if the terminal is in 85H mode and the
#    85e entry if it is in 920 emulation mode. They are incompatible in
#    some places and NOT software settable i.e., :is: can't fix change it)
# 3) In 85h mode, the arrow keys and special functions transmit when
#    the terminal is in dup-edit, and work only locally in local-edit.
#    Vi won't swallow `del char' for instance, but :vs: turns on
#    dup-edit anyway so that the arrow keys will work right. If the
#    arrow keys don't work the way you like, change :vs:, :ve:, and :is:.
#    920E mode does not have software commands to toggle between dup
#    and local edit, so you get whatever was set last on the terminal.
# 4) :vb: attribute is nice, but seems too slow to work correctly (\Eb<pad>\Ed)
# 5) Make sure `hidden' attributes are selected. If `embedded' attributes
#    are selected, the entries :sg@: and :ug@: should be removed.
# 6) auto new-line should be on (selectable from setup mode only)
#
# From: Erik Fair <fair@ucbarpa>  Sun Oct 27 07:21:05 1985
abm85h|85H|85h|Kimtron ABM 85H, 85H mode:\
	:hs:\
	:sg@:ug@:\
	:ds=\Ee:fs=^M:im=\EZ:\
	:is=\EC\EN\EX\024\016\EA\Ea\E%\E9\Ee\Er\En\E"\E}\E'\E(\Ef\r\EG0\Ed\E.4\El:\
	:kd=^V:me=\E(\EG0:mh=\E):mr=\EG4:se=\EG0:so=\EG4:\
	:ts=\Eg\Ef:ue=\EG0:us=\EG8:vb@:ve=\E.4:vs=\E.2:tc=abm85:
abm85e|85E|85e|Kimtron ABM 85H, 920E mode:\
	:sg@:ug@:\
	:im=\EZ:\
	:is=\EC\EX\EA\E%\E9\Ee\Er\En\E"\E}\E'\E(\Ef\r\Ek\Eq\Em:\
	:me=\E(\Ek:mh=\E):mr=\Ej:vb@:tc=abm85:
abm85h-o|oabm85h|o85h|Kimtron ABM 85H, old firmware rev.:\
	:sg@:ug@:\
	:im=\EZ:\
	:is=\E}\EC\EX\Ee\En\E%\Er\E(\Ek\Em\Eq\Ed\ET\EC\E9\EF:\
	:me=\E(\Ek:mh=\E):mr=\Ej:\
	:vb=\200\200\200\007\200\200\200:tc=abm85:
# From: <malman@bbn-vax.arpa>
# (kt7: removed obsolete ":ko=ic,dc,al,dl,cl,ce,cd,bt:", ":ma=^V^J^L :";
# mapped ":pt:" to default tabs -- esr)
kt7|kimtron model kt-7:\
	:am:bs:pt:\
	:co#80:li#24:\
	:al=\EE:bt=\EI:cd=\EY:ce=\ET:cl=^Z:cm=\E=%+ %+ :\
	:dc=\EW:dl=\ER:do=^V:ei=:fs=\Eg:ho=^^:ic=\EQ:\
	:if=/usr/share/tabset/stdcrt:im=:is=\El\E":k0=^AI\r:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=^H:kd=^V:\
	:kh=^^:kl=^H:kr=^L:ku=^K:nd=^L:se=\EG0:so=\EG4:\
	:ts=\Ef:ue=\EG0:up=^K:us=\EG8:

#### Microterm (act, mime)
#
# The mime1 entries refer to the Microterm Mime I or Mime II.
# The default mime is assumed to be in enhanced act iv mode.
#

# New "safe" cursor movement (5/87) from reuss@umd5.umd.edu.  Prevents freakout with
# out-of-range args on Sytek multiplexors.  No ":so=^N:" and ":se=^N:" since 
# it gets confused and it's too dim anyway.  No ic since Sytek insists ^S 
# means xoff.
# (act4: found ":ic=2^S:ei=:im=:ip=.1*^V:" commented out in 8.3 -- esr)
act4|microterm|microterm act iv:\
	:am:bs:\
	:co#80:li#24:\
	:al=2.3*\001<2.3*/>:bl=^G:cd=2.2*\037:ce=.1*\036:\
	:cl=12\014:cm=\024%+^X%>/0%+P:cr=^M:dc=.1*\004:\
	:dl=2.3*\027:do=^K:ho=^]:kd=^K:kl=^H:kr=^X:ku=^Z:\
	:le=^H:nd=^X:sf=^J:up=^Z:
# The padding on :sr: and :ta: for act5 and mime is a guess and not final.
# The act 5 has hardware tabs, but they are in columns 8, 16, 24, 32, 41 (!)...
# (microterm5: removed obsolete ":ma==^Z^P^Xl^Kj:" -- esr)
act5|microterm5|microterm act v:\
	:kd=^K:kl=^H:kr=^X:ku=^Z:sr=\EH:uc=^H\EA:tc=act4:
# Act V in split screen mode.  act5s is not tested and said not to work.
act5s|skinny act5:\
	:co#39:li#48:\
	:te=\EQ:ti=\EP:tc=act5:
# Mimes using brightness for standout.  Half bright is really dim unless
# you turn up the brightness so far that lines show up on the screen.
mime-fb|full bright mime1:\
	:is=^S\E:se=^S:so=^Y:tc=mime:
mime-hb|half bright mime1:\
	:is=^Y\E:se=^Y:so=^S:tc=mime:
# (mime: removed obsolete ":ma=^X ^K^J^Z^P:"; removed ":do=^K:" that overrode
# the more plausible ":do=^J:"; mapped ":pt:" to ":it#8:" -- esr)
# uc was at one time disabled to get around a curses bug, be wary of it
mime|mime1|mime2|mimei|mimeii|microterm mime1:\
	:am:bs:pt:\
	:co#80:it#8:li#24:vt#9:\
	:al=\001:bl=^G:cd=^_:ce=^^:cl=^]^C:\
	:cm=\024%+^X%> 0%+P:cr=^M:dl=\027:do=^J:ho=^]:\
	:is=^S\E^Q:kd=^K:kl=^H:kr=^X:ku=^Z:le=^H:nd=^X:sf=^J:\
	:sr=\022:ta=\011:uc=^U:up=^Z:
# These termcaps (for mime 2a) put the terminal in low intensity mode
# since high intensity mode is so obnoxious.
mime2a-s|microterm mime2a (emulating an enhanced soroc iq120):\
	:am:bs:\
	:co#80:li#24:\
	:al=\001:bl=^G:cd=\EJ:ce=\EK:cl=\EL:cm=\E=%+ %+ :\
	:cr=^M:dc=\ED:dl=\027:do=^J:ei=^Z:ho=^^:im=\EE:ip=:\
	:is=\E):kd=^J:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:se=\E;:\
	:sf=^J:so=\E\072:sr=\EI:ue=\E7:up=\EI:us=\E6:
# This is the preferred mode (but ^X can't be used as a kill character)
# (mime2a: replaced ":pt:" with SCO's "it#8" -- esr)
mime2a|mime2a-v|microterm mime2a (emulating an enhanced vt52):\
	:bs:pt:\
	:co#80:it#8:li#24:\
	:al=\001:bl=^G:cd=\EQ:ce=\EP:cl=\EL:cm=\EY%+ %+ :\
	:cr=^M:dc=^N:dl=\027:do=^J:ei=^Z:ho=\EH:im=^O:ip=:\
	:is=^Y:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:\
	:se=\E9:sf=^J:so=\E8:sr=\EA:ta=^I:ue=\E5:up=\EA:\
	:us=\E4:
# (mime3a: removed obsolete ":ma=^X ^K^J^Z^P:" -- esr)
mime3a|mime1 emulating 3a:\
	:am@:\
	:kd=^K:kl=^H:kr=^X:ku=^Z:tc=adm3a:
# (mime3ax: mapped ":pt:" to default tabs -- esr)
mime3ax|mime-3ax|mime1 emulating enhanced 3a:\
	:pt:\
	:it#8:\
	:al=\001:cd=^_:ce=^X:dl=\027:ta=\011:tc=mime3a:
# Wed Mar  9 18:53:21 1983
# We run our terminals at 2400 baud, so there might be some timing problems at
# higher speeds. The major improvements in this model are the terminal now 
# scrolls down and insert mode works without redrawing the rest of the line
# to the right of the cursor. This is done with a bit of a kludge using the
# exit graphics mode to get out of insert, but it does not appear to hurt
# anything when using vi at least. If you have some users using act4s with
# programs that use curses and graphics mode this could be a problem.
mime314|mm314|mime 314:\
	:am:\
	:co#80:li#24:\
	:al=^A:cd=^_:ce=^^:cl=^L:cm=\024%.%.:dc=^D:dl=^W:\
	:ei=^V:ho=^]:im=^S:kd=^K:kl=^H:kr=^X:ku=^Z:le=^H:\
	:nd=^X:ta=^I:up=^Z:
# Fri Aug  5 08:11:57 1983
# This entry works for the ergo 4000 with the following setups:
# ansi,wraparound,newline disabled, xon/xoff disabled in both
# setup a & c.
#	
# WARNING!!! There are multiple versions of ERGO 4000 microcode
# Be advised that very early versions DO NOT WORK RIGHT !!  
# Microterm does have a ROM exchange program- use it or lose big
ergo4000|microterm ergo 4000:\
	:da:db:ms:\
	:co#80:li#66:\
	:AL=\E[1L:bl=^G:cd=\E[0J:ce=\E[0K:cl=\E[H\E[2J:\
	:cm=\E[%i%d;%dH:cr=^M:dc=\E[1P:dl=\E[1M:do=\E[B:\
	:ei=\E[4l:im=\E[4h:\
	:is=\E<\E=\E[?1l\E[?4l\E[?5l\E[?7h\E[?8h:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:kd=\E[B:ke=\E=:kl=\E[D:\
	:kr=\E[C:ks=\E=:ku=\E[A:l1=pf1:l2=pf2:l3=pf3:l4=pf4:\
	:le=^H:nd=\E[C:se=\E[0m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:\
	:up=\E[A:

#### NCR 
#
# NCR's terminal group was merged with AT&T's when AT&T bought the company.
# For what happened to that group, see the ADDS section.
#

# From <root@goliath.un.atlantaga.NCR.COM>, init string hacked by SCO.
ncr7900i|7900i|ncr7900|7900|ncr 7900 model 1:\
	:am:bw:ul:\
	:co#80:li#24:sg#1:ug#1:\
	:bl=^G:cd=\Ek:ce=\EK:cl=^L:cm=\E1%r%.%.:cr=^M:do=^J:\
	:is=\E0@\010\E3\E4\E7:kd=^J:kh=^A:kl=^U:kr=^F:ku=^Z:\
	:le=^H:ll=^A:mb=\E0B:me=\E0@:mh=\E0A:mr=\E0P:nd=^F:\
	:pf=^T:po=^R:\
	:..sa=\E0%p5%'@'%+%p4%{2}%*%+%p3%{16}%*%+%p2%{32}%*%+%p1%{17}%*%+%c:\
	:se=\E0@:sf=^J:so=\E0Q:ue=\E0@:up=^Z:us=\E0`:
ncr7900i-na|ncr7900-na|7900-na|ncr 7900 model 1 with no arrows:\
	:kd@:kl@:kr@:ku@:tc=ncr7900i:
ncr7900iv|ncr 7900 model 4:\
	:am:bw:es:hs:\
	:co#80:li#24:\
	:al=\E^N:bl=^G:cl=^L:cm=\013%+@\E\005%02:cr=^M:\
	:dl=\E^O:do=^J:ds=\Ey1:fs=\Ek\Ey5:ho=\013@\E^E00:\
	:k1=\ES:k2=\ET:k3=\EU:k4=\EV:k5=\EW:k6=\EP:k7=\EQ:\
	:k8=\ER:kb=^H:kd=\EB:kh=\EH:kl=\ED:kr=\EC:ku=\EA:\
	:l6=blue:l7=red:l8=white:le=^H:nw=^M^J:sf=^J:\
	:ts=\Ej\Ex5\Ex1\EY8%p1%{32}%+%c\Eo:
ncr7901|7901|ncr 7901 model:\
	:am:bw:ul:\
	:co#80:li#24:\
	:bl=^G:cd=\Ek:ce=\EK:ch=\020%+^J:cl=^L:cm=\EY%+ %+ :\
	:cr=^M:cv=\013%+@:do=^J:is=\E4^O:kC=^L:kd=^J:kh=^H:\
	:kl=^U:kr=^F:ku=^Z:le=^H:ll=^A:mb=\E0B:me=^O:mh=\E0A:\
	:mr=\E0P:nd=^F:pf=^T:po=^R:\
	:..sa=\E0%p5%'@'%+%p4%{2}%*%+%p3%{16}%*%+%p2%{32}%*%+%p1%{17}%*%+%c\016:\
	:se=^O:sf=^J:so=\E0Q\016:ue=^O:up=^Z:us=\E0`\016:\
	:ve=^X:vi=^W:

#### Perkin-Elmer (Owl)
#
# These are official terminfo entries from within Perkin-Elmer.
#

bantam|pe550|pe6100|perkin elmer 550:\
	:co#80:li#24:\
	:bl=^G:ce=\EI:cl=\EK:cm=\EX%+ \EY%+ :cr=^M:do=^J:\
	:ho=\EH:le=^H:ll=\EH\EA:nd=\EC:sf=^J:up=\EA:
fox|pe1100|perkin elmer 1100:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cd=\EJ:ce=\EI:cl=\EH\EJ:cm=\EX%+ \EY%+ :cr=^M:\
	:ct=\E3:do=^J:ho=\EH:le=^H:ll=\EH\EA:nd=\EC:sf=^J:\
	:st=\E1:up=\EA:vb=\020\002\020\003:
owl|pe1200|perkin elmer 1200:\
	:am:in:\
	:co#80:li#24:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EI:cl=\EH\EJ:\
	:cm=\EX%+ \EY%+ :cr=^M:ct=\E3:dc=\EO:dl=\EM:do=^J:\
	:ei=:ho=\EH:ic=\EN:im=:ip=:k0=\ERJ:k1=\ERA:k2=\ERB:\
	:k3=\ERC:k4=\ERD:k5=\ERE:k6=\ERF:k7=\ERG:k8=\ERH:\
	:k9=\ERI:kb=^H:le=^H:ll=\EH\EA:nd=\EC:se=\E!\200:\
	:sf=^J:so=\E!^H:st=\E1:up=\EA:vb=\020\002\020\003:
pe1251|pe6300|pe6312|perkin elmer 1251:\
	:am:\
	:co#80:it#8:li#24:pb#300:sg#1:vt#8:\
	:bl=^G:cd=\EJ:ce=\EI:cl=\EK:cm=\EX%+ \EY%+ :cr=^M:\
	:ct=\E3:do=\EB:ho=\EH:k0=\ERA:k1=\ERB:k2=\ERC:\
	:k3=\ERD:k4=\ERE:k5=\ERF:k6=\ERG:k7=\ERH:k8=\ERI:\
	:k9=\ERJ:k;=\ERK:le=\ED:nd=\EC:sf=^J:st=\E1:up=\EA:
pe7000m|perkin elmer 7000 series monochrome monitor:\
	:am:\
	:co#80:li#24:\
	:bl=^G:bt=\E!Y:cd=\EJ:ce=\EI:cl=\EK:cm=\ES%+ %+ :\
	:cr=^M:do=\EB:ho=\EH:i1=\E!\200\EW  7o\Egf\ES7 :\
	:k0=\E!\200:k1=\E!^A:k2=\E!^B:k3=\E!^C:k4=\E!^D:\
	:k5=\E!^E:k6=\E!^F:k7=\E!^G:k8=\E!^H:k9=\E!^I:\
	:k;=\E!^J:kb=^H:kd=\E!U:kh=\E!S:kl=\E!V:kr=\E!W:\
	:ku=\E!T:le=\ED:ll=\ES7 :nd=\EC:se=\E!\200:sf=^J:\
	:so=\E!^H:sr=\ER:ue=\E!\200:up=\EA:us=\E! :
pe7000c|perkin elmer 7000 series colour monitor:\
	:am:\
	:co#80:li#24:\
	:bl=^G:bt=\E!Y:cd=\EJ:ce=\EI:cl=\EK:cm=\ES%+ %+ :\
	:cr=^M:do=\EB:ho=\EH:\
	:i1=\E!\200\EW  7o\Egf\Eb0\Ec7\ES7 :k0=\E!\200:\
	:k1=\E!^A:k2=\E!^B:k3=\E!^C:k4=\E!^D:k5=\E!^E:\
	:k6=\E!^F:k7=\E!^G:k8=\E!^H:k9=\E!^I:k;=\E!^J:kb=^H:\
	:kd=\E!U:kh=\E!S:kl=\E!V:kr=\E!W:ku=\E!T:le=\ED:\
	:ll=\ES7 :nd=\EC:se=\Eb0:sf=^J:so=\Eb2:sr=\ER:\
	:ue=\E!\200:up=\EA:us=\E! :

#### Sperry Univac
#
# Sperry Univac has merged with Burroughs to form Unisys.
#

# This entry is for the Sperry UTS30 terminal running the TTY 
# utility under control of CP/M Plus 1R1. The functionality 
# provided is comparable to the DEC vt100.
uts30|sperry uts30 with cp/m@1R1:\
	:am:bw:hs:\
	:co#80:li#24:ws#40:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:\
	:LE=\E[%dD:RI=\E[%dC:SF=\E[%dB:SR=\E[%dA:UP=\E[%dA:\
	:ae=\Ed:al=\EN:as=\EF:bl=^G:cd=\E[J:ce=\E[K:cl=^L:\
	:cm=\E[%i%d;%dH:cr=^M:cs=\EU%+ %+ :dc=\EM:dl=\EL:\
	:do=\EB:ei=:fs=^M:ho=\E[H:ic=\EO:im=:\
	:is=\E[U 7\E[24;1H:kb=^H:kd=\EOB:kh=\E[H:kl=\EOD:\
	:kr=\EOC:ku=\EOA:le=^H:mb=\E[5m:md=\E[1m:me=\E[m:\
	:mr=\E[7m:nd=\EC:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\EX:\
	:rf=/usr/lib/tabset/vt100:sc=\EW:se=\E[m:sf=^J:\
	:so=\E[7m:sr=\EI:ta=^I:ts=\E]:uc=\EPB:ue=\E[m:\
	:up=\E[A:us=\E[4m:ve=\ES:vi=\ER:

#### Tandem
#
# Tandem builds these things for use with its line of fault-tolerant
# transaction-processing computers.  They aren't generally available
# on the merchant market, and so are fairly uncommon.
#

tandem6510|adm3a repackaged by Tandem:\
	:tc=adm3a:

# A funny series of terminal that TANDEM uses.  The actual model numbers
# have a fourth digit after 653 that designates minor variants.  These are
# natively block-mode and rather ugly, but they have a character mode which
# this doubtless(?) exploits.  There is a 6520 that is slightly dumber.
# (tandem653: had ":sb=\ES:", probably someone's mistake for sf -- esr)
tandem653|t653x|Tandem 653x multipage terminal:\
	:am:bs:da:db:hs:\
	:co#80:li#24:sg#1:ug#1:ws#64:\
	:cd=\EJ:ce=\EK:cl=\EI:cm=\023%+ %+ :do=^J:ds=\Eo\r:\
	:fs=^M:ho=\EH:if=/usr/share/tabset/tandem653:le=^H:\
	:nd=\EC:se=\E6 :sf=\ES:so=\E6$:sr=\ET:ts=\Eo:ue=\E6 :\
	:up=\EA:us=\E60:

#### Tandy/Radio Shack
#
# Tandy has a line of VDTs distinct from its microcomputers.
#

dmterm|deskmate terminal:\
	:am:bw:\
	:co#80:li#24:\
	:al=\EP:bl=^G:cd=\EJ:ce=\EK:cl=\Ej:cm=\EY%+ %+ :\
	:cr=^M:dc=\ES:dl=\ER:do=\EB:ei=:ho=\EH:ic=\EQ:im=:\
	:k0=\E1:k1=\E2:k2=\E3:k3=\E4:k4=\E5:k5=\E6:k6=\E7:\
	:k7=\E8:k8=\E9:k9=\E0:kd=\EB:kh=\EH:kl=\ED:kr=\EC:\
	:ku=\EA:l0=f1:l1=f2:l2=f3:l3=f4:l4=f5:l5=f6:l6=f7:\
	:l7=f8:l8=f9:l9=f10:le=^H:ll=\EE:nd=\EC:se=\EG0:\
	:sf=\EX:so=\EG4:ta=^I:up=\EA:ve=\EG6:vi=\EG5:
dt100|dt-100|Tandy DT-100 terminal:\
	:xo:\
	:co#80:li#24:sg#1:ug#1:\
	:ac=kkllmmjjnnwwvvttuuqqxx:ae=^O:al=\E[L:as=^N:bl=^G:\
	:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:cm=\010\E[%i%d;%dH:\
	:cr=^M:cs=\E[%2;%2r:dc=\E[P:dl=\E[M:do=\E[B:ei=:\
	:ho=\E[H:ic=\E[@:im=:is=\E[?3l\E)0\E(B:k1=\E[?3i:\
	:k2=\E[2i:k3=\E[@:k4=\E[M:k5=\E[17~:k6=\E[18~:\
	:k7=\E[19~:k8=\E[20~:k9=\E[21~:k;=\E[?5i:kN=\E[29~:\
	:kP=\E[28~:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:\
	:l1=f1:l2=f2:l3=f3:l4=f4:l5=f5:l6=f6:l7=f7:l8=f8:\
	:le=^H:nd=\E[C:se=\E[m:sf=^J:so=\E[7m:sr=\EM:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:ve=\E[?25h:vi=\E[?25l:
dt100w|dt-100w|Tandy DT-100 terminal:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:is=\E[?3l\E)0\E(B:sf=^J:tc=dt100:
dt110|Tandy DT-110 emulating ansi:\
	:xo:\
	:co#80:li#24:\
	:@7=\E[K:ac=kkllmmjjnnwwvvuuttqqxx:ae=^O:al=\E[0L:\
	:as=^N:bl=^G:cd=\E[0J:ce=\E[0K:cl=\E[;H\E[2J:\
	:cm=\010\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:dc=\E[0P:\
	:dl=\E[0M:do=\E[0B:eA=\E(B\E)0:ei=:ho=\E[H:ic=\E[0@:\
	:im=:is=\E[?3l\E)0\E(B:k1=\E[1~:k2=\E[2~:k3=\E[3~:\
	:k4=\E[4~:k5=\E[5~:k6=\E[6~:k7=\E[7~:k8=\E[8~:\
	:k9=\E[9~:k;=\E[10~:kI=\E[@:kN=\E[26~:kP=\E[25~:\
	:kd=\E[B:kh=\E[G:kl=\E[D:kr=\E[C:ku=\E[A:l0=f1:l1=f2:\
	:l2=f3:l3=f4:l4=f5:l5=f6:l6=f7:l7=f8:l8=f9:l9=f10:\
	:le=^H:nd=\E[C:se=\E[0m:sf=^J:so=\E[7m:sr=\EM:ta=^I:\
	:ue=\E[0m:up=\E[0A:us=\E[4m:ve=\E[?25h:vi=\E[?25l:
dt200|td200|Tandy 200:\
	:am:xt:\
	:co#40:li#16:\
	:al=\EL:bl=^G:cd=^L:ce=\EK:cl=\EE:cm=\EY%+ %+ :cr=^M:\
	:dl=\EM:do=^_:kd=^_:kl=^]:kr=^\:ku=^^:le=^H:nd=^\:\
	:se=\Eq:sf=^J:so=\Ep:up=\EA:
pt210|TRS-80 PT-210 printing terminal:\
	:hc:os:\
	:co#80:\
	:bl=^G:cr=^M:do=^J:sf=^J:

#### Tektronix (tek)
#
# Tektronix tubes are graphics terminals.  Most of them use modified 
# oscilloscope technology incorporating a long-persistence green phosphor,
# and support vector graphics on a main screen with an attached "dialogue
# area" for interactive text.
#

tek|tek4012|4012|tektronix 4012:\
	:os:\
	:co#75:li#35:\
	:bl=^G:cl=\E\014:cr=^M:do=^J:ff=\014:is=\E^O:le=^H:
tek4013|4013|tektronix 4013:\
	:ae=\E^O:as=\E^N:tc=tek4012:
tek4014|4014|tektronix 4014:\
	:co#81:li#38:\
	:is=\E\017\E9:tc=tek4012:
tek4015|4015|tektronix 4015:\
	:ae=\E^O:as=\E^N:tc=tek4014:
tek4014-sm|4014-sm|tektronix 4014 in small font:\
	:co#121:li#58:\
	:is=\E\017\E\072:tc=tek4014:
tek4015-sm|4015-sm|tektronix 4015 in small font:\
	:ae=\E^O:as=\E^N:tc=tek4014-sm:
tek4023|4023|tex|tektronix 4023:\
	:am:\
	:co#80:li#24:vt#4:\
	:bl=^G:cl=\E\014:cm=\034%r%+ %+ :cr=^M:do=^J:le=^H:\
	:nd=^I:se=^_@:sf=^J:so=^_P:
# It is recommended that you run the 4025 at 4800 baud or less;
# various bugs in the terminal appear at 9600.  It wedges at the
# bottom of memory (try "cat /usr/dict/words"); ^S and ^Q typed
# on keyboard don't work.  You have to hit BREAK twice to get
# one break at any speed - this is a documented feature.
# Can't use cursor motion because it's memory relative, and 
# because it only works in the workspace, not the monitor.  
# Same for home. Likewise, standout only works in the workspace.
# 
# el was commented out since vi and rogue seem to work better 
# simulating it with lots of spaces!
# 
# il1 and il had 145ms of padding, but that slowed down vi's ^U 
# and didn't seem necessary.
#
tek4024|tek4025|tek4027|tektronix 4024/4025/4027:\
	:am:da:db:\
	:co#80:it#8:li#34:lm#0:\
	:AL=\037up\r\037ili %d\r:CC=^_:DL=\037dli %d\r\006:\
	:DO=\037dow %d\r:LE=\037lef %d\r:RI=\037rig %d\r:\
	:UP=\037up %d\r:al=\037up\r\037ili\r:bl=^G:\
	:cd=\037dli 50\r:cl=\037era\r\n\n:cr=^M:dc=\037dch\r:\
	:dl=\037dli\r\006:do=^F^J:ei=:ic=\037ich\r \010:im=:\
	:is=!com 31\r\n\037sto 9 17 25 33 41 49 57 65 73\r:\
	:ke=\037lea p2\r\037lea p4\r\037lea p6\r\037lea p8\r\037lea f5\r:\
	:ks=\037lea p4 /h/\r\037lea p8 /k/\r\037lea p6 / /\r\037lea p2 /j/\r\037lea f5 /H/\r:\
	:le=^H:nd=\037rig\r:sf=^F^J:ta=^I:up=^K:
tek4025-17|4025-17|4027-17|tek 4025 17 line window:\
	:li#17:\
	:tc=tek4025:
tek4025-17-ws|4025-17-ws|4025-17ws|4027-17ws|4027-17-ws|tek 4025 17 line window in workspace:\
	:is=!com 31\r\n\037sto 9 17 25 33 41 49 57 65 73\r\037wor 17\r\037mon 17\r:\
	:se=\037att s\r:so=\037att e\r:te=\037mon h\r:\
	:ti=\037wor h\r:tc=tek4025-17:
tek4025-ex|tek4027-ex|tek 4025/4027 w/!:\
	:is=\037com 33\r\n!sto 9 17 25 33 41 49 57 65 73\r:\
	:te=\037com 33\r:ti=!com 31\r:tc=tek4025:
# Tektronix 4025a
# From: Doug Gwyn <gwyn@brl-smoke.ARPA>
# The following status modes are assumed for normal operation (replace the
# initial "!" by whatever the current command character is):
#	!COM 29			# NOTE: changes command character to GS (^])
#	^]DUP
#	^]ECH R
#	^]EOL
#	^]RSS T
#	^]SNO N
#	^]STO 9 17 25 33 41 49 57 65 73
# Other modes may be set according to communication requirements.
# If the command character is inadvertently changed, termcap can't restore it.
# Insert-character cannot be made to work on both top and bottom rows.
# Clear-to-end-of-display emulation via !DLI 988 is too groady to use, alas.
# There also seems to be a problem with vertical motion, perhaps involving
# delete/insert-line, following a typed carriage return.  This terminal sucks.
# Delays not specified; use "stty ixon -ixany" to enable DC3/DC1 flow control!
# (tek4025a: mapped ":pt:" to default tabs; removed obsolete ":xx:".
# This may mean the tek4025a entry won't work any more. -- esr)
tek4025a|4025a|Tektronix 4025A:\
	:am:bs:bw:da:db:pt:xo:\
	:co#80:li#34:\
	:CC=^]:DC=\035dch %d;:DL=\035dli %d;:DO=\035dow %d;:\
	:LE=\035lef %d;:RI=\035rig %d;:SF=\035dow %d;:\
	:UP=\035up %d;:al=\013\035ili;:bl=^G:bt=\035bac;:\
	:ce=\035dch 80;:ch=\r\035rig %d;:\
	:cl=\035era;\n\035rup;:cr=^M:ct=\035sto;:dc=\035dch;:\
	:dl=\035dli;:do=^J:le=^H:nd=\035rig;:\
	:rs=!com 29\035del 0\035rss t\035buf\035buf n\035cle\035dis\035dup\035ech r\035eol\035era g\035for n\035pad 203\035pad 209\035sno n\035sto 9 17 25 33 41 49 57 65 73\035wor 0;:\
	:sf=^J:ta=^I:up=^K:
# From: cbosg!teklabs!davem Wed Sep 16 21:11:41 1981
# Here's the command file that I use to get rogue to work on the 4025.
# It should work with any program using the old curses (e.g. it better
# not try to scroll, or cursor addressing won't work.  Also, you can't
# see the cursor.)
# (This "learns" the arrow keys for rogue. I have adapted it for termcap - mrh)
# (tek4025-cr: mapped ":pt:" to default tabs -- esr)
tek4025-cr|4025-cr|tek 4025 for curses and rogue:\
	:am:bs:pt:\
	:co#80:li#33:\
	:cl=\037era;:cm=\037jum%i%d\054%d;:do=^F^J:\
	:is=!com 31\r\n\037sto 9 17 25 33 41 49 57 65 73\r:\
	:le=^H:nd=\037rig;:nl=^F^J:te=\037wor 0:\
	:ti=\037wor 33h:up=^K:
# next two lines commented out since curses only allows 128 chars, sigh.
#	:ti=\037lea p1/b/\037lea p2/j/\037lea p3/n/\037lea p4/h/\037lea p5/ /\037lea p6/l/\037lea p7/y/\037lea p8/k/\037lea p9/u/\037lea p./f/\037lea pt/`era w/13\037lea p0/s/\037wor 33h:\
#	:te=\037lea p1\037lea p2\037lea p3\037lea p4\037lea pt\037lea p5\037lea p6\037lea p7\037lea p8\037lea p9/la/13\037lea p.\037lea p0\037wor 0:
tek4025ex|4025ex|4027ex|tek 4025 w/!:\
	:is=\037com 33\r\n!sto 9\05417\05425\05433\05441\05449\05457\05465\05473\r:\
	:te=\037com 33\r:ti=!com 31\r:tc=tek4025:
tek4105|4105|tektronix 4105:\
	:am:mi:ms:ul:xn:xt:\
	:co#79:it#8:li#29:\
	:ae=\E[0m:al=\E[1L:as=\E[1m:bl=^G:bt=\E[Z:cd=\E[J:\
	:ce=\E[K:cl=\E[2J\E[H:cm=\E[%i%2;%2H:cr=^M:ct=\E[1g:\
	:dc=\E[1P:dl=\E[1M:do=\E[1B:ei=\E[4l:ho=\E[H:\
	:i1=\E%!1\E[0m:im=\E[4h:is=\E%!1\E[?6141\E[0m:kb=^H:\
	:kd=\E[1B:kl=\E[1D:kr=\E[1C:ku=\E[1A:mb=\E[=3;<7m:\
	:md=\E[=7;<4m:me=\E[=0;<1m:mh=\E[=1;<6m:mk=\E[=6;<5:\
	:mr=\E[=1;<3m:nd=\E[1C:se=\E[=0;<1m:sf=\E[S:\
	:so=\E[=2;<3m:sr=\E[T:ta=^I:ti=\E%!1\E[?6l\E[2J:\
	:ue=\E[=0;<1m:up=\E[1A:us=\E[=5;<2m:

tek4105-30|4105-30|4015 emulating 30 line vt100:\
	:am:mi:ms:xn:xo:\
	:co#80:it#8:li#30:vt#3:\
	:@8=\EOM:DO=\E[%dB:K1=\EOq:K2=\EOr:K3=\EOs:K4=\EOp:\
	:K5=\EOn:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:as=^N:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:do=^J:eA=\E(B\E)0:ho=\E[H:k0=\EOy:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\EOt:k6=\EOu:k7=\EOv:\
	:k8=\EOl:k9=\EOw:k;=\EOx:kb=^H:kd=\EOB:ke=\E[?1l\E>:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m\017:mr=\E[7m:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:..sa=\E[0%?%p1%p6%|%t;1%;%?%p2%t;4%;%?%p1%p3%|%t;7%;%?%p4%t;5%;m%?%p9%t\016%e\017%;:\
	:sc=\E7:se=\E[m:sf=^J:so=\E[1;7m:sr=\EM:st=\EH:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:

tek4107|tek4109|4107|4109|tektronix terminals 4107 4109:\
	:am:mi:ms:ul:xn:xt:\
	:co#79:it#8:li#29:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\ELZ:cm=\EY%+ %+ :cr=^M:\
	:do=^J:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=^H:\
	:mb=\E%!1\E[5m\E%!0:md=\E%!1\E[1m\E%!0:\
	:me=\E%!1\E[m\E%!0:mh=\E%!1\E[<0m\E%!0:\
	:mr=\E%!1\E[7m\E%0:nd=\EC:\
	:..sa=\E%%!1\E[%?%p1%t;7%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p6%t;1%;m\E%%!0:\
	:se=\E%!1\E[m\E%!0:sf=^J:so=\E%!1\E[7;5m\E%!0:sr=\EI:\
	:ta=^I:ue=\E%!1\E[m\E%!0:up=\EA:us=\E%!1\E[4m\E%!0:\
	:ve=\E%!0:vs=\E%!3:
# Tektronix 4207 with sysline.  In the ancestral termcap file this was 4107-s;
# see the note attached to tek4207.
tek4207-s|Tektronix 4207 with sysline but no memory:\
	:es:hs:\
	:ds=\E7\E[?6l\E[2K\E[?6h\E8:fs=\E[?6h\E8:\
	:i2=\E7\E[?6l\E[2K\E[?6h\E8:\
	:is=\E%!1\E[2;32r\E[132D\E[2g\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[J:\
	:ts=\E7\E[?6l\E[2K\E[;%i%df:tc=tek4107:

# The 4110 series may be a wonderful graphics series, but they make the 4025
# look good for screen editing.  In the dialog area, you can't move the cursor
# off the bottom line.  Out of the dialog area, ^K moves it up, but there
# is no way to scroll.
# 
# Note that there is a floppy for free from Tek that makes the 
# 4112 emulate the vt52 (use the vt52 termcap). There is also
# an expected enhancement that will use ANSI standard sequences.
# 
# 4112 in non-dialog area pretending to scroll. It really wraps 
# but vi is said to work (more or less) in this mode.
# 
# 'vi' works reasonably well with this entry.
#
otek4112|o4112-nd|otek4113|otek4114|tektronix 4110 series:\
	:am:\
	:co#80:li#34:\
	:bl=^G:cl=\E^L:cr=^M:do=^J:le=^H:sf=^J:te=\EKA1\ELV1:\
	:ti=\EKA0\ELV0\EMG0:up=^K:
# The 4112 with the ANSI compatibility enhancement
tek4112|tek4114|tektronix 4110 series:\
	:am:bs:db:\
	:co#80:li#34:\
	:al=\E[L:bt=\E[Z:cd=\E[0J:ce=\E[0K:cl=\E[2J\E[0;0H:\
	:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:ei=:ic=\E[@:im=:\
	:is=\E3!1:nd=\E[C:se=\E[m:sf=\E7\E[0;0H\E[M\E8:\
	:so=\E[7m:sr=\E7\E[0;0H\E[L\E8:ue=\E[m:up=\EM:\
	:us=\E[4m:ve=:vs=:
tek4112-nd|4112-nd|4112 not in dialog area:\
	:ns:\
	:up=^K:tc=tek4112:
tek4112-5|4112-5|4112 in 5 line dialog area:\
	:li#5:\
	:tc=tek4112:
# (tek4113: this used to have ":nd=\LM1 \LM0:", someone's mistake;
# removed ":as=\E^N:ae=\E^O:", which had been commented out in 8.3.
# Note, the !0 and !1 sequences in :te:/:ti:/:ve:/:vs: were previously \0410
# and \0411 sequences...I don't *think* they were supposed to be 4-digit
# octal -- esr)
tek4113|tektronix 4113 color graphics, 5 line dialog area:\
	:am:bs:da:eo:\
	:co#80:li#5:\
	:cl=\ELZ:do=^J:is=\EKA1\ELL5\ELV0\ELV1:le=^H:\
	:nd=\ELM1 \ELM0:uc=\010\ELM1_\ELM0:\
	:vb=\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERB0:
tek4113-34|4113-34|tektronix 4113 color graphics, 34 line dialog area:\
	:li#34:\
	:is=\EKA1\ELLB2\ELV0\ELV1:tc=tek4113:
# :ns: left off to allow vi visual mode. APL font (:as=\E^N:/:ae=\E^O:) not 
# supported here. :uc: is slow, but looks nice. Suggest setenv MORE -up .
# :vb: needs enough delay to let you see the background color being toggled.
# (tek4113-nd: mapped ":pt:" to default tabs -- esr)
tek4113-nd|4113-nd|tektronix 4113 color graphics, no dialog area:\
	:am:bs:eo:pt:\
	:co#80:li#34:\
	:cl=\E^L:do=^J:ho=\ELF7l\177 @:\
	:is=\ELZ\EKA0\ELF7l\177 @:le=^H:ll=\ELF hl @:nd=^I:\
	:se=\EMT1:so=\EMT2:uc=\010\EMG1_\EMG0:up=^K:\
	:vb=\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERBA4\ERB0:\
	:vs=\ELZ\EKA0:
# This entry is from Tek. Inc.  (Brian Biehl)
# (tek4115: mapped ":pt:" to default tabs; :bc: renamed to :le: -- esr)
otek4115|Tektronix 4115:\
	:am:bs:da:db:eo:pt:\
	:co#80:li#34:\
	:al=\E[L:bt=\E[Z:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:\
	:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:do=\E[B:ei=\E[4l:\
	:ho=\E[;H:if=/usr/share/tabset/vt100:im=\E[4h:\
	:is=\E%!0\E%\014\ELV0\EKA1\ELBB2\ENU@=\ELLB2\ELM0\ELV1\EKYA?\E%!1\E[<1l\E[?7h\E[?8h\E[34;1H\E[34B\E[0m:\
	:kb=^H:ke=\E>:ks=\E=:le=\E[D:nd=\E[C:se=\E[m:\
	:so=\E[7m:sr=\EM:te=\E%!0\ELBG8\E%!1\E[34;1H\E[J:\
	:ti=\E%!0\ELBB2\E%!1:ue=\E[m:up=\E[A:us=\E[4m:\
	:ve=\E%!0\ELBG8\E%!1\E[34;1H:vs=\E%!0\ELBB2\E%!1:
tek4115|newer tektronix 4115 entry with more ANSI capabilities:\
	:am:xo:\
	:co#80:li#34:\
	:AL=\E[%dL:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:LE=\E[%dD:\
	:RI=\E[%dC:UP=\E[%dA:al=\E[L:bl=^G:bt=\E[Z:cd=\E[J:\
	:ce=\E[K:ch=\E[%+^AG:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:cr=^M:ct=\E[2g:cv=\E[%+^Ad:dc=\E[P:dl=\E[M:do=^J:\
	:ei=:ho=\E[H:ic=\E[@:im=:kb=^H:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[0m:mk=\E[8m:mr=\E[7m:nd=\E[C:\
	:..rp=%p1%c\E[%p2%{1}%-%db:\
	:..sa=\E[%?%p1%t7;%;%?%p2%t4;%;%?%p3%t7;%;%?%p4%t5;%;%?%p6%t1;%;m:\
	:se=\E[m:sf=^J:so=\E[7m:st=\EH:ta=^I:ue=\E[m:up=\E[A:\
	:us=\E[4m:
# The tek4125 emulates a vt100 incorrectly - the scrolling region
# command is ignored.  The following entry replaces the :cs: with the needed
# :al:, :dl:, and :im:; removes some cursor pad commands that the tek4125
# chokes on; and adds a lot of initialization for the tek dialog area.
# Note that this entry uses all 34 lines and sets the cursor color to green.
# Steve Jacobson 8/85
# (tek4125: there were two "\!"s in the is that I replaced with "\E!" -- esr)
tek4125|4125:\
	:li#34:\
	:al=\E[1L:cs@:dl=\E[1M:im=\E1:\
	:is=\E%\E!0\EQD1\EUX03\EKA\ELBB2\ELCE0\ELI100\ELJ2\ELLB2\ELM0\ELS1\ELX00\ELV1\E%\E!1\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:\
	:ks=\E=:rc@:sc@:tc=vt100:

# From: <jcoker@ucbic>
# (tek4107: mapped ":pt:" to default tabs.  This was the termcap file's
# entry for the 4107/4207, but SCO supplied another, less capable 4107 entry. 
# So we'll use that for 4107 and note that if jcoker wasn't confused you
# may be able to use this one. -- esr)
tek4207|Tektronix 4207 graphics terminal with memory:\
	:am:bs:bw:mi:pt:ul:xn:\
	:co#80:li#32:\
	:al=3\E[L:bt=\E[Z:cd=\E[J:ce=5\E[K:cl=156\E[H\E[J:\
	:cm=\E[%i%d;%dH:dc=4\E[P:dl=3\E[M:do=^J:ei=:ho=\E[H:\
	:ic=4\E[@:im=:\
	:is=\E%!0\ELBP0\E%!1\E[H\E[2g\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[8C\EH\E[J:\
	:kd=\ED:kh=\E[H:kl=\E[D:kr=\E[C:ku=\EM:le=^H:\
	:mb=\E[5m:md=\E[1m:me=\E[m:mr=\E[7m:nd=\E[C:se=\E[m:\
	:so=\E[7m:te=\E[?6h\E%!0\ELBP0\E%!1\E[32;1f:\
	:ti=\E[?6l\E[H\E[J:ue=\E[m:up=\EM:us=\E[4m:

# From: <carolyn@dali.berkeley.edu>  Thu Oct 31 12:54:27 1985
# (tek4404: There was a "\!" in :ti: that I replaced with "\E!";
# also mapped ":pt:" to default tabs -- esr)
tek4404|4404:\
	:bs:pt:\
	:co#80:li#32:\
	:al=\E[1L:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:\
	:cm=\E[%i%d;%dH:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[1M:\
	:do=^J:ei=\E[4l:ho=\E[H:im=\E[4h:kd=\E[B:ke=\E[?1h:\
	:kl=\E[D:kr=\E[C:ks=\E[?1l:ku=\E[A:mb=\E[5m:md=\E[1m:\
	:me=\E[m:nd=\E[C:rc=\E8:sc=\E7:se=\E[27m:so=\E[7m:\
	:ta=\E[2I:te=\E[1;1H\E[0J\E[?6h\E[?1l:\
	:ti=\E%\E!1\E[1;32r\E[?6l\E>:ue=\E[m:up=\E[A:\
	:us=\E[4m:
# t500 is a local entry for the oddball Tek 500 owned by Fluke 
# Labs
#
t500|Tek series 500:\
	:am:bw:\
	:co#80:li#25:\
	:bl=^G:cl=\005:cm=\E=%+ %+ :cr=^M:do=^J:ho=^T:le=^H:\
	:sf=^J:
# I added the is string - straight Unix has ESC ; in the login 
# string which sets a ct8500 into monitor mode (aka 4025 snoopy 
# mode). The is string here cleans up a few things (but not 
# everything).
#
ct8500|tektronix ct8500:\
	:am:bw:da:db:\
	:co#80:li#25:\
	:al=\E^L:bl=^G:bt=\E^I:cd=\E^U:ce=\E^T:cl=\E^E:\
	:cm=\E|%+ %+ :cr=^M:dc=\E^]:dl=\E^M:do=^J:ei=:\
	:ic=\E^\:im=:is=\037\EZ\Ek:le=^H:me=\E :nd=\ES:\
	:se=\E :sf=^J:so=\E$:sr=\E^A:ta=^I:ue=\E :up=\ER:\
	:us=\E!:

# Tektronix 4205 terminal.
#
# am is not defined because the wrap around occurs not when the char.
# is placed in the 80'th column, but when we are attempting to type
# the 81'st character on the line.
#
# Bold, dim, and standout are simulated by colors and thus not allowed
# with colors.  The tektronix color table is mapped into the RGB color
# table by setf/setb. All colors are reset to factory specifications by oc.
# The initc cap uses RGB notation to define colors.  for arguments 1-3 the 
# interval (0-1000) is broken into 8 smaller sub-intervals (125).  Each sub-
# interval then maps into pre-defined value.
# (untranslatable capabilities removed to fit entry within 1023 bytes)
# WARNING: this entry, 1264 bytes long, may core-dump older termcap libraries!
tek4205|4205|tektronix 4205:\
	:cc:mi:ms:\
	:Co#8:NC#49:co#80:it#8:li#30:pa#63:\
	:AL=\E[%dL:DO=\E[%dB:IC=\E[%d@::LE=\E[%dD:RI=\E[%dC::\
	::UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[1L:as=^N:bl=^G:bt=\E[Z:cb=\E[1K:cd=\E[J:\
	:ce=\E[K:cl=\E[2J\E[H:cm=\E[%i%d;%dH:cr=^M:ct=\E[1g:\
	:dc=\E[1P:dl=\E[1M:do=\E[B:eA=\E)0:ec=\E%dX:ei=\E[4l:\
	:ho=\E[H:i1=\E%!0\ETM1\E%!1\E[0m:im=\E[4h:k0=\EOA:\
	:k1=\EOB:k2=\EOC:k3=\EOD:k4=\EP:k5=\EQ:k6=\ER:k7=\ES:\
	:kb=^H:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:le=\E[D:\
	:mb=\E[5m:md=\E[=7;<4m:me=\E[=0;<1m\E[24;25;27m\017:\
	:mh=\E[=1;<6m:mk=\E[=6;<5:mr=\E[7m:nd=\E[C:\
	:oc=\E%!0\n\ETFB0\n0000\n1F4F4F4\n2F400\n30F40\n4A4C<F4\n50F4F4\n6F40F4\n7F4F40\n\E%!1:\
	:op=\E[39;40m:se=\E[=0;<1m:sf=\ED:so=\E[=2;<3m:\
	:sr=\EM:ta=^I:ti=\E%%!1\E[?6l\E[2J:ue=\E[24m:up=\E[A:\
	:us=\E[4m:

#### Teletype (tty)
#
# These are the hardcopy Teletypes from before AT&T bought the company,
# clattering electromechanical dinosaurs in Bakelite cases that printed on
# pulpy yellow roll paper.  If you remember these you go back a ways.
# Teletype-branded VDTs are listed in the AT&T section.
#
# The earliest UNIXes were designed to use these clunkers; nroff and a few
# other programs still default to emitting codes for the Model 37.
#

tty33|model 33 teletype:\
	:hc:os:xo:\
	:co#72:\
	:bl=^G:cr=^M:do=^J:sf=^J:
tty35|model 35 teletype:\
	:tc=tty33:
tty37|model 37 teletype:\
	:bs:hc:os:xo:\
	:bl=^G:cr=^M:do=^J:hd=\E9:hu=\E8:le=^H:sf=^J:up=\E7:

# There are known to be at least three flavors of the tty40, all seem more
# like IBM half duplex forms fillers than ASCII terminals.  They have lots of
# awful braindamage, such as printing a visible newline indicator after each
# newline.  The 40-1 is a half duplex terminal and is hopeless.  The 40-2 is
# braindamaged but has hope and is described here.  The 40-4 is a 3270
# lookalike and beyond hope.  The terminal has visible bell but I don't know
# it - it's null here to prevent it from showing the BL character.
# There is an \EG in :nl: because of a bug in old vi (if stty says you have
# a "newline" style terminal (-crmode) vi figures all it needs is nl
# to get crlf, even if :cr: is not ^M.)
# (tty40: removed obsolete ":nl=\EG\EB:", it's just do+cr -- esr)
tty40|ds40|ds40-2|dataspeed40|teletype dataspeed 40/2:\
	:xo:\
	:co#80:li#24:\
	:al=\EL:cd=\EJ:cl=\EH\EJ:cr=\EG:ct=\EH\E2:dc=\EP:\
	:dl=\EM:do=\EB:ei=:ho=\EH:ic=\E^:im=:kb=^]:kl=^H:\
	:le=^H:nd=\EC:pf=^T:po=\022:r2=\023\ER:se=\E4:sf=\ES:\
	:so=\E3:sr=\ET:st=\E1:ta=\E@:up=\E7:
tty43|model 43 teletype:\
	:am:bs:hc:os:xo:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:kb=^H:le=^H:sf=^J:

#### Tymshare
#

scanset|sc410|sc415|Tymshare Scan Set:\
	:am:bw:ms:\
	:co#80:li#24:\
	:ac=l<m-k4j%q\\\054x5:ae=^O:as=^N:bl=^G:cd=\EJ:\
	:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :cr=^M:do=^J:ho=\EH:\
	:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=^I:pf=\E;0:\
	:po=\E;0:ps=\E;3:r1=\E>:rc=^C:sc=^B:sf=^J:up=^K:

scanset-n|Tymshare Scan Set in 40 col mode:\
	:r2=\E<:tc=scanset:

#### Volker-Craig (vc)
#

# Missing in vc303a and vc303 descriptions:  they scroll 2 lines at a time
# every other linefeed.
vc303a|vc403a|volker-craig 303a:\
	:am:bs:ns:\
	:co#80:li#24:\
	:bl=^G:ce=\026:cl=\030:cr=^M:do=^J:ho=\031:kd=^J:\
	:kl=^H:kr=^U:ku=^Z:le=^H:ll=^P:nd=^U:up=^Z:
vc303|vc103|vc203|volker-craig 303:\
	:am:bs:ns:\
	:co#80:li#24:\
	:bl=^G:cl=\014:cr=^M:do=^J:ho=\013:kd=^J:kl=^H:kr=^I:\
	:ku=^N:le=^H:ll=\017W:nd=^I:up=^N:
# (vc404: removed obsolete ":ma=^Z^P^U :" -- esr)
vc404|volker-craig 404:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cd=\027:ce=\026:cl=\030:cm=\020%+ %+ :cr=^M:\
	:do=^J:ho=\031:kd=^J:kl=^H:kr=^U:ku=^Z:le=^H:nd=^U:\
	:sf=^J:up=^Z:
vc404-s|volker-craig 404 w/standout mode:\
	:do=^J:se=^O:so=^N:tc=vc404:
# (vc404-na: removed obsolete ":ma@:" -- esr)
vc404-na|volker-craig 404 w/no arrow keys:\
	:kr@:ku@:tc=vc404:
vc404-s-na|volker-craig 404 w/standout mode and no arrow keys:\
	:se=^O:so=^N:tc=vc404-na:
# From: <wolfgang@cs.sfu.ca>
vc414|vc414h|Volker-Craig 414H in sane escape mode.:\
	:am:bs:\
	:co#80:li#24:\
	:al=\E\032:cd=\E^X:ce=10\E\017:cl=\E\034:dc=\E3:\
	:do=\E^K:ei=:ic=\E\072:im=:k0=\EA:k1=\EB:k2=\EC:\
	:k3=\ED:k4=\EE:k5=\EF:k6=\EG:k7=\EH:kd=\E^K:kh=\E^R:\
	:kl=^H:kr=^P:ku=\E^L:l0=PF1:l1=PF2:l2=PF3:l3=PF4:\
	:l4=PF5:l5=PF6:l6=PF7:l7=PF8:nd=^P:se=\E^_:so=\E^Y:\
	:up=\E^L:
vc414h-noxon:\
	:cm=\E\021%r%.%.:dl=\E\023:ho=\E^R:tc=vc414h:
vc415|volker-craig 415:\
	:cl=^L:tc=vc404:

######## OBSOLETE PERSONAL-MICRO CONSOLES AND EMULATIONS
#

#### IBM PC and clones
#

# The pcplot IBM-PC terminal emulation program is really messed up. It is
# supposed to emulate a vt-100, but emulates the wraparound bug incorrectly,
# doesn't support scrolling regions, ignores add line commands, and ignores
# delete line commands. Consequently, the resulting behavior looks like a
# crude adm3a-type terminal.
# Steve Jacobson 8/85
pcplot:\
	:xn@:\
	:cs@:rc@:sc@:tc=vt100:
# (kaypro: removed obsolete ":ma=^K^P:" -- esr)
kaypro|kaypro2|kaypro II:\
	:am:bs:\
	:co#80:li#24:\
	:cl=1\032:cm=\E=%+ %+ :ho=^^:kd=^J:kl=^H:kr=^L:ku=^K:\
	:nd=^L:up=^K:
sanyo55|sanyo|sanyo mbc-55x pc compatible:\
	:am:bs:\
	:co#80:li#25:\
	:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:nd=\E[C:\
	:se=\E[m:so=\E[7m:ue=\E[m:up=\E[A:us=\E[4m:

# From IBM, Thu May  5 19:35:27 1983
ibmpc|ibm-pc|ibm5051|5051|IBM Personal Computer (no ANSI.SYS):\
	:am:\
	:co#80:li#24:\
	:bl=^G:cl=^L^K:cr=^M^^:do=^J:ho=^K:im=\200R:kd=^_:\
	:le=^]:nd=^\:sf=\n:up=^^:

#### Apple
#

# apple -- works with an Apple ][+ that is equipped with a Videx 80 column
# card in slot 3. A special routine must be installed at the apple end to
# enable scroll down, here indicated with a ^U.  The Videx card must have 
# inverse char set, which is used as standout.
apple|apple-v80|Apple][+ w/Videx80 & custom scroll down:\
	:am:xn:\
	:co#80:li#24:\
	:ae=^Z3:as=^Z2:bl=^G:cd=\013:ce=\035:cl=\014:\
	:..cm=\r\036%r%p1%{32}%+%c%p2%{32}%+%c$<6>:cr=^M:\
	:do=^J:ho=\031:le=\010:nd=^\:se=^Z2:sf=^J:so=^Z3:\
	:sr=^P:up=^_:
# (appleII: mapped ":pt:" to default tabs -- esr)
appleII|apple ii plus:\
	:am:bs:pt:\
	:co#80:li#24:\
	:cd=^K:ce=^]:cl=^L:cm=\036%r%+ %+ :do=^J:ho=\E^Y:\
	:is=\024T1\016:kd=^J:kr=^U:nd=^\:se=^N:so=^O:up=^_:\
	:vb=\024G1\024T1:ve=^TC2:vs=^TC6:
# Originally by Gary Ford 21NOV83
# From: <ee178aci%sdcc7@SDCSVAX.ARPA>  Fri Oct 11 21:27:00 1985
apple-80|apple II with smarterm 80 col:\
	:am:bs:bw:\
	:co#80:li#24:\
	:bt=^R:cd=10*\013:ce=10\035:cl=10*\014:\
	:cm=\036%r%+ %+ :cr=10*\r:do=^J:ho=^Y:le=^H:nd=^\:\
	:up=^_:
apple-soroc|apple emulating soroc 120:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cd=\EY:ce=\ET:cl=\E*:cm=\E=%+ %+ :cr=^M:do=^J:\
	:ho=^^:kd=^J:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:sf=^J:\
	:up=^K:
# From Peter Harrison, Computer Graphics Lab, San Francisco
#   ucbvax!ucsfmis!harrison  .....uucp
#   ucbvax!ucsfmis!harrison@BERKELEY   .......ARPA
# "These two work.  If you don't have the inverse video chip for the
# Apple with videx then remove the so and se fields."
# (DaleApple: mapped ":pt:" to default tabs -- esr)
DaleApple|Apple with videx videoterm 80 column board with inverse video:\
	:am:bs:pt:xn:\
	:co#80:li#24:\
	:cd=^K:ce=^]:cl=300\014:cm=\036%r%+ %+ :do=^J:ho=^Y:\
	:kd=^J:kh=^Y:kl=^H:kr=^U:le=^H:nd=^\:se=^Z2:so=^Z3:\
	:up=^_:
# (lisa: this had forms-drawing capabilities
#	:GV=`:GH=a:G1=c:G2=f:G3=e:G4=d:GU=u:GD=s:GC=b:GL=v:GR=t:
# I renamed GS/GE/CO/CF, mapped ":pt:" to default tabs -- esr)
lisa|apple lisa console display, black on white:\
	:am:bs:eo:ms:pt:\
	:co#88:li#32:\
	:ae=\E[10m:al=\E[L:as=\E[11m:cd=\E[J:ce=\E[K:cl=^L:\
	:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:do=\E[B:ei=:ho=\E[H:\
	:ic=\E[@:im=:is=\E>\E[0m\014:kb=^H:kd=\E[B:kl=\E[D:\
	:kr=\E[C:ku=\E[A:nd=\E[C:se=\E[m:so=\E[7m:ue=\E[m:\
	:up=\E[A:us=\E[4m:vi=\E[5h:vs=\E[5l:
liswb|apple lisa console display, white on black:\
	:is=\E>\E[0;7m\014:se=\E[0;7m:so=\E[0m:ue=\E[0;7m:\
	:us=\E[4m:tc=lisa:
mac|macintosh|Macintosh with MacTerminal:\
	:xn:\
	:dN#30:\
	:al=20\E[L:dc=7\E[P:dl=20\E[M:ei=:ic=9\E[@:im=:ip=7:tc=vt100:

#### Radio Shack/Tandy
#

# (coco3: This had "ta" used incorrectly as a boolean and bl given as "bl#7".
# I read these as mistakes for ":it#8:" and ":bl=\007:" respectively -- esr)
# From: <{pbrown,ctl}@ocf.berkeley.edu> 12 Mar 90
coco3|os9LII|Tandy CoCo3 24*80 OS9 Level II:\
	:am:bs:\
	:co#80:it#8:li#24:\
	:al=^_0:bl=^G:cd=^K:ce=^D:cl=5*\014:cm=2\002%r%+ %+ :\
	:dl=^_1:do=^J:ho=^A:kd=^J:kl=^H:kr=^I:ku=^L:mb=^_":\
	:md=\E\072^A:me=\037!\E\072\200:mr=^_ :nd=^F:se=^_!:\
	:so=^_ :ue=^_#:up=^I:us=^_":ve=^E!:vi=^E :
trs80|trs-80|radio shack trs-80 Model I:\
	:am:bs:\
	:co#64:li#16:\
	:bl=^G:cr=^M:do=^J:le=^H:sf=^J:
# (trs2: mapped ":pt:" to default tabs; removed obsolete ":nl=^_:" -- esr)
trs2|trsII|trs80II|Radio Shack Model II using P&T CP/M:\
	:am:bs:ms:pt:\
	:co#80:li#24:\
	:al=^D:bl=^G:cd=^B:ce=^A:cl=^L:cm=\EY%+ %+ :cr=^M:\
	:dl=^K:do=^_:ho=^F:kb=^H:kd=^_:kl=^\:kr=^]:ku=^^:\
	:nd=^]:se=^O:sf=^J:so=^N:up=^^:
# From: Kevin Braunsdorf <ksb@mentor.cc.purdue.edu>
# (This had unknown capabilities
#	:GV=s:GH=u:GU=e:GD=c:G1=`:G2=_:G3=b:G4=a:\
#	:BN=\E[?33h:BF=\E[?33l:UC=\E[_ q:BC=\E[\177 q:\
#	:CN=\ERC:CF=\ERc:NR=\ERD:NM=\ER@:
# I renamed GS/GE,also deleted the unnecessary ":kn#2:", ":sg#0:"
# and mapped ":pt:" to default tabs -- esr)
trs16|trs-80 model 16 console:\
	:am:bs:pt:\
	:co#80:li#24:sg#0:\
	:ae=\ERg:al=\EL:as=\ERG:bl=^G:cd=\EJ:ce=\EK:cl=^L:\
	:cm=\EY%+ %+ :cr=^M:dc=\EQ:dl=\EM:do=\EB:ei=:ho=\EH:\
	:ic=\EP:im=:k0=^A:k1=^B:k2=^D:k3=^L:k4=^U:k5=^P:\
	:k6=^N:k7=^S:kb=^H:kd=\EB:kh=^W:kl=\ED:kr=\EC:ku=\EA:\
	:l0=f1:l1=f2:l2=f3:l3=f4:l4=f5:l5=f6:l6=f7:l7=f8:\
	:le=^H:nd=\EC:pf=\E]+:po=\E]=:se=\ER@:sf=^J:so=\ERD:\
	:ta=^I:up=\EA:ve=\ERC:vi=\ERc:
# From: Suk Lee <..!{decvax,linus,allegra,ihnp4}!utcsrgv!spoo>
# (civis/cnorm added from SCO description)
trs100|Radio Shack Model 100:\
	:am:bs:xt:\
	:co#40:li#8:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EK:cl=\EE:cm=\EY%+ %+ :\
	:cr=^M:dl=\EM:do=^J:ho=\EH:kb=^H:kd=^_:kl=^]:kr=^\:\
	:ku=^^:le=^H:nd=\EC:se=\Eq:sf=^J:so=\Ep:up=\EA:\
	:ve=\EP:vi=\EQ:
trs200|Tandy 200:\
	:am:xt:\
	:co#40:li#16:\
	:al=\EL:bl=^G:cd=^L:ce=\EK:cl=\EE:cm=\EY%+ %+ :cr=^M:\
	:dl=\EM:do=^_:kd=^_:kl=^]:kr=^\:ku=^^:le=^H:nd=^\:\
	:se=\Eq:sf=^J:so=\Ep:up=\EA:
trs600|Tandy Model 600:\
	:am:\
	:co#80:li#15:\
	:bl=^G:cl=\EH\EE:cm=\EY%+ 040%+ :cr=^M:do=\EB:kd=\EB:\
	:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:sf=^J:ta=^I:\
	:up=\EA:

#### Atari ST
#

# From: Simson L. Garfinkel <simsong@media-lab.mit.edu>
# (atari: mapped ":pt:" to default tabs -- esr)
atari|atari st:\
	:am:bs:pt:\
	:co#80:li#25:\
	:al=\EL:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :dl=\EM:\
	:do=\EB:kd=\EB:kl=\ED:kr=\EC:ku=\EA:nd=\EC:se=\Eq:\
	:so=\Ep:sr=\EI:up=\EA:
# UniTerm terminal program for the Atari ST:  49-line VT220 emulation mode
# From: Paul M. Aoki <aoki@ucbvax.berkeley.edu>
uniterm|uniterm49|UniTerm VT220 emulator, 49 lines:\
	:li#49:\
	:is=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h\E[1;49r\E[49;1H:tc=vt220:

#### Commodore Business Machines
#
# Formerly located in West Chester, PA; went spectacularly bust in 1994
# after years of shaky engineering and egregious mismanagement.  Made one
# really nice machine (the Amiga) and boatloads of nasty ones (PET, C-64,
# C-128, VIC-20).  The C-64 is said to have been the most popular machine
# ever (most units sold); they can still be found gathering dust in closets
# everywhere.
#

# From: Kent Polk <kent@swrinde.nde.swri.edu>, 30 May 90
# Added a few more entries, converted caret-type control sequence (^x) entries
# to '\0xx' entries since a couple of people mentioned losing '^x' sequences.
#
# :as:, :ae:			Support for alternate character sets.
# :ve=\E[\040p:vi=\E[\060\040p:	cursor visible/invisible.
# :xn:  vt100 kludginess at column 80/NEWLINE ignore after 80 cols(Concept)
#     This one appears to fix a problem I always had with a line ending
#     at 'width+1' (I think) followed by a blank line in vi. The blank
#     line tended to disappear and reappear depending on how the screen
#     was refreshed. Note that this is probably needed only if you use
#     something like a Dnet Fterm with the window sized to some peculiar
#     dimension larger than 80 columns.
# :k0=\E9~:	map F10 to k0 - could have F0-9 -> k0-9, but ... F10 was 'k;'
# (amiga: removed obsolete ":kn#10:" -- esr)
amiga|Amiga ANSI:\
	:am:bs:bw:xn:\
	:co#80:li#24:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:\
	:LE=\E[%dD:RI=\E[%dC:SF=\E[%dS:SR=\E[%dT:UP=\E[%dA:\
	:ae=^O:al=\E[L:as=^N:bl=^G:bt=\E[Z:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:do=\E[B:\
	:ei=:ho=\E[H:ic=\E[@:im=:is=\E[20l:k0=\E9~:k1=\E0~:\
	:k2=\E1~:k3=\E2~:k4=\E3~:k5=\E4~:k6=\E5~:k7=\E6~:\
	:k8=\E7~:k9=\E8~:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:\
	:le=\E[D:mb=\E[7;2m:md=\E[1m:me=\E[0m:mh=\E[2m:\
	:mk=\E[8m:mr=\E[7m:nd=\E[C:rs=\Ec:se=\E[0m:sf=\E[S:\
	:so=\E[7m:sr=\E[T:ue=\E[0m:up=\E[A:us=\E[4m:vb=^G:\
	:ve=\E[ p:vi=\E[0 p:

# The legendary home of B1FF...
vic20|vic|VIC-20 Personal Computer:\
	:am:\
	:co#22:li#20:\
	:bl=^G:cl=^K^L:cr=^M:do=^J:ho=^L:nd=^\:sf=^J:up=^^:

#### CompuColor
#
# These were consoles for a line of Z80-based micros dating from around 1977.
#

# These compucolors appear similar, but they at least have different
# sized screens.  I don't know what's going on here.
# (compucolor: removed obsolete ":bc=^Z:" -- esr)
compucolor|isc8001|intecolor:\
	:am:\
	:co#80:li#47:\
	:al=\EU:bl=^G:cl=\014:cr=\r:dl=\EV\034:do=\n:\
	:ei=\022\EK:im=\023\EQ:kd=^J:kh=^H:kl=^Z:kr=^Y:ku=^\:\
	:le=\032:nd=\031:sf=\n:ue=\022:up=\034:us=\021:
# (compucolor2: mapped ":pt:" to default tabs,
# removed obsolete ":bc=^Z:" -- esr)
compucolor2|compucolorII:\
	:am:pt:\
	:co#64:li#32:\
	:bl=^G:cl=^L:cm=\003%r%.%.:cr=^M:do=^J:ho=^H:le=^Z:\
	:nd=^Y:sf=^J:ta=^I:up=^\:

#### Exidy Sorcerer
#

# (exidy: mapped ":pt:" to default tabs -- esr)
exidy|exidy2500|exidy sorcerer as dm2500:\
	:am:\
	:co#64:li#30:\
	:al=^P^J^X:bl=^G:cd=^X:ce=^W:cl=^^:\
	:..cm=\014%p2%'`'%^%c%p1%'`'%^%c:cr=^M:dc=^H:\
	:dl=^P^Z^X:dm=^P:do=^J:ei=^X:ho=^B:ic=^\:im=^P:le=^H:\
	:nd=^\:se=^X:sf=^J:so=^N:ta=^I:up=^Z:
ex3000:\
	:co#80:li#24:\
	:bl=^G:cr=^M:do=^J:ho=^Q:sf=^J:
# This came from the comp ctr who got it from some user.  Smart indeed!
# (sexidy: looks like an Exidy Sorcerer in some bizarre emulation mode;
# removed obsolete ":ma=^x^J:"; removed obsolete ":bc=^A:"; removed 
# incorrect (and overridden) ":le=^H:" -- esr)
sexidy|exidy smart:\
	:bs:\
	:co#64:li#24:\
	:bl=^G:cl=^L:cr=^M:do=^J:ho=^Q:kd=^S:le=^A:nd=^S:\
	:sf=^J:up=^W:

#### Osborne
#
# Thu Jul  7 03:55:16 1983
#	
# As an aside, be careful; it may sound like an anomaly on the 
# Osborne, but with the 80-column upgrade, it's too easy to 
# enter lines >80 columns!
#	
# I've already had several comments...
# The Osborne-1 with the 80-col option is capable of being 
# 52,80, or 104 characters wide; default to 80 for compatibility 
# with most systems.
#	
# The tab is destructive on the Ozzie; make sure to 'stty -tabs'.
ozzie|osborne|osborne1|osborne 1:\
	:ms:ul:xt:\
	:co#104:li#24:\
	:al=\EE:bl=^G:ce=\ET:cl=^Z:cm=\E=%+ %+ :cr=^M:dc=\EW:\
	:dl=\ER:do=^J:ei=:ic=\EQ:im=:kd=^J:kl=^H:kr=^L:ku=^K:\
	:le=^H:nd=^L:se=\E(:sf=^J:so=\E):ue=\Em:up=^K:us=\El:

#### Console types for UNIX clones
#

# According to the Coherent 2.3 manual, the PC console is similar
# to a z19. The differences seem to be (1) 25 lines, (2) no status
# line, (3) standout is broken, (4) ins/del line is broken, (5)
# has blinking and bold.
pc-coherent|pcz19|coherent|IBM PC console running Coherent:\
	:am:mi:\
	:co#80:it#8:li#25:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EE:cm=\EY%+ %+ :cr=^M:\
	:dc=\EN:do=\EB:ei=\EO:ho=\EH:im=\E@:kb=^H:kd=\EB:\
	:kh=\EH:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:se=\Eq:\
	:sf=^J:so=\Ep:sr=\EI:ta=^I:up=\EA:

# According to the Venix 1.1 manual, the PC console is similar
# to a DEC vt52.  Differences seem to be (1) arrow keys send 
# different strings, (2) enhanced standout, (3) added insert/delete line.
# Note in particular that it doesn't have automatic margins (am).
# There are other keys (f1-f10, pgup, pgdn, backtab, insch, delch)
# not described here.
pc-venix|venix|IBM PC console running Venix:\
	:co#80:it#8:li#25:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :\
	:cr=^M:dl=\EM:do=^J:kb=^H:kd=\EP:kh=\EG:kl=\EK:\
	:kr=\EM:ku=\EH:le=^H:nd=\EC:sf=^J:sr=\EI:ta=^I:\
	:up=\EA:

#### Miscellaneous microcomputer consoles
#
# If you know anything more about any of these, please tell me.

# I don't know which, if either, of these sols to believe.
# ^S is an arrow key!  Boy is this guy in for a surprise...
sol|sol1|sol terminal computer:\
	:am:\
	:co#64:li#16:\
	:bl=^G:cl=^K:cm=\E\021%.\E\022%.:cr=^M:do=^J:ho=^N:\
	:kd=^Z:kl=^A:kr=^S:ku=^W:le=^H:nd=^S:sf=^J:up=^W:
sol2|sol terminal computer:\
	:am:mi:xn:\
	:co#64:li#16:\
	:al=20\EL:bl=^G:cd=20\EJ:ce=\EK:cl=20\EE:\
	:cm=\EY%+ %+ :cr=^M:dc=\EN:dl=20\EM:do=^J:ei=\EO:\
	:ho=\EH:im=\E@:kd=\ED:kh=\EH:kl=\EL:kr=\ER:ku=\EU:\
	:le=^H:nd=\EC:sf=\n:ta=^I:up=\EA:ve=\EX:vs=^N^Lv:
# basis from Peter Harrison, Computer Graphics Lab, San Francisco
#   ucbvax!ucsfmis!harrison ...uucp / ucbvax!ucsfmis!harrison@BERKELEY ...ARPA
# (basis: removed obsolete ":ma=^K^P^R^L^L :nl=5000*^J:" -- esr)
basis|BASIS108 computer with terminal translation table active:\
	:cd=\EY:ce=\ET:cl=300\E*:do=5000\n:kb=^H:kd=^J:kl=^H:\
	:kr=^L:ku=^K:se=\E):so=\E(:tc=adm3a:
# luna's BMC terminal emulator
luna|luna68k|LUNA68K Bitmap console:\
	:co#88:li#46:\
	:tc=ansi-mini:
microkit|mkt|microkit terminal computer:\
	:am:mi:xn:\
	:co#40:li#23:\
	:al=\El:bl=^G:cd=\Ej:ce=\Ek:cl=\Ee:cm=\Ey%+ %+ :\
	:cr=^M:dc=\En:dl=\Em:do=^J:ei=\Eo:ho=\Eh:im=\E@:\
	:kd=\Ed:kh=\Eh:kl=\El:kr=\Er:ku=\Eu:le=^H:nd=\Ec:\
	:sf=^J:ta=^I:up=\Ea:ve=\Ex:vs=\016\014zv:
megatek|pegasus workstation terminal emulator:\
	:am:os:\
	:co#83:li#60:\
	:
# The Xerox 820 was an early Z80 micro that went nowhere (I think)
xerox820|x820|Xerox 820:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cd=^Q:ce=^X:cl=1^Z:cm=\E=%+ %+ :cr=^M:do=^J:\
	:ho=^^:le=^H:nd=^L:sf=^J:up=^K:

#### Videotex and teletext
#

# standard-issue France Telecom minitel terminal (made by Philips)
# (m2-nam: had unknown ":zd=\E[1m:zb=\E[5m:zc=lkmjqxtuwvn:";
# also deleted unnecessary ":ug#0:sg#0:"; mapped ":pt:" to "" -- esr)
m2-nam|minitel|minitel-2|minitel-2-nam|France Telecom Minitel:\
	:am@:bs:pt:xn:\
	:co#80:it#8:li#24:\
	:ae=\E(B:al=\E[L:as=\E(0:cd=\E[J:ce=\E[K:cl=\E[H\E[J:\
	:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:ei=\E[4l:ho=\E[H:\
	:im=\E[4h:ip=7:is=\E[1;24r\E[24;1H:k1=\EOP:k2=\EOQ:\
	:k3=\EOR:k4=\EOS:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:\
	:ku=\E[A:nd=\E[C:se=\E[m:sf=^J:so=\E[7m:sr=\EM:\
	:ue=\E[m:up=\E[A:us=\E[4m:
# From: Joel Rubin <jmrubin@coral.berkeley.edu>
# This is a preliminary TERMCAP for VIDTEX, a terminal program sold by 
# Compuserve.  Line and column numbers are computer-dependent (I have a
# Commodore '64); you should use the meta-B option to shut off clean-breaking
# of lines.  No key codes included since some of them are programmable and
# most are machine-specific.  Works on vi if you don't use clean-breaking.
# Very similar to the IBM 3101 termcap.  Escape-D used for backspace because
# control-H is destructive backspace.  There seem to be a few weirdnesses
# (especially at the beginning of a wrapped line), and the cursor does not,
# unfortunately, flash.
# (vid: mapped ":pt:" to default tabs; changed :bc: to :le: -- esr)
vid|vidtex|Compuserve vidtex program:\
	:am:pt:\
	:co#40:li#25:\
	:cd=\EJ:ce=\EK:cl=^L:cm=\EY%+ %+ :ho=\EH:le=\ED:\
	:nd=\EC:up=\EA:
# This (inherited from the Emacs termcap.dat file) is probably *way* obsolete!
rsvidtx|Radio Shack VIDEOTEX:\
	:co#32:li#16:\
	:cd=\EJ:ce=\EK:cl=\EH\EJ:..cm=\EY%+ %+ :cr=^M:do=^J:\
	:kb=^H:kd=^J:kl=^H:nd=\EC:nw=^M^J:sf=^J:ta=^I:up=\EA:

######## OBSOLETE VDT TYPES
#
# These terminals are *long* dead -- these entries are retained for
# historical interest only.

#### AED
#
# Advanced Electronic Devices made its name manufacturing super-expensive
# vector-graphics displays and frame buffers in the late 1970s.  They used
# to be in Sunnyvale CA 94086 on Pastoria Avenue.  They're long gone now.
#

# From: Giles Billingsley <gilesb%ucbcad@berkeley.edu>
# rewritten 8/82 for newer AEDs and better operation of vi, etc.
# (bel/cr/cub1/cud1/ind added from SCO entry, which doesn't have db or the
# humongous is2, thus they are commented out here -- esr)
aed|AED|aed512|AED512|aed 512:\
	:bs:\
	:co#64:li#40:\
	:bl=^G:cl=^L:cr=^M:do=^J:le=^H:nd=\Ei0800\001:\
	:se=\E[00C80\001:\
	:sf=\E;1100\072004=000200??;1300'\200\001\n\E\072004=0002??00;1200\001\n:\
	:so=\E\07200>8000140[80C00\001:\
	:te=\E\07200>8000100{804<0??00001000L80\072004=000200??\001:\
	:ti=\E\07200>8000140{<04<0??00001010L<0\072004=0002??00\001:\
	:uc=\Ei???>l0800i0102\001:ue=\E\07200>8000100\001:\
	:up=^K:us=\E\07200>8000140\001:\
	:vb=\EK0001??0000K0001202080\001:\
	:ve=\E\072004=000200??\001:
aed-ucb|AED-UCB|aed512-ucb|AED512-UCB|aed 512 w/o UCB ROM:\
	:bs:db:\
	:co#64:li#40:\
	:cl=^L:if=/usr/share/tabset/aed512:nd=\Ei0800\001:\
	:se=\E[00C80\001:so=\E\07200>8000140[80C00\001:\
	:te=\E\07200>8000100{804<0??00001000L80\072004=000200??\001:\
	:ti=\E\07200>8000140{<04<0??00001010L<0\072004=0002??00\001:\
	:uc=\Ei???>l0800i0102\001:ue=\E\07200>8000100\001:\
	:up=^K:us=\E\07200>8000140\001:\
	:vb=\EK0001??0000K0001202080\001:\
	:ve=\E\E\E\E\E\E\E\072004=000200??\001:

#### Amtek Business Machines
#

# (abm80: early versions of this entry apparently had ":se=\E^_:so=\E^Y",
# but these caps were commented out in 8.3; also, removed overridden
# ":do=^J:" -- esr)
abm80|amtek business machines 80:\
	:am:bs:bw:\
	:co#80:li#24:\
	:al=\E^Z:bt=^T:cd=\E^X:ce=\E^O:cl=\E^\:\
	:cm=\E\021%r%+ %+ :dl=\E^S:do=\E^K:ho=\E^R:le=^H:\
	:nd=^P:up=\E^L:

#### Bell Labs blit terminals
#
# These were AT&T's official entries.
#

blit|jerq|blit running teletype rom:\
	:am:eo:ul:xo:\
	:co#87:it#8:li#72:\
	:AL=\EF%+ :DC=\Ee%+ :DL=\EE%+ :IC=\Ef%+ :al=\EF!:\
	:bl=^G:ce=\EK:cl=^L:cm=\EY%r%+ %+ :cr=^M:dc=\Ee!:\
	:dl=\EE!:do=^J:ei=:ic=\Ef!:im=:k1=\Ex:k2=\Ey:k3=\Ez:\
	:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=\ED:nd=\EC:\
	:sf=^J:ta=^I:up=\EA:

cbblit|fixterm|blit running columbus code:\
	:co#88:\
	:cd=\EJ:ei=\ER:ic@:im=\EQ:pO=\EP%03:pf=^T:po=^R:\
	:se=\EV!:so=\EU!:ue=\EV":us=\EU":vb=\E^G:tc=blit:

oblit|ojerq|first version of blit rom:\
	:am:da:db:eo:mi:ul:xo:\
	:co#88:it#8:li#72:\
	:AL=\Ef%+ :DL=\Ee%+ :al=\EF:bl=^G:cd=\EJ:ce=\EK:\
	:cl=^L:cm=\EY%r%+ %+ :cr=^M:dc=\EO:dl=\EE:do=^J:\
	:ei=\ER:im=\EQ:kb=^H:le=\ED:nd=\EC:sf=^J:ta=^I:\
	:up=\EA:vb=\E^G:

daleblit|daleterm|blit running Dale DeJager's ROM:\
	:da@:db@:\
	:kd=\EB:kl=\ED:kr=\EC:ku=\EA:se=\EV!:so=\EU!:ue=\EV":\
	:us=\EU":tc=oblit:

#### Bolt, Beranek & Newman (bbn)
#
# The BitGraph was a product of the now-defunct BBN Computer Corporation.
# The parent company, best known as the architects of the Internet, is
# still around.
#

# Entries for the BitGraph terminals.  The problem 
# with scrolling in vi can only be fixed by getting BBN to put 
# smarter scroll logic in the terminal or changing vi or padding 
# scrolls with about 500 ms delay.
#	
# I always thought the problem was related to the terminal 
# counting newlines in its input buffer before scrolling and 
# then moving the screen that much. Then vi comes along and 
# paints lines in on the bottom line of the screen, so you get 
# this big white gap.

bitgraph|bbn bitgraph:\
	:tc=bg3.10rv:
bg3.10rv|bgrv|bbn bitgraph (reverse video):\
	:tc=bg2.0rv:
bg3.10nv|bgnv|bbn bitgraph (normal video):\
	:tc=bg2.0nv:
bg3.10|bgn|bbn bitgraph (no init):\
	:tc=bg2.0:
bg2.0rv|bbn bitgraph (reverse video):\
	:is=\E>\E[?5h\E[?7h:vb=\E[?5l\E[?5h:tc=bg2.0:
bg2.0nv|bbn bitgraph (normal video):\
	:is=\E>\E[?5l\E[?7h:vb=\E[?5h\E[?5l:tc=bg2.0:
bg2.0|bbn bitgraph (no init):\
	:xn:\
	:co#85:li#64:\
	:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[J:\
	:cm=%i\E[%d;%dH:cr=^M:cs=\E[%i%d;%dr:dl=\E[M:do=\E[B:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:kd=\E[B:ke=\E>:\
	:kl=\E[D:kr=\E[C:ks=\E=:ku=\E[A:l1=PF1:l2=PF2:l3=PF3:\
	:l4=PF4:le=^H:nd=\E[C:rc=\E8:sc=\E7:se=\E[0m:sf=\n:\
	:so=\E[7m:ta=^I:up=\E[A:
bg1.25rv|bbn bitgraph (reverse video):\
	:is=\E>\E[?5h\E[?7h:vb=\E[?5l\E[?5h:tc=bg1.25:
bg1.25nv|bbn bitgraph (normal video):\
	:is=\E>\E[?5l\E[?7h:vb=\E[?5h\E[?5l:tc=bg1.25:
bg1.25|bbn bitgraph:\
	:co#85:li#64:\
	:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\E[H\E[J:\
	:cm=%i\E[%d;%dH:cr=^M:dl=\E[M:do=\E[B:k1=\EP:k2=\EQ:\
	:k3=\ER:k4=\ES:kd=\EB:ke=\E>:kl=\ED:kr=\EC:ks=\E=:\
	:ku=\EA:l1=PF1:l2=PF2:l3=PF3:l4=PF4:le=^H:\
	:ll=\E[64;1H:nd=\E[C:se=\E[0m:sf=\n:so=\E[7m:ta=^I:\
	:up=\E[A:

#### Chromatics
#

# cg7900: Following is revised version. As I mentioned, I recompiled 
# curses in order to accomadate the large amount of definition.
# I have put the long strings in ti/te. Ti sets up a window 
# that is smaller than the screen, and puts up a warning message 
# outside the window. Te erases the warning message, puts the 
# window back to be the whole screen, and puts the cursor at just
# below the small window. A defined vs and ve to really turn 
# the cursor on and off, but I have taken this out since I don't 
# like the cursor being turned off when vi exits.   
cg7900|chromatics|chromatics 7900:\
	:am:\
	:co#80:li#40:\
	:al=^A>2:bl=^G:cd=^Al:ce=^A`:cl=^L:\
	:cm=\001M%r%d\\\054%d\\\054:cr=^M:dc=^A<1:dl=^A<2:\
	:do=^J:ei=:ho=^\:ic=^A>1:im=:le=^H:ll=^A|:nd=^]:\
	:se=\001C1\\\054\001c2\\\054:sf=^J:\
	:so=\001C4\\\054\001c7\\\054:\
	:te=\001W0\\\05440\\\05485\\\05448\\\054\014\001W0\\\0540\\\05485\\\05448\\\054\001M0\\\05440\\\054:\
	:ti=\001P0\001O1\001R1\001C4\\\054\001c0\\\054\014\001M0\\\05442\\\054WARNING DOUBLE ENTER ESCAPE and \025\001C1\\\054\001c2\\\054\001W0\\\0540\\\05479\\\05439\\\054:\
	:uc=\001\001_\001\200:up=^K:

#### Computer Automation
#

ca22851|computer automation 22851:\
	:am:\
	:co#80:li#24:\
	:bl=^G:cd=^\:ce=^]:cl=\014:cm=\002%i%.%.:cr=^M:do=^J:\
	:ho=^^:kd=^W:kh=^^:kl=^U:ku=^V:le=^U:nd=^I:sf=^J:\
	:up=^V:

#### Cybernex
#

# This entry has correct padding and the undocumented "ri" capability
cyb83|xl83|cybernex xl-83:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cd=\020:ce=\017:cl=\014:cm=\027%+ %+ :cr=^M:\
	:do=^J:ho=^K:kd=^J:kl=^H:kr=^I:ku=^N:le=^H:nd=^I:\
	:sf=^J:sr=^N:up=^N:
# (mdl110: removed obsolete ":ma=^Z^P:" and overridden ":cd=145^NA^W:" -- esr)
cyb110|mdl110|cybernex mdl-110:\
	:am:bs:\
	:co#80:li#24:\
	:al=\016A\016\035:bl=^G:cd=\016@\026:ce=\016@\026:\
	:cl=\030:cm=\020%+ %+ :cr=^M:dc=\016A\036:\
	:dl=\016A\016\036:do=^J:ei=:ho=^Y:ic=\016A\035:im=:\
	:le=^H:nd=^U:se=^NG:sf=^J:so=^NF:ta=\011:up=^Z:

#### Datapoint
#
# Datapoint is gone.  They used to be headquartered in Texas.
# They created ARCnet, an Ethernet competitor that flourished for a while
# in the early 1980s before 3COM got wise and cut its prices.  The service
# side of Datapoint still lives (1995) in the form of Intelogic Trace.
#

dp3360|datapoint|datapoint 3360:\
	:am:bs:\
	:co#82:li#25:\
	:bl=^G:cd=^_:ce=^^:cl=^]^_:cr=^M:do=^J:ho=^]:le=^H:\
	:nd=^X:sf=^J:up=^Z:

#### DEC terminals (Obsolete types: DECwriter and vt40/42/50)
#
# These entries are DEC's official terminfos for its older terminals.
# Contact Bill Hedberg <hedberg@hannah.enet.dec.com> of Terminal Support
# Engineering for more information.  Updated terminfos and termcaps 
# are kept available at ftp://gatekeeper.dec.com/pub/DEC/termcaps.
#

gt40|dec gt40:\
	:os:\
	:co#72:li#30:\
	:bl=^G:cr=^M:do=^J:le=^H:
gt42|dec gt42:\
	:os:\
	:co#72:li#40:\
	:bl=^G:cr=^M:do=^J:le=^H:
vt50|dec vt50:\
	:co#80:li#12:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:cr=^M:do=^J:le=^H:\
	:nd=\EC:sf=^J:ta=^I:up=\EA:
vt50h|dec vt50h:\
	:co#80:li#12:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :cr=^M:\
	:do=^J:le=^H:nd=\EC:sf=^J:sr=\EI:ta=^I:up=\EA:
vt52|dec vt52:\
	:co#80:it#8:li#24:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :cr=^M:\
	:do=^J:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=^H:\
	:nd=\EC:sf=^J:sr=\EI:ta=^I:up=\EA:
vt61|vt-61|vt61.5:\
	:co#80:li#24:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :cr=\r:\
	:do=^J:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:\
	:sf=\n:sr=\EI:ta=^I:up=\EA:

# The gigi does standout with red!
gigi|vk100|dec gigi graphics terminal:\
	:am:xn:\
	:co#84:li#24:\
	:DO=\E[%dB:LE=\E[%r%dD:RI=\E[%dC:UP=\E[%dA:bl=^G:\
	:cd=\E[J:ce=\E[K:cl=\E[;H\E[2J:cm=\E[%i%d;%dH:cr=^M:\
	:do=^J:is=\E>\E[?3l\E[?4l\E[?5l\E[?20l\E[?7h\E[?8h:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:kd=\EOB:\
	:ke=\E[?1l\E>:kh=\E[H:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:\
	:ku=\EOA:le=^H:nd=\E[C:se=\E[m:sf=^J:so=\E[7;31m:\
	:sr=\EM:ta=^I:ue=\E[m:up=\E[A:us=\E[4m:

# DEC PRO-350 console (VT220-style).  The 350 was DEC's attempt to produce
# a PC differentiated from the IBM clones.  It was a total, ludicrous,
# grossly-overpriced failure (among other things, DEC's OS didn't include
# a format program, so you had to buy pre-formatted floppies from DEC at
# a hefty premium!).
# (pro350: mapped ":pt:" to default tabs -- esr)
pro350|decpro|dec pro console:\
	:bs:pt:\
	:co#80:li#24:\
	:ae=\EG:as=\EF:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :\
	:do=\EB:ho=\EH:k0=\EE:k1=\EF:k2=\EG:k3=\EH:k4=\EI:\
	:k5=\EJ:k6=\Ei:k7=\Ej:kd=\EB:kh=\EH:kl=\ED:kr=\EC:\
	:ku=\EA:nd=\EC:se=\E^N:so=\E^H:sr=\EI:ue=\E^C:up=\EA:\
	:us=\E^D:

dw1|decwriter I:\
	:hc:os:\
	:co#72:\
	:bl=^G:cr=^M:do=^J:le=^H:sf=^J:
dw2|decwriter|dw|decwriter II:\
	:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:kb=^H:le=^H:sf=^J:

# \E(B		Use U.S. character set (otherwise # => british pound !)
# \E[20l	Disable "linefeed newline" mode (else puts \r after \n,\f,\v)
# \E[w   	10 char/in pitch
# \E[1;132	full width horizontal margins
# \E[2g		clear all tab stops
# \E[z		6 lines/in
# \E[66t	66 lines/page (for \f)
# \E[1;66r	full vertical page can be printed
# \E[4g		clear vertical tab stops
# \E>		disable alternate keypad mode (so it transmits numbers!)
# \E[%i%du	set tab stop at column %d (origin == 1)
#		(Full syntax is \E[n;n;n;n;n;...;nu where each 'n' is 
#		a tab stop)
#
#       The dw3 does standout with wide characters.
#
dw3|la120|decwriter III:\
	:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:\
	:i1=\E(B\E[20l\E[w\E[0;132s\E[2g\E[z\E[66t\E[1;66r\E[4g\E>:\
	:is=\E[9;17;25;33;41;49;57;65;73;81;89;97;105;113;121;129u\r:\
	:kb=^H:le=^H:se=\E[w:sf=^J:so=\E[6w:ta=^I:
dw4|decwriter IV:\
	:am:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:is=\Ec:k0=\EOP:k1=\EOQ:k2=\EOR:\
	:k3=\EOS:kb=^H:le=^H:sf=^J:ta=^I:

#### Delta Data (dd)
#

# Untested. The cup sequence is hairy enough that it probably needs work.
# The idea is ctrl(O), dd(row), dd(col), where dd(x) is x - 2*(x%16) + '9'.
# There are BSD-derived termcap entries floating around for this puppy
# that are *certainly* wrong.
delta|dd5000|delta data 5000:\
	:am:\
	:co#80:li#27:\
	:bl=^G:ce=^NU:cl=^NR:cm=\017%+^P%+^P:dc=^NV:do=^J:\
	:ho=^NQ:le=^H:nd=^Y:sf=^J:up=^Z:

#### Digital Data Research (ddr)
#

# (ddr: mapped ":pt:" to default tabs -- esr)
ddr|rebus3180|ddr3180|Rebus/DDR 3180 vt100 emulator:\
	:am:bs:pt:xn:\
	:co#80:li#24:vt#3:\
	:cd=50\E[J:ce=3\E[K:cl=50\E[;H\E[2J:cm=5\E[%i%d;%dH:\
	:cs=\E[%i%d;%dr:do=^J:ho=\E[H:is=\E[1;24r\E[24;1H:\
	:k1=\EOP:k2=\EOQ:k3=\EOR:k4=\EOS:kb=^H:kd=\E[B:\
	:ke=\E[?1l\E>:kl=\E[D:kr=\E[C:ks=\E[?1h\E=:ku=\E[A:\
	:le=^H:mb=2\E[5m:md=2\E[1m:me=2\E[m:mr=2\E[7m:\
	:nd=2\E[C:rc=\E8:rf=/usr/share/lib/tabset/vt100:\
	:rs=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:sc=\E7:se=\E[m:\
	:sf=5\ED:so=\E[7m:sr=5\EM:ue=2\E[m:up=2\E[A:\
	:us=2\E[4m:

#### General Electric (ge)
#

terminet1200|terminet300|tn1200|tn300|terminet|GE terminet 1200:\
	:hc:os:\
	:co#120:\
	:bl=^G:cr=^M:do=^J:sf=^J:

#### Heathkit/Zenith
#

h19-a|heath-ansi|heathkit-a|heathkit h19 ansi mode:\
	:am:mi:ms:\
	:co#80:it#8:li#24:\
	:ae=\E[11m:al=\E[1L:as=\E[10m:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[2J:cm=\E[%i%d;%dH:cr=^M:dc=\E[1P:dl=\E[1M:\
	:do=\E[1B:ei=\E[4l:ho=\E[H:im=\E[4h:\
	:is=\E<\E[>1;2;3;4;5;6;7;8;9l\E[0m\E[11m\E[?7h:\
	:k1=\EOS:k2=\EOT:k3=\EOU:k4=\EOV:k5=\EOW:k6=\EOP:\
	:k7=\EOQ:k8=\EOR:kb=^H:kd=\E[1B:kh=\E[H:kl=\E[1D:\
	:kr=\E[1C:ku=\E[1A:l6=blue:l7=red:l8=white:le=^H:\
	:nd=\E[1C:se=\E[0m:sf=^J:so=\E[7m:sr=\EM:ta=^I:\
	:up=\E[1A:ve=\E[>4l:vs=\E[>4h:
h19-bs|heathkit w/keypad shifted:\
	:ke=\Eu:ks=\Et:tc=h19-b:
h19-smul|heathkit w/keypad shifted/underscore cursor:\
	:ke=\Eu:ks=\Et:tc=h19-u:
h19|heath|h19-b|heathkit|heath-19|z19|zenith|heathkit h19:\
	:am:es:hs:mi:ms:\
	:co#80:it#8:li#24:\
	:ae=\EG:al=\EL:as=\EF:bl=^G:cd=\EJ:ce=\EK:cl=\EE:\
	:cm=\EY%+ %+ :cr=^M:dc=\EN:dl=\EM:do=\EB:ei=\EO:\
	:fs=\Ek\Ey5:ho=\EH:im=\E@:k1=\ES:k2=\ET:k3=\EU:\
	:k4=\EV:k5=\EW:k6=\EP:k7=\EQ:k8=\ER:kb=^H:kd=\EB:\
	:kh=\EH:kl=\ED:kr=\EC:ku=\EA:l6=blue:l7=red:l8=white:\
	:le=^H:nd=\EC:se=\Eq:sf=^J:so=\Ep:sr=\EI:ta=^I:\
	:ts=\Ej\Ex5\EY8%p1%{32}%+%c\Eo\Eo:up=\EA:ve=\Ey4:\
	:vs=\Ex4:
h19-u|heathkit with underscore cursor:\
	:ve@:vs@:tc=h19-b:
alto-h19|altoh19|altoheath|alto-heath|alto emulating heathkit h19:\
	:li#60:\
	:al=\EL:dl=\EM:tc=h19:

# The major problem with the Z29 is that it requires more 
# padding than the Z19. Once again, here's a little termcap 
# entry for it that will do the trick. 
# 
# The problem declaring an H19 to be synonomous with a Z29 is that
# it needs more padding. It especially loses if a program attempts
# to put the Z29 into insert mode and insert text at 9600 baud. It
# even loses worse if the program attempts to insert tabs at 9600
# baud. Adding padding to text that is inserted loses because in 
# order to make the Z29 not die, one must add so much padding that
# whenever the program tries to use insert mode, the effective 
# rate is about 110 baud.
# 
# What program would want to put the terminal into insert mode 
# and shove stuff at it at 9600 baud you ask?  
# 
# Emacs. Emacs seems to want to do the mathematically optimal 
# thing in doing a redisplay rather than the practical thing.
# When it is about to output a line on top of a line that is 
# already on the screen, instead of just killing to the end of 
# the line and outputing the new line, it compares the old line 
# and the new line and if there are any similarities, it 
# constructs the new line by deleting the text on the old line 
# on the terminal that is already there and then inserting new
# text into the line to transform it into the new line that is 
# to be displayed. The Z29 does not react kindly to this.
# 
# But don't cry for too long.... There is a solution. You can make
# a termcap entry for the Z29 that says the Z29 has no insert mode.
# Then Emacs cannot use it. "Oh, no, but now inserting into a 
# line will be really slow", you say. Well there is a sort of a
# solution to that too. There is an insert character option on 
# the Z29 that will insert one character. Unfortunately, it 
# involves putting the terminal into ansi mode, inserting the 
# character, and changing it back to H19 mode. All this takes 12 
# characters. Pretty expensive to insert one character, but it 
# works. Either Emacs doesn't try to use its inserting hack when 
# it's only given an insert character ability or the Z29 doesn't 
# require padding with this (the former is probably more likely, 
# but I haven't checked it out).
z29|zenith29|z29b|zenith z29b:\
	:am:ms:\
	:co#80:li#24:\
	:ae=\EF:al=\EL:as=\EG:bl=^G:bt=\E-:cd=\EJ:ce=\EK:\
	:cl=\EE:cm=\EY%+ %+ :cr=^M:dc=\EN:dl=\EM:do=\EB:ei=:\
	:ho=\EH:ic=\E<\E[1@\E[?2h:im=:is=\E<\E[?2h\Ev:k0=\E~:\
	:k1=\ES:k2=\ET:k3=\EU:k4=\EV:k5=\EW:k6=\EP:k7=\EQ:\
	:k8=\ER:k9=\E0I:kb=^H:kd=\EB:kh=\EH:kl=\ED:kr=\EC:\
	:ku=\EA:l0=home:le=^H:nd=\EC:se=\Eq:sf=\n:so=\Ep:\
	:sr=\EI:ta=^I:ue=\Es0:up=\EA:us=\Es8:ve=\Ey4:vs=\Ex4:

# From: Brad Brahms <Brahms@USC-ECLC>
z100|h100|z110|z-100|h-100|heath/zenith z-100 pc with color monitor:\
	:ve=\Ey4\Em70:vs=\Ex4\Em71:tc=z100bw:
# (z100bw: removed obsolete ":kn#10:"; mapped ":pt:" to default tabs -- esr)
z100bw|h100bw|z110bw|z-100bw|h-100bw|heath/zenith z-100 pc:\
	:bs:mi:ms:pt:\
	:co#80:li#24:\
	:ae=\EG:al=5*\EL:as=\EF:cd=\EJ:ce=\EK:cl=5*\EE:\
	:cm=1*\EY%+ %+ :dc=1*\EN:dl=5*\EM:do=\EB:ei=\EO:\
	:ho=\EH:im=\E@:k0=\EJ:k1=\ES:k2=\ET:k3=\EU:k4=\EV:\
	:k5=\EW:k6=\EP:k7=\EQ:k8=\ER:k9=\EOI:kb=^H:kd=\EB:\
	:kh=\EH:kl=\ED:kr=\EC:ku=\EA:nd=\EC:se=\Eq:so=\Ep:\
	:sr=\EI:up=\EA:ve=\Ey4:vs=\Ex4:
p19:\
	:al=2*\EL:dl=2*\EM:tc=h19-b:
# From: <ucscc!B.fiatlux@ucbvax.berkeley.edu>
# (ztx: mapped ":pt:" to default tabs; removed duplicate :sr: -- esr)
ztx|ztx11|zt-1|htx11|ztx-1-a|ztx-10/11:\
	:am:bs:es:hs:pt:\
	:co#80:li#24:\
	:al=\EL:cd=\EJ:ce=\EK:cl=\EE:cm=\EY%+ %+ :dl=\EM:\
	:do=^J:ds=\Ey1:fs=\Ek\Ey5:ho=\EH:\
	:is=\Ej\EH\Eq\Ek\Ev\Ey1\Ey5\EG\Ey8\Ey9\Ey>:k0=\ES:\
	:k1=\EB:k2=\EU:k3=\EV:k4=\EW:k5=\EP:k6=\EQ:k7=\ER:\
	:kb=^H:kd=\EB:kl=\ED:kr=\EC:ku=\EA:le=^H:nd=\EC:\
	:se=\Eq:so=\Es5:sr=\EI:ts=\Ej\Ex5\Ex1\EY8%+ \Eo:\
	:ue=\Eq:up=\EA:us=\Es2:

#### IMS International (ims)
#
# There was a company called IMS International located in Carson City, 
# Nevada, that flourished from the mid-70s to mid-80s.  They made S-100
# bus/Z80 hardware and a line of terminals called Ultimas.  

# From: Erik Fair <fair@ucbarpa.berkeley.edu>  Sun Oct 27 07:21:05 1985
ims950-b|bare ims950 no init string:\
	:is@:tc=ims950:
ims950-ns|ims950 w/no standout:\
	:se@:so@:ue@:us@:tc=ims950:
# (ims950: removed obsolete ":ko@:" -- esr)
ims950|ims televideo 950 emulation:\
	:xn@:\
	:k0@:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:k9@:kb@:kd@:kh@:\
	:kl@:kr@:ku@:vb@:tc=tvi950:
# (ims950-rv: removed obsolete ":ko@:" -- esr)
ims950-rv|ims tvi950 rev video:\
	:xn@:\
	:k0@:k1@:k2@:k3@:k4@:k5@:k6@:k7@:k8@:k9@:kb@:kd@:kh@:\
	:kl@:kr@:ku@:vb@:tc=tvi950-rv:
# (ims-ansi: mapped ":pt:" to default tabs -- esr)
ims-ansi|ultima2|ultimaII|IMS Ultima II:\
	:am:bs:pt:\
	:co#80:li#24:\
	:cd=\E[0J:ce=\E[0K:cl=\E[;H\E[2J:cm=\E[%i%2;%2H:\
	:do=\ED:if=/usr/share/tabset/vt100:\
	:is=\E[0m\E[>14l\E[?1;?5;20l\E>\E[1m\r:kd=\E[B:\
	:kh=\E[H:kl=\E[D:kr=\E[C:ku=\E[A:se=\E[0m\E[1m:\
	:so=\E[7m:sr=\EM:ue=\E[0m\E[1m:up=\EM:us=\E[4m:

#### Intertec Data Systems
#
# I think this company is long dead as of 1995.  They made an early CP/M
# micro called the "Intertec Superbrain" that was moderately popular,
# then sank out of sight.
#

superbrain|intertec superbrain:\
	:am:bw:\
	:co#80:li#24:\
	:bl=^G:cd=\E~k<10*>:ce=\E~K:cl=\014:cm=\EY%+ %+ :\
	:cr=^M:do=^J:kd=^J:kl=^U:kr=^F:ku=^K:le=^H:nd=^F:\
	:sf=^J:ta=^I:te=^L:ti=^L:up=^K:
intertube|intertec|Intertec InterTube:\
	:am:\
	:co#80:li#25:\
	:bl=^G:cl=^L:cm=\EY%+ %+ :cr=^M:do=^J:ho=^A:le=^H:\
	:nd=^F:se=\E0@:sf=^J:so=\E0P:up=^Z:
# The intertube 2 has the "full duplex" problem like the tek 4025: if you
# are typing and a command comes in, the keystrokes you type get interspersed
# with the command and it messes up
it2|intertube2|intertec data systems intertube 2:\
	:am:\
	:co#80:li#25:\
	:bl=^G:ce=\EK:ch=\020%+^J:cl=^L:cm=\016%.\020%+^J:\
	:cr=^M:cv=\013%.:do=^J:ho=^A:le=^H:ll=^K^X\r:nd=^F:\
	:se=\E0@:sf=^J:so=\E0P:up=^Z:

#### Modgraph
#
# These people used to be reachable at:
#
#	Modgraph, Inc
#	1393 Main Street,
#	Waltham, MA 02154
#	Vox: (617)-890-5796.
#
# However, if you call that number today you'll get an insurance company.
# I think Modgraph is long gone.
#

modgraph|mod|modgraph terminal emulating vt100:\
	:xn@:\
	:co#80:li#24:\
	:is=\E^9;0s\E^7;1s\E[3g\E^11;9s\E^11;17s\E^11;25s\E^11;33s\E^11;41s\E^11;49s\E^11;57s\E^11;65s\E^11;73s\E^11;81s\E^11;89s:\
	:rf@:sr=5\EM\E[K:vs=\E^9;0s\E^7;1s:tc=vt100:
# (modgraph2: mapped ":pt:" to default tabs -- esr)
# The GX-1000 manual is dated 1984
modgraph2|modgraph gx-1000, set to 80x24, keypad not enabled:\
	:am:bs:da:db:pt:\
	:co#80:li#24:\
	:cd=50\EJ:ce=3\EK:cl=50\EH\EJ:cm=5\EY%+ %+ :\
	:is=\E<\E^5;2s\E^7;1s\E[3g\E^11;9s\E^11;17s\E^11;25s\E^11;33s\E^11;41s\E^11;49s\E^11;57s\E^11;65s\E^11;73s\E^11;81s\E^11;89s\E^12;0s\E^14;2s\E^15;9s\E^25;1s\E^9;1s\E^27;1:\
	:nd=2\EC:sr=5\EI:up=2\EA:

#### Morrow Designs
# 
# This was George Morrow's company.  They started in the late 1970s making
# S100-bus machines.  They used to be reachable at:
#
#        Morrow
#        600 McCormick St.
#        San Leandro, CA 94577
#
# but they're long gone now (1995).
#

# The mt70 terminal was shipped with the Morrow MD-3 microcomputer. 
# Jeff's specimen was dated June 1984.
# From: Jeff Wieland <wieland@acn.purdue.edu> 24 Feb 1995
mt70|mt-70|Morrow MD-70; native Morrow mode:\
	:am:mi:ms:xo:\
	:co#80:it#8:li#24:\
	:%1=^AO\r:F1=^A`\r:F2=^Aa\r:F3=^Ab\r:F4=^Ac\r:\
	:F5=^Ad\r:F6=^Ae\r:F7=^Af\r:F8=^Ag\r:F9=^Ah\r:\
	:FA=^Ai\r:ac=+z\\\054{.yOi-x`|jGkFlEmDnHtLuKvNwMxIqJ:\
	:ae=\E%:al=\EE:as=\E$:bl=^G:bt=\EI:cd=\EY:ce=\ET:\
	:cl=^Z:cm=\E=%+ %+ :cr=^M:ct=\E0:dc=\EW:dl=\ER:do=^J:\
	:ei=:ho=^^:i1=\E"2\EG0\E]:ic=\EQ:im=:k1=^A@\r:\
	:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:k6=^AE\r:\
	:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kB=^A^Z\r:\
	:kC=^An\r:kD=\177:kb=^H:kd=^AK\r:kh=^AN\r:kl=^AL\r:\
	:kr=^AM\r:ku=^AJ\r:le=^H:me=\EG0:mh=\EG2:mr=\EG4:\
	:nd=^L:nw=^_:se=\EG0:sf=^J:so=\EG4:ta=^I:\
	:ti=\E"2\EG0\E]:up=^K:us=\EG1:vb=\EK1\EK0:ve=\E"2:\
	:vi=\E"0:

#### Netronics
#
# The Netronics Smarterm 80 was a kit-built terminal that came in at least two
# flavors, a first 40-column version, and a second 64-column version released
# about 1983.

# (netx: removed obsolete ":ma=j^Jk^Pl :" -- esr)
netx|netronics:\
	:bs:\
	:co#64:li#16:\
	:bl=^G:cd=\006\005:ce=\005:cl=\014:cm=\E=%+@%+@:\
	:cr=^M:do=^J:ho=^D:le=^H:nd=\E+@A:sf=^J:sr=\E=@@\013:\
	:up=^K:
smartvid|Netronics Smartvid 80:\
	:am:bw:eo:ms:xs:\
	:co#80:li#24:sg#1:ug#1:\
	:ae=\EGB:as=\EG@:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=^L:\
	:cm=\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=^J:ei=\ED:ho=^Z:\
	:ic=\EQ:im=\EC:le=^H:ll=^Z^K:nd=^A:se=\EG@:sf=^J:\
	:so=\EGC:sr=^K:ta=\Ei:te=^Z^K:ue=\EG@:up=^K:us=\EGA:\
	:ve=^Z^K:
smarterm|smarterm-s|netronics smarterm 80x24 naked terminal:\
	:am:ul:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EE:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=^L:\
	:cm=\E=%+ %+ :cr=^M:dc=\EW:dl=\ER:do=^J:ei=\ED:ho=^Z:\
	:ic=\EQ:im=\EC:le=^H:nd=^A:sf=^J:ta=^I:ue=\EG@:\
	:us=\EGA:

#### Omron
#
# This company is still around in 1995, manufacturing point-of-sale systems.

omron|Omron 8025AG:\
	:am:bs:da:db:\
	:co#80:li#24:\
	:al=\EL:bl=^G:cd=\ER:ce=\EK:cl=\EJ:cr=^M:dc=\EP:\
	:dl=\EM:do=^J:ho=\EH:le=^H:nd=\EC:se=\E4:sf=\ES:\
	:so=\Ef:sr=\ET:up=\EA:vs=\EN:

#### Soroc
#

# (soroc120: removed obsolete ":ma=^K^P^R^L^L :" -- esr)
soroc120|iq120|soroc iq120:\
	:cd=\EY:ce=\ET:cl=\E*:do=^J:kd=^J:kl=^H:kr=^L:ku=^K:tc=adm3a:
soroc140|iq140|soroc iq140:\
	:am:mi:\
	:co#80:li#24:\
	:al=\Ee:bl=^G:bt=\EI:cd=\Ey:ce=\Et:cl=\E+:\
	:cm=\E=%+ %+ :cr=^M:dc=\Ew:dl=\Er:do=^J:ei=\E8:ho=^^:\
	:im=\E9:k0=^A0\r:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:\
	:k5=^AD\r:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:kb=^H:\
	:kh=^^:kr=^L:ku=^K:le=^H:ll=^^^K:nd=^L:se=\E\177:\
	:sf=^J:so=\E\177:ue=\E^A:up=^K:us=\E^A:

#### Southwest Technical Products
#
# These guys made an early personal micro called the M6800.  
# The ct82 was probably its console terminal.
#

# (swtp: removed obsolete ":bc=^D:" -- esr)
swtp|ct82|southwest technical products ct82:\
	:am:\
	:co#82:li#20:\
	:al=^^Y:bl=^G:cd=^V:ce=^F:cl=^L:cm=\013%r%.%.:cr=^M:\
	:dc=^^H:dl=^Z:do=^J:ei=:ho=^P:ic=^^X:im=:\
	:is=\034\022\036\023\036\004\035\027\011\023\036\035\036\017\035\027\022\011:\
	:le=^D:ll=^C:nd=^S:se=^^^F:sf=^N:so=^^^V:sr=^O:up=^A:

#### Synertek
#
# Bob Manson <manson@pattyr.acs.ohio-state.edu> writes (28 Apr 1995):
#
# Synertek used to make ICs, various 6502-based single-board process
# control and hobbyist computers, and assorted peripherals including a
# series of small inexpensive terminals (I think they were one of the
# first to have a "terminal-on-a-keyboard", where the terminal itself
# was only slightly larger than the keyboard).
#
# They apparently had a KTM-1 model, which I've never seen. The KTM-2/40
# was a 40x24 terminal that could connect to a standard TV through a
# video modulator.  The KTM-2/80 was the 80-column version (the 2/40
# could be upgraded to the 2/80 by adding 2 2114 SRAMs and a new ROM).
# I have a KTM-2/80 still in working order.  The KTM-2s had fully
# socketed parts, used 2 6507s, a 6532 as keyboard scanner, a program
# ROM and 2 ROMs as character generators. They were incredibly simple,
# and I've never had any problems with mine (witness the fact that mine
# was made in 1981 and is still working great... I've blown the video
# output transistor a couple of times, but it's a 2N2222 :-)
#
# The KTM-3 (which is what is listed in the terminfo file) was their
# attempt at putting a KTM-2 in a box (and some models came with a
# CRT). It wasn't much different from the KTM-2 hardware-wise, but the
# control and escape sequences are very different. The KTM-3 was always
# real broken, at least according to the folks I've talked to about it.
# 
# The padding in the entry is probably off--these terminals were very
# slow (it takes like 100ms for the KTM-2 to clear the screen...) And
# anyone with any sanity replaced the ROMs with something that provided
# a reasonable subset of VT100 functionality, since the usual ROMs were
# obviously very primitive... oh, you could get an upgraded ROM from
# Synertek for some incredible amount of money, but what hacker with an
# EPROM burner would do that? :)
# 
# Sorry I don't have any contact info; I believe they were located in
# Sunnyvale, and I'm fairly sure they are still manufacturing ICs
# (they've gone to ASICs and FPGAs), but I doubt they're in the computer
# business these days.

# Tested, seems to work fine with vi.
synertek|ktm|synertek380|synertek ktm 3/80 tubeless terminal:\
	:am:\
	:co#80:li#24:\
	:cd=\EJ:ce=\EK:cl=^Z:cm=\E=%+ %+ :le=^H:nd=^L:up=^K:

#### Tab Office Products
#
#	TAB Products Co. - Palo Alto, California
#	Electronic Office Products,
#	1451 California Avenue 94304
#
# I think they're out of business.
#

# The tab 132 uses xon/xoff, so no padding needed.
# :ks:/:ke: have nothing to do with arrow keys.
# :is: sets 80 col mode, normal video, autowrap on (for :am:).
# Seems to be no way to get rid of status line.
# The manual for this puppy was dated June 1981.  It claims to be VT52-
# compatible.
tab132|tab|tab132-15|tab 132/15:\
	:da:db:\
	:co#80:dN@:li#24:lm#96:\
	:al=\E[L:cm=\E[%i%d;%dH:dc=\E[P:dl=\E[M:do=^J:\
	:ei=\E[4l:im=\E[4h:is=\E[?7h\E[?3l\E[?5l:kd=\E[B:ke@:\
	:kl=\E[D:ks@:ku=\E[A:tc=vt100:
tab132-w:\
	:co#132:\
	:is=\E[?7h\E[?3h\E[?5l:tc=tab132:
tab132-rv:\
	:is=\E[?7h\E[?3l\E[?5h:tc=tab132:
tab132-w-rv:\
	:is=\E[?7h\E[?3h\E[?5h:tc=tab132-w:


#### Teleray
#
#	Research Incorporated
#	6425 Flying Cloud Drive
#	Eden Prairie, MN 55344
#	Vox: (612)-941-3300
#
# The Teleray terminals were all discontinued in 1992-93.  RI still services
# and repairs these beasts, but no longer manufactures them.  The Teleray
# people believe that all the types listed below are very rare now (1995).
# There was a newer line of Telerays (Model 7, Model 20, Model 30, and
# Model 100) that were ANSI-compatible.
#
# Note two things called "teleray".  Reorder should move the common one
# to the front if you have either.  A dumb teleray with the cursor stuck
# on the bottom and no obvious model number is probably a 3700.
#

t3700|dumb teleray 3700:\
	:bs:\
	:co#80:li#24:\
	:bl=^G:cl=^L:cr=^M:do=^J:le=^H:sf=^J:
# (t3800: mapped ":pt:" to default tabs -- esr)
t3800|teleray 3800 series:\
	:bs:pt:\
	:co#80:li#24:\
	:bl=^G:cd=\EJ:ce=\EK:cl=^L:cm=\EY%+ %+ :cr=^M:do=^J:\
	:ho=\EH:le=^H:ll=\EY7 :nd=\EC:sf=^J:ta=^I:up=^K:
# (t1061: mapped ":pt:" to default tabs -- esr)
t1061|teleray|teleray 1061:\
	:am:km:xs:xt:\
	:co#80:li#24:sg#1:ug#1:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EK:cl=\014:cm=\EY%+ %+ :\
	:cr=^M:ct=\EG:dc=\EQ:dl=\EM:do=^J:ei=:ho=\EH:ic=\EP:\
	:im=:ip=:\
	:is=\Ee\EU01^Z1\EV\EU02^Z2\EV\EU03^Z3\EV\EU04^Z4\EV\EU05^Z5\EV\EU06^Z6\EV\EU07^Z7\EV\EU08^Z8\EV\Ef:\
	:k1=^Z1:k2=^Z2:k3=^Z3:k4=^Z4:k5=^Z5:k6=^Z6:k7=^Z7:\
	:k8=^Z8:le=^H:nd=\EC:se=\ER@:sf=^J:so= \ERD:st=\EF:\
	:ta=^I:ue=\ER@:up=\EA:us=\ERH:
t1061f|teleray 1061 with fast PROMs:\
	:al=\EL:dl=\EM:ip@:tc=t1061:
# "Teleray Arpa Special", offically designated as
# "Teleray Arpa network model 10" with "Special feature 720".
# This is the new (1981) fast microcode updating the older "arpa" proms
# (which gave meta-key and progmmable-fxn keys).  720 is much much faster,
# converts the keypad to programmable function keys, and has other goodies.
# Standout mode is still broken (magic cookie, etc) so is suppressed as no
# programs handle such lossage properly.
# Note: this is NOT the old termcap's "t1061f with fast proms."
# From: J. Lepreau <lepreau@utah-cs> Tue Feb  1 06:39:37 1983, Univ of Utah
# (t10: mapped ":pt:" to default tabs;
# removed overridden ":so@:se@:us@:ue@:" -- esr)
t10|teleray 10 special:\
	:bs:km:pt:xs:xt:\
	:co#80:li#24:sg#2:ug#1:\
	:al=\EL:cd=\EJ:ce=\EK:cl=30\Ej:cm=\EY%+ %+ :dc=\EQ:\
	:dl=\EM:ei=:ho=\EH:ic=\EP:im=:nd=\EC:pc=\200:se=\ER@:\
	:sf=\Eq:so=\ERD:sr=\Ep:ue=\ER@:up=\EA:us=\ERH:
# teleray 16 - map the arrow keys for vi/rogue, shifted to up/down page, and
# back/forth words. Put the function keys (f1-f10) where they can be
# found, and turn off the other magic keys along the top row, except
# for line/local. Do the magic appropriate to make the page shifts work.
# Also toggle ^S/^Q for those of us who use Emacs.
t16|teleray 16:\
	:am:da:db:mi:xs:xt:\
	:co#80:li#24:\
	:al=\E[L:bl=^G:cd=\E[0J:ce=\E[0K:cl=\E[H\E[2J:\
	:cm=%i\E[%d;%df:cr=^M:dc=\E[P:dl=\E[M:do=\E[B:\
	:ei=\E[4l:ho=\E[H:im=\E[4h:k1=^Z1:k2=^Z2:k3=^Z3:\
	:k4=^Z4:k5=^Z5:k6=^Z6:k7=^Z7:k8=^Z8:k9=^Z9:k;=^Z0:\
	:le=^H:nd=\E[C:se=\E[m:sf=^J:so=\E[7m:sr=\E[T:ta=^I:\
	:te=\E[V\E[24;1f\E[?38h:ti=\E[U\E[?38l:ue=\E[m:\
	:up=\E[A:us=\E[4m:

#### Texas Instruments (ti)
#

ti700|ti733|ti735|ti silent 700:\
	:bs:hc:os:\
	:co#80:dC#162:\
	:bl=^G:cr=\r:do=^J:le=^H:sf=^J:
ti743|ti745|ti silent 745:\
	:bs:hc:os:\
	:co#80:\
	:bl=^G:cr=^M:do=^J:le=^H:sf=^J:
ti800|ti omni 800:\
	:bs:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:le=^H:sf=^J:
ti924|Texas Instruments 924 VDT 8859/1 7 bit CTRL:\
	:am:xo:\
	:co#80:it#8:li#24:\
	:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\E[2J\E[H:\
	:cm=%i\E[%d;%dH:cr=^M:cs=%i\E[%d;%dr:ct=\E[3g:\
	:dl=\E[M:do=\E[B:ho=\E[H:k1=\EOP:k2=\EOQ:k3=\EOR:\
	:k4=\EOS:k5=\E[16~:k6=\E[17~:k7=\E[18~:k8=\E[19~:\
	:k9=\E[20~:kD=\E[P:kI=\E[@:kb=^H:kd=\E[B:kl=\E[D:\
	:kr=\E[C:ku=\E[A:le=\E[D:mb=\E[5m:md=\E[1m:me=\E[0m:\
	:mr=\E[7m:nd=\E[C:rc=\E8:sc=\E7:se=\E[m:sf=\ED:\
	:so=\E[7m:sr=\EM:st=\EH:ta=^I:ue=\E[m:up=\E[A:\
	:us=\E[4m:ve=\E[?25h:vi=\E[?25l:vs=\E[?31h:
ti924-8|Texas Instruments 924 VDT 8859/1 8 bit CTRL:\
	:am:xo:\
	:co#80:it#8:li#24:\
	:al=\E[L:bl=^G:cd=\E[J:ce=\E[K:cl=\E[2J\E[H:\
	:cm=%i\E[%d;%dH:cr=^M:cs=%i\E[%d;%dr:ct=\E[3g:\
	:dl=\E[M:do=\E[B:ho=\E[H:k1=P\217>:k2=Q\217>:\
	:k3=R\217>:k4=S\217>:k5=~\23316>:k6=~\23317>:\
	:k7=~\23318>:k8=~\23319>:k9=~\23320>:kD=P\233>:\
	:kI=@\233>:kb=^H:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:\
	:le=\E[D:mb=\E[5m:md=\E[1m:me=\E[0m:mr=\E[7m:nd=\E[C:\
	:rc=\E8:sc=\E7:se=\E[m:sf=\ED:so=\E[7m:sr=\EM:st=\EH:\
	:ta=^I:ue=\E[m:up=\E[A:us=\E[4m:ve=\E[?25h:\
	:vi=\E[?25l:vs=\E[?31h:
ti924w|Texas Instruments 924 VDT 7 bit - 132 column mode:\
	:co#132:\
	:tc=ti924:
ti924-8w|Texas Instruments 924 VDT 8 bit - 132 column mode:\
	:co#132:\
	:tc=ti924-8:
em931-9|Texas Instruments 924 Emulator in the 931 Mode:\
	:tc=ti931:
em924|Texas Instruments 924 Emulator in the 924 Mode:\
	:tc=ti924:
em931|Texas Instruments 931 Emulator:\
	:tc=ti931:
ti931|Texas Instruments 931 VDT:\
	:am:xo:\
	:co#80:li#24:\
	:LE=ENTR:al=\EN:bl=^G:cd=\EJ:ce=\EI:cl=\EL:\
	:cm=\EY%+ %+ :cr=^M:dc=\EQ:dl=\EO:do=\EB:ei=:ho=\EH:\
	:ic=\ER\EP\EM:im=:is=\EGB\E(@B@@\E):k1=\Ei1:k2=\Ei2:\
	:k3=\Ei3:k4=\Ei4:k5=\Ei5:k6=\Ei6:k7=\Ei7:k8=\Ei8:\
	:k9=\Ei9:kA=\EN:kD=\EQ:kI=\EP:kL=\EO:kd=\EB:kl=\ED:\
	:kr=\EC:ku=\EA:le=\ED:mb=\E4P:me=\E4@:mk=\E4H:\
	:mr=\E4B:nd=\EC:se=\E4@:sf=\Ea:so=\E4A:sr=\Eb:\
	:ue=\E4@:up=\EA:us=\E4D:ve=\E4@:
ti926|Texas Instruments 926 VDT 8859/1 7 bit CTRL:\
	:cs@:sf=\E[1S:sr=\E[1T:tc=ti924:
ti926-8|Texas Instruments 926 VDT 8859/1 8 bit CTRL:\
	:cs@:sf=S\2331>:sr=T\2331>:tc=ti924-8:
ti_ansi|basic entry for ti928:\
	:am:eo:ut:xn:xo:\
	:Co#8:co#80:it#8:li#25:pa#64:\
	:@7=\E[F:Sb=\E[4%dm:Sf=\E[3%dm:al=\E[L:bl=^G:bt=\E[Z:\
	:cd=\E[J:ce=\E[K:cl=\E[2J\E[H:cm=\E[%i%d;%dH:cr=^M:\
	:cs=\E[%i%d;%dr:dc=\E[P:dl=\E[M:do=\E[B:ei=:ho=\E[H:\
	:ic=\E[@:im=:k0=\E[V:k1=\E[M:k2=\E[N:k3=\E[O:k4=\E[P:\
	:k5=\E[Q:k6=\E[R:k7=\E[S:k8=\E[T:k9=\E[U:kN=\E[G:\
	:kP=\E[I:kb=^H:kd=\E[B:kh=\E[H:kl=\E[D:kr=\E[C:\
	:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:me=\E[m:nd=\E[C:\
	:op=\E[37;40m:se=\E[m:sf=\E[S:so=\E[7m:sr=\E[T:ta=^I:\
	:ue=\E[m:up=\E[A:us=\E[4m:
#
#       928 VDT 7 bit control mode
#
ti928|Texas Instruments 928 VDT 8859/1 7 bit CTRL::\
	:%9=\E[35~:@7=\E_1\E\\:@8=\E[8~:F1=\E[29~:F2=\E[31~:\
	:F3=\E[32~:F5=\E[34~:k1=\E[17~:k2=\E[18~:k3=\E[19~:\
	:k4=\E[20~:k5=\E[21~:k6=\E[23~:k7=\E[24~:k8=\E[25~:\
	:k9=\E[26~:k;=\E[28~:kD=\E[P:kI=\E[@:kN=\E[S:kP=\E[T:tc=ti_ansi:
#
#       928 VDT 8 bit control mode
#
ti928-8|Texas Instruments 928 VDT 8859/1 8 bit CTRL::\
	:%9=\23335~:@7=\2371\234:@8=\2338~:F1=\23329~:\
	:F2=\23331~:F3=\23332~:F5=\23334~:k1=\23317~:\
	:k2=\23318~:k3=\23319~:k4=\23320~:k5=\23321~:\
	:k6=\23323~:k7=\23324~:k8=\23325~:k9=\23326~:\
	:k;=\23328~:kD=\233P:kI=\233@:kN=\233S:kP=\233T:\
	:kh=\233H:tc=ti_ansi:

#### Zentec (zen)
#

# (zen30: removed obsolete ":ma=^L ^R^L^K^P:" -- esr)
zen30|z30|zentec 30:\
	:am:bs:mi:ul:\
	:co#80:li#24:\
	:al=\EE:bl=^G:cd=\EY:ce=\ET:cl=\E*:cm=\E=%+ %+ :\
	:cr=^M:dc=\EW:dl=\ER:do=^J:ei=\Er:ho=^^:im=\Eq:le=^H:\
	:nd=^L:se=\EG0:sf=^J:so=\EG6:up=^K:
# (zen50: this had unknown capabilities
#	:BS=^U:CL=^V:CR=^B:
# UK/DK/RK/LK/HM were someone's aliases for ku/kd/kl/kr/kh,
# which were also in the original entry -- esr)
# (zen50: removed obsolete ":ma=^Hh^Ll^Jj^Kk:" -- esr)
zen50|z50|zentec zephyr:\
	:am:bs:\
	:co#80:li#24:sg#1:\
	:al=\EE:cd=\EY:ce=\ET:cl=\E+:cm=\E=%+ %+ :dc=\EW:\
	:dl=\ER:ei=:ic=\EQ:im=:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:\
	:se=\EGO:so=\EG4:up=^K:

######## OTHER OBSOLETE TYPES
#
# These terminals are *long* dead -- these entries are retained for
# historical interest only.

#### Obsolete non-ANSI software emulations
#

# CTRM terminal emulator
# 1. underlining is not allowed with colors: first, is is simulated by 
# black on white, second, it disables background color manipulations.
# 2. BLINKING, REVERSE and BOLD are allowed with colors,
# so we have to save their status in the static registers A, B and H
# respectively, to be able to restore them when color changes
# (because any color change turns off ALL attributes)
# 3. "enter_bold_mode" and "enter_reverse_mode" sequences alternates modes,
# rather then simply  entering them.  Thus we have to check the
# static register B and H to determine the status, before sending the 
# escape sequence.
# 4. sgr0 now must set the status of all 3 register (A,B,H) to zero
# and then reset colors
# 5. implementation of the protect mode would badly penalize the performance.
# we would have to use \E&bn sequence to turn off colors (as well as all
# other attributes), and keep the status of protect mode in yet another
# static variable.  If someone really need this mode, they would have to
# create another terminfo entry.
# 6. original color-pair is white on black.
# store the information about colors into static registers
# 7. set foreground color.  it performs the following steps.
#   1) turn off all attributes
#   2) turn on the background and video attribues that have been turned
#      on before (this information is stored in static registers X,Y,Z,A,B,H,D).
#   3) turn on foreground attributes
#   4) store information about foreground into U,V,W static registers
# 8. turn on background: similar to turn on foreground above
ctrm|C terminal emulator:\
	:am:ut:xo:\
	:Co#8:NC#2:Nl#0:co#80:lh#0:li#24:lm#0:lw#0:pa#63:\
	:pb#19200:vt#6:\
	:..Sb=\E&bn\n%?%gA%t\E&dA%;\n%?%gB%t\E&dB%;\n%?%gH%t\E&dH%;\n%?%gU%t\E&bR%;\n%?%gV%t\E&bG%;\n%?%gW%t\E&bB%;\n\n%?%p1%{1}%&%t\E&bb%{1}%e%{0}%;%PZ\n%?%p1%{2}%&%t\E&bg%{1}%e%{0}%;%PY\n%?%p1%{4}%&%t\E&br%{1}%e%{0}%;%PX:\
	:..Sf=\E&bn\n%?%gA%t\E&dA%;\n%?%gB%t\E&dB%;\n%?%gH%t\E&dH%;\n%?%gX%t\E&br%;\n%?%gY%t\E&bg%;\n%?%gZ%t\E&bb%;\n\n%?%p1%{1}%&%t\E&bB%{1}%e%{0}%;%PW\n%?%p1%{2}%&%t\E&bG%{1}%e%{0}%;%PV\n%?%p1%{4}%&%t\E&bR%{1}%e%{0}%;%PU:\
	:al=\EL:bl=^G:bt=\Ei:cd=\EJ:ce=\EK:ch=\E&a%dC:\
	:cl=\EH\EJ:cm=\E&a%r%dc%dY:cr=^M:ct=\E3:cv=\E&a%dY:\
	:dc=\EP:dl=\EM:do=^J:ei=\ER:im=\EQ:ip=:is=\E&jA\r:\
	:k1=\Ep\r:k2=\Eq\r:k3=\Er\r:k4=\Es\r:k5=\Et\r:\
	:k6=\Eu\r:k7=\Ev\r:k8=\Ew\r:kb=^H:kd=\Ew\r:ke=\E&jA:\
	:kh=\Ep\r:kl=\Eu\r:kr=\Ev\r:ks=\E&jB:ku=\Et\r:le=^H:\
	:mb=\E&dA%{1}%PA:md=%?%gH%{0}%=%t\E&dH%{1}%PH%;:\
	:me=\E&d@%{0}%PA%{0}%PB%{0}%PH:\
	:mr=%?%gB%{0}%=%t\E&dB%{1}%PB%;:nd=\EC:\
	:op=\E&bn\E&bB\E&bG\E&bR\n%{0}%PX%{0}%PY%{0}%PZ\n%{1}%PW%{1}%PV%{1}%PU:\
	:..sa=\E&d@%{0}%PA%{0}%PB%{0}%PD%{0}%PH\n%?%p1%p3%p5%|%|%t\E&dB%{1}%PB%;\n%?%p4%t\E&dA%{1}%PA%;\n%?%p6%t\E&dH%{1}%PH%;\n%?%p2%t\E&dD%;:\
	:sf=^J:so=\E&dD:st=\E1:ta=\011:up=\EA:us=\E&dD:

# gs6300 - can't use blue foreground, it clashes with underline;
# it's simulated with cyan
gs6300|emots|AT&T PC6300 with EMOTS Terminal Emulator:\
	:am:ms:ut:xo:\
	:Co#8:co#80:it#8:li#24:pa#63:\
	:AL=\E[%dL:DC=\E[%dP:DL=\E[%dM:DO=\E[%dB:IC=\E[%d@:\
	:LE=\E[%dD:LF=\E|:RI=\E[%dC:Sb=\E[?;%dm:\
	:..Sf=\E[?%?%p1%{0}%=%t0\n%e%p1%{1}%=%t2\n%e%p1%{1}%-%d%;m:\
	:UP=\E[%dA:\
	:ac=\\\054\\\054..--++``aaffgghhiijjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=\E[10m:al=\E[L:as=\E[11m:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:dc=\E[P:dl=\E[M:\
	:do=^J:ei=:ho=\E[H:ic=\E[@:im=:is=\E[0m:k1=\E[0s:\
	:k2=\E[24s:k3=\E[1s:k4=\E[23s:k5=\E[2s:k6=\E[22s:\
	:k7=\E[3s:k8=\E[21s:kB=^R^I:kb=^H:kd=\E[B:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:mb=\E[5m:md=\E[1m:\
	:me=\E[m\E[10m:mr=\E[7m:nd=\E[C:op=\E[?;m:pf=\E[4i:\
	:po=\E[5i:r1=\Ec:sf=^J:so=\E[1m:sr=\E[L:ta=^I:\
	:up=\E[A:us=\E[4m:

# From: <earle@smeagol.UUCP> 29 Oct 85 05:40:18 GMT
# MS-Kermit with Heath-19 emulation mode enabled
# (h19k: changed ":pt@:" to ":it@"
h19k|h19kermit|heathkit emulation provided by Kermit (no auto margin):\
	:am@:da:db:xt:\
	:it@:\
	:ta@:tc=h19-u:

# pc52 - can't use blue foreground, it clashes with underline;
# it's simulated with cyan
# bold means: white on black bold, so it not allowed with colors
# rev means: black on white, also not allowed
# smso and dim are simulated with colors, ditto
# smul is allowed, even though it always means white foreground:
# it is too important to leave out.
pc52|dec vt52 for PC:\
	:am:ms:ut:\
	:Co#8:NC#53:co#80:it#8:li#25:pa#63:\
	:Sb=\Ec%d:..Sf=\Eb%?%p1%{1}%=%t3\n%e%p1%d%;:al=\EL:\
	:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\EY%+ %+ :cr=^M:\
	:dl=\EM:do=^J:k1=\Ea:k2=\Eb:k3=\Ec:k4=\Ed:k5=\Ee:\
	:k6=\Ef:k7=\Eg:k8=\Eh:k9=\Ei:k;=\Ej:kb=^H:kd=\ED:\
	:kl=\EL:kr=\ER:ku=\EU:le=^H:mb=\Eo:md=\Ebo\Ec0:\
	:me=\Eb7\Ec0\Et:mh=\Eb3\Ec0:mr=\Ep:nd=\EC:\
	:op=\Eb7\Ec0:se=\Eb7\Ec0:sf=^J:so=\Eb6\Ec4:sr=\EI:\
	:ta=^I:up=\EA:us=\Es:

# vs100 emulator using tsim
# From: <lai@decwrl.dec.com>
# (vs100t: had Al/Dl in front of obvious AL/DL capabilities;
# also mapped ":pt:" to default tabs -- esr)
vs100t|tsim|vs100-tsim:\
	:am:bs:pt:\
	:co#80:li#24:\
	:AL=\E+%+ :DL=\E-%+ :al=\EI:cd=\EQ:ce=\EL:cl=\EE:\
	:cm=\EM%+ %+ :cs=\ES%+ %+ :dc=\Ed:dl=\ED:do=^J:ei=:\
	:ho=\EH:ic=\Ei:im=:is=\ER:nd=\En:rs=\ER:se=\Er:\
	:so=\Eh:ue=\Ev:up=^K:us=\Eu:

# From: Rick Thomas <ihnp4!btlunix!rbt>
xtalk|IBM PC with xtalk communication program (versions up to 3.4):\
	:am:mi:ms:xo:\
	:co#80:it#8:li#24:sg#1:vt#3:\
	:@8=\EOM:DO=\E[%dB:K1=\EOq:K2=\EOr:K3=\EOs:K4=\EOp:\
	:K5=\EOn:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:al=\E[L:as=^N:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:ct=\E[3g:dl=\E[M:\
	:do=^J:eA=\E(B\E)0:ho=\E[H:k0=\EOy:k1=\EOP:k2=\EOQ:\
	:k3=\EOR:k4=\EOS:k5=\EOt:k6=\EOu:k7=\EOv:k8=\EOl:\
	:k9=\EOw:k;=\EOx:kb=^H:kd=\EOB:ke=\E[?1l\E>:kl=\EOD:\
	:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:nd=\E[C:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:se=\E[m :sf=^J:\
	:so=\E[7m :sr=\EM:st=\EH:ta=^I:up=\E[A:

# YTERM standard version 1.0.
# Straight old ascii keyboard except function keys are Yale (e.g.,ASCII.KBD).
# Only 80 tab columns (else yterm 1.1 bug).  No :xn: in 1.0.
# Cannot use termcap :sr=\EM: because vi will not work, too bad.
# vi string is given so that yterm is reset each vi startup.
# (yterm10: removed obsolete ":EP:" and ":ma=h^JjklH:" capabilities;
# mapped ":pt:" to default tabs -- esr)
# From: greg small <gts@populi.berkeley.edu> 9-25-84
yterm10|yterm 1.0 UCB ascii.kbd:\
	:am:bs:pt:\
	:co#80:li#24:\
	:cd=^K:ce=^]:cl=^L:cm=\036%r%+ %+ :ho=^Y:\
	:is=\017\E[7i\E[m\E[?7h\E[?3g\r\EHY0  for \EHYTERM 1.\EH0 with A\EHSCII.KBD\EH 9-13-84\EH        \EH        \EH        \EH        \EH\n:\
	:k0=\E0:k1=\E1:k2=\E2:k3=\E3:k4=\E4:k5=\E5:k6=\E6:\
	:k7=\E7:k8=\E8:k9=\E9:kd=^J:kh=^^:kl=^H:kr=^L:ku=^K:\
	:nd=^\:rc=\E8:sc=\E7:se=\E[m:so=\E[7m:ue=\E[m:up=^_:\
	:us=\E[4m:\
	:vs=\017\E[7i\E[m\E[?7h\E[?3g\r\EHY0      \EH        \EH        \EH        \EH        \EH        \EH        \EH        \EH        \EH\r:
# YTERM variant version 1.1.  Version 1.1 has :xn:.
# From: greg small <gts@populi.berkeley.edu> 9-13-84
yterm11|yterm 1.1 UCB ascii.kbd:\
	:xn:\
	:is=\017\E[7i\E[m\E[?7h\E[?3g\r\EHY1  for \EHYTERM 1.\EH1 with A\EHSCII.KBD\EH 9-13-84\EH        \EH        \EH        \EH        \EH\n:tc=yterm10:
# YTERM 1.0 variant no autowrap or tabs
# X does not remember autowrap or tabs when T is deleted and restarted.
# (yterm: changed ":pt@:" to ":it@:" -- esr)
yterm10nat|yterm 1.0 UCB ascii.kbd no autowrap or tabs:\
	:am@:\
	:it@:\
	:is=\017\E[7i\E[m\E[?7l\E[?3g\rY2  for YTERM 1.0 with ASCII.KBD 9-20-84 no autowrap or tabs\n:\
	:vs=\017\E[7i\E[m\E[?7l\E[?3g\rY2\r:tc=yterm10:

# The official PC terminal emulator program of the AT&T Product Centers.
# Note - insert mode commented out - doesn't seem to work on AT&T PC.
simterm|attpc running simterm:\
	:am:\
	:co#80:li#24:\
	:al=\EL:bl=^G:cd=\EJ:ce=\EK:cl=\EH\EJ:cm=\E=%+ %+ :\
	:cr=^M:dc=\ER:dl=\EM:do=\EB:ho=\EH:im=\EQ:le=^H:\
	:nd=\EC:sf=^J:so=\E&dB:te=\EVE:ti=\EVS:up=\EA:

#### Daisy wheel printers
#

# This section collects Diablo, DTC, Xerox, Qume, and other daisy
# wheel terminals.  These are now largely obsolete.
#
# This is an "experimental" entry for the SRI Agiles.
# It has been tried in a minimal way -- the Agile did not blow up!
# However, it has not been exhaustively tested.
# Anyone who tries it and finds it wanting should get in touch with:
# From: Ralph Keirstead <ralph@sri-unix>
#	EK352; SRI International; 333 Ravenswood Avenue; Menlo Park, CA 94025
# (agile: I removed an incorrect ":pl:" -- esr)
agile|agiles|sri agiles:\
	:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:ct=\E2:do=^J:hd=\E9:hu=\E0:is=\EE\EF\EJ:\
	:kb=^H:le=^H:sf=^J:st=\E1:ta=^I:up=\E^J:
# (1620: mapped ":pt:" to default tabs -- esr)
diablo1620|diablo1720|diablo450|ipsi|diablo 1620:\
	:bs:hc:os:pt:\
	:co#132:\
	:ch=\E\011%i%.:ct=\E2:do=^J:hd=\ED:hu=\EU:\
	:if=/usr/share/tabset/xerox1720:kb=^H:le=^H:st=\E1:\
	:up=\E^J:
diablo1620-m8|diablo1640-m8|diablo 1620 w/8 column left margin:\
	:co#124:\
	:do=^J:is=\r        \E9:tc=diablo1620:
diablo1640|diablo1730|diablo1740|diablo630|x1700|diablo|xerox|diablo 1640:\
	:bl=^G:if=/usr/share/tabset/xerox1730:se=\E&:so=\EW:\
	:ue=\ER:us=\EE:tc=diablo1620:
diablo1640-lm|diablo-lm|xerox-lm|diablo 1640 with indented left margin:\
	:co#124:\
	:if=/usr/share/tabset/xerox1730-lm:se=\E&:so=\EW:\
	:ue=\ER:us=\EE:tc=diablo1620:
diablo1740-lm|630-lm|1730-lm|x1700-lm:\
	:tc=diablo1640-lm:
# DTC 382 with VDU.  Has no :cd: so we fake it with :ce:.  Standout
# (so="^P \002^PF:") works but won't go away without dynamite (":se=^P \200:").
# The terminal has tabs, but I'm getting tired of fighting the braindamage. 
# If no tab is set or the terminal's in a bad mood, it glitches the screen
# around all of memory.  Note that return puts a blank ("a return character")
# in the space the cursor was at, so we use ^P return (and thus ^P newline for
# newline).  Note also that if you turn off pt and let Unix expand tabs,
# curses won't work (current version) because it doesn't turn off this bit,
# and cursor addressing sends a tab for row/column 9.  What a losing terminal!
# I have been unable to get tabs set in all 96 lines - it always leaves at
# least one line with no tabs in it, and once you tab through that line,
# it completely weirds out.
dtc382|DTC 382:\
	:am:da:db:xs:\
	:co#80:li#24:lm#96:\
	:al=^P^Z:bl=^G:cd=\020\025\020\023\020\023:ce=^P^U:\
	:cl=\020\035:cm=\020\021%r%.%.:cr=^P^M:dc=^X:dl=^P^S:\
	:ei=^Pi:ho=^P^R:im=^PI:le=^H:nd=^PR:pc=\177:sf=^J:\
	:te=\020\035:ue=^P \200:up=^P^L:us=^P ^P:ve=^Pb:\
	:vs=^PB:
dtc300s|DTC 300s:\
	:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:ct=\E3:do=^J:ff=^L:hd=\Eh:hu=\EH:kb=^H:\
	:le=^H:sf=^J:st=\E1:ta=^I:up=^Z:
gsi:\
	:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:hd=\Eh:hu=\EH:le=^H:sf=^J:ta=^I:\
	:up=^Z:
aj830|aj832|aj|anderson jacobson:\
	:bs:hc:os:\
	:bl=^G:cr=^M:do=^J:hd=\E9:hu=\E8:le=^H:sf=^J:up=\E7:
# From: Chris Torek <chris@gyre.umd.edu> Thu, 7 Nov 85 18:21:58 EST
aj510|AJ510|Anderson-Jacobson model 510:\
	:am:bs:mi:\
	:co#80:li#24:\
	:al=2*\E&I:cd=\E'P:ce=\E'L:cl=^L:cm=\E#%+ %+ :\
	:dc=.1*\E'D:dl=2*\E&D:ei=\E'J:ic=:im=\E'I:ip=.1*:\
	:kd=\EZ:kl=\EW:kr=\EX:ku=\EY:nd=\EX:pc=\177:se=\E"I:\
	:so=\E"I:te=\E"N:ti=\E"N:ue=\E"U:up=\EY:us=\E"U:
# From: <cbosg!ucbvax!pur-ee!cincy!chris> Thu Aug 20 09:09:18 1981
# This is incomplete, but it's a start.
# (5520: mapped ":pt:" to default tabs -- esr)
nec5520|nec|spinwriter|nec 5520:\
	:bs:hc:os:pt:\
	:co#132:\
	:bl=^G:cr=^M:ct=\E3:do=^J:ff=^L:hd=\E]s\n\E]W:\
	:hu=\E]s\E9\E]W:kb=^H:le=^H:sf=^J:st=\E1:ta=^I:\
	:up=\E9:
# (qume5: mapped ":pt:" to default tabs -- esr)
qume5|qume|Qume Sprint 5:\
	:bs:hc:os:pt:\
	:co#80:\
	:bl=^G:cr=^M:ct=\E3:do=^J:ff=^L:hd=\Eh:hu=\EH:kb=^H:\
	:le=^H:sf=^J:st=\E1:ta=^I:up=^Z:
# I suspect the xerox1720 is the same as the diablo 1620.
# (x1720: mapped ":pt:" to default tabs -- esr)
xerox1720|x1720|x1750|xerox 1720:\
	:bs:hc:os:pt:\
	:co#132:\
	:bl=^G:cr=^M:ct=\E2:do=^J:ff=^L:le=^H:sf=^J:st=\E1:\
	:ta=^I:

#### Miscellaneous obsolete terminals, manufacturers unknown
#
# If you have any information about these (like, a manufacturer's name, 
# and a date on the serial-number plate) please send it!

cad68-3|cgc3|cad68 basic monitor transparent mode size 3 chars:\
	:am:bs:\
	:co#73:li#36:\
	:cl=^Z:ho=^^:nd=^L:up=^K:
cad68-2|cgc2|cad68 basic monitor transparent mode size 2 chars:\
	:am:bs:\
	:co#85:li#39:\
	:cl=^Z:ho=^^:k1=\E5:k2=\E6:k3=\E7:k4=\E8:kd=\E2:\
	:kl=\E3:kr=\E4:ku=\E1:nd=^L:se=\Em^C:so=\Em^L:up=^K:
cdi|cdi1203:\
	:am:bs:hc:os:\
	:co#80:\
	:bl=^G:cr=\r:do=^J:le=^H:sf=^J:
cops10|cops|cops-10:\
	:am:bw:\
	:co#80:li#24:\
	:bl=^G:cd=^W:ce=^V:cl=30^X:cm=\020%+ %+ :cr=^M:do=^J:\
	:kb=^H:kd=^J:kh=^Y:kl=^H:kr=^L:ku=^K:le=^H:nd=^L:\
	:sf=^J:up=^K:
# (d132: removed duplicate ":ic=\E5:" -- esr)
d132|datagraphix|datagraphix 132a:\
	:da:db:in:\
	:co#80:li#30:\
	:al=\E3:bl=^G:cl=^L:cr=^M:dc=\E6:do=^J:ei=:ho=\Et:\
	:ic=\E5:im=:nd=\El:sf=\Ev:sr=\Ew:up=\Ek:ve=\Em\En:\
	:vs=\Ex:
# I'm told the d800 was an early portable terminal that looked a lot like the
# original Compaq portable.
# (d800: mapped ":pt:" to default tabs -- esr)
d800|Direct 800/A:\
	:am:bs:da:db:ms:pt:xs:\
	:co#80:li#24:\
	:ae=\E[0m:as=\E[1m:bl=^G:cd=\E[J:ce=\E[K:\
	:cl=\E[1;1H\E[2J:cm=\E[%i%d;%dH:cr=^M:do=^J:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\EOT:k6=\EOU:k7=\EOV:\
	:k8=\EOW:kd=\E[B:kl=\E[D:kr=\E[C:ku=\E[A:le=^H:\
	:nd=\E[C:se=\E[0m:sf=\ED:so=\E[7m:sr=\EM:ta=^I:\
	:ue=\E[0m:up=\E[A:us=\E[4m:ve=\E[>12h:vs=\E[>12l:
digilog|digilog 333:\
	:bs:\
	:co#80:li#16:\
	:bl=^G:ce=^X:cr=^M:do=^J:ho=^N:le=^H:nd=^I:sf=^J:\
	:up=^O:
env230|envision230|envision 230 graphics terminal:\
	:am:mi:ms:xo:\
	:co#80:it#8:li#24:vt#3:\
	:@8=\EOM:DO=\E[%dB:K1=\EOq:K2=\EOr:K3=\EOs:K4=\EOp:\
	:K5=\EOn:LE=\E[%dD:RI=\E[%dC:UP=\E[%dA:\
	:ac=``aaffggjjkkllmmnnooppqqrrssttuuvvwwxxyyzz{{||}}~~:\
	:ae=^O:as=^N:bl=^G:cb=\E[1K:cd=\E[J:ce=\E[K:\
	:cl=\E[H\E[J:cm=\E[%i%d;%dH:cr=^M:cs=\E[%i%d;%dr:\
	:ct=\E[3g:do=^J:eA=\E(B\E)0:ho=\E[H:k0=\EOy:k1=\EOP:\
	:k2=\EOQ:k3=\EOR:k4=\EOS:k5=\EOt:k6=\EOu:k7=\EOv:\
	:k8=\EOl:k9=\EOw:k;=\EOx:kb=^H:kd=\EOB:ke=\E[?1l\E>:\
	:kl=\EOD:kr=\EOC:ks=\E[?1h\E=:ku=\EOA:le=^H:mb=\E[5m:\
	:md=\E[1m:me=\E[m\017:mr=\E[7m:nd=\E[C:pf=\E[4i:\
	:po=\E[5i:ps=\E[0i:\
	:r2=\E>\E[?3l\E[?4l\E[?5l\E[?7h\E[?8h:rc=\E8:\
	:..sa=\E[%?%p1%t;1%;%?%p2%t;4%;%?%p3%t;7%;%?%p4%t;5%;%?%p6%t;1%;m:\
	:sc=\E7:se=\E[0m<2>:sf=^J:so=\E[1m<2>:sr=\EM:st=\EH:\
	:ta=^I:ue=\E[m:up=\E[A:us=\E[4m:
# These execuports were impact-printer ttys with a 30- or maybe 15-cps acoustic
# coupler attached, the whole rig fitting in a suitcase and more or less
# portable.  Hot stuff for c.1977 :-) -- esr
ep48|ep4080|execuport 4080:\
	:am:bs:os:\
	:co#80:\
	:bl=^G:cr=^M:do=^J:hd=^\:hu=^^:le=^H:sf=^J:
ep40|ep4000|execuport 4000:\
	:am:bs:os:\
	:co#136:\
	:bl=^G:cr=^M:do=^J:hd=^\:hu=^^:le=^H:sf=^J:
# From: Paul Leondis <unllab@amber.berkeley.edu>
ifmr|Informer D304:\
	:am:bs:\
	:co#80:li#24:\
	:cd=\E/:ce=\EQ:cl=\EZ:cm=\EY%r%+ %+ :dc=\E\\:do=^J:\
	:ei=:ho=\EH:ic=\E[:im=:nd=\EC:se=\EK:so=\EJ:sr=\En:\
	:up=\EA:
# This used to say "de#001202" which presumably refers to the stty bits
# that need to be set for some version of Unix.  We need the real delay
# requirements in MS.
mw2|Multiwriter 2:\
	:hc:os:\
	:co#132:\
	:bl=^G:cr=^M:do=^J:sf=^J:
# Entry largely based on wy60 and has the features of wy60ak.
opus3n1+|Esprit  Opus3n1+ in wy60 mode with ANSI arrow keys +:\
	:am:bw:hs:km:mi:ms:ul:xo:\
	:Nl#8:co#80:lh#1:li#24:lw#8:ws#80:\
	:#2=\E{:%9=\EP:&3=\Er:@7=\E[F:@8=\E7:F1=^AJ\r:\
	:F2=^AK\r:F3=^AL\r:F4=^AM\r:F5=^AN\r:F6=^AO\r:\
	:LF=\EA11:LO=\EA10:RA=\Ed.:RX=\Ec20:SA=\Ed/:SX=\Ec21:\
	:ac=0wa_h[jukslrmqnxqzttuyv]wpxv:ae=\EH^C:al=\EE:\
	:as=\EH^B:bl=^G:bt=\EI:cd=\EY:ce=\ET:cl=\E*:\
	:cm=\Ea%i%dR%dC:cr=^M:ct=\E0:dc=\EW:dl=\ER:do=^J:\
	:ds=\Ez(\r:ei=\Er:fs=^M:ho=\036:\
	:if=/usr/lib/tabset/std:im=\Eq:ip=:\
	:is=\E`\072\Ee(\EO\Ee6\Ec41\E~4\Ec21\Ed/\Ezz&\E[A\037\Ezz'\E[B\037\Ezz(\E[D\037\Ezz)\E[C\037\Ezz<\E[Q\037\Ezz`\E[F\037\EA1*\EZH12:\
	:k1=^A@\r:k2=^AA\r:k3=^AB\r:k4=^AC\r:k5=^AD\r:\
	:k6=^AE\r:k7=^AF\r:k8=^AG\r:k9=^AH\r:k;=^AI\r:kA=\EE:\
	:kB=\EI:kD=\EW:kE=\ET:kI=\EQ:kL=\ER:kN=\EK:kP=\EJ:\
	:kS=\EY:kb=^H:kd=\E[B:kh=^^:kl=\E[D:kr=\E[C:ku=\E[A:\
	:le=^H:mb=\EG2:me=\E(\EH\003\EG0\EcD:mh=\EGp:mk=\EG1:\
	:mp=\E):mr=\EG4:nd=^L:nw=\r\n:pf=^T:pl=\EZ2%+?%s\177:\
	:pn=\Ez%+/%s\r:po=^R:ps=\EP:px=\EZ1%+?%s\177:\
	:r1=\E~!\E~4:r2=\EeF:r3=\EwG\Ee(:\
	:..sa=%?%p8%t\E)%e\E(%;%?%p9%t\EH\002%e\EH\003%;\EG%'0'%?%p2%p6%|%t%{8}%|%;%?%p1%p3%|%p6%|%t%{4}%|%;%?%p4%t%{2}%|%;%?%p1%p5%|%t%{64}%|%;%?%p7%t%{1}%|%;%c:\
	:se=\EG0:sf=^J:so=\EG4:sr=\Ej:st=\E1:ta=\011:\
	:ti=\Ezz&\E[A\037\Ezz'\E[B\037\Ezz(\E[D\037\Ezz)\E[C\037\Ezz<\E[Q\037:\
	:ts=\Ez(:uc=\EG8%p1%c\EG0:ue=\EG0:up=^K:us=\EG8:\
	:ve=\E`1:vi=\E`0:
# (ps300: changed ":pt@:" to "it@" -- esr)
ps300|Picture System 300:\
	:xt:\
	:it@:\
	:se@:so@:ue@:us@:tc=vt100:
ramtek|ramtek 6000:\
	:am:\
	:co#78:li#24:\
	:bl=^G:cl=[alpha]\n[erase]\n:cr=^M:do=^J:le=^H:sf=^J:
# Upper case terminal, uses lower case for control sequences!!!
tec400|tec scope:\
	:sg#1:\
	:al=e:cd=s:ce=c:cl=f:..cm=l%p2%~%c%p1%~%c:dc=t:dl=u:\
	:do=h:ei=:ho=i:ic=d:im=:le=w:nd=g:se=|:so={:up=x:
# From: <ucbvax!geoff> Mon Sep 21 21:15:45 1981
# This entry has been tested.
tec500|tec 500:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cl=\032:cm=\E=%+ %+ :cr=^M:do=^J:ho=^^:le=^H:\
	:nd=^L:se=^\:sf=^J:so=^]:up=^K:
# tec is untested, and taken from CB/Unix virtual terminal driver.
# I would appreciate more information on this terminal, such as the
# manufacturer and the model number.  There are too many tecs in here.
# (tec: removed obsolete ":ma=^K^P^_ :" -- esr)
tec:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cl=^L:cr=^M:do=^J:ho=^^:le=^H:nd=^_:sf=^J:\
	:up=^K:
teletec|Teletec Datascreen:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cl=^L:cr=^M:do=^J:ho=^^:le=^H:nd=^_:sf=^J:\
	:up=^K:
# Terak made a PDP-11 based box with a bitmapped display that ran UCSD
# Pascal as the native O/S. It was quite a nice box, and there were several
# at Berkeley.
terak|Terak emulating Datamedia 1520:\
	:tc=dm1520:
# From: Mark Dornfeld <romwa@ucbvax.berkeley.edu>
#		This termcap is for the LANPAR Technologies VISION 3220
#	terminal.  The function key definitions k0-k5 represent the
#	edit keypad: FIND, INSERT HERE, REMOVE, SELECT, PREV SCREEN,
#	NEXT SCREEN. The key definitions k6-k9 represent the PF1 to
#	PF4 keys.
# (v3220: mapped ":pt:" to default tabs, removed obsolete ":kn#10:" -- esr)
v3220|LANPAR Vision II model 3220/3221/3222:\
	:am:bs:mi:pt:xn:\
	:co#80:li#24:\
	:al=\E[L:cd=\E[J:ce=\E[K:cl=\E[H\E[J:cm=\E[%i%d;%dH:\
	:dc=\E[P:dl=\E[M:ei=\E[4l:im=\E[4h:\
	:is=\E>\E[?3l\E[?7h\E[?8h\E[p:k0=\E[1~:k1=\E[2~:\
	:k2=\E[3~:k3=\E[4~:k4=\E[5~:k5=\E[6~:k6=\E[OP:\
	:k7=\E[OQ:k8=\E[OR:k9=\E[OS:kd=\E[B:ke=\E>:kh=\E[H:\
	:kl=\E[D:kr=\E[C:ks=\E=:ku=\E[A:nd=\E[C:se=\E[m:\
	:so=\E[7m:sr=\EM:ue=\E[m:up=\E[A:us=\E[4m:
# Does anybody know where these "wind" terminals came from?
wind:\
	:bs:\
	:co#80:li#24:\
	:cl=\EnP(\Eo:cm=\Ep%r%.%.:ho=\Ep\200\200:k1=\E5:\
	:k2=\E6:k3=\E7:k4=\E8:kd=\E2:kl=\E3:kr=\E4:ku=\E1:\
	:nd=^L:nl=^]:se=\Em^C:so=\Em^L:up=^K:
wind16:\
	:bs:\
	:co#80:li#16:\
	:cl=\EnP\020\Eo:cm=\Ep%r%.%.:ho=\Ep\200\200:nd=^L:\
	:nl=^]:se=\Em^C:so=\Em^L:up=^K:
wind40:\
	:bs:\
	:co#80:li#40:\
	:cl=\EnP(\Eo:cm=\Ep%r%.%.:ho=\Ep\200\200:nd=^L:nl=^]:\
	:se=\Em^C:so=\Em^L:up=^K:
# (wind50: corrected :cl=\EnP\128\062\Eo: -- esr)
wind50:\
	:bs:\
	:co#88:li#50:\
	:cl=\EnP2\Eo:cm=\Ep%r%.%.:ho=\Ep\200\200:k1=\E5:\
	:k2=\E6:k3=\E7:k4=\E8:kd=\E2:kl=\E3:kr=\E4:ku=\E1:\
	:nd=^L:nl=^]:se=\Em^C:so=\Em^L:up=^K:
# (xitex: removed obsolete ":ma=j^Jk^Pl :" -- esr)
xitex|xitex sct-100:\
	:bs:\
	:co#64:li#16:\
	:bl=^G:cd=\006\005:ce=\005:cl=\014:cm=\E=%+@%+@:\
	:cr=^M:do=^J:ho=^D:le=^H:nd=\E+@A:sf=^J:sr=\E=@@\013:\
	:up=^K:
plasma|plasma panel:\
	:am:bs:\
	:co#85:li#45:\
	:bl=^G:cl=^L:cr=^M:do=^J:ho=^^:le=^H:nd=^X:sf=^J:\
	:up=^V:

#### Homebrew and custom terminals
#

# Nu machine parameters taken from mit-vax.
# 						smc - 5/21/85
#
nuterminal:\
	:am:mi:ms:\
	:co#80:it#8:li#24:\
	:ae=\EG:al=1*\EL:as=\EF:cd=60\EJ:ce=10\EK:cl=60\EE:\
	:..cm=\EY%+ %+ :cr=^M:dc=2.5*\EN:dl=1*\EM:do=\EB:\
	:ei=\EO:ho=\EH:im=\E@:ip=2.5*:k1=\ES:k2=\ET:k3=\EU:\
	:k4=\EV:k5=\EW:k6=\EP:k7=\EQ:k8=\ER:kb=^H:kd=\EB:\
	:kh=\EH:kl=\ED:kr=\EC:ku=\EA:l6=blue:l7=red:l8=white:\
	:le=^H:nd=\EC:nw=^M^J:se=\Eq:sf=^J:so=\Ep:sr=\EI:\
	:ta=^I:up=\EA:ve=\Ey4:vs=\Ex4:
nu24|nuwindow:\
	:mi:ms:\
	:co#86:it#8:li#24:\
	:ae=\EG:al=1*\EL:as=\EF:cd=\EJ:ce=\EK:cl=\EE:\
	:..cm=\EY%+ %+ :cr=^M:dl=1*\EM:do=\EB:ei=\EO:ho=\EH:\
	:im=\E@:ip=2.5*:kb=^H:kd=\EB:kh=\EH:kl=\ED:kr=\EC:\
	:ku=\EA:le=^H:nd=\EC:nw=^M^J:se=\Eq:sf=^J:so=\Ep:\
	:sr=\EI:ta=^I:up=\EA:ve=\Ey4:vs=\Ex4:
bnu|nu51|bnuwindow:\
	:co#86:li#51:\
	:tc=nuterminal:
fnu|nu61|fnuwindow:\
	:co#86:li#61:\
	:tc=nuterminal:
nunix-30|nu-telnet-30|nu-half -- Half nu screen thru telnet:\
	:am:\
	:co#78:it#8:li#30:\
	:al=\EL:cd=\EJ:ce=\EK:cl=\EE:..cm=\EY%+ %+ :cr=^M:\
	:dl=\EM:do=\EB:ho=\EH:ip=2.5*:kb=^H:kd=^J:kl=^H:\
	:le=^H:nd=\EC:nw=^M^J:se=\Eq:sf=^J:so=\Ep:sr=\EI:\
	:ta=^I:up=\EA:
nunix-61|nu-telnet-61|nu-full| Full nu screen thru telnet:\
	:co#78:li#61:\
	:tc=nunix-30:

bch|bc|bill croft homebrew:\
	:am:bs:\
	:co#96:li#72:\
	:cl=^Z:cm=\E=%+ %+ :do=^J:ho=^^:le=^H:nd=^L:up=^K:\
	:vb=:
nucterm|rayterm|NUC homebrew:\
	:am:bs:\
	:co#80:li#24:\
	:bl=^G:cd=^E:ce=^A:cl=\014:cr=^M:do=^J:ho=^B:le=^H:\
	:ll=^K:nd=^C:sf=^J:up=^N:
carlock|klc:\
	:am:bs:\
	:co#80:li#24:\
	:al=^E:bl=^G:ce=^U:cl=\032:cm=\E=%+ %+ :cr=^M:\
	:dc=\177:dl=^D:do=^J:ei=^T:ho=^^:im=^T:nd=^L:se=^V:\
	:sf=^J:so=^V:up=^K:vb=\EV\EV:
# uVAX
qdss|qdcons|qdss glass tty:\
	:am:bs:\
	:co#128:li#57:\
	:cl=1\032:cm=\E=%.%.:do=^J:le=^H:nd=^L:up=^K:
# (ubell: removed obsolete ":ma=j^Jk^P^K^Pl :";
# mapped ":pt:" to default tabs; removed obsolete ":bc=^Y:" -- esr)
ubell|ubellchar:\
	:am:bs:pt:\
	:co#80:li#24:\
	:bl=^G:ce=\Ed:cl=^Z:cm=\E=%+ %+ :cr=^M:do=^J:ho=^^:\
	:le=^H:nd=^L:sf=^J:ta=^I:up=^K:
ttywilliams:\
	:am:\
	:co#80:li#12:\
	:bl=^G:ce=^_:cl=^^:cr=^M:do=^K:ho=^]:le=^Y:nd=^X:\
	:sf=^J:up=^Z:
######## ICH/ICH1 VERSUS RMIR/SMIR
#
# Some non-curses applications get confused if both ich/ich1 and rmir/smir
# are present; the symptom is doubled characters in an update using insert.
# These applications are technically correct; in both 4.3BSD termcap and
# terminfo, you're not actually supposed to specify both ich/ich1 and rmir/smir
# unless the terminal needs both.  This requirement is now rare; most ich
# sequences do not require previous smir, and most smir insert modes do not
# require ich1 before each character.
#
# For ncurses-based applications this is not a problem, as ncurses uses
# one or the other as appropriate but never mixes the two.  Therefore we
# have not corrected entries like `linux' and `xterm' that specify both.
# If you see doubled characters from these, use the linux-nic and xterm-nic
# entries that suppress ich/ich1.
#
######## ANSI/VT100/PC-TERM TERMINAL STANDARDS
#
# ANSI Standard (X3.64) Control Sequences for Video Terminals and Peripherals
# 
# Most of the content of this comment is adapted from a table prepared by
# Richard Shuford, based on a 1984 Byte article.  Terminfo correspondences
# and discussion of some terminfo-related issues have been added.
#
# The table is a complete list of the defined ANSI X.364 control sequences.
# In the main table, \E stands for an escape (\033) character, SPC for space.
# Pn stands for a single numeric parameter to be inserted in decimal ASCII.
# Ps stands for a list of such parameters separated by semicolons
#
#                                                   Default    Type
# Sequence     Sequence                             Parameter   or
# Mnemonic     Name              Sequence           Value      Mode   terminfo
# -----------------------------------------------------------------------------
# APC  Applicatn Program Command \E Fe               -         Delim  -
# CBT  Cursor Backward Tab       \E [ Pn Z           1         eF     cbt
# CCH  Cancel Previous Character \E T                -         -      -
# CHA  Cursor Horzntal Absolute  \E [ Pn G           1         eF     hpa (1)
# CHT  Cursor Horizontal Tab     \E [ Pn I           1         eF     tab (2)
# CNL  Cursor Next Line          \E [ Pn E           1         eF     nel (3)
# CPL  Cursor Preceding Line     \E [ Pn F           1         eF     -
# CPR  Cursor Position Report    \E [ Pn ; Pn R      1, 1      -      -
# CSI  Control Sequence Intro    \E [                -         Intro  -
# CTC  Cursor Tab Control        \E [ Ps W           0         eF     -
# CUB  Cursor Backward           \E [ Pn D           1         eF     cub
# CUD  Cursor Down               \E [ Pn B           1         eF     cud
# CUF  Cursor Forward            \E [ Pn C           1         eF     cuf
# CUP  Cursor Position           \E [ Pn ; Pn H      1, 1      eF     cup (4)
# CUU  Cursor Up                 \E [ Pn A           1         eF     cuu
# CVT  Cursor Vertical Tab       \E [ Pn Y           -         eF     -
# DA   Device Attributes         \E [ Pn c           0         -      -
# DAQ  Define Area Qualification \E [ Ps o           0         -      -
# DCH  Delete Character          \E [ Pn P           1         eF     dch
# DCS  Device Control String     \E P                -         Delim  -
# DL   Delete Line               \E [ Pn M           1         eF     dl
# DMI  Disable Manual Input      \E \                -         Fs     -
# DSR  Device Status Report      \E [ Ps n           0         -      -
# EA   Erase in Area             \E [ Ps O           0         eF     -
# ECH  Erase Character           \E [ Pn X           1         eF     ech
# ED   Erase in Display          \E [ Ps J           0         eF     ed  (5)
# EF   Erase in Field            \E [ Ps N           0         eF     -
# EL   Erase in Line             \E [ Ps K           0         eF     el  (5)
# EMI  Enable Manual Input       \E b                          Fs     -
# EPA  End of Protected Area     \E W                -         -      -
# ESA  End of Selected Area      \E G                -         -      -
# FNT  Font Selection            \E [ Pn ; Pn SPC D  0, 0      FE     -
# GSM  Graphic Size Modify       \E [ Pn ; Pn SPC B  100, 100  FE     -
# GSS  Graphic Size Selection    \E [ Pn SPC C       none      FE     -
# HPA  Horz Position Absolute    \E [ Pn `           1         FE     (1)
# HPR  Horz Position Relative    \E [ Pn a           1         FE     (6)
# HTJ  Horz Tab w/Justification  \E I                -         FE     (2)
# HTS  Horizontal Tab Set        \E H                -         FE     hts
# HVP  Horz & Vertical Position  \E [ Pn ; Pn f      1, 1      FE     (4)
# ICH  Insert Character          \E [ Pn @           1         eF     ich
# IL   Insert Line               \E [ Pn L           1         eF     il
# IND  Index                     \E D                -         FE     -
# INT  Interrupt                 \E a                -         Fs     -
# JFY  Justify                   \E [ Ps SPC F       0         FE     -
# MC   Media Copy                \E [ Ps i           0         -      -
# MW   Message Waiting           \E U                -         -      -
# NEL  Next Line                 \E E                -         FE     nel (3)
# NP   Next Page                 \E [ Pn U           1         eF     -
# OSC  Operating System Command  \E ]                -         Delim  -
# PLD  Partial Line Down         \E K                -         FE     -
# PLU  Partial Line Up           \E L                -         FE     -
# PM   Privacy Message           \E ^                -         Delim  -
# PP   Preceding Page            \E [ Pn V           1         eF     -
# PU1  Private Use 1             \E Q                -         -      -
# PU2  Private Use 2             \E R                -         -      -
# QUAD Typographic Quadding      \E [ Ps SPC H       0         FE     -
# REP  Repeat Char or Control    \E [ Pn b           1         -      rep
# RI   Reverse Index             \E M                -         FE     -
# RIS  Reset to Initial State    \E c                -         Fs     -
# RM   Reset Mode                \E [ Ps l           none      -      -
# SD   Scroll Down               \E [ Pn T           1         eF     rin
# SEM  Select Edit Extent Mode   \E [ Ps Q           0         -      -
# SGR  Select Graphic Rendition  \E [ Ps m           0         FE     sgr (7)
# SL   Scroll Left               \E [ Pn SPC @       1         eF     -
# SM   Select Mode               \E [ Ps h           none      -      -
# SPA  Start of Protected Area   \E V                -         -      -
# SPI  Spacing Increment         \E [ Pn ; Pn SPC G  none      FE     -
# SR   Scroll Right              \E [ Pn SPC A       1         eF     -
# SS2  Single Shift 2 (G2 set)   \E N                -         Intro  -
# SS3  Single Shift 3 (G3 set)   \E O                -         Intro  -
# SSA  Start of Selected Area    \E F                -         -      -
# ST   String Terminator         \E \                -         Delim  -
# STS  Set Transmit State        \E S                -         -      -
# SU   Scroll Up                 \E [ Pn S           1         eF     indn
# TBC  Tab Clear                 \E [ Ps g           0         FE     tbc
# TSS  Thin Space Specification  \E [ Pn SC E        none      FE     -
# VPA  Vert Position Absolute    \E [ Pn d           1         FE     vpa
# VPR  Vert Position Relative    \E [ Pn e           1         FE     (8)
# VTS  Vertical Tabulation Set   \E J                -         FE     -
# 
# ---------------------------------------------------------------------------
#
# Notes:
#
# (1) There seems to be some confusion abroad between CHA and HPA.  Most
# `ANSI' terminals accept the CHA sequence, not the HPA. but terminfo calls
# the capability (hpa).
#
# (2) CHT corresponds to terminfo (tab).  Usually it has the value ^I.
# Occasionally (as on, for example, certain HP terminals) this has the HTJ
# value.
#
# (3) terminfo (nel) is usually \r\n rather than ANSI \EE.
#
# (4) CUP and HVP are identical in effect.  Some ANSI.SYS versions accept
# HVP, but always allow CUP as an alternate.
#
# (5) See the VT100 discussion for the meaning of the ED parameter.
# 
# (6) Some ANSI.SYS versions accept HPR, but more commonly `ANSI' terminals
# use CUF for this function and ignore HPR
#
# (7) In SGR, the ANSI.SYS values for attributes are now nearly universal.
#
# (8) Some ANSI.SYS versions accept VPR, but more commonly `ANSI' terminals
# use CUD for this function and ignore VPR.
#
# ---------------------------------------------------------------------------
# 
# Abbreviations:
#
# Intro  an Introducer of some kind of defined sequence; the normal 7-bit
#        X3.64 Control Sequence Introducer is the two characters "Escape ["
# 
# Delim  a Delimiter
# 
# x/y    identifies a character by position in the ASCII table (column/row)
# 
# eF     editor function (see explanation)
# 
# FE     format effector (see explanation)
# 
# F      is a Final character in
#             an Escape sequence (F from 3/0 to 7/14 in the ASCII table)
#             a control sequence (F from 4/0 to 7/14)
# 
# Gs     is a graphic character appearing in strings (Gs ranges from
#        2/0 to 7/14) in the ASCII table
# 
# Ce     is a control represented as a single bit combination in the C1 set
#        of controls in an 8-bit character set
# 
# C0     the familiar set of 7-bit ASCII control characters
# 
# C1     roughly, the set of control characters available only in 8-bit systems.
#        This is too complicated to explain fully here, so read Jim Fleming's
#        article in the February 1983 BYTE, especially pages 214 through 224.
# 
# Fe     is a Final character of a 2-character Escape sequence that has an
#        equivalent representation in an 8-bit environment as a Ce-type
#        (Fe ranges from 4/0 to 5/15)
# 
# Fs     is a Final character of a 2-character Escape sequence that is
#        standardized internationally with identical representation in 7-bit
#        and 8-bit environments and is independent of the currently
#        designated C0 and C1 control sets (Fs ranges from 6/0 to 7/14)
# 
# I      is an Intermediate character from 2/0 to 2/15 (inclusive) in the
#        ASCII table
# 
# P      is a parameter character from 3/0 to 3/15 (inclusive) in the ASCII
#        table
# 
# Pn     is a numeric parameter in a control sequence, a string of zero or
#        more characters ranging from 3/0 to 3/9 in the ASCII table
# 
# Ps     is a variable number of selective parameters in a control sequence
#        with each selective parameter separated from the other by the code
#        3/11 (which usually represents a semicolon); Ps ranges from
#        3/0 to 3/9 and includes 3/11
# 
# Format Effectors versus Editor Functions
# 
# A format effector specifies how following output is to be displayed.
# An editor function allows you to modify the display.  Informally
# format effectors may be destructive; format effectors should not be.
# 
# For instance, a format effector that moves the "active position" (the 
# cursor or equivalent) one space to the left would be useful when you want to
# create an overstrike, a compound character made of two standard characters
# overlaid. Control-H, the Backspace character, is actually supposed to be a
# format effector, so you can do this. But many systems use it in a
# nonstandard fashion, as an editor function, deleting the character to the
# left of the cursor and moving the cursor left. When Control-H is assumed to
# be an editor function, you cannot predict whether its use will create an
# overstrike unless you also know whether the output device is in an "insert
# mode" or an "overwrite mode". When Control-H is used as a format effector,
# its effect can always be predicted. The familiar characters carriage
# return, linefeed, formfeed, etc., are defined as format effectors.
#
# The ANSI Standard
# 
# The complete document describing the standard,  "ANSI X3.64-1979:
# Additional Controls for Use with the American National Standard
# Code for Information Interchange," can be ordered for $13.50 (plus
# $4 postage) from
# 
#      Standards Sales Department
#      American National Standards Institute
#      1430 Broadway
#      New York, NY 10018
#      212/354-3300
# 
# It's best to read the full standard before using it. It also helps
# to have copies of the related standards "X3.4-1977: American
# National Standard Code for Information Interchange" (the ASCII
# standard) and "X3.41.1974: Code-Extension Techniques for Use with
# the 7-Bit Coded Character Set of American National Standard for
# Information Interchange."
# 
# NOTES ON THE DEC VT100 IMPLEMENTATION
# 
# Control sequences implemented in the VT100 are as follows:
# 
#      CPR, CUB, CUD, CUF, CUP, CUU, DA, DSR, ED, EL, HTS, HVP, IND,
#      LNM, NEL, RI, RIS, RM, SGR, SM, TBC
# 
# plus several private DEC commands.
# 
# Erasing parts of the display (EL and ED) in the VT100 is performed thus:
# 
#      Erase from cursor to end of line           Esc [ 0 K    or Esc [ K
#      Erase from beginning of line to cursor     Esc [ 1 K
#      Erase line containing cursor               Esc [ 2 K
#      Erase from cursor to end of screen         Esc [ 0 J    or Esc [ J
#      Erase from beginning of screen to cursor   Esc [ 1 J
#      Erase entire screen                        Esc [ 2 J
# 
# The VT100 responds to receiving the DA (Device Attributes) control
# 
#      Esc [ c    (or Esc [ 0 c)
# 
# by transmitting the sequence
# 
#      Esc [ ? l ; Ps c
# 
# where Ps is a character that describes installed options.
# 
# The VT100's cursor location can be read with the DSR (Device Status
# Report) control
# 
#      Esc [ 6 n
# 
# The VT100 reports by transmitting the CPR sequence
# 
#      Esc [ Pl ; Pc R
# 
# where Pl is the line number and Pc is the column number (in decimal).
# 
# The specification for the DEC VT100 is document EK-VT100-UG-003.
# 
# NOTES ON `PC-TERM' COMPATIBILITY
#
# The MS-DOS ANSI.SYS driver has set the de-facto standard for attribute
# and color values in the SGR string.  These are as follows:
#
# 0	all attributes off
# 1	foreground bright
# 4	underscore on
# 5	blink on/background bright (not reliable with brown)
# 7	reverse-video
# 8	set blank (non-display)
# 10	set primary font
# 11	set first alternate font (on PCs, display ROM characters 1-31)
# 12	set second alternate font (on PCs, display IBM high-half chars)
#
#			Color attribute sets
# 3n	set foreground color       / 0=black, 1=red,     2=green, 3=brown,
# 4n	set background color       \ 4=blue,  5=magenta, 6=cyan,  7=white
# Bright black becomes gray.  Bright brown becomes yellow,
#	
# * Many VGA cards (such as the Paradise and compatibles) do the wrong thing
#   when you try to set a "bright brown" (yellow) background with attribute
#   5 (you get a blinking yellow foreground instead).  A few displays
#   (including the System V console) support an attribute 6 that undoes this
#   braindamage.
#
# * Some older versions of ANSI.SYS have a bug that causes thems to require
#   ESC [ Pn k as EL rather than the ANSI ESC [ Pn K.

######## NONSTANDARD CAPABILITY TRANSLATIONS USED IN THIS FILE
#
# The historical termcap file entries were written primarily in 4.4BSD termcap.
# The 4.4BSD termcap set was substantially larger than the original 4.1BSD set,
# with the extension names chosen for compatibility with the termcap names
# assigned in System V terminfo.  There are some variant extension sets out
# there.  We try to describe them here.
#
# XENIX extensions:
#
# The XENIX extensions include a set of function-key capabilities as follows:
#
#       code	XENIX variable name	terminfo name	name clashes?
#	----	-------------------	-------------	-----------------------
#	CL	key_char_left
#	CR	key_char_right
#	CW	key_change_window			create_window
#	EN	key_end          	kend
#	HM	key_home		khome
#	HP	??
#	LD	key_delete_line  	kdl1
#	LF	key_linefeed     			label_off
#	NU	key_next_unlocked_cell
#	PD	key_page_down   	knp
#	PL	??
#	PN	start_print		mc5
#	PR	??
#	PS	stop_print		mc4
#	PU	key_page_up     	kpp		pulse
#	RC	key_recalc				remove_clock
#	RF	key_toggle_ref				req_for_input
#	RT	key_return      	kent
#	UP	key_up_arrow           	kcuu1   	parm_up_cursor
#	WL	key_word_left
#	WR	key_word_right
#
# The XENIX extensions also include the following character-set and highlight
# capabilities:
#
#	XENIX	terminfo	function
#	-----	--------	------------------------------
#	GS	smacs		start alternate character set
#	GE	rmacs		end alternate character set
#	GG			:as:/:ae: glitch (analogous to :sg:/:ug:)
#	bo	blink		begin blink (not used in /etc/termcap)
#	be			end blink (not used in /etc/termcap)
#	bb			blink glitch  (not used in /etc/termcap)
#	it	dim		begin dim (not used in /etc/termcap)
#	ie			end dim (not used in /etc/termcap)
#	ig			dim glitch  (not used in /etc/termcap)
#
# XENIX also supposedly uses the following forms-drawing capabilities:
#
#	single	double type
#	------	------	-------------
#	gv	GV	vertical line (|)
#	gh	GH	horizontal line (-)
#	g1	G1	top right corner
#	g4	G4	bottom right corner (_|)
#	g2	G2	top left corner
#	g3	G3	bottom left corner (|_)
#	gd	GD	down-tick character (T)
#	gl	GL	left-tick character (-|)
#	gr	GR	right-tick character (|-)
#	gc	GC	middle intersection (-|-)
#	gu	GU	up-tick character (_|_)
#
# However, there is some confusion about case.  The scoansi entry uses
# mixed-case versions of these, and the historical ibmpcx, lisa, trs16, and fos
# entries have only the uppercase versions.  Accordingly, the ncurses tools
# don't try to translate these.
#
# AT&T Extensions:
#
# The old AT&T 5410, 5420, 5425, pc6300plus, 610, and s4 entries used a set of
# nonstandard capabilities.  Its signature is the KM capability, used to name
# some sort of keymap file.  EE, BO, CI, CV, XS, DS, FL and FE are in this
# set.  Comments in the original, and a little cross-checking with other AT&T
# documentation, seem to establish that BO=:mr: (start reverse video), DS=:mh:
# (start dim), XS=:mk: (secure/invisible mode), EE=:me: (end highlights),
# FL=:LO: (enable soft labels), FE=:LF: (disable soft labels), CI=:vi: (make
# cursor invisible), and CV=:ve: (make cursor normal).
#
# TC Extensions:
#
# There is a set of extended termcaps associated with something
# called the "Terminal Control" or TC package created by MainStream Systems,
# Winfield Kansas.  This one also uses GS/GE for as/ae, and also uses
# CF for civis and CO for cvvis.  Finally, they define a boolean :ct:
# that flags color terminals.

######## CHANGE HISTORY
#
# 9.1.0 (Wed Feb  1 04:50:32 EST 1995):
#	* First terminfo master translated from 8.3.
# 9.2.0 (Wed Feb  1 12:21:45 EST 1995):
#	* Replaced Wyse entries with updated entries supplied by vendor.
# 9.3.0 (Mon Feb  6 19:14:40 EST 1995):
#	* Added contact & status info from G. Clark Brown <clark@sssi.com>.
# 9.3.1 (Tue Feb  7 12:00:24 EST 1995):
#	* Better XENIX keycap translation.  Describe TC termcaps.
#	* Contact and history info supplied by Qume.
# 9.3.2 (Sat Feb 11 23:40:02 EST 1995):
#	* Raided the Shufort FTP site for recent termcaps/terminfos.
#	* Added information on X3.64 and VT100 standard escape sequences.
# 9.3.3 (Mon Feb 13 12:26:15 EST 1995):
#	* Added a correct X11R6 xterm entry.
#	* Fixed terminfo translations of padding.
# 9.3.4 (Wed Feb 22 19:27:34 EST 1995):
#	* Added correct acsc/smacs/rmacs strings for vt100 and xterm.
#	* Added u6/u7/u8/u9 capabilities.
#	* Added PCVT entry.
# 9.3.5 (Thu Feb 23 09:37:12 EST 1995):
#	* Emacs uses :so:, not :mr:, for its mode line.  Fix linux entry
#	  to use reverse-video standout so Emacs will look right.
#	* Added el1 capability to ansi.
#	* Added smacs/rmacs to ansi.sys.
# 9.4.0 (Sat Feb 25 16:43:25 EST 1995):
#	* New mt70 entry.
#	* Added COPYRIGHTS AND OTHER DELUSIONS.
#	* Added AT&T 23xx & 500/513, vt220 and vt420, opus3n1+, netronics
#	  smartvid & smarterm, ampex 175 & 219 & 232,
#	  env230, falco ts100, fluke, intertube, superbrain, ncr7901, vic20,
#	  ozzie, trs200, tr600, Tandy & Texas Instruments VDTs, intext2,
#	  screwpoint, fviewpoint, Contel Business Systems, Datamedia Colorscan,
#	  adm36, mime314, ergo4000, ca22851.  Replaced att7300, esprit, dd5500.
#	* Replaced the Perkin-Elmer entries with vendor's official ones.
#	* Restored the old minimal-ansi entry, luna needs it.
#	* Fixed some incorrect ip and proportional-padding translations.
# 9.4.1 (Mon Feb 27 14:18:33 EST 1995):
#	* Fix linux & AT386 sgr strings to do A_ALTCHARSET turnoff correctly.
#	* Make the xterm entry 65 lines again; create xterm25 and xterm24
#	  to force a particular height.
#	* Added beehive4 and reorganized other Harris entries.
# 9.4.2 (Thu Mar  9 01:45:44 EST 1995):
#	* Merged in DEC's official entries for its terminals.  The only old
#	  entry I kept was Doug Gwyn's alternate vt100 (as vt100-avo).
#	* Replaced the translated BBN Bitgraph entries with purpose-built
#	  ones from AT&T's SVr3.
#	* Replaced the AT&T entries with AT&T's official terminfos.
#	* Added teleray 16, vc415, cops10. 
#	* Merged in many individual capabilities from SCO terminfo files.
# 9.4.3 (Mon Mar 13 02:37:53 EST 1995):
#	* Typo fixes.
#	* Change linux entry so A_PROTECT enables IBM-PC ROM characters.
# 9.4.4 (Mon Mar 27 12:32:35 EST 1995):
#	* Added tty35, Ann Arbor Guru series. vi300 and 550, cg7900, tvi803,
#	  pt210, ibm3164, IBM System 1, ctrm, Tymshare scanset, dt200, adm21,
#	  simterm, citoh and variants.
#	* Replaced sol entry with sol1 and sol2.
#	* Replaced Qume QVT and Freedom-series entries with purpose-built
#	  terminfo entries.
#	* Enhanced vt220, tvi910, tvi924, hpterm, hp2645, adm42, tek
#	  and dg200 entries using caps from from SCO.
#	* Added the usual set of function-key mappings to ANSI entry.
#	* Corrected xterm's function-key capabilities.
# 9.4.5 (Tue Mar 28 14:27:49 EST 1995):
#	* Fix in xterm entry, cub and cud are not reliable under X11R6.
# 9.4.6 (Thu Mar 30 14:52:15 EST 1995):
#	* Fix in xterm entry, get the arrow keys right.
#	* Change some \0 escapes to \200.
# 9.4.7 (Tue Apr  4 11:27:11 EDT 1995)
#	* Added apple (Videx card), adm1a, oadm31.
#	* Fixed malformed ampex csr.
#	* Fixed act4, cyb110; they had old-style prefix padding left in. 
#	* Changed mandatory to advisory padding in many entries.
#	* Replaced HP entries up to hpsub with purpose-built ones.
#	* Blank rmir/smir/rmdc/smdc capabilities removed.
#	* Small fixes merged in from SCO entries for lpr, fos, tvi910+, tvi924.
# 9.4.8 (Fri Apr  7 09:36:34 EDT 199):
#	* Replaced the Ann Arbor entries with SCO's, the init strings are
#	  more efficient (but the entries otherwise identical).
#	* Added dg211 from Shuford archive.
#	* Added synertek, apple-soroc, ibmpc, pc-venix, pc-coherent, xtalk,
#	  adm42-nl, pc52, gs6300, xerox820, uts30.
#	* Pull SCO's padding into vi200 entry.
#	* Improved capabilities for tvi4107 and other Televideo and Viewpoint
#	  entries merged in from SCO's descriptions.
#	* Fixed old-style prefix padding on zen50, h1500.
#	* Moved old superbee entry to superbee-xsb, pulled in new superbee
#	  entry from SCO's description.
#	* Reorganized the special entries.
#	* Added lm#0 to cbunix and virtual entries.
#
# 9.5.0 (Mon Apr 10 11:30:00 EDT 1995):
#	* Restored cdc456tst.
#	* Fixed sb1 entry, SCO erroneously left out the xsb glitch.
#	* Added megatek, beacon, microkit.
#	* Freeze for ncurses-1.9 release.
#
# 9.5.1 (Fri Apr 21 12:46:42 EDT 1995):
#	* Added historical data for TAB.
#	* Comment fixes from David MacKenzie.
#	* Added the new BSDI pc3 entry.
#
# 9.5.2 (Tue Apr 25 17:27:52 EDT 1995)
#	* A change in the tic -C logic now ensures that all entries in 
#	  the termcap translation will fit in < 1024 bytes.
#	* Added `bobcat' and `gator' HP consoles and the Nu machine entries
#	  from GNU termcap file.  This merges in all their local information.
#
# 9.5.3 (Tue Apr 25 22:28:13 EDT 1995)
#	* Changed tic -C logic to dump all capabilities used by GNU termcap.
#	* Added warnings about entries with long translations (restoring
#	  all the GNU termcaps pushes a few over the edge).
#
# 9.5.4 (Wed Apr 26 15:35:09 EDT 1995)
#	* Yet another tic change, and a couple of entry tweaks, to reduce the
#	  number of long (> 1024) termcap translations back to 0.
#
# 9.6.0 (Mon May  1 10:35:54 EDT 1995)
#	* Added kf13-kf20 to Linux entry.
#	* Regularize Prime terminal names.
#	* Historical data on Synertek.
#	* Freeze for ncurses-1.9.1.
#
# 9.6.1 (Sat May  6 02:00:52 EDT 1995):
#	* Added true xterm-color entry, renamed djm's pseudo-color entry.
#	* Eliminate whitespace in short name fields, this tanks some scripts.
#	* Name field changes to shorten some long entries.
#	* Termcap translation now automatically generates empty rmir/smir
#	  when ich1/ich is present (copes with an ancient vi bug).
#	* Added `screen' entries from FSF's screen-3.6.2.
#	* Added linux-nic and xterm-nic entries.
#
# 9.6.2 (Sat May  6 17:00:55 EDT 1995):
#	* Change linux entry to use smacs=\E[11m and have an explicit acsc,
#	  eliminating some special-case code in ncurses.
#
# 9.7.0 (Tue May  9 18:03:12 EDT 1995):
#	* Added vt320-k3, rsvidtx from the Emacs termcap.dat file.  I think
#	  that captures everything unique from it.
#	* Added reorder script generator.
#	* Freeze for ncurses 1.9.2 release.
#
# 9.7.1 (Thu Jun 29 09:35:22 EDT 1995):
#	* Added Sean Farley's kspd, flash, rs1 capabilities for linux.
#	* Added Olaf Siebert's corrections for adm12.
#	* ansi-pc-color now includes the colors and pairs caps, so that
#	  entries which use it will inherit them automatically.
#	* The linux entry can now recognize the center (keypad 5) key.
#	* Removed some junk that found its way into Linux acsc.
#
# 9.8.0 (Fri Jul  7 04:46:57 EDT 1995):
#	* Add 50% cut mark as a desperate hack to reduce tic's core usage.
#	* xterm doesn't try to use application keypad mode any more.
#	* Freeze for ncurses-1.9.3 release.
#
# 9.8.1 (Thu Jul 19 17:02:12 EDT 1995):
#	* Added corrected sun entry from vendor.
#	* Added csr capability to linux entry.
#	* Peter Wemm says the at386 hpa should be \E[%i%p1%dG, not \E[%p1%dG.
#	* Added vt102-nsgr to cope with stupid IBM PC `VT100' emulators.
#	* Some commented-out caps in long entries come back in, my code 
#	  for computing string-table lengths had a bug in it.
#	* pcansi series modified to fit comm-program reality better.
#
######## REORDER
#
# Older termcap distributions featured a kluge called `reorder' intended to
# time-optimize access to selected terminals by moving them to the front of
# the file.  This is obsolete under terminfo, but for completeness's sake
# we give a reorder script generator here (strip off the leading #s to use).
#
#: mkreorder --  generate script to optimize access to given terminal types
#:
#: entries named on command line will be sorted to the front in reverse order
#echo "ed -- termcap <<EOF"
#for x in $*
#do
#	echo "/^$x[|:]/;.,/^[a-z#]/-1m0"
#done
#echo "0a"
#echo "."
#echo "w termcap.sorted"
#echo "q"
#echo "EOF"
#:end of script
#
# Invoke this script like this:
#
#	mkreorder h19 wy60 vt100 >reorder
#
# The following sets edit modes for GNU EMACS
# Local Variables:
# fill-prefix:"\t"
# fill-column:75
# End:
######## SHANTIH!  SHANTIH!  SHANTIH!
