Q:	My machine won't swap to my swapdisk (SCSI address 6).  However, I think this used to work.

A:	You may have a removable media device at a lower SCSI address than your swap disk.  Devices with no media in them cannot return a disk label, causing checkswap to return FSR_NONE.   The file /etc/rc.swap has a line

        case $swapstatus in
	            0)
                # No such disk was actually connected.
                break;
                ;;

This can be fixed by removing the line with break in it. You end up with:

        case $swapstatus in
	            0)
                # No such disk was actually connected.
                ;;

The downside is that the script always scans for all SCSI devices looking for a swap device.

QA861

Valid for 2.0, 3.0