#!/bin/sh
#
# This is an example script for using netperf. Feel free to modify it 
# as necessary, but I would suggest that you copy this one first.
#
# 
# This version has been modified to take advantage of the confidence
# interval support in revision 2.0 of netperf. it has also been altered
# to make submitting its resutls to the netperf database easier
# raj 11/94
#
# usage: tcp_rr_script hostname [CPU]
#

if [ $# -gt 2 ]; then
  echo "try again, correctly -> tcp_rr_script hostname [CPU]"
  exit 1
fi

if [ $# -eq 0 ]; then
  echo "try again, correctly -> tcp_rr_script hostname [CPU]"
  exit 1
fi

# where the programs are
NETHOME=/etc/netperf
#NETHOME="/opt/netperf"
#NETHOME=.

# at what port will netserver be waiting? If you decide to run
# netserver at a differnet port than the default of 12865, then set
# the value of PORT apropriately
#PORT="-p some_other_portnum"
PORT=""

# The test length in seconds
TEST_TIME=60

# How accurate we want the estimate of performance: 
#      maximum and minimum test iterations (-i)
#      confidence level (99 or 95) and interval (percent)
STATS_STUFF="-i 10,3 -I 99,5"

# The socket sizes that we will be testing - using zero will let it 
# be the system default.
SOCKET_SIZES="0"

# The request,response sizes that we will be using. The netperf
# command parser will treat "1" the same as "1,1" - I use 1,1 to
# remember that it is "request,response"
RR_SIZES="1,1 64,64 100,200 128,8192"

# if there are two parms, parm one it the hostname and parm two will
# be a CPU indicator. actually, anything as a second parm will cause
# the CPU to be measured, but we will "advertise" it should be "CPU"

if [ $# -eq 2 ]; then
  REM_HOST=$1
  LOC_CPU="-c"
  REM_CPU="-C"
fi

if [ $# -eq 1 ]; then
  REM_HOST=$1
fi

# If we are measuring CPU utilization, then we can save beaucoup
# time by saving the results of the CPU calibration and passing
# them in during the real tests. So, we execute the new CPU "tests"
# of netperf and put the values into shell vars.
case $LOC_CPU in
\-c) LOC_RATE=`$NETHOME/netperf $PORT -t LOC_CPU`;;
*) LOC_RATE=""
esac

case $REM_CPU in
\-C) REM_RATE=`$NETHOME/netperf $PORT -t REM_CPU -H $REM_HOST`;;
*) REM_RATE=""
esac

# This disables header display
NO_HDR="-P 0"

for SOCKET_SIZE in $SOCKET_SIZES
 do
  for RR_SIZE in $RR_SIZES
   do
   echo
   echo ------------------------------------------------------
   echo Testing with the following command line:
   # we echo the command line for cut and paste to th database
   echo $NETHOME/netperf $PORT -l $TEST_TIME -H $REM_HOST -t TCP_RR \
        $LOC_CPU $LOC_RATE $REM_CPU $REM_RATE $STATS_STUFF --\
        -r $RR_SIZE -s $SOCKET_SIZE -S $SOCKET_SIZE
   echo
   # since we have the confidence interval stuff, we do not
   # need to repeat a test multiple times from the shell
   $NETHOME/netperf $PORT -l $TEST_TIME -H $REM_HOST -t TCP_RR \
   $LOC_CPU $LOC_RATE $REM_CPU $REM_RATE $STATS_STUFF --\
   -r $RR_SIZE -s $SOCKET_SIZE -S $SOCKET_SIZE
 done
done
echo
echo If you wish to submit these results to the netperf database at
echo http://www.cup.hp.com/netperf/NetperfPage.html, please submit each
echo datapoint individually. Individual datapoints are separated by
echo lines of dashes. 
