# PCMCIA Default Driver Bindings File 
# /boot/home/config/settings/kernel/drivers/pcmcia.default
#
# PLEASE DO NOT MODIFY THIS FILE -- Place any custom entries in the file:
# /boot/home/config/settings/kernel/drivers/pcmcia
#
# Each "card" entry must contain a "bind" directive to indicate which driver
# to bind the specified card to (note that the driver must already have
# pcmcia support -- just naming a driver here doesn't magically make pcmcia
# work with it).  The "card" entry must also have either a "manfid" specifier
# or a "version" specifier -- the command "cardctl ident" will show the
# manfid and version (called "product info") of any cards present in a 
# pcmcia socket

# Some pcmcia controllers have problems with some interrupts (one laptop
# we tested just would not work with irq 9, but 10 and 11 were fine).
# You can use a line like the following to avoid problem irqs:
#
# disable_irq 9

card { # Linksys NetworkEverywhere 10-base-T Card
	manfid 0x0149 0xc1ab
	bind ne2k
}

card { # D-Link DE-660 Ethernet Card
	version "D-Link" "DE-660"
	bind ne2k
}

card { # Linksys EtherCard - discontinued
	version "LINKSYS" "E-CARD" "Ver 02.00"
	bind ne2k
}

card { # Linksys EtherCard
	version "Linksys" "Combo PCMCIA EthernetCard (EC2T)" "2.0"
	bind ne2k
}

card { # Kingston EtherRX
	version "Kingston" "KNE-PC2"
	bind ne2k
}

card { # ATA CDROM Adapter (some VAIOs have these)
	version " " "NinjaATA-" "V1.0"
	bind ide_cs
}

card { # SanDisk CompactFlash Adapter
	manfid 0x0045 0x0401
	bind ide_cs
}

card { # Advantech CompactFlash
	version "CF" "32M" ""
	manfid 0x000a 0x0000
	bind ide_cs
}

card { # FIC CompactFlash
	manfid 0x026a 0x0000
	bind ide_cs
}

card { # Hitachi CompaqFlash
	manfid 0x0007 0x0000
	bind ide_cs
}

card { # Cirrus Logic 14.4L Fax Modem
	version "CIRRUS LOGIC" "FAX MODEM"
	bind zz
}

card { # TDK Data-Fax Modem
	verion "TDK" "DF5600 Data-Fax Modem" "TDK Systems"
	bind zz
}

card { # Gold Card FaxModem
	version "Psion Dacom" "Gold Card Global 56K+Fax" "56K+Fax"
	bind zz
}

card { # Com1 Platinum card 
	version "COM1 SA" "MC220 CARD" 
	bind zz 
}

card { # Cirrus Logic 56K Modem 
	version "CIRRUS LOGIC 56K MODEM" "CL-MD56XX" 
	bind zz 
}

card { # SohoWare
   version "Socket Communications, Inc.", "Ethernet EA Lan Adapter",
   bind ne2k
}

card { # Farallon clone of 3Com 3c589
   version "Farallon" "ENet"
   bind tcm589
}

card { # 3Com 3c589
   manfid 0x0101 0x0589
   bind tcm589
}
card { #Lucent Wavelan
   version  "Lucent Technologies" "WaveLAN/IEEE"
   bind wavelan
}
