*PPD-Adobe: "4.3"
*% Adobe Systems PostScript(R) Printer Description File
*% Copyright 1987-1995 Adobe Systems Incorporated. 
*% All Rights Reserved. 
*% Permission is granted for redistribution of this file as
*% long as this copyright notice is intact and the contents
*% of the file is not altered in any way from its original form.
*% End of Copyright statement

*% Copyright (c) Tektronix, Incorporated.  All rights reserved.
*% Tektronix (R) is a registered trademark of Tektronix, Inc.
*% TekColor TM is a trademark of Tektronix, Inc.
*% Phaser (R) is a registered trademark of Tektronix, Inc., for color
*%  printers and related products.

*FormatVersion: "4.3"
*FileVersion: "1.2"
*LanguageEncoding: ISOLatin1
*LanguageVersion: English
*Product: "(Phaser 560)"
*PSVersion: "(2015.105) 14"
*Manufacturer: "Tektronix"
*ModelName: "Tektronix Phaser 560 Extended"
*ShortNickName: "Tektronix Phaser 560 Extended"
*NickName: "Tektronix Phaser 560 with Extended Features"
*PCFileName: "TKP560P1.PPD"

*% === Installable Options ===========
*OpenGroup: InstallableOptions/Options Installed

*OpenUI *InstalledMemory/Memory Configuration: PickOne
*OrderDependency: 69.0 AnySetup *InstalledMemory
*DefaultInstalledMemory: None
*InstalledMemory None/Standard 40 MB RAM: ""
*InstalledMemory 56Meg/56 MB Total RAM: ""
*InstalledMemory 72Meg/72 MB Total RAM: ""
*?InstalledMemory: "% InstalledMemory 
 currentsystemparams /RamSize get
 16#100000 div round cvi
 dup 42 lt
 { pop (None) } {2 string cvs print (Meg) } ifelse
 print (\n) print flush"
*End
*CloseUI: *InstalledMemory

*OpenUI *Option3/Optional Lower Trays: Boolean
*OrderDependency: 69.2 AnySetup *Option3
*DefaultOption3: False
*Option3 True/Installed: ""
*Option3 False/Not Installed: ""
*?Option3: "
currentpagedevice /InputAttributes get 1 known
{ (True) } { (False) } ifelse = flush"
*End
*CloseUI: *Option3

*OpenUI *Option1/Optional Hard Drive: Boolean
*OrderDependency: 69.4 AnySetup *Option1
*DefaultOption1: False
*Option1 True/Installed: ""
*Option1 False/Not Installed: ""
*?Option1: "
 false
 (%disk?%)
 { currentdevparams dup /Writeable known
   { /Writeable get {pop true} if }  {pop} ifelse
 } 10 string /IODevice resourceforall
 {(True)}{(False)} ifelse = flush"
*End
*CloseUI: *Option1

*OpenUI *Option2/Optional Network Card: PickOne
*OrderDependency: 69.6 AnySetup *Option2
*DefaultOption2: None
*Option2 None/Not Installed: ""
*Option2 P1/EtherTalk, NetWare and TCP/IP: ""
*Option2 P3/LocalTalk and Serial: ""
*Option2 P4/TokenTalk, NetWare and TCP/IP: ""
*?Option2: "% Option2
 (%EthernetPhysical%) /IODevice resourcestatus
 {pop pop (P1) }
 {
   (%LocalTalk%) /IODevice resourcestatus
   {pop pop (P3) }
   {
     (%TokenRingPhysical%) /IODevice resourcestatus
     {pop pop (P4) } { (None) } ifelse
   } ifelse
 } ifelse = flush"
*End
*CloseUI: *Option2

*CloseGroup: InstallableOptions

*% === Constraints ===================

*UIConstraints: *Option3 False *InputSlot Middle
*UIConstraints: *Option3 False *InputSlot Lower

*UIConstraints: *InputSlot Middle *Option3 False
*UIConstraints: *InputSlot Lower *Option3 False

*% === Basic Device Capabilities ============

*LanguageLevel: "2"
*Protocols: BCP

*FreeVM: "5700000"
*VMOption None/40 MB Standard RAM: "5700000"
*VMOption 56Meg/56 MB Total RAM: "17700000"
*VMOption 72Meg/72 MB Total RAM: "4200000"

*ColorDevice: True
*DefaultColorSpace: CMYK
*AccurateScreensSupport: True
*SuggestedJobTimeout: "0"
*SuggestedWaitTimeout: "300"
*SuggestedManualFeedTimeout: "60"
*1284Modes Parallel: Compat Nibble
*1284DeviceID: "
  MANUFACTURER:Tektronix;COMMAND SET:Adobe Level 2 PostScript;
  MODEL:Phaser 560;CLASS:Printer;DESCRIPTION:
  Phaser 560 Color Laser Printer, PostScript Level 2, Letter/Legal/A4 Size;
  COMPATIBLE_ID:"
*End
*TTRasterizer: Type42
*?TTRasterizer: "
  42 /FontType resourcestatus
  { pop pop (Type42)} {pop pop (None)} ifelse = flush"
*End

*FileSystem: True
*?FileSystem: "
  false
  (%disk?%)
  { currentdevparams dup /Writeable known
    { /Writeable get {pop true} if }  {pop} ifelse
  } 10 string /IODevice resourceforall
  {(True)}{(False)} ifelse = flush"
*End
*Throughput: "14"
*Password: "0"
*ExitServer: "
  count 0 eq
  { false } { true exch startjob } ifelse
  not
  { (WARNING: Cannot modify initial VM.) =
    (Missing or invalid password.) =
    (Please contact the author of this software.) = flush quit
  } if"
*End
*Reset: "
  count 0 eq
  { false } { true exch startjob } ifelse
  not
  { (WARNING: Cannot reset printer.) =
    (Missing or invalid password.) =
    (Please contact the author of this software.) = flush quit
  } if
  systemdict /quit get exec
  (WARNING : Printer Reset Failed.) = flush"
*End

*DefaultResolution: 600dpi
*SetResolution 600dpi : ""
*SetResolution 1200dpi : ""
*?Resolution: "
  currentpagedevice /HWResolution get 0 get (    ) cvs print (dpi) = flush"
*End

*% Halftone Information =================
*DefaultHalftoneType: 9
*ScreenFreq: "60.0"
*ScreenAngle: "45.0"
*DefaultScreenProc: Dot
*ScreenProc Dot: "{180 mul cos exch 180 mul cos add 2 div} bind"
*DefaultTransfer: Null
*Transfer Null: "{ }"
*Transfer Null.Inverse: "{1 exch sub} bind"


*% Tray Selection ============

*OpenUI *TKMPFMedia/MP Manual Feed Media: PickOne
*OrderDependency: 45.0 AnySetup *TKMPFMedia
*DefaultTKMPFMedia: Paper
*TKMPFMedia Paper: "userdict /MFMedia (Paper) put"
*TKMPFMedia Duplex/Paper 2nd Side: "userdict /MFMedia (Duplex) put"
*TKMPFMedia Transparency: "userdict /MFMedia (Transparency) put"
*TKMPFMedia CoatedPaper/Coated Paper: "userdict /MFMedia (CoatedPaper) put"
*TKMPFMedia CardStock/Card or Envelope: "userdict /MFMedia (CardStock) put"
*TKMPFMedia Label: "userdict /MFMedia (Label) put"
*TKMPFMedia FabricTransfer/Fabric Transfer: "
 userdict /MFMedia (FabricTransfer) put"
*End 
*?TKMPFMedia: "
  /MFMedia where {/MFMedia get}{(Unknown)} ifelse
  = flush"
*End
*CloseUI: *TKMPFMedia

*OpenUI *InputSlot: PickOne
*OrderDependency: 46.0 AnySetup *InputSlot
*DefaultInputSlot: Paper
*InputSlot Paper: "
  <<
    /MediaPosition null
    /MediaType (Paper)
    /TraySwitch true
    /ManualFeed false
  >> setpagedevice"
*End
*InputSlot Transparency: "
  <<
    /MediaPosition null
    /MediaType (Transparency)
    /TraySwitch true
    /ManualFeed false
  >> setpagedevice"
*End
*InputSlot Upper: "
  <<
    /MediaPosition 0
    /MediaType null
    /TraySwitch false
    /ManualFeed false
  >> setpagedevice"
*End
*InputSlot Middle: "
  <<
    /MediaPosition 1
    /MediaType null
    /TraySwitch false
    /ManualFeed false
  >> setpagedevice"
*End
*InputSlot Lower: "
  <<
    /MediaPosition 2
    /MediaType null
    /TraySwitch false
    /ManualFeed false
  >> setpagedevice"
*End
*InputSlot MPTray/Multi-Purpose Tray: "
  <<
    /MediaPosition 3
    /MediaType null
    /TraySwitch false
    /ManualFeed false
  >> setpagedevice"
*End
*InputSlot MPMF/Multi-Purpose Manual Feed: "
    <<
      /MediaPosition null
      /MediaType /MFMedia where {/MFMedia get }{(Paper)}ifelse
      /TraySwitch false
      /ManualFeed true
    >> setpagedevice"
*End
*?InputSlot: "
currentpagedevice begin ManualFeed 
{(MPMF)} 
{MediaPosition null eq {MediaType}
 {[(Upper) (Middle) (Lower) (MPTray)] MediaPosition get}ifelse
}ifelse end
= flush"
*End
*CloseUI: *InputSlot


*% Paper Handling ===================

*% Use these entries to set paper size most of the time, unless there is
*% specific reason to use PageRegion.
*OpenUI *PageSize: PickOne
*OrderDependency: 56.0 AnySetup *PageSize
*DefaultPageSize: Letter
*PageSize Letter: "<< /PageSize [612 792] /ImagingBBox null >> setpagedevice"
*PageSize Legal: "<< /PageSize [612 1008] /ImagingBBox null >> setpagedevice"
*PageSize A4: "<< /PageSize [595 842] /ImagingBBox null >> setpagedevice"
*?PageSize: "
  currentpagedevice /PageSize get aload pop 
  2 copy gt {exch} if (Unknown)
  <<
  [612 792] (Letter)
  [612 1008] (Legal)
  [595 842] (A4) >>
  { exch aload pop 4 index sub abs 5 le exch 5 index sub abs 5 le and 
      { exch pop exit } { pop } ifelse
  } bind forall = flush pop pop"
*End
*CloseUI: *PageSize

*% These entries will set up the frame buffer. Usually used with manual feed.
*OpenUI *PageRegion: PickOne
*OrderDependency: 56.0 AnySetup *PageRegion
*DefaultPageRegion: Letter
*PageRegion Letter: "<< /PageSize [612 792] /ImagingBBox null >> setpagedevice"
*PageRegion Legal: "<< /PageSize [612 1008] /ImagingBBox null >> setpagedevice"
*PageRegion A4: "<< /PageSize [595 842] /ImagingBBox null >> setpagedevice"
*CloseUI: *PageRegion

*% The following entries provide information about specific paper keywords.
*DefaultImageableArea: Letter
*ImageableArea Letter: "10.32 15.91 601.68 776.22"
*ImageableArea Legal: "10.32 16.39 601.68 991.74"
*ImageableArea A4: "13.45 14.47 581.76 828.54"
*?ImageableArea: "
  currentpagedevice pop
  clippath pathbbox
  /cvp {16 string cvs print ( ) print} def
  4 3 roll 100 mul ceiling 100 div cvp
  3 2 roll 100 mul ceiling 100 div cvp
  exch 100 mul floor 100 div cvp
  100 mul floor 100 div = flush
  userdict /cvp undef"
*End

*% These provide the physical dimensions of the paper (by keyword)
*DefaultPaperDimension: Letter
*PaperDimension Letter: "612 792"
*PaperDimension Legal: "612 1008"
*PaperDimension A4: "595 842"

*RequiresPageRegion All: True


*% TKColor Selections  ===================

*OpenUI *TKColor/Color Correction: PickOne
*OrderDependency: 40.0 AnySetup *TKColor
*DefaultTKColor: Automatic
*TKColor Automatic: "
  <<
    /DeviceRenderingInfo <<
      /Type 2
      /VirtualColorDevice <<
        /Type 3
        /ColorTransform /Automatic
      >>
    >>
  >> setpagedevice"
*End
*TKColor NoAdjust/None: "
  <<
    /DeviceRenderingInfo <<
      /Type 2
      /VirtualColorDevice null
    >>
  >> setpagedevice"
*End
*TKColor VividColor/Vivid Color: "
  <<
    /DeviceRenderingInfo <<
      /Type 2
      /VirtualColorDevice <<
        /Type 3
        /ColorTransform /TekBlue
      >>
    >>
  >> setpagedevice"
*End
*TKColor SimulateDisplay/Simulate Display: "
  <<
    /DeviceRenderingInfo <<
      /Type 2
      /VirtualColorDevice <<
        /Type 3
        /ColorTransform /TekDisplay
      >>
    >>
  >> setpagedevice"
*End
*TKColor SWOPPress/SWOP Press: "
  <<
    /DeviceRenderingInfo <<
      /Type 2
      /VirtualColorDevice <<
        /Type 3
        /ColorTransform /SWOP-Coated
      >>
    >>
  >> setpagedevice"
*End
*TKColor EuroscalePress/Euroscale Press: "
  <<
    /DeviceRenderingInfo <<
      /Type 2
      /VirtualColorDevice <<
        /Type 3
        /ColorTransform /Euroscale-Coated
      >>
    >>
  >> setpagedevice"
*End
*TKColor CommercialPress/Commercial Press: "
  <<
    /DeviceRenderingInfo <<
      /Type 2
      /VirtualColorDevice <<
        /Type 3
        /ColorTransform /Commercial-Coated
      >>
    >>
  >> setpagedevice"
*End
*TKColor UsePrinterSetting/Use Printer Setting: ""
*?TKColor: "
  { currentpagedevice /DeviceRenderingInfo get
    /VirtualColorDevice get
    dup null eq
    { pop (NoAdjust) }
    { /ColorTransform get
      <<
        /Automatic         (Automatic)
        /TekBlue           (VividColor)
        /TekDisplay        (SimulateDisplay)
        /SWOP-Coated       (SWOPPress)
        /Euroscale-Coated  (EuroscalePress)
        /Commercial-Coated (CommercialPress)
      >>
      exch get
    } ifelse
  } stopped
  { % error in PostScript code execution
    pop pop (Unknown)
  } if
  = flush"
*End
*CloseUI: *TKColor

*% Print Quality Selection  ===================

*OpenUI *OutputMode/Print Quality: PickOne
*OrderDependency: 47.0 AnySetup *OutputMode
*DefaultOutputMode: Standard
*OutputMode FastMono/Fast Monochrome  600x600 dpi: "
  <<
    /HWResolution [600 600]
    /ProcessColorModel /DeviceGray
  >> setpagedevice"
*End
*OutputMode FastColor/Fast Color  600x600 dpi: "
  <<
    /HWResolution [600 600]
    /ProcessColorModel /DeviceCMY
  >> setpagedevice"
*End
*OutputMode Presentation/Presentation  600x600 dpi: "
  <<
    /HWResolution [600 600]
    /ProcessColorModel /DeviceCMYK
    /PostRenderingEnhance true
    /PostRenderingEnhanceDetails <<
       /OutputMode (Presentation)
    >>
  >> setpagedevice"
*End
*OutputMode Standard/Standard  600x600 dpi: "
  <<
    /HWResolution [600 600]
    /ProcessColorModel /DeviceCMYK
    /PostRenderingEnhance true
    /PostRenderingEnhanceDetails <<
      /OutputMode (Standard)
    >>
  >> setpagedevice"
*End
*OutputMode Premium/Premium  1200x1200 dpi: "
  <<
    /HWResolution [1200 1200]
    /ProcessColorModel /DeviceCMYK
    /PostRenderingEnhance true
    /PostRenderingEnhanceDetails <<
      /OutputMode (Standard)
    >>
  >> setpagedevice"
*End
*?OutputMode: "
  currentpagedevice /ProcessColorModel get dup /DeviceGray eq 
  {
    pop (FastMono) 
  }
  {
    /DeviceCMY eq 
    {
      (FastColor)
    }
    {
      currentpagedevice /HWResolution get 0 get 1200 eq 
      {
        (Premium)
      }
      {
        currentpagedevice /PostRenderingEnhanceDetails get /OutputMode get
      } ifelse
    } ifelse
  } ifelse
  = flush"
*End
*CloseUI: *OutputMode

*OpenUI *TKImageSmoothing/Image Smoothing: Boolean
*OrderDependency: 52.0 AnySetup *TKImageSmoothing
*DefaultTKImageSmoothing: False
*TKImageSmoothing False/Off: "
  false /RRCustomProcs /ProcSet findresource /setforceinterpolate get exec"
*End
*TKImageSmoothing True/On: "
  true /RRCustomProcs /ProcSet findresource /setforceinterpolate get exec"
*End
*?TKImageSmoothing: "
  /RRCustomProcs /ProcSet findresource /currentforceinterpolate get exec
  {(True)}{(False)} ifelse
  = flush"
*End
*CloseUI: *TKImageSmoothing

*OpenUI *OutputOrder/Output Order: PickOne
*OrderDependency: 44.0 AnySetup *OutputOrder
*DefaultOutputOrder: Reverse
*OutputOrder Normal/Face Down: "  << /OutputFaceUp false >> setpagedevice"
*OutputOrder Reverse/Face Up: "  << /OutputFaceUp true >> setpagedevice"
*?OutputOrder: "
  currentpagedevice /OutputFaceUp get
  { (Reverse) }
  { (Normal)  } ifelse
  = flush"
*End
*CloseUI: *OutputOrder

*OpenUI *TKCollate/Quick Collate: Boolean
*OrderDependency: 50.0 AnySetup *TKCollate
*DefaultTKCollate: False
*TKCollate False/Off: "<< /Collate false >> setpagedevice"
*TKCollate True/On: "<< /Collate true >> setpagedevice"
*?TKCollate: "
  save
  currentpagedevice /Collate get {(True)}{(False)}ifelse
  = flush restore"
*End
*CloseUI: *TKCollate

*OpenUI *TKCheckPrint/Check Print: Boolean
*OrderDependency: 55.0 AnySetup *TKCheckPrint
*DefaultTKCheckPrint: False
*TKCheckPrint False/Off: ""
*TKCheckPrint True/On: "
  /RRCustomProcs /ProcSet findresource /setcheckprint get exec"
*End
*?TKCheckPrint: "
  /RRCustomProcs /ProcSet findresource
  /currentcheckprint get exec {(True)}{(False)}ifelse
  = flush"
*End
*CloseUI: *TKCheckPrint

*% Font Information =====================
*DefaultFont: Courier
*Font AvantGarde-Book: Standard "(001.006S)" Standard ROM
*Font AvantGarde-BookOblique: Standard "(001.006S)" Standard ROM
*Font AvantGarde-Demi: Standard "(001.007S)" Standard ROM
*Font AvantGarde-DemiOblique: Standard "(001.007S)" Standard ROM
*Font Bookman-Demi: Standard "(001.004S)" Standard ROM
*Font Bookman-DemiItalic: Standard "(001.004S)" Standard ROM
*Font Bookman-Light: Standard "(001.004S)" Standard ROM
*Font Bookman-LightItalic: Standard "(001.004S)" Standard ROM
*Font Courier: Standard "(002.004S)" Standard ROM
*Font Courier-Bold: Standard "(002.004S)" Standard ROM
*Font Courier-BoldOblique: Standard "(002.004S)" Standard ROM
*Font Courier-Oblique: Standard "(002.004S)" Standard ROM
*Font Helvetica: Standard "(001.006S)" Standard ROM
*Font Helvetica-Bold: Standard "(001.007S)" Standard ROM
*Font Helvetica-BoldOblique: Standard "(001.007S)" Standard ROM
*Font Helvetica-Condensed: Standard "(001.001)" Standard ROM
*Font Helvetica-Condensed-Bold: Standard "(001.002)" Standard ROM
*Font Helvetica-Condensed-BoldObl: Standard "(001.002)" Standard ROM
*Font Helvetica-Condensed-Oblique: Standard "(001.001)" Standard ROM
*Font Helvetica-Narrow: Standard "(001.006S)" Standard ROM
*Font Helvetica-Narrow-Bold: Standard "(001.007S)" Standard ROM
*Font Helvetica-Narrow-BoldOblique: Standard "(001.007S)" Standard ROM
*Font Helvetica-Narrow-Oblique: Standard "(001.006S)" Standard ROM
*Font Helvetica-Oblique: Standard "(001.006S)" Standard ROM
*Font NewCenturySchlbk-Bold: Standard "(001.009S)" Standard ROM
*Font NewCenturySchlbk-BoldItalic: Standard "(001.007S)" Standard ROM
*Font NewCenturySchlbk-Italic: Standard "(001.006S)" Standard ROM
*Font NewCenturySchlbk-Roman: Standard "(001.007S)" Standard ROM
*Font Palatino-Bold: Standard "(001.005S)" Standard ROM
*Font Palatino-BoldItalic: Standard "(001.005S)" Standard ROM
*Font Palatino-Italic: Standard "(001.005S)" Standard ROM
*Font Palatino-Roman: Standard "(001.005S)" Standard ROM
*Font Symbol: Special "(001.007S)" Special ROM
*Font Times-Bold: Standard "(001.007S)" Standard ROM
*Font Times-BoldItalic: Standard "(001.009S)" Standard ROM
*Font Times-Italic: Standard "(001.007S)" Standard ROM
*Font Times-Roman: Standard "(001.007S)" Standard ROM
*Font ZapfChancery-MediumItalic: Standard "(001.007S)" Standard ROM
*Font ZapfDingbats: Special "(001.004S)" Special ROM
*?FontQuery: "
  { count 1 gt
    { exch dup 127 string cvs (/) print print (:) print
     /Font resourcestatus {pop pop (Yes)} {(No)} ifelse = 
    } { exit } ifelse
  } bind loop
  (*) = flush"
*End

*?FontList: "(*) {cvn ==} 128 string /Font resourceforall (*) = flush"

*InkName: ProcessBlack/Process Black
*InkName: CustomColor/Custom Color
*InkName: ProcessCyan/Process Cyan
*InkName: ProcessMagenta/Process Magenta
*InkName: ProcessYellow/Process Yellow

*DefaultColorSep: ProcessBlack.60lpi.600dpi/60 lpi / 600 dpi

*%  For 60 lpi / 600 dpi ================================

*ColorSepScreenAngle ProcessBlack.60lpi.600dpi/60 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle CustomColor.60lpi.600dpi/60 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle ProcessCyan.60lpi.600dpi/60 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle ProcessMagenta.60lpi.600dpi/60 lpi / 600 dpi: "45.0"
*ColorSepScreenAngle ProcessYellow.60lpi.600dpi/60 lpi / 600 dpi: "45.0"

*ColorSepScreenFreq ProcessBlack.60lpi.600dpi/60 lpi / 600 dpi: "60.0"
*ColorSepScreenFreq CustomColor.60lpi.600dpi/60 lpi / 600 dpi: "60.0"
*ColorSepScreenFreq ProcessCyan.60lpi.600dpi/60 lpi / 600 dpi: "60.0"
*ColorSepScreenFreq ProcessMagenta.60lpi.600dpi/60 lpi / 600 dpi: "60.0"
*ColorSepScreenFreq ProcessYellow.60lpi.600dpi/60 lpi / 600 dpi: "60.0"

*% The byte count of this file should be exactly 018572 or 019207
*% depending on the filesystem it resides in.
*% end of PPD file for Tektronix Phaser 560 Extended
