# configuration manager settings
#
# This file should be moved to the directory
# /boot/home/config/settings/kernel/drivers/
#
# This file contains runtime configuration options for the configuration
# manager. If you want to enable any of these options, move this file to
# the proper directory and uncomment the appropriate line by removing the
# initial # sign.

# The following four options control the verbosity of the driver. This is only
# meaningful if you are trying to debug a configuration manager problem and
# will otherwise only serve to slow down your boot process.
# verbosity <1-9>
# isaverbosity <1-9>
# isabiosverbosity <1-9>
# isapnpverbosity <1-9>

# The following option allows the configuration manager to reconfigure any
# motherboard devices that you might have, e.g. serial ports, parallel ports,
# built-in sound cards.
# WARNING: This option works properly only on certain BIOSes.
# ENABLING THIS OPTION MAY RENDER YOUR SYSTEM UNBOOTABLE.
# bios_reconfig enabled

# The following option allows you to reserve irqs, marking them unavailable
# to ISA PnP devices during the initial configuration scan. This is
# typically used to keep irqs free for PCMCIA cards and is generally useless
# without the bios_reconfig option enabled. THIS OPTION IS CURRENTLY
# EXPERIMENTAL AND ITS USE MAY RENDER YOUR SYSTEM UNBOOTABLE.
# reserve_irq	<irq-list>	# example: reserve_irq 4 7

# Should the use of any of the experimental options cause your system to hang
# during boot, you may recover by booting into safe mode and removing the
# setting file.
